{"text_format":"1","workbook":"xlsx","n_sheets":29,"sheets":["README","Certification","Certification Table","LSE Showing","Resource Custom Profiles","Unoptimized Showing","Profile Optimization","Validation Overview","Check Capacity","Check Custom Profiles","Check Storage SOC","Check Grouped Resources","Check Hybrid Deliverability","Check Demand Response","LSE Showing Complete","Hourly Availability Chart","Hourly Availability","Local Availability Chart","Local Availability","Flex Availability Chart","Flex Availability","Requirements and Allocations","Resource Database","Resource Default Profiles","Regions","Expanded Default Profiles","Resource Profile Categories","VER Categories","Query Statuses"],"not_rendered":{"charts":6,"images":1,"macros":1,"external_links":0,"defined_names":125,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Hourly Availability Chart","index":15,"reason":"not_a_worksheet"},{"sheet":"Local Availability Chart","index":17,"reason":"not_a_worksheet"},{"sheet":"Flex Availability Chart","index":19,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"README","index":0,"n_rows":15,"n_cols":3,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Resource Adequacy Slice-of-Day Showing Template\n\nThis template processes data from tables in various worksheets, and uses queries to route identifying data throughout the workbook and setup lookup calculations in cell formulas. Validation test results are evaluated in several hidden worksheets and summarized in the \"Validation Overview\" worksheet with a golden tab. All queries can be accessed from the \"Data\" menu -> \"Queries & Connections\" -> \"Queries & Connections\" or by pressing [Alt]+[F12].\n\nA valid monthly showing consists of general resource allocations specified in the table on the A1\"LSE Showing\" worksheet along with custom slice-of-day profiles for any resources for which the default profile is not desired, and a certification of showing with information about the load-serving entity submitting the showing. The \"LSEShowing\" query merges the general showing, custom profiles, and default profiles to build the complete showing data table. Only the three worksheets corresponding to these tables, denoted with blue tabs, should be altered when preparing a monthly showing: \"Certification\", \"LSE Showing\", and \"Resource Custom Profiles\". A fourth worksheet labelled \"Profile Optimization\" provides a tool for automatically allocating operating hours for resources shown using default profiles from the Resource Database.\n\nAll showing data for each resource, including custom and optimized profiles along, is presented in the \"LSE Showing Complete\" worksheet. This sheet is for reference only and should not be edited directly.\n\nValidation tests are summarized on the Validation Overview worksheet. All tests should refresh automatically when accessing this worksheet. Tests may be inspected by clicking the associated \"Go To Sheet\" buttons. Other hidden worksheets may be unhidden by right-clicking on any tab and selecting \"Unhide Sheets\". Three chart sheets rely on supporting data in hidden sheets which can be accessed using similar buttons located at the top left corner of each chart.\n\nSee the User's Guide for more detailed information and instructions."]
[]
[null,"Information"]
[null,"Template Version:",30]
[null,"Resource Database Source:","2024 MRD 16may24.xlsx"]
[]
[null,"Tools"]
[]
[null,"Clear All Input Data:"]
[]
[null,"Clear Requirements and Allocations:"]
[]
[null,"Refresh Resource Database:"]
[]
[null,"Autofill LSE Showing Values:"]

{"sheet":"Certification","index":1,"n_rows":28,"n_cols":1,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,0,0,2],[9,0,9,1],[16,0,16,1],[22,0,22,1],[7,0,7,2]]}
["Monthly Showing Certification Form"]
["Load Serving Entity Full Name:"]
["Load Serving Entity Abbreviation:"]
["Showing Type:"]
["Showing Month:"]
["Date of Filing:"]
[]
["Consistent with Rules 1 and 2.4 of the CPUC's Rules of Practice and Procedure, this resource adequacy showing has been verified by an officer of the corporation, who shall expressly certify, under penalty of perjury, the following:\n1. I have responsibility for the activities reflected in this showing;\n2. I have reviewed, or have caused to be reviewed, this showing;\n3. Based on my knowledge, information, or belief, this filing does not contain any untrue statement of a material fact or omit to state a material fact necessary to make the statements made;\n4. Based on my knowledge, information, or belief, this filing contains all of the information required to be provided by CPUC orders, rules, and regulations."]
[]
["LSE Officer Information"]
["Title:"]
["Name:"]
["Email:"]
["Phone:"]
["Signature:"]
[]
["Backup Contact Information"]
["Title:"]
["Name:"]
["Email:"]
["Phone:"]
[]
["Load Serving Entity Information"]
["LSE Address Line 1:"]
["LSE Address Line 2:"]
["LSE City:"]
["LSE State:"]
["LSE Zip:"]

{"sheet":"Certification Table","index":2,"n_rows":22,"n_cols":2,"rows_kept":22,"cut":false,"hidden":true,"merged":[]}
["Key","Value"]
["Load Serving Entity Full Name",{"$f":"LSEFullName","v":0}]
["Load Serving Entity Abbreviation",{"$f":"LSEAbbreviation","v":0}]
["Showing Type",{"$f":"ShowingType","v":0}]
["Showing Month",{"$f":"ShowingMonth","v":"00:00:00"}]
["Date of Filing",{"$f":"FilingDate","v":"00:00:00"}]
["Contact 1 Title",{"$f":"LSETitle1","v":"00:00:00"}]
["Contact 1 Name",{"$f":"LSEName1","v":"00:00:00"}]
["Contact 1 Email",{"$f":"LSEEmail1","v":"00:00:00"}]
["Contact 1 Phone",{"$f":"LSEPhone1","v":0}]
["Contact 2 Title",{"$f":"LSETitle2","v":0}]
["Contact 2 Name",{"$f":"LSEName2","v":0}]
["Contact 2 Email",{"$f":"LSEEmail2","v":0}]
["Contact 2 Phone",{"$f":"LSEPhone2","v":0}]
["Address 1",{"$f":"LSEAddressStreet1","v":0}]
["Address 2",{"$f":"LSEAddressStreet2","v":0}]
["City",{"$f":"LSEAddressCity","v":0}]
["State",{"$f":"LSEAddressState","v":0}]
["Zip",{"$f":"LSEAddressZip","v":0}]
["Month Ahead Coefficient",1]
["Year Ahead Coefficient",0.9]
["Maximum DR Ratio",8.3000000000000004E-2]

{"sheet":"LSE Showing","index":3,"n_rows":4,"n_cols":12,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Contract ID","Resource ID","Resource SubID","NQC Under Contract (MW)","Local RA (MW)","Committed Flexible RA (MW)","Capacity Effective Start Date","Capacity Effective End Date","SCID or Counterparty if not available","MCC Bucket 4","Unspecified Import","Use Default Profile"]
["CAM Storage","CAM Storage Allocation Single Cycle",null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                *(RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=LSEShowing[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    0\n)","v":0},0,0,{"$f":"IFERROR(EOMONTH(ShowingMonth,-1)+1,DATEVALUE(\"1900-01-01\"))","v":"1900-01-01"},{"$f":"IFERROR(EOMONTH(ShowingMonth,0),DATEVALUE(\"1900-01-31\"))","v":"1900-01-31"},"Allocation",false,false,false]
["CAM Storage","CAM Storage Allocation Multi Cycle",null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                *(RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=LSEShowing[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    0\n)","v":0},0,0,"1900-01-01","1900-01-31","Allocation",false,false,false]
["CAM Peakers","CAM Peaker Allocation",null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                *(RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=LSEShowing[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    0\n)","v":0},0,0,"1900-01-01","1900-01-31","Allocation",false,false,true]

{"sheet":"Resource Custom Profiles","index":4,"n_rows":1,"n_cols":26,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Resource ID","Resource SubID","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]

{"sheet":"Unoptimized Showing","index":5,"n_rows":1,"n_cols":36,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Profile Source","Resource Type","Default Profile Category","Chart Label","Region","NQC Under Contract (MW)","Resource NQC","Resource Pmax","Deliverability","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]

{"sheet":"Profile Optimization","index":6,"n_rows":29,"n_cols":36,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,1,2],[28,18,73,22]]}
["Status:",null,null,null,null,null,"Optimized Showings",null,null,null,null,null,null,null,null,null,null,null,"Capacity Deficits",null,null,null,null,null,"Storage Properties"]
["Alternate Optimizer:\r\nComplete After 11 Iterations",null,null,null,null,null,"Resource ID","Resource SubID","Hour Ending","Shown Colocated Capacity (MW)","Capacity Available for Charging (MW)","Maximum Capacity (MW)","Charging Priority","Shown MW","Objective","State-of-Charge Day 1","State-of-Charge Day 2",null,"Hour Ending","Deficit (MW)","Maximum Capacity (MW)","Total Shown MW","Difference (MW)",null,"Resource ID","Resource SubID","Allows Grid Charging","Maximum Capacity (MW)","Maximum Available Capacity (MW)","Maximum Daily Storage Cycles","Storage Efficiency","Maximum Continuous Energy (MWh)","Maximum Possible Energy (MWh)","Shown Energy (MWh)","Difference Energy (MWh)","Minimum State-of-Charge"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,"Pre-Optimization Information:",null,null,null,null,null,null,null,null,null,null,null,"0.00",{"$f":"SUM(SODProfilesForSOC[Objective])","v":0},null,{"$f":"MIN(SODProfilesForSOC[[State-of-Charge Day 1]:[State-of-Charge Day 2]])","v":0},null,2,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,"Minimum:",{"$f":"SUBTOTAL(105,StorageProperties[Difference Energy (MWh)])","v":0},{"$f":"SUBTOTAL(105,StorageProperties[Minimum State-of-Charge])","v":0}]
[null,null,"Total Deficit:",{"$f":"SUM(SODCapacityDeficits[Deficit (MW)])","v":{"$error":"#N/A"}},"MWh",null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Maximum Possible Energy:",{"$f":"SUM(StorageProperties[Maximum Possible Energy (MWh)])","v":0},"MWh",null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Minimum (Maximum Capacity-Deficit):",{"$f":"MIN(SODCapacityDeficits[Maximum Capacity (MW)]-SODCapacityDeficits[Deficit (MW)])","v":{"$error":"#N/A"}},"MW",null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,"Optimization Run Information:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Iteration Number:",11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Objective:",{"$f":"SODProfilesForSOC[[#Totals],[Objective]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Minimum Objective:",15905.470389079597,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,"Optimization Settings:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Maximum Iterations:",24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Objective Threshold Coefficient:",1E-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"SOC Adjustment Coefficient:",1.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Energy Adjustment Coefficient:",0.95,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,"Efficiency Prioritization Coefficient:",0.85,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"MAX(\n    INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n    * (\n        1 + INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                0\n            )\n        ) / 100\n    )\n    * INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n            0\n        )\n    )\n    - SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                UnoptimizedShowing[],\n                UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n            ),\n            (\n                (UnoptimizedShowing[Deliverability]<>\"EO\")\n                    * (UnoptimizedShowing[Contract ID]<>\"DR Allocation\")\n                    * (UnoptimizedShowing[Chart Label]<>\"Demand Response\")\n            )=1,\n            0\n        )\n    )\n    - MIN(\n        SUM(\n            _xlfn._xlws.FILTER(\n                _xlfn._xlws.FILTER(\n                    UnoptimizedShowing[],\n                    UnoptimizedShowing[#Headers]=\"MW HE \" & SODCapacityDeficits[[#This Row],[Hour Ending]]\n                ),\n                ((UnoptimizedShowing[Contract ID]=\"DR Allocation\") + (UnoptimizedShowing[Chart Label]=\"Demand Response\"))>0,\n                0\n            )\n        ),\n        MaximumDRRatio\n        * INDEX(Certification[Value],MATCH(ShowingType & \" Coefficient\",Certification[Key],0))\n        * (\n            1 + INDEX(\n                RequirementsAndAllocations[Value],\n                MATCH(\n                    1,\n                    (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                        * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                        * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                        * (RequirementsAndAllocations[Name]=\"Planning Reserve Margin\"),\n                    0\n                )\n            ) / 100\n        )\n        * INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Load Forecast\")\n                    * (RequirementsAndAllocations[Option]=\"HE \"&SODCapacityDeficits[[#This Row],[Hour Ending]]),\n                0\n            )\n        )\n    ),\n    0\n)","v":{"$error":"#N/A"}},{"$f":"SUMIFS(\n    SODProfilesForSOC[Maximum Capacity (MW)],\n    SODProfilesForSOC[Hour Ending],\n    SODCapacityDeficits[[#This Row],[Hour Ending]]\n)","v":0},{"$f":"ROUND(\n    SUMIFS(\n        SODProfilesForSOC[Shown MW],\n        SODProfilesForSOC[Hour Ending],\n        SODCapacityDeficits[[#This Row],[Hour Ending]]\n    ),\n    6\n)","v":0},{"$f":"ROUND(\n    SODCapacityDeficits[[#This Row],[Total Shown MW]] - SODCapacityDeficits[[#This Row],[Deficit (MW)]],\n    4\n)","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Minimum:",{"$f":"MIN(SODCapacityDeficits[Difference (MW)])","v":{"$error":"#N/A"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"How to Optimize Storage Resources:\n1. Add one or more storage resources to the LSE Showing worksheet and set \"Default Profile\" to \"FALSE\".\n2. Do not create an entry in the Resource Custom Profiles worksheet for these resources.\n3. Click the \"Optimize Shown Hours\" button and wait for the three tables to finish updating (refresh status appears at the bottom of the Excel window), then for Solver to find a solution, if possible.\n6. Check that values in the \"Difference (MW)\" column of the \"Capacity Deficits\" table are all zero, indicating all capacity deficits are met.\n7. If the optimizer fails to run, check the \"Status\" cell above for information about why. You may need to adjust which storage and non-resources resources are shown on the LSE Showing worksheet, or adjust the initial conditions in the \"Fractional Showing\" column of the \"Optimization\" table.\n\nAbout the Optimizer:\nThis sheet uses a custom algorithm implemented in Excel VBA to minimize the objective cell at the bottom of the Objective Function column, subject to a variety of constraints. The VBA script sets and iteratively adjusts capacities in the \"Shown MW\" column of the \"Optimized Showings\" column.\n\nThe objective cell calculates the energy required to charge the showing across all resources, thereby accounting for shown capacities and resource efficiencies. The VBA script cycles through three steps: increasing the showing among higher-efficiency resources, reducing showings so that each resource does not fall below zero state-of-charge, and reallocating any differences between the \"Deficit (MW)\" and \"Total Shown (MW)\" columns of the Capacity Deficits table.\n\nThe State-of-Charge columns approximate the hourly states of charge across two consecutive days assuming 100% charge at midnight of day 1, charging at a rate equal to the capacity available for charging for the given hour multiplied by the storage efficiency for hours during which 0 capacity is shown, and subtracting shown capacity from the accumulated charge. This calculation ensures that multi-cycle storage has sufficient time to charge between discharge cycles, and implicitly applies a constraint for maximum continuous energy. Both single- and multi-cycle storage are additionally constrained by total daily MWh.\n\nNote:\nSolutions are not guaranteed to be the absolute optimum, and results should be checked using the \"Validation Overview\" worksheet as not all validation tests are incorporated into the optimization."]

{"sheet":"Validation Overview","index":7,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[[9,3,10,3],[9,4,10,4],[1,3,7,3],[1,4,7,4]]}
["Test","Result","Description","Worksheet","Review"]
["Hourly System Capacity",{"$f":"_xlfn.IFS(\n    INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n    \"Refreshing ...\",\n    MIN(CheckCapacity[[#Totals],[MW HE 1]:[MW HE 24]])>=0,\n    \"Pass\",\n    TRUE,\n    \"Fail\"\n)","v":"Pass"},"Checks whether the total MWh shown available across all 24 hours meet the hourly requirements.","Check Capacity"]
["Local Capacity",{"$f":"_xlfn.IFS(\n    INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n    \"Refreshing ...\",\n    MIN(CheckCapacity[[#Totals],[LA Basin (MW)]:[NBNC (MW)]])>=0,\n    \"Pass\",\n    TRUE,\n    \"Fail\"\n)","v":"Pass"},"Checks whether shown local capacity meets local requirements."]
["Flexible Capacity",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        SUM(CheckCapacity[[#Totals],[Flexible Category 1 (MW)]:[Flexible Category 2 (MW)]])\n        >=-INDEX(CheckCapacity[Flexible Category 2 (MW)],MATCH(\"Requirements\",CheckCapacity[Contract ID],0))\n        -INDEX(CheckCapacity[Flexible Category 3 (MW)],MATCH(\"Requirements\",CheckCapacity[Contract ID],0)),\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"N/A"},"Checks whether shown flexible capacity meets flex requirements."]
["Contract Date",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        CheckCapacity[[#Totals],[Check Dates]],\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"N/A"},"Checks that each shown resource is available for the current showing month according to the contract period."]
["Shown Hours",{"$f":"_xlfn.IFS(\n    INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n    \"Refreshing ...\",\n    IFERROR(\n        CheckCapacity[[#Totals],[Valid Hours]],\n        FALSE\n    ),\n    \"Pass\",\n    TRUE,\n    \"Fail\"\n)","v":"Fail"},"Passes if the shown hours of usage for each resource are within those allowed in the resource database."]
["Storage Excess Capacity",{"$f":"_xlfn.IFS(\n    INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n    \"Refreshing ...\",\n    CheckCapacity[[#Totals],[Grid Capacity (MWh)]]-CheckCapacity[[#Totals],[Grid Charging Requirement (MWh)]]>=0,\n    \"Pass\",\n    TRUE,\n    \"Fail\"\n)","v":"Pass"},"Checks that sufficient excess capacity above system requirements across all hours are shown to supply the total storage charging needs, accounting for efficiency losses."]
["MCC Bucket 4 Storage Excess Capacity",{"$f":"_xlfn.IFS(\n    INDEX(Queries[Status],MATCH(\"CheckCapacity\",Queries[Output Query Table],0))=\"STALE\",\n    \"Refreshing ...\",\n    CheckCapacity[[#Totals],[Grid Capacity (MWh)]]-CheckCapacity[[#Totals],[MCC Bucket 4 Charging Requirement (MWh)]]>=0,\n    \"Pass\",\n    TRUE,\n    \"Fail\"\n)","v":"Pass"},"Applies the Storage Excess Capacity test only to Storage Resources indicated with the MCC Bucket 4 flag"]
["Custom Profile",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckCustomProfiles\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        AND(CheckCustomProfiles[Check]),\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"N/A"},"Checks whether any custom slice-of-day profiles exceed their resource’s NQC or VER value.","Check Custom Profiles"]
["Storage Minimum State-of-Charge",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckStorageSOC\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        CheckStorageSOC[[#Totals],[Minimum SOC]]>=0,\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"Pass"},"Checks the state-of-charge for each hour across two consecutive days to ensure storage resources maintain greater than zero stored energy.","Check Storage SOC"]
["Storage Energy",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckStorageSOC\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        CheckStorageSOC[[#Totals],[Delta Daily Energy (MWh)]]>=0,\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"Pass"},"Checks that storage resources do not show more than their listed maximum daily energy capacities."]
["Grouped Resource Interconnection",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckGroupedResources\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        AND(\n            CheckGroupedResources[Difference (MW)]>=0\n        ),\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"Pass"},"Checks that groups of resources--either hybrid pairs or colocated resources--do not exceed interconnection limits.","Check Grouped Resources"]
["Hybrid Deliverability",{"$f":"IFERROR(\n    _xlfn.IFS(\n        INDEX(Queries[Status],MATCH(\"CheckHybridDeliverability\",Queries[Output Query Table],0))=\"STALE\",\n        \"Refreshing ...\",\n        AND(CheckHybridDeliverability[Hybrid Check]),\n        \"Pass\",\n        TRUE,\n        \"Fail\"\n    ),\n    \"N/A\"\n)","v":"N/A"},"Checks hybrid solar resources against their paired storage according to their deliverability statuses.","Check Hybrid Deliverability"]
["Demand Response",{"$f":"IF(\n    CheckDemandResponse[[#Totals],[Demand Response Ratio]]<=INDEX(Certification[Value],MATCH(\"Maximum DR Ratio\",Certification[Key],0)),\n    \"Pass\",\n    \"Fail\"\n)","v":{"$error":"#N/A"}},{"$f":"\"Checks that shown demand response capacity does not exceed \" & TEXT(INDEX(Certification[Value],MATCH(\"Maximum DR Ratio\",Certification[Key],0)),\"0.0%\") & \" of requirements in any hour.\"","v":"Checks that shown demand response capacity does not exceed 8.3% of requirements in any hour."},"Check Demand Response"]
["Overall",{"$f":"_xlfn.IFS(\n    OR(B2:B14=\"Refreshing ...\"),\n    \"Refreshing …\",\n    OR(B2:B14=\"Fail\"),\n    \"Fail\",\n    TRUE,\n    \"Pass\"\n)","v":{"$error":"#N/A"}},"All applicable individual tests above must pass."]

{"sheet":"Check Capacity","index":8,"n_rows":3,"n_cols":60,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Colocated Resource IDs","Chart Label","Deliverability Status","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24","LA Basin (MW)","Big Creek-Ventura (MW)","San Diego-IV (MW)","Bay Area (MW)","Fresno (MW)","Sierra (MW)","Stockton (MW)","Kern (MW)","Humboldt (MW)","NBNC (MW)","Flexible Category 1 (MW)","Flexible Category 2 (MW)","Flexible Category 3 (MW)","Excess Capacity Group","Storage Efficiency","Total Energy Shown (MWh)","Grid Capacity (MWh)","Onsite Energy-Only Capacity (MWh)","Grid Charging Requirement (MWh)","MCC Bucket 4 Charging Requirement (MWh)","First Hour Shown","Last Hour Shown","Total Hours Shown","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours","Capacity Effective Start Date","Capacity Effective End Date","Valid Hours","Check Dates"]
[]
[null,null,"Total",null,null,null,{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 1]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 2]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 3]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 4]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 5]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 6]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 7]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 8]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 9]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 10]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 11]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 12]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 13]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 14]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 15]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 16]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 17]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 18]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 19]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 20]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 21]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 22]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 23]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[MW HE 24]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[LA Basin (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Big Creek-Ventura (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[San Diego-IV (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Bay Area (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Fresno (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Sierra (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Stockton (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Kern (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[Humboldt (MW)]),2)","v":0},{"$f":"ROUND(SUBTOTAL(109,CheckCapacity[NBNC (MW)]),2)","v":0},{"$f":"ROUND(\n    SUMIFS(CheckCapacity[Flexible Category 1 (MW)],CheckCapacity[Contract ID],\"<>Requirements\"),\n    2\n)","v":0},{"$f":"_xlfn.IFNA(\n    ROUND(\n        MIN(\n            -INDEX(CheckCapacity[Flexible Category 2 (MW)],MATCH(\"Requirements\",CheckCapacity[Contract ID],0)),\n            SUMIFS(CheckCapacity[Flexible Category 2 (MW)],CheckCapacity[Contract ID],\"<>Requirements\")\n            +CheckCapacity[[#Totals],[Flexible Category 3 (MW)]]\n        ),\n        2\n    ),\n    0\n)","v":0},{"$f":"_xlfn.IFNA(\n    ROUND(\n        MIN(\n            -INDEX(CheckCapacity[Flexible Category 3 (MW)],MATCH(\"Requirements\",CheckCapacity[Contract ID],0)),\n            SUMIFS(CheckCapacity[Flexible Category 3 (MW)],CheckCapacity[Contract ID],\"<>Requirements\")\n        ),\n        2\n    ),\n    0\n)","v":0},null,null,null,{"$f":"SUBTOTAL(109,CheckCapacity[Grid Capacity (MWh)])","v":0},null,{"$f":"SUBTOTAL(109,CheckCapacity[Grid Charging Requirement (MWh)])","v":0},{"$f":"SUBTOTAL(109,CheckCapacity[MCC Bucket 4 Charging Requirement (MWh)])","v":0},null,null,null,null,null,null,null,null,{"$f":"AND(CheckCapacity[Valid Hours])","v":{"$error":"#VALUE!"}},{"$f":"AND(CheckCapacity[Check Dates])","v":{"$error":"#VALUE!"}}]

{"sheet":"Check Custom Profiles","index":9,"n_rows":1,"n_cols":33,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Resource ID","Resource SubID","Chart Label","NQC (MW)","Pmax (MW)","NQC Under Contract (MW)","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24","Maximum Shown Capacity (MW)","Maximum Shown Capacity HE","Check"]

{"sheet":"Check Storage SOC","index":10,"n_rows":3,"n_cols":108,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Colocated Resource IDs","Allows Grid Charging","Storage Efficiency","Maximum Continuous Energy (MWh)","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24","Available Charging MW HE 1","Available Charging MW HE 2","Available Charging MW HE 3","Available Charging MW HE 4","Available Charging MW HE 5","Available Charging MW HE 6","Available Charging MW HE 7","Available Charging MW HE 8","Available Charging MW HE 9","Available Charging MW HE 10","Available Charging MW HE 11","Available Charging MW HE 12","Available Charging MW HE 13","Available Charging MW HE 14","Available Charging MW HE 15","Available Charging MW HE 16","Available Charging MW HE 17","Available Charging MW HE 18","Available Charging MW HE 19","Available Charging MW HE 20","Available Charging MW HE 21","Available Charging MW HE 22","Available Charging MW HE 23","Available Charging MW HE 24","SOC Day 1 HE 1","SOC Day 1 HE 2","SOC Day 1 HE 3","SOC Day 1 HE 4","SOC Day 1 HE 5","SOC Day 1 HE 6","SOC Day 1 HE 7","SOC Day 1 HE 8","SOC Day 1 HE 9","SOC Day 1 HE 10","SOC Day 1 HE 11","SOC Day 1 HE 12","SOC Day 1 HE 13","SOC Day 1 HE 14","SOC Day 1 HE 15","SOC Day 1 HE 16","SOC Day 1 HE 17","SOC Day 1 HE 18","SOC Day 1 HE 19","SOC Day 1 HE 20","SOC Day 1 HE 21","SOC Day 1 HE 22","SOC Day 1 HE 23","SOC Day 1 HE 24","SOC Day 2 HE 1","SOC Day 2 HE 2","SOC Day 2 HE 3","SOC Day 2 HE 4","SOC Day 2 HE 5","SOC Day 2 HE 6","SOC Day 2 HE 7","SOC Day 2 HE 8","SOC Day 2 HE 9","SOC Day 2 HE 10","SOC Day 2 HE 11","SOC Day 2 HE 12","SOC Day 2 HE 13","SOC Day 2 HE 14","SOC Day 2 HE 15","SOC Day 2 HE 16","SOC Day 2 HE 17","SOC Day 2 HE 18","SOC Day 2 HE 19","SOC Day 2 HE 20","SOC Day 2 HE 21","SOC Day 2 HE 22","SOC Day 2 HE 23","SOC Day 2 HE 24","Minimum SOC","Minimum SOC Day and HE","Maximum Daily Energy (MWh)","Shown Energy (MWh)","Delta Daily Energy (MWh)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Minimum:",{"$f":"SUBTOTAL(105,CheckStorageSOC[Minimum SOC])","v":0},null,null,"Minimum:",{"$f":"SUBTOTAL(105,CheckStorageSOC[Delta Daily Energy (MWh)])","v":0}]

{"sheet":"Check Grouped Resources","index":11,"n_rows":1,"n_cols":28,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Associated Resources","Interconnection Limit (MW)","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24","Maximum Total MW","Difference (MW)"]

{"sheet":"Check Hybrid Deliverability","index":12,"n_rows":1,"n_cols":38,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Resource Type","Pmax (MW)","NQC (MW)","NQC Under Contract (MW)","Interconnection Limit (MW)","Deliverable %","Deliverable MW","Deliverability Status","Calculated Deliverable MW","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24","Hybrid Pair","Hybrid Check"]

{"sheet":"Check Demand Response","index":13,"n_rows":26,"n_cols":4,"rows_kept":26,"cut":false,"hidden":true,"merged":[]}
["Hour Ending","Demand Response (MW)","System Requirement (MW)","Demand Response Ratio"]
[1,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[2,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[3,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[4,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[5,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[6,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[7,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[8,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[9,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[10,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[11,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[12,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[13,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[14,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[15,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[16,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[17,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[18,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[19,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[20,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[21,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[22,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[23,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[24,{"$f":"SUM(\n    _xlfn._xlws.FILTER(\n        _xlfn._xlws.FILTER(\n           LSEShowingComplete[],\n           LSEShowingComplete[#Headers]=\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]]\n        ),\n        (LSEShowingComplete[Chart Label]=\"Demand Response\")+(LSEShowingComplete[Resource ID]=\"DR Allocation\")>0,\n        0\n    )\n)","v":0},{"$f":"-INDEX(\n    CheckCapacity[],\n    MATCH(\"Requirements\",CheckCapacity[Contract ID],0),\n    MATCH(\"MW HE \"&CheckDemandResponse[[#This Row],[Hour Ending]],CheckCapacity[#Headers],0)\n)","v":{"$error":"#N/A"}},{"$f":"CheckDemandResponse[[#This Row],[Demand Response (MW)]]/CheckDemandResponse[[#This Row],[System Requirement (MW)]]","v":{"$error":"#N/A"}}]
[null,null,"Max:",{"$f":"MAX(CheckDemandResponse[Demand Response Ratio])","v":{"$error":"#N/A"}}]

{"sheet":"LSE Showing Complete","index":14,"n_rows":1,"n_cols":56,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Contract ID","Resource ID","Resource SubID","Colocated Resource IDs","Resource Type","Fuel","Chart Label","Pmax (MW)","NQC (MW)","NQC Under Contract (MW)","Local RA (MW)","Local Capacity Area","Committed Flexible RA (MW)","Flexible Category","Deliverability Status","Deliverable %","Deliverable MW","Capacity Effective Start Date","Capacity Effective End Date","Path 26 Designation","Allows Grid Charging","Daily Storage Cycle Physical Capability","Storage Efficiency","Maximum Continuous Energy (MWh)","Storage Maximum Daily MWh","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours","Interconnection Limit (MW)","MCC Bucket 4","Unspecified Import","Profile Source","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]

{"sheet":"Hourly Availability","index":16,"n_rows":17,"n_cols":25,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["Label","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24"]
["Requirements and Allocations",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Nuclear",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Hydro",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Pumped Hydro",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Thermal",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["CHP",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Unspecified Imports",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Biogas",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Biomass",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Geothermal",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Solar",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Wind",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Fuel Cell",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Other",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Battery Storage",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]
["Demand Response",{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0},{"$f":"_xlfn.IFS(\n    HourlyAvailability[[#This Row],[Label]]=\"Requirements and Allocations\",\n    -SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    ),\n    TRUE,\n    SUM(\n        _xlfn._xlws.FILTER(\n            _xlfn._xlws.FILTER(\n                CheckCapacity[],\n                CheckCapacity[#Headers]=\"MW HE \"&INT(INDEX(HourlyAvailability[#Headers],COLUMN()))\n            ),\n            CheckCapacity[Chart Label]=HourlyAvailability[[#This Row],[Label]],\n            0\n        )\n    )\n)","v":0}]

{"sheet":"Local Availability","index":18,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["Label","LA Basin","Big Creek-Ventura","San Diego-IV","Bay Area","Fresno","Sierra","Stockton","Kern","Humboldt","NBNC"]
["Local Requirement",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Nuclear",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Hydro",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Pumped Hydro",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Thermal",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["CHP",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Unspecified Imports",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Biogas",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Biomass",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Geothermal",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Solar",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Wind",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Fuel Cell",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Other",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Battery Storage",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]
["Demand Response",{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0},{"$f":"IF(LocalAvailability[[#This Row],[Label]]=\"Local Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Local Requirement\")\n                    * (RequirementsAndAllocations[Option]=INDEX(LocalAvailability[#Headers],1,COLUMN())),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Local RA (MW)],\n        LSEShowingComplete[Chart Label],\n        LocalAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Local Capacity Area],\n        INDEX(LocalAvailability[#Headers],1,COLUMN())\n    )\n)","v":0}]

{"sheet":"Flex Availability","index":20,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["Label","Flexible Category 1","Flexible Category 2","Flexible Category 3"]
["Flexible Requirement",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Nuclear",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Hydro",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Pumped Hydro",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Thermal",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["CHP",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Unspecified Imports",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Biogas",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Biomass",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Geothermal",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Solar",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Wind",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Fuel Cell",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Other",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Battery Storage",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]
["Demand Response",{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0},{"$f":"IF(FlexAvailability[[#This Row],[Label]]=\"Flexible Requirement\",\n    IFERROR(\n        INDEX(\n            RequirementsAndAllocations[Value],\n            MATCH(\n                1,\n                (RequirementsAndAllocations[LSE]=LSEAbbreviation)\n                    * (RequirementsAndAllocations[Year]=YEAR(ShowingMonth))\n                    * (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                    * (RequirementsAndAllocations[Name]=\"Flexible Requirement\")\n                    * (RequirementsAndAllocations[Option]=SUBSTITUTE(INDEX(FlexAvailability[#Headers],1,COLUMN()),\"Flexible \",\"\")),\n                0\n            )\n        ),\n        0\n    ),\n    SUMIFS(\n        LSEShowingComplete[Committed Flexible RA (MW)],\n        LSEShowingComplete[Chart Label],\n        FlexAvailability[[#This Row],[Label]],\n        LSEShowingComplete[Flexible Category],\n        INDEX(_xlfn.TEXTSPLIT(INDEX(FlexAvailability[#Headers],1,COLUMN()),\" \"),3)\n    )\n)","v":0}]

{"sheet":"Requirements and Allocations","index":21,"n_rows":1,"n_cols":7,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["LSE","Year","Month","Name","Option","Value","Units"]

{"sheet":"Resource Database","index":22,"n_rows":1794,"n_cols":37,"rows_kept":1794,"cut":false,"hidden":false,"merged":[]}
["Resource ID","Resource SubID","Resource Name","Colocated Resource IDs","Technology","Resource Type","Fuel","Balancing Authority Area","Path 26 Designation","Local Capacity Area","Sub-Local Capacity Area","Flexible Category","Pmax (MW)","Interconnection Limit (MW)","Deliverability Status","Deliverable %","Deliverable MW","Allows Grid Charging","Daily Storage Cycle Physical Capability","Storage Efficiency","Maximum Continuous Energy (MWh)","Storage Maximum Daily MWh","First Available Hour (HE)","Last Available Hour (HE)","Maximum Daily Run Hours","January NQC (MW)","February NQC (MW)","March NQC (MW)","April NQC (MW)","May NQC (MW)","June NQC (MW)","July NQC (MW)","August NQC (MW)","September NQC (MW)","October NQC (MW)","November NQC (MW)","December NQC (MW)"]
["CAM Storage Allocation Single Cycle",null,"CAM Storage Allocation Single Cycle",null,"OTHER","Battery Storage","LESR","CISO",null,null,null,null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    0\n)","v":0},null,null,null,null,true,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Daily Storage Cycle Physical Capability\"),\n            0\n        )\n    ),\n    0\n)","v":0},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Storage Efficiency\"),\n            0\n        )\n    ),\n    0\n)","v":0},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Maximum Continuous Energy\"),\n            0\n        )\n    ),\n    0\n)","v":0},{"$f":"ResourceDatabase[[#This Row],[Maximum Continuous Energy (MWh)]]*ResourceDatabase[[#This Row],[Daily Storage Cycle Physical Capability]]","v":0},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B4))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"First Hour Available\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B4))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Last Hour Available\"),\n            0\n        )\n    ),\n    24\n)","v":24},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B4))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Maximum Daily Run Hours\"),\n            0\n        )\n    ),\n    ResourceDatabase[[#This Row],[Last Available Hour (HE)]]-ResourceDatabase[[#This Row],[First Available Hour (HE)]]+1\n)","v":24},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=1)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=2)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=3)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=4)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=5)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=6)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=7)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=8)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=9)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=10)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=11)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=12)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1}]
["CAM Storage Allocation Multi Cycle",null,"CAM Storage Allocation Multi Cycle",null,"OTHER","Battery Storage","LESR","CISO",null,null,null,null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    0\n)","v":0},null,null,null,null,true,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Daily Storage Cycle Physical Capability\"),\n            0\n        )\n    ),\n    0\n)","v":0},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Storage Efficiency\"),\n            0\n        )\n    ),\n    0\n)","v":0},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Maximum Continuous Energy\"),\n            0\n        )\n    ),\n    0\n)","v":0},{"$f":"ResourceDatabase[[#This Row],[Maximum Continuous Energy (MWh)]]*ResourceDatabase[[#This Row],[Daily Storage Cycle Physical Capability]]","v":0},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B5))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"First Hour Available\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B5))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Last Hour Available\"),\n            0\n        )\n    ),\n    24\n)","v":24},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B5))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Maximum Daily Run Hours\"),\n            0\n        )\n    ),\n    ResourceDatabase[[#This Row],[Last Available Hour (HE)]]-ResourceDatabase[[#This Row],[First Available Hour (HE)]]+1\n)","v":24},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=1)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=2)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=3)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=4)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=5)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=6)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=7)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=8)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=9)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=10)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=11)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=12)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1}]
["CAM Peaker Allocation",null,"CAM Peakers",null,"OTHER","CAM Peaker","NATURAL GAS","CISO",null,null,null,null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH(ShowingMonth))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    0\n)","v":0},null,null,null,"",null,null,null,null,null,{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B6))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"First Hour Available\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B6))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Last Hour Available\"),\n            0\n        )\n    ),\n    24\n)","v":24},{"$f":"IFERROR(\n    INDEX(\n        RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=MONTH('Certification'!B6))\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Maximum Daily Run Hours\"),\n            0\n        )\n    ),\n    ResourceDatabase[[#This Row],[Last Available Hour (HE)]]-ResourceDatabase[[#This Row],[First Available Hour (HE)]]+1\n)","v":24},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=1)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=2)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=3)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=4)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=5)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=6)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=7)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=8)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=9)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=10)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=11)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1},{"$f":"IFERROR(\n    INDEX(\n       RequirementsAndAllocations[Value],\n        MATCH(\n            1,\n            (RequirementsAndAllocations[Month]=12)\n                *(RequirementsAndAllocations[Name]=ResourceDatabase[[#This Row],[Resource ID]])\n                *(RequirementsAndAllocations[Option]=\"Net Qualifying Capacity\"),\n            0\n        )\n    ),\n    1\n)","v":1}]
["7STDRD_1_SOLAR1",null,"Shafter Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern Oil",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["ACACIA_6_SOLAR",null,"West Antelope Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.54,0.1,3.79,5.18,10.09,8.67,0.46,0.1,0.1,0.1]
["ADERA_1_SOLAR1",null,"Adera Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ADLIN_1_UNITS",null,"GEYSERS AIDLIN AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",1,22,null,"FC","","",null," "," "," "," ",1,24,24,22,22,22,22,22,22,22,22,22,22,22,22]
["ADMEST_6_SOLAR",null,"Adams East",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon",null,19,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.16,5.69,6.92,11.47,9.86,1.01,0.1,0.1,0.1]
["ADOBEE_1_SOLAR",null,"Adobe Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["AGRICO_6_PL3N5",null,"Fresno Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon",1,22.69,null,"FC","","",null," "," "," "," ",1,24,24,22.69,22.69,22.69,22.69,22.69,22.69,22.69,22.69,22.69,22.69,22.69,22.69]
["AGRICO_7_UNIT",null,"Fresno Cogen",null,"OTHER","CHP","NATURAL GAS","CISO","North","Fresno","Herndon",1,50.6,null,"FC","","",null," "," "," "," ",1,24,24,50.6,50.6,50.6,50.6,50.6,50.6,50.6,50.6,50.6,50.6,50.6,50.6]
["AGUCAL_5_SOLAR1",null,"Agua Caliente Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,290,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["AKINGS_6_AMESR1",null,"American Kings Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Hanford",null,123,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.75,1.27,53.76,67.38,91.84,77.12,6.42,0.11,0.1,0.1]
["ALAMIT_2_PL1X3",null,"Alamitos Energy Center Unit 7",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",1,674.7,null,"FC","","",null," "," "," "," ",1,24,24,674.7,674.7,674.7,674.7,674.7,674.7,674.7,674.7,674.7,674.7,674.7,674.7]
["ALAMIT_7_ES1",null,"Alamitos Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",1,100,null,"FC","","",null,2.8553459119496862,0.90800000000000003,400,1142.1383647798746,1,24,11.421383647798745,100,100,100,100,100,100,100,100,100,100,100,100]
["ALAMIT_7_UNIT 3",null,"ALAMITOS GEN STA. UNIT 3",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",1,326.76,null,"FC","","",null," "," "," "," ",1,24,24,326.76,326.76,326.76,326.76,326.76,326.76,326.76,326.76,326.76,326.76,326.76,326.76]
["ALAMIT_7_UNIT 4",null,"ALAMITOS GEN STA. UNIT 4",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",1,334.43,null,"FC","","",null," "," "," "," ",1,24,24,334.43,334.43,334.43,334.43,334.43,334.43,334.43,334.43,334.43,334.43,334.43,334.43]
["ALAMIT_7_UNIT 5",null,"ALAMITOS GEN STA. UNIT 5",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",1,480,null,"FC","","",null," "," "," "," ",1,24,24,480,480,480,480,480,480,480,480,480,480,480,480]
["ALAMO_6_UNIT",null,"ALAMO POWER PLANT ",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,2,17,null,"FC","","",null," "," "," "," ",1,24,24,13.22,14,12.02,13.92,13.71,14,14,14,9.5399999999999991,9.7200000000000006,13.63,11.53]
["ALHMBR_1_ALHSLR",null,"Alhambra (Solar Gen 2) ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID","South",null,null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.35,0.1,9.4700000000000006,12.94,25.23,21.69,1.1499999999999999,0.1,0.1,0.1]
["ALLGNY_6_HYDRO1",null,"Salmon Creek Hydroelectric Project",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,null,0.52,null,"FC","","",null," "," "," "," ",1,24,24,0.14000000000000001,0.25,0.32,0.48,0.48,0.14000000000000001,0.03,0,0,0.03,0.14000000000000001,0.08]
["ALMASL_2_AL6BT6",null,"Almasol 6 BES","ALMASL_2_GS6SR6","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,50,150,"FC","","",false,1,0.8,200,200,1,24,4,50,50,50,50,50,50,50,50,50,50,50,50]
["ALMASL_2_GS1SR1",null,"Almasol Generating Station 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,125,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.51,0.37,41.04,53.05,82.25,70.989999999999995,3.81,0.1,0.1,0.1]
["ALMASL_2_GS4SR4",null,"Almasol Generating Station 4",null,"PHOTO VOLTAIC","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["ALMASL_2_GS6SR6",null,"Almasol Generating Station 6","ALMASL_2_AL6BT6","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,150,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["ALMASL_2_GS7SR7",null,"Almasol Generating Station 7",null,"PHOTO VOLTAIC","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,132,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.7,0.39,43.34,56.02,86.85,74.97,4.0199999999999996,0.1,0.1,0.1]
["ALMEGT_1_UNIT 1",null,"ALAMEDA GT UNIT 1",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Oakland",1,25,null,"FC","","",null," "," "," "," ",1,24,24,23.4,23.4,23.4,23.4,23.4,23.4,23.4,23.4,23.4,23.4,23.4,23.4]
["ALMEGT_1_UNIT 2",null,"ALAMEDA GT UNIT 2",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Oakland",1,25,null,"FC","","",null," "," "," "," ",1,24,24,23.5,23.5,23.5,23.5,23.5,23.5,23.5,23.5,23.5,23.5,23.5,23.5]
["ALPSLR_1_NTHSLR",null,"Alpaugh North, LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["ALPSLR_1_SPSSLR",null,"Alpaugh 50 LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,50,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.61,0.42,14.98,18.22,30.18,25.96,2.66,0.1,0.1,0.1]
["ALT6DN_2_WIND7",null,"Pinyon Pines 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,164.31,null,"FC","","",null," "," "," "," ",1,24,24,8.9600000000000009,19.329999999999998,20.88,66.3,70.66,62.3,54.75,47.95,32.869999999999997,15.38,7.11,7.54]
["ALT6DS_2_WIND9",null,"Pinyon Pines 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,132,null,"FC","","",null," "," "," "," ",1,24,24,7.2,15.53,16.77,53.26,56.77,50.05,43.99,38.520000000000003,26.41,12.36,5.71,6.06]
["ALTA3A_2_CPCE4",null,"Alta Wind 4",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,102,null,"FC","","",null," "," "," "," ",1,24,24,5.56,12,12.96,41.16,43.86,38.67,33.99,29.76,20.41,9.5500000000000007,4.41,4.68]
["ALTA3A_2_CPCE5",null,"Alta Wind 5",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,168,null,"FC","","",null," "," "," "," ",1,24,24,9.16,19.760000000000002,21.35,67.78,72.25,63.69,55.98,49.02,33.61,15.73,7.27,7.71]
["ALTA3A_2_CPCE8",null,"Alta Wind 8",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,8.18,17.64,19.059999999999999,60.52,64.510000000000005,56.87,49.98,43.77,30.01,14.04,6.49,6.89]
["ALTA4A_2_CPCW1",null,"Alta Wind 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,8.18,17.64,19.059999999999999,60.52,64.510000000000005,56.87,49.98,43.77,30.01,14.04,6.49,6.89]
["ALTA4B_2_CPCW2",null,"Alta Wind 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,8.18,17.64,19.059999999999999,60.52,64.510000000000005,56.87,49.98,43.77,30.01,14.04,6.49,6.89]
["ALTA4B_2_CPCW3",null,"Alta Wind 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,8.18,17.64,19.059999999999999,60.52,64.510000000000005,56.87,49.98,43.77,30.01,14.04,6.49,6.89]
["ALTA4B_2_CPCW6",null,"Mustang Hills",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,8.18,17.64,19.059999999999999,60.52,64.510000000000005,56.87,49.98,43.77,30.01,14.04,6.49,6.89]
["ALTA6B_2_WIND11",null,"Alta Wind 11",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,88.15,null,"FC","","",null," "," "," "," ",1,24,24,4.8099999999999996,10.37,11.2,35.57,37.909999999999997,33.42,29.37,25.72,17.64,8.25,3.81,4.05]
["ALTA6E_2_WIND10",null,"Alta Wind 10",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,134.84,null,"FC","","",null," "," "," "," ",1,24,24,7.35,15.86,17.14,54.41,57.99,51.12,44.93,39.35,26.98,12.62,5.83,6.19]
["ALTWD_2_AT3WD3",null,"Altech 3",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,9.8000000000000007,null,"FC","","",null," "," "," "," ",1,24,24,0.53,1.1499999999999999,1.25,3.95,4.21,3.72,3.27,2.86,1.96,0.92,0.42,0.45]
["ALTWD_2_COAWD1",null,"Coachella 1",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,50.4,null,"FC","","",null," "," "," "," ",1,24,24,2.75,5.93,6.4,20.34,21.67,19.11,16.79,14.71,10.08,4.72,2.1800000000000002,2.31]
["ANAHM_2_CANYN1",null,"CANYON POWER PLANT UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,49.21,null,"FC","","",null," "," "," "," ",1,24,24,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21]
["ANAHM_2_CANYN2",null,"CANYON POWER PLANT UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,48.04,null,"FC","","",null," "," "," "," ",1,24,24,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04]
["ANAHM_2_CANYN3",null,"CANYON POWER PLANT UNIT 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,46.49,null,"FC","","",null," "," "," "," ",1,24,24,46.49,46.49,46.49,46.49,46.49,46.49,46.49,46.49,46.49,46.49,46.49,46.49]
["ANAHM_2_CANYN4",null,"CANYON POWER PLANT UNIT 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,49.8,null,"FC","","",null," "," "," "," ",1,24,24,49.8,49.8,49.8,49.8,49.8,49.8,49.8,49.8,49.8,49.8,49.8,49.8]
["ANZA_6_SOLAR1",null,"Seville Solar One",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","IID","South",null,null,1,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["APLHIL_1_SFKHY1",null,"South Fork Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",1,2.68,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["AQUAWS_2_AQWSR1",null,"Aquamarine Westside",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,250,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,7.61,2.59,109.27,136.94999999999999,186.66,156.75,13.05,0.22,0.1,0.1]
["ARBWD_6_QF",null,"Wind Resource II",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,19.95,null,"FC","","",null," "," "," "," ",1,24,24,1.0900000000000001,2.35,2.54,8.0500000000000007,8.58,7.56,6.65,5.82,3.99,1.87,0.86,0.92]
["ARCOGN_2_UNITS",null,"WATSON COGENERATION",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","South","LA Basin","Western",1,305,null,"FC","","",null," "," "," "," ",1,24,24,305,305,305,305,305,305,305,305,305,305,305,305]
["ARKANS_1_ARKSLR",null,"Arkansas (Solar Gen 2)",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID","South",null,null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.35,0.1,9.4700000000000006,12.94,25.23,21.69,1.1499999999999999,0.1,0.1,0.1]
["ARLINT_5_SCEDYN",null,"Arlington Valley CC",null,"COMBINED CYCLE","CCGT","NATURAL GAS","AZPS","South",null,null,null,565,null,"FC","","",null," "," "," "," ",1,24,24,565,565,565,565,565,565,565,565,565,565,565,565]
["ARLNTN_2_AR1SR1",null,"Arlington","SUNCAT_2_A2ABT2, SUNCAT_2_A2BSR2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,269,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["ARLNTN_2_ASUSR1",null,"Arlington Solar Unit 1","SUNCAT_2_A1ABT1, SUNCAT_2_A1BBT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,131,131,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3.68,0.39,43.01,55.6,86.19,74.400000000000006,3.99,0.1,0.1,0.1]
["ARLVAL_5_SOLAR",null,"Arlington Valley Solar Energy II",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","SRP","South",null,null,null,127,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.43,0.18,24.05,32.869999999999997,64.09,55.08,2.92,0.1,0.1,0.1]
["ARVINN_6_ORION1",null,"Orion 1 Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,12,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.39,0.1,3.6,4.37,7.24,6.23,0.64,0.1,0.1,0.1]
["ARVINN_6_ORION2",null,"Orion 2 Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,8,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.24,0.1,3.5,4.38,5.97,5.0199999999999996,0.42,0.1,0.1,0.1]
["ASTORA_2_SOLAR1",null,"Astoria 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["ASTORA_2_SOLAR2",null,"Astoria 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,75,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.1,0.22,24.62,31.83,49.35,42.59,2.2799999999999998,0.1,0.1,0.1]
["ATHOS_5_AP1X2",null,"Athos Power Plant",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,250,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,7.01,0.74,82.08,106.11,164.49,141.97999999999999,7.61,0.1,0.1,0.1]
["ATHOS_5_AP2X2",null,"Athos Power Plant 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,200,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,5.61,0.59,65.66,84.89,131.59,113.59,6.09,0.1,0.1,0.1]
["ATWEL2_1_SOLAR1",null,"Atwell West",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["ATWELL_1_SOLAR",null,"Atwell Island PV Solar Generating Faci.",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["AVENAL_6_AVPARK",null,"Avenal Park Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,6,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.19,0.1,1.8,2.19,3.62,3.11,0.32,0.1,0.1,0.1]
["AVENAL_6_AVSLR1",null,"Avenal Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga",null,7.9,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["AVENAL_6_AVSLR2",null,"Avenal Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga",null,7.9,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["AVENAL_6_SANDDG",null,"Sand Drag Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,19,null,"ID",0.83579999999999999,"",null," "," "," "," ",1,24,24,0.1,0.1,0.51,0.13,4.76,5.79,9.58,8.24,0.85,0.1,0.1,0.1]
["AVENAL_6_SUNCTY",null,"Sun City Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["AVSOLR_2_SOLAR",null,"AV SOLAR RANCH 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,241.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,6.53,0.34,45.73,62.5,121.87,104.75,5.55,0.1,0.1,0.1]
["BAHIA_2_LKHSR1",null,"Lake Herman Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["BALCHS_7_UNIT 1",null,"BALCH 1 PH UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",1,31,null,"FC","","",null," "," "," "," ",1,24,24,24.8,24.8,24.8,24.8,24.8,24.8,31,31,31,28.2,24.8,24.8]
["BALCHS_7_UNIT 2",null,"BALCH 2 PH UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",1,52.5,null,"FC","","",null," "," "," "," ",1,24,24,42,42,0,42,52.5,52.5,52.5,52.5,52.5,52.5,52.5,52.5]
["BALCHS_7_UNIT 3",null,"BALCH 2 PH UNIT 3",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",1,54.6,null,"FC","","",null," "," "," "," ",1,24,24,43.68,0,24.8,43.68,54.18,54.6,54.6,54.6,54.6,54.6,54.6,43.68]
["BANKPP_2_NSPIN",null,"BANKPP_2_NSPIN",null,"PUMP","Pump","WATER","CISO","North","Bay Area","Contra Costa",1,270,null,"FC","","",null," "," "," "," ",1,24,24,127,127,127,127,127,127,127,127,127,127,127,127]
["BARRE_2_ALASB1","BARRE_2_ALASB1_SUN","Los Alamitos 1",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","LA Basin",null,null,10,10,"FC","","",null,null,null,null,null,1,24,24,0.1,0.1,0.28000000000000003,0.03,3.28,4.24,6.58,5.68,0.3,0.1,0.1,0.1]
["BARRE_2_ALASB1","BARRE_2_ALASB1_LESR","Los Alamitos 1",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","LA Basin",null,null,10,10,"FC","","",false,1,0.8,20,20,1,24,24,5,5,5,5,5,5,5,5,5,5,5,5]
["BARRE_2_QF",null,"BARRE QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Western",null,0.2,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0.01,0.01,0,0,0,0,0,0,0,0]
["BARRE_6_PEAKER",null,"Barre Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,49,null,"FC","","",null," "," "," ",449.18,1,24,9.1669387755102036,49,49,49,49,49,49,49,49,49,49,49,49]
["BASICE_2_UNITS",null,"King City Cogen",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,120,null,"FC","","",null," "," "," "," ",1,24,24,120,120,120,120,120,120,120,120,120,120,120,120]
["BCTSYS_5_PWXDYN",null,"BCTSYS_5_PWXDYN",null,"HYDRO","Hydro","WATER","BPAT","North",null,null,1,428,null,"FC","","",null," "," "," "," ",1,24,24,428,428,428,428,428,428,428,428,428,428,428,428]
["BDGRCK_1_UNITS",null,"BADGER CREEK LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",1,48.08,null,"FC","","",null," "," "," "," ",1,24,24,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08]
["BEARDS_7_UNIT 1",null,"Beardsley Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",1,11.5,null,"FC","","",null," "," "," "," ",1,24,24,4.3,2.74,2,6.54,5.96,9.1,5.54,5.94,3.8,3.2,2.72,6.18]
["BEARMT_1_UNIT",null,"Bear Mountain Limited",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP, Westpark",1,49.21,null,"FC","","",null," "," "," "," ",1,24,24,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21,49.21]
["BEJNLS_5_BV2SCEDYN",null,"Broadview 2",null,"WIND","Wind","WIND","AZPS","South",null,null,1,167,null,"FC","","",null," "," "," "," ",1,24,24,33.5,35.450000000000003,33.5,48.94,36.74,27.63,16.7,10.02,19.440000000000001,11.32,17.21,25.15]
["BEKWJS_5_BV1SCEDYN",null,"Broadview 1",null,"WIND","Wind","WIND","AZPS","South",null,null,1,130,null,"FC","","",null," "," "," "," ",1,24,24,26.08,27.59,26.08,38.090000000000003,28.6,21.51,13,7.8,15.14,8.81,13.39,19.579999999999998]
["BELDEN_7_UNIT 1",null,"BELDEN HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,119,null,"FC","",38.700000000000003,null," "," "," "," ",1,24,24,1.6,1.6,0,0,0,35.200000000000003,38.700000000000003,38.700000000000003,38.700000000000003,38.700000000000003,0,1.6]
["BGSKYN_2_AS2SR1",null,"Wise Hydro Unit 1","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,105,562,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,2.95,0.31,34.47,44.57,69.09,59.63,3.2,0.1,0.1,0.1]
["BGSKYN_2_ASPSR2",null,"Whitewater Hill Wind Project","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,100,562,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["BGSKYN_2_ASSR1B",null,"Antelope Solar 1B ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_AS2SR2, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,17,562,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,0.48,0.1,5.58,7.22,11.19,9.65,0.52,0.1,0.1,0.1]
["BGSKYN_2_ASSR3A",null,"Antelope Solar 3A ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,15,562,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.42,0.1,4.92,6.37,9.8699999999999992,8.52,0.46,0.1,0.1,0.1]
["BGSKYN_2_ASSR3B",null,"Antelope Solar 3B ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,5,562,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,1.64,2.12,3.29,2.84,0.15,0.1,0.1,0.1]
["BGSKYN_2_BS3SR3",null,"Big Sky Solar 3","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGCRK_2_EXESWD",null,"BIG CREEK HYDRO PROJECT PSP",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",1,820,null,"FC","","",null," "," "," "," ",1,24,24,490.44,553.79999999999995,507,561.6,700,728.6,706.43,700,700,455.76,483,498.28]
["BIGCRK_7_DAM7",null,"DAM 7 AT BIG CREEK (FISHWATER GEN)",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,0.3,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["BIGCRK_7_MAMRES",null,"MAMMOTH POOL RESERVOIR (FISHWATER",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,1.25,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["BIGSKY_2_AS2BT1",null,"Antelope Solar 2 LAB","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3","OTHER","Paired_BattStorage","LESR","CISO","South","Big Creek-Ventura",null,2,127,562,"ID",1,"",false,1,0.8,508,508,1,24,4,127,127,127,127,127,127,127,127,127,127,127,127]
["BIGSKY_2_ASLBT2",null,"Antelope Solar 2 Luna",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura",null,2,100,null,"ID",1,"",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["BIGSKY_2_BSKSR6",null,"Big Sky Solar 6","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2,BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGSKY_2_BSKSR7",null,"Big Sky Solar 7","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGSKY_2_BSKSR8",null,"Big Sky Solar 8","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGSKY_2_SOLAR1",null,"Antelope Big Sky Ranch ","BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGSKY_2_SOLAR2",null,"Big Sky Solar 4","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,40,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.1200000000000001,0.12,13.13,16.98,26.32,22.72,1.22,0.1,0.1,0.1]
["BIGSKY_2_SOLAR3",null,"Big Sky Summer ","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2,BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGSKY_2_SOLAR4",null,"Western Antelope Blue Sky Ranch B","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["BIGSKY_2_SOLAR5",null,"Big Sky Solar 2","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR6, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,5,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,1.64,2.12,3.29,2.84,0.15,0.1,0.1,0.1]
["BIGSKY_2_SOLAR6",null,"Digger Creek Ranch Hydro","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR7, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,85,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.38,0.25,27.91,36.08,55.93,48.27,2.59,0.1,0.1,0.1]
["BIGSKY_2_SOLAR7",null,"Bailey Creek Ranch","BIGSKY_2_SOLAR1, BIGSKY_2_SOLAR2, BIGSKY_2_SOLAR3, BIGSKY_2_SOLAR4, BIGSKY_2_SOLAR5, BIGSKY_2_SOLAR6, BGSKYN_2_ASSR1B, BGSKYN_2_AS2SR1, BGSKYN_2_ASSR3A, BGSKYN_2_ASSR3B, BGSKYN_2_ASPSR2, BIGSKY_2_BSKSR6, BIGSKY_2_BSKSR7, BIGSKY_2_BSKSR8, BGSKYN_2_BS3SR3, BIGSKY_2_AS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,50,562,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.4,0.15,16.420000000000002,21.22,32.9,28.4,1.52,0.1,0.1,0.1]
["BIOMAS_1_UNIT 1",null,"WOODLAND BIOMASS",null,"STEAM","Biomass","BIOMASS","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,25.5,null,"FC","","",null," "," "," "," ",1,24,24,15.98,15.69,7.86,8.07,8.06,7.5,7.93,8.07,15.24,8.0299999999999994,12.07,16.22]
["BISHOP_1_ALAMO",null,"BISHOP CREEK PLANT 2  AND  6",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,13.4,null,"FC","","",null," "," "," "," ",1,24,24,3.13,2.38,2.6,3.84,7.55,7.84,6.7,6.15,4.45,3.01,2.57,2.08]
["BISHOP_1_UNITS",null,"BISHOP CREEK PLANT 3  AND  4",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,15.8,null,"FC","","",null," "," "," "," ",1,24,24,4.91,3.68,2.96,6.32,10.33,10.75,9.3800000000000008,7.28,6.91,5.04,4.13,4.3]
["BKRFLD_2_SOLAR1",null,"Bakersfield 111",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP",null,1.38,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.6,0.76,1.03,0.87,0.1,0.1,0.1,0.1]
["BLACK_7_UNIT 1",null,"JAMES B. BLACK 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,85,null,"FC","","",null," "," "," "," ",1,24,24,84.2,82.4,82.4,82.4,84,84.6,84.4,84.4,82,68,68,84]
["BLACK_7_UNIT 2",null,"JAMES B. BLACK 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,84.1,null,"FC","","",null," "," "," "," ",1,24,24,83.48,83.28,83.28,82,83.28,83.88,84.08,84.08,84.08,67.28,83.48,83.28]
["BLAST_1_WIND",null,"Mountain View IV Wind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,49,null,"FC","","",null," "," "," "," ",1,24,24,2.67,5.76,6.23,19.77,21.07,18.579999999999998,16.329999999999998,14.3,9.8000000000000007,4.59,2.12,2.25]
["BLCKBT_2_STONEY",null,"BLACK BUTTE HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,6.2,null,"FC","","",null," "," "," "," ",1,24,24,2.04,1.6,1.3,3.5,2.7,2.57,2.02,1.83,1.5,1.5,2.1,2.5099999999999998]
["BLCKWL_6_SOLAR1",null,"Blackwell Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,12,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.37,0.12,5.24,6.57,8.9600000000000009,7.52,0.63,0.1,0.1,0.1]
["BLKCRK_2_GMCBT1",null,"Genesis McCoy Bess","BLKCRK_2_SOLAR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,230,250,"FC","","",false,2.843766438716465,0.90100000000000002,920,2616.2651236191477,1,24,11.37506575486586,230,230,230,230,230,230,230,230,230,230,230,230]
["BLKCRK_2_SOLAR1",null,"McCoy Station","BLKCRK_2_GMCBT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,250,250,"EO","","",null," "," "," "," ",1,24,24,0.1,0.1,7.01,0.74,82.08,106.11,164.49,141.97999999999999,7.61,0.02,0.1,0.1]
["BLKDIA_2_BDEBT1",null,"Black Diamond Energy Storage ",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","Pittsburg",1,200,null,"FC","","",null,1,0.8,800,800,1,24,4,200,200,200,200,200,200,200,200,200,200,200,200]
["BLM W_2_COSBT1",null,"Coso Battery Storage",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,2,60,null,"FC","","",null,1,0.8,240,240,1,24,4,60,60,60,60,60,60,60,60,60,60,60,60]
["BLM_2_UNITS",null,"BLM EAST Facility",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,1,72,null,"PD","",47,null," "," "," "," ",1,24,24,47,47,47,47,47,47,47,47,47,47,47,47]
["BLVRDE_6_BLVBT1",null,"Sycamore Cogeneration Unit 2",null,"FTUR","Battery Storage","NATURAL GAS","CISO","South","San Diego-IV",null,null,76,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,9.75,9.75,9.75,9.75,9.75,9.75,9.75,9.75,9.75]
["BLYTHE_1_SOLAR1",null,"Blythe Solar 1 Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,21,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["BLYTHE_1_SOLAR2",null,"Blythe Green 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["BNNIEN_7_ALTAPH",null,"ALTA POWER HOUSE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.34,0.3,0.3,0.4,0.2,0.39,0.4,0.61,0.42,0.53,0.41,0.3]
["BOGUE_1_UNITA1",null,"Feather River Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","Bogue, Drum-Rio Oso",1,48.69,null,"FC","","",null," "," "," "," ",1,24,24,47.38,47.38,47.38,47.38,47.38,47.38,47.38,47.38,47.38,47.38,47.38,47.38]
["BORDER_6_UNITA1",null,"CalPeak Power Border Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, Border",1,51.25,null,"FC","","",null," "," "," "," ",1,24,24,51.25,51.25,51.25,51.25,51.25,51.25,51.25,51.25,51.25,51.25,51.25,51.25]
["BOWMN_6_HYDRO",null,"NID Hydro Bowman Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,3.6,null,"FC","","",null," "," "," "," ",1,24,24,0.15,0.06,7.0000000000000007E-2,0.21,1.6,1.23,2.1800000000000002,2,1.5,1.03,0.24,0.18]
["BRDGVL_7_BAKER",null,"Baker Station Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,1.49,null,"FC","","",null," "," "," "," ",1,24,24,0.47,0.45,0.37,0.28000000000000003,0.13,0.01,0,0,0,0.01,0.06,0.46]
["BRDSLD_2_HIWIND",null,"High Winds Energy Center",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,162,null,"FC","","",null," "," "," "," ",1,24,24,6.87,11.87,15.97,49.51,77.89,49.77,63.8,34.85,12.02,2.91,4.58,6.94]
["BRDSLD_2_MTZUM2",null,"NextEra Energy Montezuma Wind II",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,78.2,null,"FC","","",null," "," "," "," ",1,24,24,3.31,5.73,7.71,23.9,37.6,24.02,30.8,16.82,5.8,1.41,2.21,3.35]
["BRDSLD_2_MTZUMA",null,"FPL Energy Montezuma Wind",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,36.799999999999997,null,"FC","","",null," "," "," "," ",1,24,24,1.56,2.7,3.63,11.25,17.690000000000001,11.3,14.49,7.92,2.73,0.66,1.04,1.58]
["BRDSLD_2_SHILO1",null,"Shiloh I Wind Project",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,150,null,"FC","","",null," "," "," "," ",1,24,24,6.36,10.99,14.79,45.85,72.12,46.08,59.07,32.26,11.13,2.7,4.24,6.42]
["BRDSLD_2_SHILO2",null,"SHILOH WIND PROJECT 2",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,150,null,"FC","","",null," "," "," "," ",1,24,24,6.36,10.99,14.79,45.85,72.12,46.08,59.07,32.26,11.13,2.7,4.24,6.42]
["BRDSLD_2_SHLO3A",null,"Shiloh III Wind Project, LLC",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,102.5,null,"FC","","",null," "," "," "," ",1,24,24,4.34,7.51,10.11,31.33,49.28,31.49,40.369999999999997,22.05,7.6,1.84,2.9,4.3899999999999997]
["BRDSLD_2_SHLO3B",null,"Shiloh IV Wind Project",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,100,null,"FC","","",null," "," "," "," ",1,24,24,4.24,7.33,9.86,30.56,48.08,30.72,39.380000000000003,21.51,7.42,1.8,2.83,4.28]
["BREGGO_6_DEGRSL",null,"Desert Green Solar Farm",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","South","San Diego-IV","San Diego",null,6.3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.18,0.1,2.0699999999999998,2.67,4.1500000000000004,3.58,0.19,0.1,0.1,0.1]
["BREGGO_6_SOLAR",null,"NRG Borrego Solar One",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,26,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.7,0.1,4.92,6.73,13.12,11.28,0.6,0.1,0.1,0.1]
["BRODIE_2_WIND",null,"Coram Brodie Wind Project",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,102,null,"FC","","",null," "," "," "," ",1,24,24,5.56,12,12.96,41.16,43.86,38.67,33.99,29.76,20.41,9.5500000000000007,4.41,4.68]
["BUCKBL_2_PL1X3",null,"Blythe Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","CAISO System",null,1,493.63,null,"FC","","",null," "," "," "," ",1,24,24,493.63,493.63,493.63,493.63,493.63,493.63,493.63,493.63,493.63,493.63,493.63,493.63]
["BUCKCK_2_HYDRO",null,"Lassen Station Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,0.99,null,"FC",0,"",null," "," "," "," ",1,24,24,0.13,0.13,0.13,0.13,0.13,0.13,0.08,0.08,0,0.02,0.13,0.13]
["BUCKCK_7_OAKFLT",null,"Oak Flat",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",null,1.3,null,"FC",0,"",null," "," "," "," ",1,24,24,0.34,0.34,0.34,0.34,0.34,0.34,0.34,0.34,0.2,0.21,0.2,0.22]
["BUCKCK_7_PL1X2",null,"BUCKS CREEK AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,57.25,null,"FC","",24.86,null," "," "," "," ",1,24,24,24.86,24.86,24.86,24.86,24.86,24.86,24.86,24.86,24.86,24.86,24.86,24.86]
["BUCKWD_1_NPALM1",null,"North Palm Springs 1A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,2.4,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.79,1.02,1.58,1.36,0.1,0.1,0.1,0.1]
["BUCKWD_1_QF",null,"Buckwind Re-powering project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,16.5,null,"FC","","",null," "," "," "," ",1,24,24,0.9,1.94,2.1,6.66,7.1,6.26,5.5,4.8099999999999996,3.3,1.54,0.71,0.76]
["BUCKWD_7_WINTCV",null,"Wintec Energy, Ltd.",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,1.32,null,"FC","","",null," "," "," "," ",1,24,24,7.0000000000000007E-2,0.16,0.17,0.53,0.56999999999999995,0.5,0.44,0.39,0.26,0.12,0.06,0.06]
["BURNYF_2_UNIT 1",null,"Burney Forest Power",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,29,null,"FC","","",null," "," "," "," ",1,24,24,28.71,29,28.68,29,29,28.85,29,29,29,28.56,28.88,29]
["BUTTVL_7_UNIT 1",null,"BUTT VALLEY HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,39.5,null,"FC","","",null," "," "," "," ",1,24,24,38.799999999999997,31.6,31.6,31.2,32.4,32.4,39.200000000000003,39.200000000000003,39.5,32.4,32.4,38.799999999999997]
["CABALO_2_M2BSR1",null,"Mustang 2 Barbaro Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,50,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.52,0.52,21.85,27.39,37.33,31.35,2.61,0.1,0.1,0.1]
["CABALO_2_M2WSR2",null,"Mustang 2 Whirlaway Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,1,100,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3.05,1.04,43.71,54.78,74.66,62.7,5.22,0.1,0.1,0.1]
["CABZON_1_WINDA1",null,"Cabazon Wind Project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,41,null,"FC","","",null," "," "," "," ",1,24,24,2.2400000000000002,4.82,5.21,16.54,17.63,15.54,13.66,11.96,8.1999999999999993,3.84,1.77,1.88]
["CALFTN_2_CFSBT1",null,"California Flats Solar Battery","CALFTN_2_SOLAR","OTHER","Paired_BattStorage","LESR","CISO","North","CAISO System",null,3,60,130,"FC","","",false,1,0.8,240,240,1,24,4,60,60,60,60,60,60,60,60,60,60,60,60]
["CALFTN_2_SOLAR",null,"California Flats North","CALFTN_2_CFSBT1","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","North","CAISO System",null,null,130,130,"ID",0.82,"",null," "," "," "," ",1,24,24,0.1,0.1,4.1900000000000004,1.0900000000000001,38.96,47.36,78.459999999999994,67.489999999999995,6.92,0.15,0.1,0.1]
["CALFTS_2_CFSSR1",null,"California Flats Solar South",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.57,1.55,65.56,82.17,112,94.05,7.83,0.13,0.1,0.1]
["CALGEN_1_UNITS",null,"Coso Navy 1",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,1,80,null,"FC","","",null," "," "," "," ",1,24,24,80,80,80,80,80,80,80,80,80,80,80,80]
["CALPIN_1_AGNEW",null,"Agnews Power Plant",null,"COMBUSTION TURBINE","CCGT","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",1,28.56,null,"FC","","",null," "," "," "," ",1,24,24,28.56,28.56,28.56,28.56,28.56,28.56,28.56,28.56,28.56,28.56,28.56,28.56]
["CALPSS_6_SOLAR1",null,"Calipatria Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID","South",null,null,1,19.899999999999999,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.54,0.1,3.77,5.15,10.039999999999999,8.6300000000000008,0.46,0.1,0.1,0.1]
["CAMCHE_1_PL1X3",null,"CAMANCHE UNITS  1, 2 &  3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota",null,9.99,null,"FC","","",null," "," "," "," ",1,24,24,1.62,1.67,1.74,1.99,2.31,0.99,0.83,0.88,0.48,0.52,0.95,1.4]
["CAMLOT_2_SOLAR1",null,"Camelot",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,45,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.22,0.1,8.52,11.65,22.71,19.52,1.03,0.1,0.1,0.1]
["CAMLOT_2_SOLAR2",null,"Columbia Two",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,15,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.41,0.1,2.84,3.88,7.57,6.51,0.34,0.1,0.1,0.1]
["CAMPFW_7_FARWST",null,"CAMP FAR WEST HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,1,6.8,null,"FC","","",null," "," "," "," ",1,24,24,0,2.08,5.6,5.44,2.64,2.48,3.36,2.94,0,0,0,0]
["CANTUA_1_SOLAR",null,"Cantua Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Panoche 115 kV",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["CAPWD_1_QF",null,"Edom Hills Wind Farm",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,19.55,null,"FC","","",null," "," "," "," ",1,24,24,1.07,2.2999999999999998,2.48,7.89,8.41,7.41,6.51,5.7,3.91,1.83,0.85,0.9]
["CARBOU_7_PL2X3",null,"CARIBOU PH 1 UNIT 2 & 3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,49,null,"FC","","",null," "," "," "," ",1,24,24,19.2,1.6,0,0,0,0,28.8,35.36,20.8,12,0,7.2]
["CARBOU_7_PL4X5",null,"CARIBOU PH 2 UNIT 4 & 5 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,120,null,"FC","","",null," "," "," "," ",1,24,24,42.34,36.4,32,16.8,18.98,67.599999999999994,101.18,103.18,103.2,72,25.22,24.84]
["CARBOU_7_UNIT 1",null,"CARIBOU PH 1 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,24,null,"FC","","",null," "," "," "," ",1,24,24,4,1.6,0,0,0,0,9.1199999999999992,19.2,18.399999999999999,0,0,0]
["CARLS1_2_CARCT1",null,"Carlsbad 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",2,422,null,"FC","","",null," "," "," "," ",7,24,18,422,422,422,422,422,422,422,422,422,422,422,422]
["CARLS2_1_CARCT1",null,"Carlsbad 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",2,105.5,null,"FC","","",null," "," "," "," ",7,24,18,105.5,105.5,105.5,105.5,105.5,105.5,105.5,105.5,105.5,105.5,105.5,105.5]
["CASADB_1_CD4GT1",null,"Casa Diablo 4",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,1,40.700000000000003,null,"FC","","",null," "," "," "," ",1,24,24,31,31,31,31,31,31,31,31,31,31,31,31]
["CASCES_6_CESBT1",null,"Sycamore Cogeneration Unit 3",null,"FTUR","Battery Storage","NATURAL GAS","CISO","North","CAISO System",null,1,74,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,25,25,25,25,25,25,25,25,25]
["CATLNA_2_SOLAR",null,"Catalina Solar - Phases 1 and 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,110,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.97,0.16,20.83,28.47,55.51,47.71,2.5299999999999998,0.1,0.1,0.1]
["CATLNA_2_SOLAR2",null,"Catalina Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,18,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.5,0.1,5.91,7.64,11.84,10.220000000000001,0.55000000000000004,0.1,0.1,0.1]
["CAVLSR_2_BSOLAR",null,"California Valley Solar Ranch-Phase B",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,40,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.29,0.34,11.99,14.57,24.14,20.77,2.13,0.1,0.1,0.1]
["CAVLSR_2_RSOLAR",null,"California Valley Solar Ranch-Phase A",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,210,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,6.77,1.76,62.93,76.510000000000005,126.75,109.02,11.17,0.25,0.1,0.1]
["CAYTNO_2_VASCO",null,"Vasco Road",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Contra Costa",null,4.3,null,"FC","","",null," "," "," "," ",1,24,24,3.9,4.01,4.09,4.07,4.05,4.05,4.03,4,4.03,3.65,3.98,4.0999999999999996]
["CDWR07_2_GEN",null,"CDWR07_2_GEN",null,"PUMP","Pumped Hydro","WATER","CISO","North","CAISO System",null,1,415.3,null,"FC","","",null," "," "," "," ",1,24,24,115.6,115.6,115.6,115.6,115.6,115.6,115.6,115.6,115.6,115.6,115.6,115.6]
["CEDRCK_6_UNIT",null,"Water Wheel Ranch",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.98,null,"FC","","",null," "," "," "," ",1,24,24,0.28999999999999998,0.33,0.32,0.52,0.45,0.19,7.0000000000000007E-2,0.06,0.05,0.08,0.12,0.17]
["CEDUCR_2_SOLAR1",null,"Ducor Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CEDUCR_2_SOLAR2",null,"Ducor Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CEDUCR_2_SOLAR3",null,"Ducor Solar 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,15,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CEDUCR_2_SOLAR4",null,"Ducor Solar 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CENT40_1_C40SR1",null,"CENTRAL 40",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Stockton","Tesla-Bellota",null,40,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.22,0.41,17.48,21.91,29.87,25.08,2.09,0.1,0.1,0.1]
["CENTER_2_RHONDO",null,"MWD Rio Hondo Hydroelectric Recovery Pla",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",1,1.91,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CENTER_2_SOLAR1",null,"Pico Rivera",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,0.9,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CENTER_2_TECNG1",null,"TECHNICAST",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","South","LA Basin","Western",null,0.99,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CENTER_6_PEAKER",null,"Center Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,47.3,null,"FC","","",null," "," "," ",402.05,1,24,8.5,47.3,47.3,47.3,47.3,47.3,47.3,47.3,47.3,47.3,47.3,47.3,47.3]
["CENTPD_2_BMSSX2",null,"Blythe Mesa Solar","CENTPD_2_BMSX2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,223.6,223.6,"FC","","",null,null,null,null,null,1,24,24,0.1,0.1,6.27,0.66,73.41,94.9,147.12,126.99,6.81,0.1,0.1,0.1]
["CENTPD_2_BMSX2",null,"Blythe Mesa Solar 2 BESS","CENTPD_2_BMSSX2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,112,223.6,"FC","","",false,1,0.8,448,448,1,24,4,112,112,112,112,112,112,112,112,112,112,112,112]
["CENTRY_6_PL1X4",null,"CENTURY GENERATING PLANT (AGGREGATE)",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,41.4,null,"FC","","",null," "," "," "," ",1,24,24,40,40,40,40,40,40,40,40,40,40,40,40]
["CHALK_1_UNIT",null,"CHALK CLIFF LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,48.67,null,"FC","","",null," "," "," "," ",1,24,24,48.67,48.67,48.67,48.67,48.67,48.67,48.67,48.67,48.67,48.67,48.67,48.67]
["CHARMN_2_PGONG1",null,"PROCTER  AND  GAMBLE OXNARD I",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,19.87,null,"FC","","",null," "," "," "," ",1,24,24,19.170000000000002,18.8,17.87,18.55,18.27,18.02,18.39,19.61,18.64,18.899999999999999,15.88,18.73]
["CHESTN_2_CHWBX2",null,"Chestnut Westside BESS",null,"OTHER","Paired_BattStorage","LESR","CISO","North","CAISO System",null,null,135,null,"ID","","",null,null,0.8,null,null,1,24,24,135,135,135,135,135,135,135,135,135,135,135,135]
["CHESTN_2_CHWSX2",null,"Chestnut Westside PV",null,"PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","CAISO System",null,null,150,null,"ID","","",null,null,null,null,null,1,24,24,0.1,0.1,4.57,1.55,65.56,82.17,112,94.05,7.83,0.13,0.1,0.1]
["CHEVCD_6_UNIT",null,"CHEVRON USA (TAFT/CADET)",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,11.5,null,"FC","","",null," "," "," "," ",1,24,24,1.05,1.72,1.6,1.42,1.32,1.73,1.51,1.59,1.63,1.53,1.77,1.46]
["CHEVCO_6_UNIT 1",null,"CHEVRON USA (COALINGA)",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,16.5,null,"FC","","",null," "," "," "," ",1,24,24,1.1100000000000001,0.99,1.31,1.1299999999999999,1.63,1.87,1.73,2.2400000000000002,2.54,1.9,1.25,1.08]
["CHEVCO_6_UNIT 2",null,"AERA ENERGY LLC. (COALINGA)",null,"FTUR","CHP","NATURAL GAS","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,8.5,null,"FC","","",null," "," "," "," ",1,24,24,0.92,0.92,1.03,0.96,0.93,0.84,0.76,0.73,0.79,0.95,1.01,1.05]
["CHEVCY_1_UNIT",null,"CHEVRON USA (CYMRIC)",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,24.3,null,"FC","","",null," "," "," "," ",1,24,24,3.74,3.14,2.4900000000000002,2.77,2.69,2.92,2.78,1.98,1.79,2,1.75,2.15]
["CHEVMN_2_UNITS",null,"CHEVRON U.S.A. UNITS 1 & 2 AGGREGATE",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Western, El Nido",null,124.87,null,"FC","","",null," "," "," "," ",1,24,24,3.84,4.1100000000000003,8.2799999999999994,26.35,6.88,5.52,13.32,7.93,13.95,7.64,6.21,1.26]
["CHICPK_7_UNIT 1",null,"Chicago Park Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",1,42,null,"FC","","",null," "," "," "," ",1,24,24,25.04,24.54,20.239999999999998,20,20.8,24,28.06,28.04,8.8000000000000007,8,19.2,26.03]
["CHILLS_1_SYCENG",null,"Sycamore Energy 1",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.78,0.77,0.87,0.92,0.88,0.83,0.98,1,0.99,0.95,0.93,0.95]
["CHILLS_7_UNITA1",null,"Sycamore Energy 2",null,null,"Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",1,2.25,null,"FC","","",null," "," "," "," ",1,24,24,1.82,2,2,2,1.4,1.68,1.56,1.52,1.74,1.75,1.8,1.61]
["CHINO_2_APEBT1",null,"Pomona Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern",3,20,null,"FC","","",null,1,0.8,80,80,1,24,4,20,20,20,20,20,20,20,20,20,20,20,20]
["CHINO_2_JURUPA",null,"Jurupa",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CHINO_2_PESBT1",null,"Pomona Energy Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin",null,2,20,null,"FC",0,"",null,1,0.8,80,80,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["CHINO_2_QF",null,"CHINO QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Eastern",null,0.19,null,"FC","","",null," "," "," "," ",1,24,24,0,0.02,0,0,0,0,0,0,0,0,0,0]
["CHINO_2_SASOLR",null,"SS San Antonio West LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CHINO_2_SOLAR2",null,"Kona Solar - Terra Francesca",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,1.49,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CHINO_6_CIMGEN",null,"Chino Co-Generation",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","South","LA Basin","Eastern",1,26,null,"FC","","",null," "," "," "," ",1,24,24,26,26,26,26,26,26,26,26,26,26,26,26]
["CHWCHL_1_UNIT",null,"CHOW 2 PEAKER PLANT",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",1,48.6,null,"FC","","",null," "," "," "," ",1,24,24,48,48,48,48,48,48,48,48,48,48,48,48]
["CLINESCO_3_PVDYN",null,"CLINES CORNERS",null,"WIND","Wind","WIND","PNM","South",null,null,1,129.94,null,"FC","","",null," "," "," "," ",1,24,24,62.54,53.95,44.14,52.73,49.05,39.24,26.93,25.75,29.43,30.66,49.05,68.67]
["CLINESCO_3_WBDYN",null,"CLINES CORNERS B",null,"WIND","Wind","WIND","PNM","South",null,null,1,194.28,null,"FC","","",null," "," "," "," ",1,24,24,93.5,80.67,66,78.84,73.34,58.67,40.270000000000003,38.5,44,45.84,73.34,102.67]
["CLOVDL_1_SOLAR",null,"Cloverdale Solar I",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","NCNB","Eagle Rock, Fulton",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["CLOVER_2_UNIT",null,"Clover Creek",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.99,null,"FC","","",null," "," "," "," ",1,24,24,0.47,0.47,0.38,0.55000000000000004,0.45,0.26,0.1,0.04,0.01,0,0.14000000000000001,0.33]
["CLRMNT_6_CLEBT1",null,"Sycamore Cogeneration Unit 4",null,"FTUR","Battery Storage","NATURAL GAS","CISO","South","San Diego-IV",null,null,76,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,7.25,7.25,7.25,7.25,7.25,7.25,7.25,7.25,7.25]
["CLRMTK_1_QF",null,"SMALL QF AGGREGATION - OAKLAND",null,"FTUR","CHP","NATURAL GAS","CISO","North","Bay Area","Oakland",null,1.25,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CMBLND_2_DS2BT1",null,"Daggett 2 a BESS","CMBLND_2_DS2SR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,null,52,65,"ID","","",null,null,0.8,null,null,1,24,24,52,52,52,52,52,52,52,52,52,52,52,52]
["CMBLND_2_DS2BT2",null,"Daggett 2 b BESS","CMBLND_2_DS2SR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,33,65,"ID","","",null,null,0.8,null,null,1,24,24,33,33,33,33,33,33,33,33,33,33,33,33]
["CMBLND_2_DS2BT3",null,"Daggett 2 c BESS","CMBLND_2_DS2SR3","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,46,52,"ID","","",false,null,0.8,null,null,1,24,24,46,46,46,46,46,46,46,46,46,46,46,46]
["CMBLND_2_DS2SR1",null,"Daggett 2 a PV","CMBLND_2_DS2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,65,65,"ID","","",null,null,null,null,null,1,24,24,0.1,0.1,1.82,0.19,21.34,27.59,42.77,36.92,1.98,0.1,0.1,0.1]
["CMBLND_2_DS2SR2",null,"Daggett 2 b PV","CMBLND_2_DS2BT2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,65,65,"ID","","",null,null,null,null,null,1,24,24,0.1,0.1,1.82,0.19,21.34,27.59,42.77,36.92,1.98,0.1,0.1,0.1]
["CMBLND_2_DS2SR3",null,"Daggett 2 c PV","CMBLND_2_DS2BT3","PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,52,52,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,1.46,0.15,17.07,22.07,34.21,29.53,1.58,0.1,0.1,0.1]
["CNTNLA_2_SOLAR1",null,"Centinela Solar Energy I ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,125,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.38,0.18,23.67,32.35,63.08,54.22,2.87,0.1,0.1,0.1]
["CNTNLA_2_SOLAR2",null,"Centinels Solar Energy 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,45.6,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.23,0.1,8.64,11.8,23.01,19.78,1.05,0.1,0.1,0.1]
["COCOPP_2_CTG1",null,"Marsh Landing 1",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,204.2,null,"FC","","",null," "," "," "," ",1,24,24,203.08,202.82,202.21,199.04,197.87,194.63,193.62,193.09,194.72,198.97,200.43,203.72]
["COCOPP_2_CTG2",null,"Marsh Landing 2",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,202.7,null,"FC","","",null," "," "," "," ",1,24,24,202.25,201.68,201.36,198.21,197.04,193.81,192.86,192.32,193.95,198.13,199.65,202.7]
["COCOPP_2_CTG3",null,"Marsh Landing 3",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,208.96,null,"FC","","",null," "," "," "," ",1,24,24,201.79,201.31,200.92,197.81,196.72,193.1,192.03,191.57,193.18,197.81,199.11,202.45]
["COCOPP_2_CTG4",null,"Marsh Landing 4",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,204.29,null,"FC","","",null," "," "," "," ",1,24,24,203.72,203.2,202.81,199.67,198.47,194.44,193.36,192.89,194.53,199.67,200.98,204.2]
["COCOSB_6_SOLAR",null,"Oakley Solar Project",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Bay Area","Contra Costa",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["COGNAT_1_UNIT",null,"Stockton Biomas",null,"STEAM","CHP","BIOMASS","CISO","North","CAISO System",null,null,45,null,"FC","","",null," "," "," "," ",1,24,24,44.87,45,44.81,45,44.73,45,45,45,45,44.87,45,44.94]
["COLEMN_2_UNIT",null,"Coleman",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,13,null,"FC","","",null," "," "," "," ",1,24,24,4.18,5.05,5.07,4.79,4.92,2.89,2.14,0.28000000000000003,1.1100000000000001,1.3,1.7,3.27]
["COLGAT_7_UNIT 1",null,"Colgate Powerhouse Unit 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,1,176.72,null,"FC","",141.6,null," "," "," "," ",1,24,24,141.6,141.6,141.6,141.6,141.6,141.6,141.6,141.6,141.6,141.6,141.6,141.6]
["COLGAT_7_UNIT 2",null,"Colgate Powerhouse Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,1,175.67,null,"FC","",139.74,null," "," "," "," ",1,24,24,139.74,139.74,139.74,139.74,139.74,139.74,139.74,139.74,139.74,139.74,139.74,139.74]
["COLGNS_2_CNSSR1",null,"ColGreen North Shore ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","IID","South",null,null,1,74.8,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.1,0.22,24.56,31.75,49.22,42.48,2.2799999999999998,0.1,0.1,0.1]
["COLPIN_6_COLLNS",null,"Collins Pine",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,3.3,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["COLTON_6_AGUAM1",null,"AGUA MANSA UNIT 1 (CITY OF COLTON)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,43,null,"FC","","",null," "," "," "," ",1,24,24,43,43,43,43,43,43,43,43,43,43,43,43]
["COLUSA_2_PL1X3",null,"Colusa Generating Station",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,641,null,"FC","","",null," "," "," "," ",1,24,24,630,630,630,630,618,612,606,604,607,614,623,628]
["COLVIL_7_PL1X2",null,"COLLIERVILLE HYDRO UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,246.86,null,"FC","","",null," "," "," "," ",1,24,24,118.42,131.08000000000001,167.91,175.32,162.59,130,124.42,129.06,102.46,79.680000000000007,95.28,130.08000000000001]
["CONTRL_1_CASAD1",null,"Mammoth G1",null,"OTHER","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,7.2,null,"FC","","",null," "," "," "," ",1,24,24,6.97,7.2,6.97,6.85,6.73,5.74,5.0999999999999996,5.35,5.53,5.64,6.99,6.64]
["CONTRL_1_CASAD2",null,"Mammoth G2",null,"OTHER","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,1,10.5,null,"FC","","",null," "," "," "," ",1,24,24,10.11,9.9700000000000006,9.4499999999999993,8.35,8.6300000000000008,8.23,9.41,9.2799999999999994,9.17,9.16,9.99,10.199999999999999]
["CONTRL_1_CASAD3",null,"Mammoth G3",null,"OTHER","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,14,null,"FC","","",null," "," "," "," ",1,24,24,12.35,12.89,13.08,12.43,11.48,9.69,8.75,9.02,9.8800000000000008,10.72,12.99,13.07]
["CONTRL_1_LUNDY",null,"LUNDY",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.33,0.32,0.35,0.37,1.06,1.54,1.1000000000000001,0.39,0.28000000000000003,0.16,0.41,0.32]
["CONTRL_1_OXBOW",null,"Dixie Valley Geo",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,null,60,null,"FC","","",null," "," "," "," ",1,24,24,59.46,57.37,57.75,43.02,46.29,55.03,54.04,53.91,54.61,46.22,59.38,58.79]
["CONTRL_1_POOLE",null,"POOLE HYDRO PLANT 1",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,1,10.9,null,"FC","","",null," "," "," "," ",1,24,24,0.96,0.8,0.48,0.76,1.6,8.27,5.42,1.46,10.9,0.31,0.48,0.8]
["CONTRL_1_QF",null,"CONTROL QFS",null,"OTHER","CHP","OTHER","CISO","South","CAISO System",null,null,2.5499999999999998,null,"FC","","",null," "," "," "," ",1,24,24,0.56000000000000005,0.6,0.59,0.84,0.56999999999999995,0.67,0.64,0.59,0.66,0.53,0.56000000000000005,0.53]
["CONTRL_1_RUSHCK",null,"RUSH CREEK",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,1,11.94,null,"FC","","",null," "," "," "," ",1,24,24,0.8,0.82,4.82,0.82,0.8,9.4499999999999993,9.4600000000000009,1.82,11.94,1.01,0.97,0.8]
["COPMT2_2_SOLAR2",null,"CMS2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,155,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.1900000000000004,0.22,29.35,40.11,78.22,67.23,3.56,0.1,0.1,0.1]
["COPMT4_2_SOLAR4",null,"Copper Mountain Solar 4",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,92,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.4900000000000002,0.13,17.420000000000002,23.81,46.43,39.9,2.11,0.1,0.1,0.1]
["COPMTN_2_CM10",null,"Copper Mountain 10",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,10,null,"PD","",7.25,null," "," "," "," ",1,24,24,0.1,0.1,0.27,0.1,1.89,2.59,5.05,4.34,0.23,0.1,0.1,0.1]
["COPMTN_2_SOLAR1",null,"Copper Mountain 48",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,48,null,"PD","",16.5,null," "," "," "," ",1,24,24,0.1,0.1,1.3,0.1,9.09,12.42,16.5,16.5,1.1000000000000001,0.1,0.1,0.1]
["CORCAN_1_SOLAR1",null,"CID Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Hanford",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["CORCAN_1_SOLAR2",null,"Corcoran City",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon, Hanford",null,11,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.33,0.11,4.8099999999999996,6.03,8.2100000000000009,6.9,0.56999999999999995,0.1,0.1,0.1]
["CORONS_2_SOLAR",null,"Master Development Corona",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,0.99,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CORONS_6_CLRWTR",null,"Clearwater Power Plant",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Eastern",1,28,null,"FC","","",null," "," "," "," ",1,24,24,28,28,28,28,28,28,28,28,28,28,28,28]
["CORRAL_6_SJOAQN",null,"Ameresco San Joaquin",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,4.3,null,"FC","","",null," "," "," "," ",1,24,24,4.26,4.0999999999999996,4.3,4.2,4.2699999999999996,4.26,4.21,3.91,3.97,4.17,4.24,4.3]
["COTTLE_2_FRNKNH",null,"Frankenheimer Power Plant",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,5.3,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0.72,0.61,0,0,0]
["COVERD_2_HCKHY1",null,"HATCHET CREEK",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,6.89,null,"FC","","",null," "," "," "," ",1,24,24,1.77,1.66,1.39,2.5299999999999998,1.57,0.24,0,0,0,0.14000000000000001,0.09,0.41]
["COVERD_2_MCKHY1",null,"Montgomery Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,2.8,null,"FC","","",null," "," "," "," ",1,24,24,1.1499999999999999,0.81,0.85,0.98,0.54,0.09,0,0,0,0.08,0,0.62]
["COVERD_2_QFUNTS",null,"Cove Hydroelectric Project",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,5.5,null,"FC","","",null," "," "," "," ",1,24,24,0.78,1.58,1.66,3.3,3.3,0.8,0.22,0,0,0,0,0.24]
["COVERD_2_RCKHY1",null,"ROARING CREEK",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,1.01,1.07,0.22,0.49,0.18,0.15,0.01,0,0,0.04,0.09,0.27]
["COWCRK_2_UNIT",null,"Cow Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.69,0.93,0.75,0.87,0.57999999999999996,0.41,0.19,0.1,0.09,0.17,0.55000000000000004,0.82]
["CPVERD_2_SOLAR",null,"Campo Verde Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,139,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.76,0.2,26.32,35.97,70.14,60.29,3.2,0.1,0.1,0.1]
["CRELMN_6_RAMON1",null,"Ramona 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.38,0.52,1.01,0.87,0.1,0.1,0.1,0.1]
["CRELMN_6_RAMON2",null,"Ramona 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,0.95,1.29,2.52,2.17,0.11,0.1,0.1,0.1]
["CRELMN_6_RAMSR3",null,"Ramona Solar Energy",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV","San Diego",null,4.32,null,"PD",0.8,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,1.1299999999999999,1.47,2.27,1.96,0.11,0.1,0.1,0.1]
["CRESSY_1_PARKER",null,"PARKER POWERHOUSE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,2.83,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0.01,0.33,0.8,0.9,0.92,1.03,0.51,0.28000000000000003,0,0]
["CRESTA_7_PL1X2",null,"CRESTA PH UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,70.400000000000006,null,"FC","",22.06,null," "," "," "," ",1,24,24,22.06,22.06,22.06,22.06,22.06,22.06,22.06,22.06,22.06,22.06,15.7,22.06]
["CRIMSN_2_CRMBT1",null,"Crimson",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,1,200,null,"ID",1,"",null,1,0.8,800,800,1,24,4,200,200,200,200,200,200,200,200,200,200,200,200]
["CRIMSN_2_CRMBT2",null,"Crimson 2",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,1,150,null,"ID",1,"",null,1,0.8,600,600,1,24,4,150,150,150,150,150,150,150,150,150,150,150,150]
["CRNEVL_6_CRNVA",null,"Crane Valley ",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,0.9,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0.11,0.37,0.16,0.12]
["CRNEVL_6_SJQN 2",null,"SAN JOAQUIN 2",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,3.2,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0.01,0,0.28000000000000003,0.35]
["CROKET_7_UNIT",null,"CROCKETT COGEN",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,240,null,"FC","","",null," "," "," "," ",1,24,24,217.11,217.33,145.94999999999999,226.42,223.9,225.62,221.95,223,215.29,218.19,211.4,206.77]
["CRSTWD_6_KUMYAY",null,"Kumeyaay Wind Farm",null,"WIND","Wind","WIND","CISO","South","San Diego-IV","San Diego",null,50,null,"FC","","",null," "," "," "," ",1,24,24,2.73,5.88,6.35,20.170000000000002,21.5,18.96,16.66,14.59,10,4.68,2.16,2.2999999999999998]
["CRWCKS_1_SOLAR1",null,"Crow Creek Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Stockton","Tesla-Bellota",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CSCCOG_1_UNIT 1",null,"SANTA CLARA CO-GEN",null,"FTUR","CHP","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",1,7,null,"FC","","",null," "," "," "," ",1,24,24,6,6,6,6,6,6,6,6,6,6,6,6]
["CSCGNR_1_UNIT 1",null,"GIANERA PEAKER UNIT 1",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",1,24.75,null,"FC","","",null," "," "," "," ",1,24,24,24,24,24,24,24,24,24,24,24,24,24,24]
["CSCGNR_1_UNIT 2",null,"GIANERA PEAKER UNIT 2",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",1,24.75,null,"FC","","",null," "," "," "," ",1,24,24,24,24,24,24,24,24,24,24,24,24,24,24]
["CSLR4S_2_SOLAR",null,"Csolar IV South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,130,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.52,0.19,24.62,33.64,65.599999999999994,56.39,2.99,0.1,0.1,0.1]
["CSTOGA_6_LNDFIL",null,"Clover Flat Land Fill Gas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","NCNB","Fulton",null,0.85,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CSTRVL_7_PL1X2",null,"Marina Land Fill Gas",null,"RECIPROCATING ENGINE","Biogas","OTHER","CISO","North","CAISO System",null,1,4.53,null,"FC","","",null," "," "," "," ",1,24,24,4.13,3.51,3.69,4.01,3.63,3.95,4.16,4.1399999999999997,4.17,3.86,3.98,3.73]
["CSTRVL_7_QFUNTS",null,"Castroville QF Aggregate",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.04,0.06,0.15,7.0000000000000007E-2,0.04,0.08,7.0000000000000007E-2,0.09,0.09,7.0000000000000007E-2,0.05,0.03]
["CTNWDP_1_QF",null,"SMALL QF AGGREGATION - BURNEY",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.5,null,"FC","","",null," "," "," "," ",1,24,24,0.04,0.04,0.04,0.04,0.03,0.03,0.02,0.02,0.01,0.02,0.03,0.04]
["CUMBIA_1_SOLAR",null,"Columbia Solar Energy II",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Bay Area","Pittsburg",null,19,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.57999999999999996,0.2,8.3000000000000007,10.41,14.19,11.91,0.99,0.1,0.1,0.1]
["CUMMNG_6_SUNCT1",null,"SunSelect 1",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","South","CAISO System",null,1,4,null,"FC","","",null," "," "," "," ",1,24,24,3.33,3.39,3.04,3.01,3.34,3.54,3.53,3.56,3.4,3.16,3.38,3.45]
["CURTIS_1_CANLCK",null,"Canal Creek Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,0.9,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["CURTIS_1_FARFLD",null,"Fairfield Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,0.9,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0.01,0.24,0.31,0.26,0.28000000000000003,0.08,0,0,0]
["CUYAMA_6_SB3SB1","CUYAMA_6_SB3SB1_SUN","SEPV Barbara 3",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,null,3,3,"ID","","",null,null,null,null,null,1,24,24,null,0.1,0.1,0.09,0.03,1.31,2.2400000000000002,1.88,0.16,0.16,0.1,0.1]
["CUYAMA_6_SB3SB1","CUYAMA_6_SB3SB1_LESR","SEPV Barbara 3",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,null,3,3,"ID","","",false,null,0.8,null,null,1,24,24,null,3,3,3,3,3,3,3,3,3,3,3]
["CUYAMS_6_CUYSR1",null,"Cuyama Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,40,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.22,0.41,17.48,21.91,29.87,25.08,2.09,0.1,0.1,0.1]
["DAIRLD_1_MD1SL1",null,"Madera 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DAIRLD_1_MD2BM1",null,"Madera Digester Genset 2",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,null,0.8,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DAVIS_1_SOLAR1",null,"Grasslands 3",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DAVIS_1_SOLAR2",null,"Grasslands 4",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DAVIS_7_MNMETH",null,"MM Yolo Power LLC",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,4,null,"FC","","",null," "," "," "," ",1,24,24,2.14,2.4,2.42,2.4,1.94,2.0099999999999998,2,2.2599999999999998,2.3199999999999998,2.39,2.37,2.2400000000000002]
["DEADCK_1_UNIT",null,"DEADCK_1_UNIT",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",null,1.96,null,"FC","","",null," "," "," "," ",1,24,24,7.0000000000000007E-2,0.05,0.08,0.15,0,0.06,0,0,0,0,0,0]
["DEERCR_6_UNIT 1",null,"DEER CREEK",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,7,null,"FC","","",null," "," "," "," ",1,24,24,1.2,1.26,0.73,0.76,2.63,3.17,3.25,3.41,3.3,2.66,1.5,1.29]
["DELAMO_2_ALASB2","DELAMO_2_ALASB2_SUN","Los Alamitos 2",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","LA Basin",null,null,10,10,"FC","","",null,null,null,null,null,1,24,24,0.1,0.1,0.28000000000000003,0.03,3.28,4.24,6.58,5.68,0.3,0.1,0.1,0.1]
["DELAMO_2_ALASB2","DELAMO_2_ALASB2_LESR","Los Alamitos 2",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","LA Basin",null,null,10,10,"FC","","",false,1,0.8,20,20,1,24,24,5,5,5,5,5,5,5,5,5,5,5,5]
["DELAMO_2_SOLAR1",null,"Golden Springs Building H",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.49,0.64,0.99,0.85,0.1,0.1,0.1,0.1]
["DELAMO_2_SOLAR2",null,"Golden Springs Building M",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,1.75,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.56999999999999995,0.74,1.1499999999999999,0.99,0.1,0.1,0.1,0.1]
["DELAMO_2_SOLAR3",null,"Golden Springs Building G",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,1.25,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.41,0.53,0.82,0.71,0.1,0.1,0.1,0.1]
["DELAMO_2_SOLAR4",null,"Golden Springs Building F",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,1.3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.43,0.55000000000000004,0.86,0.74,0.1,0.1,0.1,0.1]
["DELAMO_2_SOLAR5",null,"Golden Springs Building L",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.33,0.42,0.66,0.56999999999999995,0.1,0.1,0.1,0.1]
["DELAMO_2_SOLAR6",null,"Freeway Springs",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Western",null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.66,0.85,1.32,1.1399999999999999,0.1,0.1,0.1,0.1]
["DELAMO_2_SOLRC1",null,"Golden Springs Building C1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Western",null,1.1599999999999999,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DELAMO_2_SOLRD",null,"Golden Solar Building D",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Western",null,1.25,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DELSUR_6_BSOLAR",null,"Central Antelope Dry Ranch B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["DELSUR_6_CREST",null,"Delsur Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,12,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DELSUR_6_DRYFRB",null,"Dry Farm Ranch B ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,1.64,2.12,3.29,2.84,0.15,0.1,0.1,0.1]
["DELSUR_6_SOLAR1",null,"Summer Solar North ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,6.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.18,0.1,2.13,2.76,4.28,3.69,0.2,0.1,0.1,0.1]
["DELSUR_6_SOLAR4",null,"Radiance Solar 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DELSUR_6_SOLAR5",null,"Radiance Solar 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DELTA_2_PL1X4",null,"DELTA ENERGY CENTER AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Pittsburg",1,880,null,"FC","","",null," "," "," "," ",1,24,24,880,880,880,875,880,880,873,873,873,880,880,880]
["DEVERS_1_SEPV05",null,"SEPV 5",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,2,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DEVERS_1_SOLAR",null,"Cascade Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,18.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DEVERS_1_SOLAR1",null,"SEPV8",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,12,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DEVERS_1_SOLAR2",null,"SEPV9",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,9,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DEVERS_2_CS2SR4",null,"Caliente Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,0.91,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DEVERS_2_DHSPG2",null,"Desert Hot Springs 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,1.4,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["DEXZEL_1_UNIT",null,"Western Power and Steam Cogeneration",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",1,20,null,"FC","","",null," "," "," "," ",1,24,24,20,20,20,20,20,20,20,20,20,20,20,20]
["DIABLO_7_UNIT 1",null,"Diablo Canyon Unit 1",null,"STEAM","Nuclear","URANIUM","CISO","North","CAISO System",null,null,1150,null,"FC","","",null," "," "," "," ",1,24,24,1140,1140,1140,1140,1140,1140,1140,1140,1140,1140,1140,1140]
["DIABLO_7_UNIT 2",null,"Diablo Canyon Unit 2",null,"STEAM","Nuclear","URANIUM","CISO","North","CAISO System",null,null,1150,null,"FC","","",null," "," "," "," ",1,24,24,1140,1140,1140,1140,1140,1140,1140,1140,1140,1140,1140,1140]
["DISCOV_1_CHEVRN",null,"CHEVRON USA (EASTRIDGE)",null,"FTUR","CHP","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",null,48.8,null,"FC","","",null," "," "," "," ",1,24,24,4.7,7.04,5.36,4.58,4.9000000000000004,5.21,5.07,6.33,6.34,3.62,4.2,4.22]
["DIXNLD_1_LNDFL",null,"Zero Waste Energy",null,"RECIPROCATING ENGINE","Biomass","BIOMASS","CISO","North","Bay Area",null,null,1.6,null,"FC","","",null," "," "," "," ",1,24,24,0.72,0.67,0.75,0.84,0.81,0.84,0.87,0.87,0.88,0.89,0.87,0.86]
["DMDVLY_1_UNITS",null,"Diamond Valley Lake Pump Gen",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,21,null,"FC","","",null," "," "," "," ",1,24,24,1.6,5.28,0.84,0.88,2.5,0.95,0.24,0.6,0,0,0,0]
["DONNLS_7_UNIT",null,"Donnells Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",1,72,null,"FC","","",null," "," "," "," ",1,24,24,72,72,72,72,72,72,72,72,72,72,72,72]
["DOSMGO_2_NSPIN",null,"DOSMGO_2_NSPIN",null,"PUMP","Pump","WATER","CISO","North","CAISO System",null,1,159,null,"FC","","",null," "," "," "," ",1,24,24,16.260000000000002,16.260000000000002,16.260000000000002,16.260000000000002,15.21,16.260000000000002,16.260000000000002,16.260000000000002,16.260000000000002,13.64,16.260000000000002,16.260000000000002]
["DOUBLC_1_UNITS",null,"DOUBLE \"C\" LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",1,52.23,null,"FC","","",null," "," "," "," ",1,24,24,52.23,52.23,52.23,52.23,52.23,52.23,52.23,52.23,52.23,52.23,52.23,52.23]
["DRACKR_2_D4SR4B",null,"Dracker Solar Unit 4B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,62.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.75,0.18,20.52,26.53,41.12,35.5,1.9,0.1,0.1,0.1]
["DRACKR_2_DS3SR3",null,"Dracker Solar Unit 3","DRACKR_2_DSUBT3","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,null,125,125,"EO","","",null," "," "," "," ",1,24,24,0.1,0.1,3.38,0.18,23.67,32.35,63.08,54.22,2.87,0.05,0.1,0.1]
["DRACKR_2_DS4SR4",null,"Dracker Solar Unit 4A","DRACKR_2_DSUBT4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,62.5,62.5,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.75,0.18,20.52,26.53,41.12,35.5,1.9,0.1,0.1,0.1]
["DRACKR_2_DSUBT1",null,"Dracker Solar Unit 1 BESS","DRACKR_2_SOLAR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,3,63,110,"FC","","",false,1,0.8,252,252,1,24,4,63,63,63,63,63,63,63,63,63,63,63,63]
["DRACKR_2_DSUBT2",null,"Dracker Solar Unit 2 BESS","DRACKR_2_SOLAR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,115,125,"FC","","",false,2.843766438716465,0.90100000000000002,460,1308.1325618095739,1,24,11.37506575486586,115,115,115,115,115,115,115,115,115,115,115,115]
["DRACKR_2_DSUBT3",null,"Dracker Solar Unit 3 BESS","DRACKR_2_DS3SR3","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,115,125,"FC","","",true,2.8487394957983194,0.90400000000000003,460,1310.420168067227,1,24,11.394957983193278,115,115,115,115,115,115,115,115,115,115,115,101.05]
["DRACKR_2_DSUBT4",null,"Dracker Solar Unit 4 BESS","DRACKR_2_DS4SR4","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,47,62.5,"FC","","",false,1,0.86,188,188,1,24,4,47,47,47,47,47,47,47,47,47,47,47,47]
["DRACKR_2_SOLAR1",null,"Dracker Solar Unit 1","DRACKR_2_DSUBT1","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,null,110,110,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.97,0.16,20.83,28.47,55.51,47.71,2.5299999999999998,0.1,0.1,0.1]
["DRACKR_2_SOLAR2",null,"Dracker Solar Unit 2","DRACKR_2_DSUBT2","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,null,125,125,"EO","","",null," "," "," "," ",1,24,24,0.1,0.1,3.38,0.18,23.67,32.35,63.08,54.22,2.87,0.05,0.1,0.1]
["DREWS_6_PL1X4",null,"Drews Generating Plant",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,41.4,null,"FC","","",null," "," "," "," ",1,24,24,40,40,40,40,40,40,40,40,40,40,40,40]
["DRUM_7_PL1X2",null,"Drum PH 1 Units 1 & 2 Aggregate",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",1,26,null,"FC","","",null," "," "," "," ",1,24,24,9.6,0,0,0,0,0,10.4,10.4,0,0,9.6,10.4]
["DRUM_7_PL3X4",null,"Drum PH 1 Units 3 & 4 Aggregate",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",1,28.9,null,"FC","","",null," "," "," "," ",1,24,24,12.8,0,0,0,12.8,12.8,12.8,12.8,0,0,12.8,12.8]
["DRUM_7_UNIT 5",null,"DRUM PH 2 UNIT 5",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",1,50,null,"FC","","",null," "," "," "," ",1,24,24,39.200000000000003,44.24,43.6,38.799999999999997,41.74,39.200000000000003,48.1,47.74,27.28,0,36,44.06]
["DSABLA_7_UNIT",null,"De Sabla Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,18.5,null,"FC","","",null," "," "," "," ",1,24,24,5.85,6.81,6.42,4.13,5.7,6.4,7.32,5.87,3.26,2.0499999999999998,3.09,3.85]
["DSFLWR_2_W9CSB1",null,"Willy 9 Chap 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,102,null,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,2.86,0.3,33.49,43.29,67.11,57.93,3.11,0.1,0.1,0.1]
["DSFLWR_2_W9CSB2",null,"Willy 9 Chap 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,72,null,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,2.02,0.21,23.64,30.56,47.37,40.89,2.19,0.1,0.1,0.1]
["DSFLWR_2_WS2SR1",null,"Willow Springs 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["DSRTHV_2_DH1SR1",null,"Desert Harvest",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,80,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.2400000000000002,0.24,26.26,33.950000000000003,52.64,45.43,2.44,0.1,0.1,0.1]
["DSRTHV_2_DH2BT1",null,"Desert Harvest BESS","DSRTHV_2_DH2SR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,35,70,"PD","",35,false,1,0.8,140,140,1,24,4,35,35,35,35,35,35,35,35,35,35,35,35]
["DSRTHV_2_DH2SR2",null,"Desert Harvest 2","DSRTHV_2_DH2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,70,70,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.96,0.21,22.98,29.71,46.06,39.75,2.13,0.1,0.1,0.1]
["DSRTSL_2_SOLAR1",null,"Desert Stateline",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,296.19,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,8.31,0.87,97.24,125.71,194.89,168.21,9.02,0.1,0.1,0.1]
["DSRTSN_2_DS2BX2",null,"Berry Cogen 18",null,"FTUR","Battery Storage","NATURAL GAS","CISO","South","CAISO System",null,1,17,null,"PD",0.94699999999999995,"",null,null,0.8,null,null,1,24,24,null,null,null,null,217.81,217.81,217.81,217.81,217.81,217.81,217.81,217.81]
["DSRTSN_2_DS2X2",null,"Desert Sunlight PV II Storage","DSRTSN_2_SOLAR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,230,250,"FC","","",false,2.7828418230563003,0.86499999999999999,920,2560.2144772117963,1,24,11.131367292225201,230,230,230,230,230,230,230,230,230,230,230,230]
["DSRTSN_2_SOLAR1",null,"Desert Sunlight 300",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,300,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,8.11,0.43,56.81,77.64,151.38999999999999,130.12,6.9,0.12,0.1,0.1]
["DSRTSN_2_SOLAR2",null,"Desert Sunlight 250","DSRTSN_2_DS2X2","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,null,250,250,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,6.76,0.36,47.34,64.7,126.16,108.43,5.75,0.1,0.1,0.1]
["DTCHWD_2_BT3WND",null,"Brookfield Tehachapi 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,4.5,null,"FC","","",null," "," "," "," ",1,24,24,0.25,0.53,0.56999999999999995,1.82,1.94,1.71,1.5,1.31,0.9,0.42,0.19,0.21]
["DTCHWD_2_BT4WND",null,"Brookfield Tehachapi 4",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,6.52,null,"FC","","",null," "," "," "," ",1,24,24,0.36,0.77,0.83,2.63,2.8,2.4700000000000002,2.17,1.9,1.3,0.61,0.28000000000000003,0.3]
["DUANE_1_PL1X3",null,"DONALD VON RAESFELD POWER PROJECT",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",1,147.80000000000001,null,"FC","","",null," "," "," "," ",1,24,24,147.80000000000001,147.80000000000001,147.80000000000001,147.80000000000001,143.5,143.5,143.5,143.5,143.5,147.80000000000001,147.80000000000001,147.80000000000001]
["DURNMESA_3_WBDYN",null,"DURAN MESA",null,"WIND","Wind","WIND","PNM","South",null,null,1,105.08,null,"FC","","",null," "," "," "," ",1,24,24,50.57,43.63,35.700000000000003,42.64,39.67,31.73,21.78,20.82,23.8,24.79,39.67,55.53]
["DUTCH1_7_UNIT 1",null,"DUTCH FLAT 1 PH",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",1,22,null,"FC","","",null," "," "," "," ",1,24,24,17.600000000000001,17.600000000000001,6.8,16.8,15.2,17.2,19.28,20.78,12.8,9.6,17.600000000000001,20.2]
["DUTCH2_7_UNIT 1",null,"DUTCH FLAT 2 PH",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",1,26,null,"FC","","",null," "," "," "," ",1,24,24,5.2,16,17.2,5.6,5.6,5.6,16,16.760000000000002,0,0,2.8,5.6]
["DVLCYN_1_UNITS",null,"DEVIL CANYON HYDRO UNITS 1-4 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",1,235,null,"FC","","",null," "," "," "," ",1,24,24,146.91,82.76,106.43,145.35,134.52000000000001,146.86000000000001,134.22,140.09,138.61000000000001,137.34,146.49,132.69999999999999]
["DYERSM_6_DSWWD1",null,"Dyer Summit Wind Repower",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,44.8,null,"FC","","",null," "," "," "," ",1,24,24,1.9,3.28,4.42,13.69,21.54,13.76,17.64,9.64,3.32,0.81,1.27,1.92]
["EASTWD_7_UNIT",null,"EASTWOOD PUMP-GEN",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",1,200,null,"FC","","",null," "," "," "," ",1,24,24,199,199,199,199,199,199,199,199,199,199,199,199]
["EDMONS_2_NSPIN",null,"EDMONS_2_NSPIN",null,"PUMP","Pump","WATER","CISO","South","Big Creek-Ventura",null,1,775.8,null,"FC","","",null," "," "," "," ",1,24,24,236,236,236,236,236,236,236,236,236,236,236,236]
["EDWARD_2_E21SB1","EDWARD_2_E21SB1_SUN","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,2,130,166,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3.65,0.38,42.68,55.18,85.54,73.83,3.96,0.1,0.1,0.1]
["EDWARD_2_E21SB1","EDWARD_2_E21SB1_LESR","EdSan 2 Edwards 1A",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,71,166,"ID",1,"",false,1,0.8,284,284,1,24,4,71,71,71,71,71,71,71,71,71,71,71,71]
["EDWARD_2_E23SB1","EDWARD_2_E23SB1_SUN","EdSan 2 Edwards 3",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,2,24,24,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.67,0.1,7.88,10.19,15.79,13.63,0.73,0.1,0.1,0.1]
["EDWARD_2_E23SB1","EDWARD_2_E23SB1_LESR","EdSan 2 Edwards 3",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,6,24,"ID",1,"",false,1,0.8,24,24,1,24,4,6,6,6,6,6,6,6,6,6,6,6,6]
["EDWARD_2_ES2BT3","EDWARD_2_ES2BT3_SUN","EdSan 2",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","South","CAISO System",null,2,118,151,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3.31,0.35,38.74,50.08,77.64,67.02,3.59,0.1,0.1,0.1]
["EDWARD_2_ES2BT3","EDWARD_2_ES2BT3_LESR","EdSan 2",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,66,151,"ID",1,"",false,1,0.8,264,264,1,24,4,66,66,66,66,66,66,66,66,66,66,66,66]
["EDWARD_2_ESSSB1",null,"Sanborn Solar 2 Edwards 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,116,null,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.25,0.34,38.08,49.23,76.33,65.88,3.53,0.1,0.1,0.1]
["EDWARD_2_ESSSB2",null,"Sanborn Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,1,132,null,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.7,0.39,43.34,56.02,86.85,74.97,4.0199999999999996,0.1,0.1,0.1]
["EEKTMN_6_SOLAR1",null,"EE K Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ELCABO_5_ECWSCEDYN",null,"El Cabo Wind",null,"WIND","Wind","WIND","AZPS","South",null,null,1,298,null,"FC","","",null," "," "," "," ",1,24,24,59.78,63.25,59.78,87.32,65.56,49.31,29.8,17.88,34.700000000000003,20.190000000000001,30.7,44.88]
["ELCAJN_6_EB1BT1",null,"Eastern BESS 1",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego, El Cajon",1,7.5,null,"FC","","",null,1,0.8,30,30,1,24,4,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5]
["ELCAJN_6_LM6K",null,"El Cajon Energy Center",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, El Cajon",1,48.1,null,"FC","","",null," "," "," "," ",1,24,24,48.1,48.1,48.1,48.1,48.1,48.1,48.1,48.1,48.1,48.1,48.1,48.1]
["ELCAJN_6_UNITA1",null,"Cuyamaca Peak Energy Plant",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, El Cajon",1,45.42,null,"FC","","",null," "," "," "," ",1,24,24,45.42,45.42,45.42,45.42,45.42,45.42,45.42,45.42,45.42,45.42,45.42,45.42]
["ELCAP_1_SOLAR",null,"2097 Helton",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ELDORO_7_UNIT 1",null,"El Dorado Unit 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Gold Hill-Drum, South of Rio Oso, South of Palermo",null,11,null,"FC","","",null," "," "," "," ",1,24,24,2.2799999999999998,3.32,2.76,5.08,7.4,4.29,4.3899999999999997,4.0999999999999996,5.44,0.14000000000000001,0,0]
["ELDORO_7_UNIT 2",null,"El Dorado Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Gold Hill-Drum, South of Rio Oso, South of Palermo",null,11,null,"FC","","",null," "," "," "," ",1,24,24,4.82,3.61,1.1599999999999999,4.93,7.78,4.33,2.04,5.19,3.49,0.14000000000000001,0,0]
["ELECTR_7_PL1X3",null,"ELECTRA PH UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,93,null,"FC","","",null," "," "," "," ",1,24,24,49.6,48,50.76,25.4,48.6,55.9,50.88,61.83,63.68,50.9,52.8,55.6]
["ELKCRK_6_STONYG",null,"STONEY GORGE HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,4.9000000000000004,null,"FC","","",null," "," "," "," ",1,24,24,0,0,1.2,1.6,1.28,1.1200000000000001,0,0,0,0,0,0]
["ELKHIL_2_PL1X3",null,"ELK HILLS COMBINED CYCLE (AGGREGATE)",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,551.70000000000005,null,"FC","","",null," "," "," "," ",1,24,24,400,400,400,400,400,400,400,400,400,400,400,400]
["ELKHRN_1_EESX3",null,"Elkhorn Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",1,182.5,null,"FC","","",null,1,0.8,730,730,1,24,4,182.5,182.5,182.5,182.5,182.5,182.5,182.5,182.5,182.5,182.5,182.5,182.5]
["ELLIOT_6_ELIBT1",null,"SMALL QF AGGREGATION - PARADISE",null,"HYDRO","Battery Storage","WATER","CISO","South","San Diego-IV",null,null,1.7,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,9.75,9.75,9.75,9.75,9.75,9.75,9.75,9.75,9.75]
["ELLIS_2_QF",null,"ELLIS QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Western",null,12,null,"FC","","",null," "," "," "," ",1,24,24,2.08,2.23,1.7,1.97,1.92,2.2000000000000002,1.6,0.76,1,1,1.01,0.98]
["ELSEGN_2_UN1011",null,"El Segundo Energy Center 5/6",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western, El Nido",1,274.31,null,"FC","","",null," "," "," "," ",1,24,24,274.31,274.31,274.31,274.31,274.31,274.31,274.31,274.31,274.31,274.31,274.31,274.31]
["ELSEGN_2_UN2021",null,"El Segundo Energy Center 7/8",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western, El Nido",1,271.74,null,"FC","","",null," "," "," "," ",1,24,24,271.74,271.74,271.74,271.74,271.74,271.74,271.74,271.74,271.74,271.74,271.74,271.74]
["ENERSJ_2_WIND",null,"ESJ Wind Energy",null,"WIND","Wind","WIND","CISO","South","San Diego-IV",null,null,151,null,"FC","","",null," "," "," "," ",1,24,24,8.23,17.760000000000002,19.190000000000001,60.93,64.94,57.25,50.32,44.06,30.21,14.13,6.53,6.93]
["ENERSJ_5_ESJWD2",null,"Energia Sierra Juarez Wind 2",null,"WIND","Wind","WIND","CISO","South","San Diego-IV",null,null,105,null,"FC","","",null," "," "," "," ",1,24,24,5.72,12.35,13.34,42.37,45.15,39.81,34.99,30.64,21.01,9.83,4.54,4.82]
["ENWIND_2_WIND1",null,"Cameron Ridge",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,47.1,null,"FC","","",null," "," "," "," ",1,24,24,2.57,5.54,5.99,19,20.260000000000002,17.86,15.69,13.74,9.42,4.41,2.04,2.16]
["ENWIND_2_WIND2",null,"Ridgetop I",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,38.24,null,"FC","","",null," "," "," "," ",1,24,24,2.08,4.5,4.8600000000000003,15.43,16.440000000000001,14.5,12.74,11.16,7.65,3.58,1.65,1.76]
["ESCNDO_6_EB1BT1",null,"Escondido BESS 1",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["ESCNDO_6_EB2BT2",null,"Escondido BESS 2",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["ESCNDO_6_EB3BT3",null,"Escondido BESS 3",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["ESCNDO_6_PL1X2",null,"MMC Escondido Aggregate",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,48.71,null,"FC","","",null," "," "," "," ",1,24,24,48.71,48.71,48.71,48.71,48.71,48.71,48.71,48.71,48.71,48.71,48.71,48.71]
["ESCNDO_6_UNITB1",null,"CalPeak Power Enterprise Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,48.04,null,"FC","","",null," "," "," "," ",1,24,24,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04,48.04]
["ESCO_6_GLMQF",null,"Goal Line Cogen",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,49.9,null,"FC","","",null," "," "," "," ",1,24,24,49.9,49.9,49.9,49.9,49.9,49.9,49.9,49.9,49.9,49.9,49.9,49.9]
["ESNHWR_2_WC1BT1",null,"Wildcat I BESS",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern, Valley-Devers",3,3,null,"ID",1,"",null,1,0.8,6,6,1,24,2,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["ESQUON_6_LNDFIL",null,"Neal Road Landfill Generating Facility",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,2.1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ESTWND_2_OPPWD1",null,"Oasis Power Plant Eastwind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,57.14,null,"FC","","",null," "," "," "," ",1,24,24,3.11,6.72,7.26,23.05,24.57,21.66,19.04,16.670000000000002,11.43,5.35,2.4700000000000002,2.62]
["ETIWND_2_CHMPNE",null,"Champagne",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ETIWND_2_FONTNA",null,"FONTANALYTLE CREEK POWERHOUSE P",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,2.56,null,"FC","","",null," "," "," "," ",1,24,24,0.94,1.02,0.53,0.78,0.78,0.56999999999999995,0.5,0.38,0.42,0.46,0.59,0.56999999999999995]
["ETIWND_2_SOLAR1",null,"Dedeaux Ontario",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.33,0.42,0.66,0.56999999999999995,0.1,0.1,0.1,0.1]
["ETIWND_2_SOLAR2",null,"Rochester",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ETIWND_2_SOLAR5",null,"Dulles",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,2,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["ETIWND_2_UNIT1",null,"ETIWND_2_UNIT1",null,"FTUR","CHP","NATURAL GAS","CISO","South","LA Basin","Eastern",1,33.6,null,"FC","","",null," "," "," "," ",1,24,24,33.6,33.6,33.6,33.6,33.6,33.6,33.6,33.6,33.6,33.6,33.6,33.6]
["ETIWND_6_GRPLND",null,"Grapeland Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,45.64,null,"FC","","",null," "," "," ",407.7,1,24,8.9329535495179666,45.64,45.64,45.64,45.64,45.64,45.64,45.64,45.64,45.64,45.64,45.64,45.64]
["ETIWND_6_MWDETI",null,"ETIWANDA RECOVERY HYDRO",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,24,null,"FC","","",null," "," "," "," ",1,24,24,1.21,2.98,0,0,0,0,0,0,0,0,0,0]
["EXCHEC_7_UNIT 1",null,"EXCHEQUER HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",1,94.5,null,"FC",0,"",null," "," "," "," ",1,24,24,94.5,94.5,94.5,94.5,94.5,94.5,94.5,94.5,94.5,94.5,94.5,94.5]
["EXCLSG_1_SOLAR",null,"Excelsior Solar ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV",null,60,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.83,0.62,26.22,32.869999999999997,44.8,37.619999999999997,3.13,0.1,0.1,0.1]
["FALBRK_6_FESBT1",null,"Fallbrook Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV",null,1,40,null,"FC","","",null,1,0.8,160,160,1,24,4,40,40,40,40,40,40,40,40,40,40,40,40]
["FELLOW_7_QFUNTS",null,"Fellow QF Aggregate",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,6.2,null,"FC","","",null," "," "," "," ",1,24,24,2.44,2.39,2.4300000000000002,2.42,2.73,2.7,2.58,2.6,2.76,2.82,2.78,2.82]
["FIFTHS_2_FSSBT",null,"Fifth Standard Battery","FIFTHS_2_FSSR1","OTHER","Battery Storage","LESR","CISO","North","CAISO System",null,2,137,null,"FC","","",null,1,0.8,548,548,1,24,4,137,137,137,137,137,137,137,137,137,137,137,137]
["FIFTHS_2_FSSR1",null,"TECOLOTE WIND","FIFTHS_2_FSSBT","WIND","Paired_Solar_1Axis","WIND","CISO","North","CAISO System",null,null,271.68,150,"PD",0.25,"",null,null,null,null,null,1,24,24,null,null,null,null,30.7,39.68,202.85,170.34,14.18,0.24,0.1,0.1]
["FLOWD_2_RT2WD2",null,"Ridgetop 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,27.39,null,"FC","","",null," "," "," "," ",1,24,24,1.49,3.22,3.48,11.05,11.78,10.38,9.1300000000000008,7.99,5.48,2.56,1.19,1.26]
["FLOWD_2_WIND1",null,"Cameron Ridge 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,11.9,null,"FC","","",null," "," "," "," ",1,24,24,0.65,1.4,1.51,4.8,5.12,4.51,3.97,3.47,2.38,1.1100000000000001,0.51,0.55000000000000004]
["FLOWD2_2_FPLWND",null,"DIABLO WINDS",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,18,null,"FC","","",null," "," "," "," ",1,24,24,0.76,1.32,1.77,5.5,8.65,5.53,7.09,3.87,1.34,0.32,0.51,0.77]
["FMEADO_6_HELLHL",null,"FMEADO_6_HELLHL",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,0.6,null,"FC","","",null," "," "," "," ",1,24,24,0.21,0.21,0.28000000000000003,0.39,0.12,0.47,0.44,0.4,0.24,0.23,0.21,0.19]
["FMEADO_7_UNIT",null,"FRENCH MEADOWS HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",1,16,null,"FC","","",null," "," "," "," ",1,24,24,16,16,16,16,16,16,16,16,16,16,16,16]
["FORBST_7_UNIT 1",null,"FORBESTOWN HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",1,37.5,null,"FC","","",null," "," "," "," ",1,24,24,35,30,30,30.25,30,30,30,36,30,30,30,30]
["FORKBU_6_UNIT",null,"Forks of Butte Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,14.3,null,"FC",0,"",null," "," "," "," ",1,24,24,6.93,7.31,7.08,9.1999999999999993,7.35,9.85,9.84,9.07,8.26,6.19,6.63,6.37]
["FRESHW_1_SOLAR1",null,"Corcoran 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["FRIANT_6_UNITS",null,"FRIANT DAM",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",null,25,null,"FC","","",null," "," "," "," ",1,24,24,3.74,2.68,1.36,1.72,3.8,7.65,7.09,4.13,2.57,2.31,0.59,1.67]
["FRNTBW_6_SOLAR1",null,"Frontier Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["FROGTN_1_UTICAA",null,"Angels Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,1.4,null,"FC","","",null," "," "," "," ",1,24,24,0.8,0.72,0.72,0.64,0.46,0.31,0.3,0.23,0.34,0.43,0,0.72]
["FROGTN_1_UTICAM",null,"Murphys Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,3.6,null,"FC","","",null," "," "," "," ",1,24,24,1.66,1.56,1.58,1.45,1.36,1.27,1.24,1.26,1.25,1.26,0,1.45]
["FTSWRD_6_TRFORK",null,"Three Forks Water Power Project",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,1.63,null,"PD",0.8,"",null," "," "," "," ",1,24,24,0.71,0.62,0.36,0.66,0.68,0.38,0.28000000000000003,0.14000000000000001,0.2,0.11,0.18,0.21]
["FTSWRD_7_QFUNTS",null,"FTSWRD_7_QFUNTS",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,1.6,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["FULTON_1_QF",null,"SMALL QF AGGREGATION - ZENIA",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Fulton",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.12,0.11,0.1,0.11,0.1,7.0000000000000007E-2,0.04,0.02,0.03,0.04,0.06,7.0000000000000007E-2]
["GALE_1_SR3SR3",null,"Sunray 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,13.8,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.39,0.1,4.53,5.86,9.08,7.84,0.42,0.1,0.1,0.1]
["GANSO_1_WSTBM1",null,"Weststar Dairy Biogas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GARLND_2_GARBT1",null,"Garland B BESS","GARLND_2_GASLR, GARLND_2_GASLRA","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,88,200,"FC","","",false,2.7590341921892723,0.85129999999999995,352,971.18003565062384,1,24,11.036136768757089,88,88,88,88,88,88,88,88,88,88,88,88]
["GARLND_2_GASLR",null,"Garland B","GARLND_2_GARBT1, GARLND_2_GASLRA","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","South","CAISO System",null,null,180,200,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.87,0.26,34.090000000000003,46.58,90.84,78.069999999999993,4.1399999999999997,0.1,0.1,0.1]
["GARLND_2_GASLRA",null,"Garland A","GARLND_2_GARBT1, GARLND_2_GASLR","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,200,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["GARNET_1_SOLAR",null,"North Palm Springs 4A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,4,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GARNET_1_SOLAR2",null,"Garnet Solar Power Generation Station 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley-Devers",null,4,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.11,0.1,1.31,1.7,2.63,2.27,0.12,0.1,0.1,0.1]
["GARNET_1_WIND",null,"GARNET WIND ENERGY CENTER",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,6.5,null,"FC","","",null," "," "," "," ",1,24,24,0.35,0.76,0.83,2.62,2.8,2.46,2.17,1.9,1.3,0.61,0.28000000000000003,0.3]
["GARNET_1_WINDS",null,"Garnet Winds Aggregation",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,22.5,null,"FC","","",null," "," "," "," ",1,24,24,1.23,2.65,2.86,9.08,9.68,8.5299999999999994,7.5,6.57,4.5,2.11,0.97,1.03]
["GARNET_1_WT3WND",null,"Wagner Wind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,6,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GARNET_2_COAWD2",null,"Coachella 2",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,10.8,null,"FC","","",null," "," "," "," ",1,24,24,0.59,1.27,1.37,4.3600000000000003,4.6399999999999997,4.09,3.6,3.15,2.16,1.01,0.47,0.5]
["GARNET_2_HYDRO",null,"Whitewater Hydro",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, Valley-Devers",null,1,null,"FC","","",null," "," "," "," ",1,24,24,7.0000000000000007E-2,0,0,0,0,0,0,0,0.08,0.27,0.24,0.54]
["GARNET_2_WIND1",null,"Phoenix",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,11.2,null,"FC","","",null," "," "," "," ",1,24,24,0.61,1.32,1.42,4.5199999999999996,4.82,4.25,3.73,3.27,2.2400000000000002,1.05,0.48,0.51]
["GARNET_2_WIND2",null,"Karen Avenue Wind Farm",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,11.7,null,"FC","","",null," "," "," "," ",1,24,24,0.64,1.38,1.49,4.72,5.03,4.4400000000000004,3.9,3.41,2.34,1.1000000000000001,0.51,0.54]
["GARNET_2_WIND3",null,"San Gorgonio East",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,12.6,null,"FC","","",null," "," "," "," ",1,24,24,0.69,1.48,1.6,5.08,5.42,4.78,4.2,3.68,2.52,1.18,0.55000000000000004,0.57999999999999996]
["GARNET_2_WIND4",null,"Windustries",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,9.8000000000000007,null,"FC","","",null," "," "," "," ",1,24,24,0.53,1.1499999999999999,1.25,3.95,4.21,3.72,3.27,2.86,1.96,0.92,0.42,0.45]
["GARNET_2_WIND5",null,"Eastwind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.16,0.35,0.38,1.21,1.29,1.1399999999999999,1,0.88,0.6,0.28000000000000003,0.13,0.14000000000000001]
["GASKW1_2_GW1SR1",null,"Gaskell West 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["GASKW1_2_GW2BT1",null,"Gaskell West 2 BESS","GASKW1_2_GW2SR1, GASKW1_2_GW2SR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,20,45,"ID",1,"",false,1,0.8,80,80,1,24,4,20,20,20,20,20,20,20,20,20,20,20,20]
["GASKW1_2_GW2SR1",null,"Gaskell West 2a","GASKW1_2_GW2BT1, GASKW1_2_GW2SR2","PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,16,45,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.45,0.1,5.25,6.79,10.53,9.09,0.49,0.1,0.1,0.1]
["GASKW1_2_GW2SR2",null,"Gaskell West 2b","GASKW1_2_GW2BT1, GASKW1_2_GW2SR1","PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,29,45,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.81,0.1,9.52,12.31,19.079999999999998,16.47,0.88,0.1,0.1,0.1]
["GASKW1_2_GW3SR1",null,"Gaskell West 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["GASKW1_2_GW4SR1",null,"Gaskell West 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["GASKW1_2_GW5SR1",null,"Gaskell West 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["GATES_2_SOLAR",null,"Gates Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["GATES_2_WSOLAR",null,"West Gates Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.32,0.1,3,3.64,6.04,5.19,0.53,0.1,0.1,0.1]
["GATEWY_2_GESBT1",null,"Gateway Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,250,null,"FC","","",null,1,0.8,700,700,1,24,4,175,175,175,175,175,175,175,175,175,175,175,175]
["GATWAY_2_PL1X3",null,"GATEWAY GENERATING STATION",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,585,null,"FC","","",null," "," "," "," ",1,24,24,546,548,545,531,519,504,494,500,504,519,538,546]
["GENESI_2_STG",null,"Genesis Station",null,"STEAM","Paired_Solar_Thermal","SUN","CISO","South","CAISO System",null,null,250,250,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.84,5.65,90.68,103.09,102.62,108.5,24.44,3.88,0.1,0.1]
["GEYS11_7_UNIT11",null,"GEYSERS UNIT 11 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",1,86.8,null,"FC","","",null," "," "," "," ",1,24,24,68,68,68,68,68,68,68,68,68,68,68,68]
["GEYS12_7_UNIT12",null,"GEYSERS UNIT 12 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",1,57,null,"FC","","",null," "," "," "," ",1,24,24,50,50,50,50,50,50,50,50,50,50,50,50]
["GEYS13_7_UNIT13",null,"GEYSERS UNIT 13 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,73,null,"FC","","",null," "," "," "," ",1,24,24,56,56,56,56,56,56,56,56,56,56,56,56]
["GEYS14_7_UNIT14",null,"GEYSERS UNIT 14 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",1,70,null,"FC","","",null," "," "," "," ",1,24,24,70,70,70,70,70,70,70,70,70,70,70,70]
["GEYS16_7_UNIT16",null,"GEYSERS UNIT 16 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",1,63,null,"FC","","",null," "," "," "," ",1,24,24,63,63,63,63,63,63,63,63,63,63,63,63]
["GEYS17_7_UNIT17",null,"GEYSERS UNIT 17 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",1,75.5,null,"FC","","",null," "," "," "," ",1,24,24,75.5,75.5,75.5,75.5,75.5,75.5,75.5,75.5,75.5,75.5,75.5,75.5]
["GEYS18_7_UNIT18",null,"GEYSERS UNIT 18 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,72,null,"FC","","",null," "," "," "," ",1,24,24,72,72,72,72,72,72,72,72,72,72,72,72]
["GEYS20_7_UNIT20",null,"GEYSERS UNIT 20 (HEALDSBURG)",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,50,50,50,50,50,50,50,50,50,50,50,50]
["GIFENS_6_BUGSL1",null,"Burford Giffen",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["GIFFEN_6_SOLAR",null,"Giffen Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon",null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.32,0.1,3,3.64,6.04,5.19,0.53,0.1,0.1,0.1]
["GIFFEN_6_SOLAR1",null,"Aspiration Solar G",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,9,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GILROY_1_UNIT",null,"GILROY COGEN AGGREGATE",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","North","Bay Area","Llagas, San Jose, South Bay-Moss Landing",1,120,null,"FC","","",null," "," "," "," ",1,24,24,120,120,120,120,115,115,115,115,115,120,120,120]
["GILRPP_1_PL1X2",null,"GILROY ENERGY CENTER UNITS 1&2 AGGREGATE",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Llagas, San Jose, South Bay-Moss Landing",1,95.2,null,"FC","","",null," "," "," "," ",1,24,24,95.2,95.2,95.2,95.2,95.2,95.2,95.2,95.2,95.2,95.2,95.2,95.2]
["GILRPP_1_PL3X4",null,"GILROY ENERGY CENTER, UNIT #3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Llagas, San Jose, South Bay-Moss Landing",1,46.2,null,"FC","","",null," "," "," "," ",1,24,24,46.2,46.2,46.2,46.2,46.2,46.2,46.2,46.2,46.2,46.2,46.2,46.2]
["GLDFGR_6_SOLAR1",null,"Portal Ridge B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["GLDFGR_6_SOLAR2",null,"Portal Ridge C",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,11.4,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.32,0.1,3.74,4.84,7.5,6.47,0.35,0.1,0.1,0.1]
["GLDTWN_6_COLUM3",null,"Columbia 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.28000000000000003,0.1,3.28,4.24,6.58,5.68,0.3,0.1,0.1,0.1]
["GLDTWN_6_SOLAR",null,"Rio Grande",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,1.64,2.12,3.29,2.84,0.15,0.1,0.1,0.1]
["GLNARM_2_UNIT 5",null,"Glenarm Turbine 5",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",1,65.81,null,"PD","",65,null," "," "," "," ",1,24,24,65,65,65,65,65,65,65,65,65,65,65,65]
["GLNARM_7_UNIT 1",null,"GLEN ARM UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,22.13,null,"FC","","",null," "," "," "," ",1,24,24,22.13,22.13,22.13,22.13,22.13,22.13,22.13,22.13,22.13,22.13,22.13,22.13]
["GLNARM_7_UNIT 2",null,"GLEN ARM UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,22.38,null,"FC","","",null," "," "," "," ",1,24,24,22.38,22.38,22.38,22.38,22.38,22.38,22.38,22.38,22.38,22.38,22.38,22.38]
["GLNARM_7_UNIT 3",null,"GLEN ARM UNIT 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,44.83,null,"FC","","",null," "," "," "," ",1,24,24,44.83,44.83,44.83,44.83,44.83,44.83,44.83,44.83,44.83,44.83,44.83,44.83]
["GLNARM_7_UNIT 4",null,"GLEN ARM UNIT 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,42.42,null,"FC","","",null," "," "," "," ",1,24,24,42.42,42.42,42.42,42.42,42.42,42.42,42.42,42.42,42.42,42.42,42.42,42.42]
["GLOW_6_SOLAR",null,"Antelope Power Plant",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GOLETA_2_GE2BT3",null,"Goleta Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura",null,3,60,null,"FC","","",null,null,0.8,null,null,1,24,24,null,40,40,40,40,40,40,40,40,40,40,40]
["GOLETA_2_QF",null,"GOLETA QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",null,0.25,null,"FC","","",null," "," "," "," ",1,24,24,0.02,0.05,0.05,0.08,0.11,0.11,0.12,0.11,0.11,0.09,0.05,0.03]
["GOLETA_2_VALBT1",null,"Vallecito Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",3,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["GOLETA_6_ELLWOD",null,"ELLWOOD ENERGY SUPPORT FACILITY",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",1,54,null,"FC","","",null," "," "," "," ",1,24,24,54,54,54,54,54,54,54,54,54,54,54,54]
["GOLETA_6_EXGEN",null,"EXXON COMPANY USA",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark, Goleta",null,48.2,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GONZLS_6_UNIT",null,"Johnson Canyon Landfill",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,1.42,null,"FC","","",null," "," "," "," ",1,24,24,1.42,1.42,1.42,1.42,1.42,1.42,1.42,1.42,1.42,1.42,1.42,1.42]
["GOOSLK_1_SOLAR1",null,"Goose Lake",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,12,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.37,0.12,5.24,6.57,8.9600000000000009,7.52,0.63,0.1,0.1,0.1]
["GRADYW_5_GDYWD1",null,"Grady Wind",null,"WIND","Wind","WIND","AZPS","South",null,null,1,200,null,"FC","","",null," "," "," "," ",1,24,24,40.119999999999997,42.45,40.119999999999997,58.61,44,33.1,20,12,23.29,13.55,20.61,30.12]
["GRIDLY_6_SOLAR",null,"GRIDLEY MAIN TWO",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Sierra","Pease",null,2.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GRIFFI_2_LSPDYN",null,"Griffith Energy",null,"COMBINED CYCLE","CCGT","NATURAL GAS","WALC","South",null,null,null,570,null,"FC","","",null," "," "," "," ",1,24,24,570,570,570,570,570,570,570,570,570,570,570,570]
["GRIZLY_1_UNIT 1",null,"GRIZZLY HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,20,null,"FC","",8.69,null," "," "," "," ",1,24,24,5.82,5.82,5.82,5.82,5.82,5.82,5.82,5.82,5.82,5.82,5.82,5.82]
["GRNLF2_1_UNIT",null,"GREENLEAF II COGEN",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Sierra","Pease, Drum-Rio Oso",1,49.2,null,"FC","","",null," "," "," "," ",1,24,24,49.2,49.2,49.2,49.2,49.2,49.2,49.2,49.2,49.2,49.2,49.2,49.2]
["GRNVLY_7_SCLAND",null,"SANTA CRUZ LANDFILL GENERATING PLANT",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,3.04,null,"FC","","",null," "," "," "," ",1,24,24,2.98,2.69,2.87,2.95,2.91,3.01,2.82,3.01,2.93,2.6,2.95,2.99]
["GRSCRK_6_BGCKWW",null,"BIG CREEK WATER WORKS - CEDAR FLAT",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.45,1.19,0.97,1.42,1.1000000000000001,0.23,0,0,0,0,0,0.02]
["GRZZLY_1_BERKLY",null,"Berkeley Cogeneration",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","North","Bay Area",null,null,26.35,null,"FC","","",null," "," "," "," ",1,24,24,0.43,7.57,0.22,2.81,0.67,0.4,0.33,0.31,0,0,0,0]
["GUERNS_6_HD3BM3",null,"Hanford Digester Genset 3",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,1,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GUERNS_6_SOLAR",null,"Guernsey Solar Station",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["GUERNS_6_VH2BM1",null,"Hanford Digester Genset 2",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,1,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["GWFPWR_1_UNITS",null,"Hanford Peaker Plant",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon, Hanford",1,98.46,null,"FC","","",null," "," "," "," ",1,24,24,98.46,98.46,98.46,98.46,98.46,98.46,98.46,98.46,98.46,98.46,98.46,98.46]
["GYS5X6_7_UNITS",null,"GEYSERS UNITS 5 & 6 AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",1,98.43,null,"FC","","",null," "," "," "," ",1,24,24,85,85,85,85,85,85,85,85,85,85,85,85]
["GYS7X8_7_UNITS",null,"GEYSERS UNITS 7 & 8 AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Eagle Rock, Fulton",1,95.8,null,"FC","","",null," "," "," "," ",1,24,24,95.8,95.8,95.8,95.8,95.8,95.8,95.8,95.8,95.8,95.8,95.8,95.8]
["GYSRVL_7_WSPRNG",null,"Warm Springs Hydro",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Fulton",null,3.75,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["HAASPH_7_PL1X2",null,"HAAS PH UNIT 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",1,144,null,"FC","","",null," "," "," "," ",1,24,24,115.2,115.2,115.2,115.2,118.2,139.19999999999999,144,144,129.6,129.6,57.6,115.2]
["HALSEY_6_UNIT",null,"HALSEY HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",1,13.5,null,"FC","","",null," "," "," "," ",1,24,24,1.96,2.8,3.28,4.2,4.8,4.33,5.92,5.52,4.16,0,0,1.78]
["HAMLIN_1_BLDSB1","HAMLIN_1_BLDSB1_SUN","Mojave 89 BESS 2B",null,"OTHER","Hybrid_Solar1Axis","LESR","CISO","South","CAISO System",null,2,70.599999999999994,150,"ID",1,"",null,null,null,null,null,1,24,4,null,null,null,null,null,63.66,98.7,85.19,4.57,0.1,0.1,0.1]
["HAMLIN_1_BLDSB1","HAMLIN_1_BLDSB1_LESR","Mojave 89 Wind",null,"OTHER","Hybrid_Battery","HYBD","CISO","South","CAISO System",null,2,75,150,"ID",1,"",null,null,0.8,null,null,1,24,4,null,null,null,null,null,75,75,75,75,75,75,75]
["HARBGN_7_UNITS",null,"HARBOR COGEN COMBINED CYCLE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",1,109.01,null,"FC","","",null," "," "," "," ",1,24,24,100,100,100,100,100,100,100,100,100,100,100,100]
["HARDWK_6_STWBM1",null,"Still Water Ranch Dairy",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Fresno",null,1,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["HATCR1_7_UNIT",null,"Hat Creek  #1 ",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,8.5,null,"FC","","",null," "," "," "," ",1,24,24,4.13,3.65,3.51,2.72,2.4700000000000002,2.63,2.58,2.42,2.31,2.75,2.84,3.33]
["HATCR2_7_UNIT",null,"Hat Creek  #2  ",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,8.5,null,"FC","","",null," "," "," "," ",1,24,24,3.98,4.8099999999999996,4.1900000000000004,2.97,2.87,3.04,2.81,2.61,2.2599999999999998,2.76,1.49,1.07]
["HATLOS_6_BWDHY1",null,"Bidwell Ditch",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,1.38,1.38,1.38,1.37,1.35,1.23,1.31,1.28,1.28,1.31,1.32,1.28]
["HATLOS_6_LSCRK",null,"Lost Creek 1 & 2 Hydro Conversion",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1.7,null,"FC","","",null," "," "," "," ",1,24,24,0.98,0.97,0.97,0.96,0.94,0.85,0.9,0.87,0.87,0.88,0.9,0.87]
["HATRDG_2_WIND",null,"Hatchet Ridge Wind Farm",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,102,null,"FC","","",null," "," "," "," ",1,24,24,4.32,7.48,10.06,31.18,49.04,31.33,40.17,21.94,7.57,1.83,2.89,4.37]
["HAYPRS_6_HAYHD1",null,"Haypress Lower",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,5.8,null,"FC","","",null," "," "," "," ",1,24,24,1.85,1.97,1.39,2.33,2.4,1.6,1.31,1.21,1.1000000000000001,0.83,0.89,0.85]
["HAYPRS_6_HAYHD2",null,"Haypress Middle",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,6.7,null,"FC","","",null," "," "," "," ",1,24,24,2.13,2.25,2.4300000000000002,2.86,2.93,1.88,1.52,1.4,1.27,0.95,1.02,0.98]
["HELMPG_7_UNIT 1",null,"HELMS PUMP-GEN UNIT 1",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","Fresno",null,1,407,null,"FC","","",null," "," "," "," ",1,24,24,407,407,407,407,407,407,407,407,407,407,407,407]
["HELMPG_7_UNIT 2",null,"HELMS PUMP-GEN UNIT 2",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","Fresno",null,1,407,null,"FC","","",null," "," "," "," ",1,24,24,407,407,407,407,407,407,407,407,407,407,407,407]
["HELMPG_7_UNIT 3",null,"HELMS PUMP-GEN UNIT 3",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","Fresno",null,1,404,null,"FC","","",null," "," "," "," ",1,24,24,404,404,404,404,404,404,404,404,404,404,404,404]
["HENRTA_6_HDEBT1",null,"Henrietta D Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Fresno",null,2,10,null,"ID",1,"",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["HENRTA_6_SOLAR1",null,"Lemoore 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.66,0.82,1.1200000000000001,0.94,0.1,0.1,0.1,0.1]
["HENRTA_6_SOLAR2",null,"Westside Solar Power PV1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,2,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["HENRTA_6_UNITA1",null,"GWF HENRIETTA PEAKER PLANT UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno",null,1,49.98,null,"FC","","",null," "," "," "," ",1,24,24,49.98,49.98,49.98,49.98,49.98,49.98,49.98,49.98,49.98,49.98,49.98,49.98]
["HENRTA_6_UNITA2",null,"GWF HENRIETTA PEAKER PLANT UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno",null,1,49.42,null,"FC","","",null," "," "," "," ",1,24,24,49.42,49.42,49.42,49.42,49.42,49.42,49.42,49.42,49.42,49.42,49.42,49.42]
["HENRTS_1_SOLAR",null,"Henrietta Solar Project",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.05,1.04,43.71,54.78,74.66,62.7,5.22,0.1,0.1,0.1]
["HERDLN_6_BYHSR1",null,"Byron Highway Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,5,null,"EO","","",null,null,null,null,null,1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["HIDSRT_2_UNITS",null,"HIGH DESERT POWER PROJECT AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","CAISO System",null,1,850,null,"FC","","",null," "," "," "," ",1,24,24,850,850,850,850,850,850,850,850,850,850,850,850]
["HIGGNS_1_COMBIE",null,"Combie South",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.88,0.68,0.53,0.76,0.65,0.24,0.12,0.01,0.04,0.04,0.67,0.78]
["HIGGNS_7_QFUNTS",null,"HIGGNS_7_QFUNTS",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,0.5,null,"FC","","",null," "," "," "," ",1,24,24,0.11,0.03,0.02,0.11,0.21,0.24,0.24,0.24,0.23,0.1,0.05,0.08]
["HIGHDS_2_H5SBT1",null,"High 5 Solar BESS","HIGHDS_2_H5SSR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,50,100,"FC","","",false,1,0.8,200,200,1,24,4,50,50,50,50,50,50,50,50,50,50,50,50]
["HIGHDS_2_H5SSR1",null,"High 5 Solar","HIGHDS_2_H5SBT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,100,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["HILAND_7_YOLOWD",null,"CLEAR LAKE UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,3.75,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["HINSON_6_LBECH1",null,"Long Beach Unit 1",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,63,null,"FC","","",null," "," "," "," ",1,24,24,63,63,63,63,63,63,63,63,63,63,63,63]
["HINSON_6_LBECH2",null,"Long Beach Unit 2",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,63,null,"FC","","",null," "," "," "," ",1,24,24,63,63,63,63,63,63,63,63,63,63,63,63]
["HINSON_6_LBECH3",null,"Long Beach Unit 3",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,63,null,"FC","","",null," "," "," "," ",1,24,24,63,63,63,63,63,63,63,63,63,63,63,63]
["HINSON_6_LBECH4",null,"Long Beach Unit 4",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,63,null,"FC","","",null," "," "," "," ",1,24,24,63,63,63,63,63,63,63,63,63,63,63,63]
["HINSON_6_SERRGN",null,"Southeast Resource Recovery",null,"STEAM","CHP","WASTE TO POWER","CISO","South","LA Basin","Western",1,34,null,"FC","","",null," "," "," "," ",1,24,24,34,34,34,34,34,34,34,34,34,34,34,34]
["HNTGBH_2_PL1X3",null,"Huntington Beach Energy",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",1,673.8,null,"FC","","",null," "," "," "," ",1,24,24,673.8,673.8,673.8,673.8,673.8,673.8,673.8,673.8,673.8,673.8,673.8,673.8]
["HNTGBH_7_UNIT 2",null,"HUNTINGTON BEACH GEN STA. UNIT 2",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","LA Basin","Western",1,226.84,null,"FC","","",null," "," "," "," ",1,24,24,226.84,226.84,226.84,226.84,226.84,226.84,226.84,226.84,226.84,226.84,226.84,226.84]
["HOLGAT_1_BORAX",null,"U.S. Borax, Unit 1",null,"OTHER","CHP","OTHER","CISO","South","CAISO System",null,null,48.2,null,"FC","","",null," "," "," "," ",1,24,24,17.170000000000002,15.12,13.09,4.87,7.33,13.88,12.08,11.68,13.9,14.74,15.84,14.94]
["HOLSTR_1_SOLAR",null,"San Benito Smart Park",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["HOLSTR_1_SOLAR2",null,"Hollister Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.66,0.82,1.1200000000000001,0.94,0.1,0.1,0.1,0.1]
["HOOV_2_ANAPT",null,"Hoover Power Plant",null,"HYDRO","Hydro","WATER","WALC","South",null,null,1,40.39,null,"FC","","",null," "," "," "," ",1,24,24,40.39,40.39,40.39,40.39,40.39,40.39,40.39,40.39,40.39,40.39,40.39,40.39]
["HOOVER_2_MWDPT",null,"HOOVER MWD",null,"HYDRO","Hydro","WATER","WALC","South",null,null,1,249,null,"FC","","",null," "," "," "," ",1,24,24,249,249,249,249,249,249,249,249,249,249,249,249]
["HOOVER_2_SCEPT",null,"Hoover DAM - SCE Share",null,"HYDRO","Hydro","WATER","WALC","South",null,null,1,287,null,"FC","","",null," "," "," "," ",1,24,24,287,287,287,287,287,287,287,287,287,287,287,287]
["HOOVER_2_VEAPT",null,"HOOVER VEA",null,"HYDRO","Hydro","WATER","WALC","South",null,null,1,16,null,"FC","","",null," "," "," "," ",1,24,24,16,16,16,16,16,16,16,16,16,16,16,16]
["HUMBPP_1_UNITS3",null,"Humboldt Bay Generating Station 3",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","Humboldt",null,1,65.08,null,"FC","","",null," "," "," "," ",1,24,24,65.08,65.08,65.08,65.08,65.08,65.08,65.08,65.08,65.08,65.08,65.08,65.08]
["HUMBPP_6_UNITS",null,"Humboldt Bay Generating Station 1",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","Humboldt",null,1,97.62,null,"FC","","",null," "," "," "," ",1,24,24,97.62,97.62,97.62,97.62,97.62,97.62,97.62,97.62,97.62,97.62,97.62,97.62]
["HURON_6_SOLAR",null,"Huron Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["HYTTHM_2_UNITS",null,"HYATT-THERMALITO PUMP-GEN (AGGREGATE)",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,933.1,null,"FC","","",null," "," "," "," ",1,24,24,56.34,149.29,371.98,238.3,220.41,291.85000000000002,632.49,567.91999999999996,501.49,283.45,199.11,303.10000000000002]
["IGNACO_1_QF",null,"SMALL QF AGGREGATION - VALLEJO/DINSMORE",null,"OTHER","CHP","OTHER","CISO","North","NCNB",null,null,0.5,null,"FC","","",null," "," "," "," ",1,24,24,0.01,0.02,0.02,0.01,0.01,0.01,0.02,0.01,0.01,0.01,0.01,0.01]
["INDIGO_1_UNIT 1",null,"INDIGO PEAKER UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,45.3,null,"FC","","",null," "," "," "," ",1,24,24,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3]
["INDIGO_1_UNIT 2",null,"INDIGO PEAKER UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,45.3,null,"FC","","",null," "," "," "," ",1,24,24,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3]
["INDIGO_1_UNIT 3",null,"INDIGO PEAKER UNIT 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,45.3,null,"FC","","",null," "," "," "," ",1,24,24,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3,45.3]
["INDVLY_1_UNITS",null,"Indian Valley Hydro",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,2.9,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0.53,1.03,1.01,0.71,0.62,0.61,0.56000000000000005,0.02,0,0]
["INTKEP_2_UNITS",null,"CCSF Hetch_Hetchy Hydro Aggregate",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,405,null,"FC","","",null," "," "," "," ",1,24,24,307,307,307,307,307,307,307,307,239,300,307,307]
["INTMNT_3_ANAHEIM",null,"Intermountain Power Project",null,"STEAM","Coal","COAL","LADWP","South",null,null,1,234,null,"FC","","",null," "," "," "," ",1,24,24,234,234,234,234,234,234,234,234,234,234,234,234]
["INTMNT_3_PASADENA",null,"Intermountain Power Project",null,"STEAM","Coal","COAL","LADWP","South",null,null,null,107,null,"FC","","",null," "," "," "," ",1,24,24,107,107,107,107,107,107,107,107,107,107,107,107]
["INTMNT_3_RIVERSIDE",null,"IPPDYN",null,"STEAM","Coal","COAL","LADWP","South",null,null,1,136,null,"FC","","",null," "," "," "," ",1,24,24,136,136,136,136,136,136,136,136,136,136,136,136]
["INTTRB_6_UNIT",null,"International Turbine Research",null,"WIND","Wind","WIND","CISO","North","Fresno",null,null,18.399999999999999,null,"FC","","",null," "," "," "," ",1,24,24,0.78,1.35,1.81,5.62,8.85,5.65,7.25,3.96,1.36,0.33,0.52,0.79]
["IVANPA_1_UNIT1",null,"Ivanpah 1",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,126,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.93,2.85,45.7,51.96,51.72,54.68,12.32,1.96,0.1,0.1]
["IVANPA_1_UNIT2",null,"Ivanpah 2",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,133,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.98,3,48.24,54.84,54.59,57.72,13,2.0699999999999998,0.1,0.1]
["IVANPA_1_UNIT3",null,"Ivanpah 3",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,133,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.98,3,48.24,54.84,54.59,57.72,13,2.0699999999999998,0.1,0.1]
["IVSLR2_2_SM2SR1",null,"Silver Ridge Mount Signal 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.21,0.44,49.25,63.66,98.7,85.19,4.57,0.1,0.1,0.1]
["IVSLRP_2_SOLAR1",null,"Silver Ridge Mount Signal",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV",null,null,200,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,5.41,0.28999999999999998,37.869999999999997,51.76,100.93,86.75,4.5999999999999996,0.1,0.1,0.1]
["IVWEST_2_SOLAR1",null,"Imperial Valley West ( Q # 608) ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.21,0.44,49.25,63.66,98.7,85.19,4.57,0.1,0.1,0.1]
["JACMSR_1_JACSR1",null,"Jacumba Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["JAVASR_1_JAVSR1",null,"Java Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,13.5,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.41,0.14000000000000001,5.9,7.4,10.08,8.4600000000000009,0.7,0.1,0.1,0.1]
["JAWBNE_2_NSRWND",null,"North Sky River Wind Project",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,160,null,"FC","","",null," "," "," "," ",1,24,24,8.7200000000000006,18.82,20.329999999999998,64.56,68.81,60.66,53.32,46.69,32.01,14.98,6.92,7.35]
["JAWBNE_2_SRWND",null,"Sky River Wind Repower A",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,30,null,"FC","","",null," "," "," "," ",1,24,24,1.64,3.53,3.81,12.1,12.9,11.37,10,8.75,6,2.81,1.3,1.38]
["JAWBNE_2_SRWWD2",null,"Sky River Wind Repower B",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,30.2,null,"FC","","",null," "," "," "," ",1,24,24,1.65,3.55,3.84,12.19,12.99,11.45,10.06,8.81,6.04,2.83,1.31,1.39]
["JAYNE_6_WLSLR",null,"Westlands Solar Farm PV 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga",null,18,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.57999999999999996,0.15,5.39,6.56,10.86,9.34,0.96,0.1,0.1,0.1]
["JOANEC_2_ST3BT3",null,"Santa Ana Storage 3",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin",null,1,40,null,"FC","","",null,1,0.8,160,160,1,24,4,40,40,40,40,40,40,40,40,40,40,40,40]
["JOANEC_2_STABT1",null,"Santa Ana Storage 1",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",2,20,null,"FC","","",null,1,0.8,80,80,1,24,4,20,20,20,20,20,20,20,20,20,20,20,20]
["JOANEC_2_STABT2",null,"Santa Ana Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",1,20,null,"FC","","",null,1,0.8,80,80,1,24,4,20,20,20,20,20,20,20,20,20,20,20,20]
["JOHANN_2_JOSBT1",null,"Johanna Storage 1",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",3,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["JOHANN_2_JOSBT2",null,"Johanna Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",2,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["JOHANN_2_OCEBT2",null,"Orange County Energy Storage 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",3,9,null,"FC","","",null,1,0.8,36,36,1,24,4,9,9,9,9,9,9,9,9,9,9,9,9]
["JOHANN_2_OCEBT3",null,"Orange County Energy Storage 3",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",3,6,null,"FC","","",null,1,0.8,24,24,1,24,4,6,6,6,6,6,6,6,6,6,6,6,6]
["KANSAS_6_SOLAR",null,"RE Kansas South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["KEARNY_6_NESBT1",null,"Kearny North Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["KEARNY_6_SESBT2",null,"Kearny South Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,10,null,"FC","","",null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["KEKAWK_6_UNIT",null,"STS HYDROPOWER LTD. (KEKAWAKA)",null,"HYDRO","Hydro","WATER","CISO","North","Humboldt",null,null,5.5,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["KELSO_2_UNITS",null,"Mariposa Energy",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,198.03,null,"FC","","",null," "," "," "," ",1,24,24,198.03,198.03,198.03,198.03,198.03,198.03,198.03,198.03,198.03,198.03,198.03,198.03]
["KELYRG_6_UNIT",null,"KELLY RIDGE HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",1,11,null,"FC","","",null," "," "," "," ",1,24,24,8.16,8,7.36,6.72,8.16,7.04,8.16,10.199999999999999,8.16,4,0,8.16]
["KERKH2_7_UNIT 1",null,"KERKHOFF PH 2 UNIT #1",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon, Wilson 115 kV",1,153.9,null,"FC","","",null," "," "," "," ",1,24,24,7.79,22.24,36,36,96.67,74.8,75.8,75,75,0,0,4]
["KERMAN_6_SOLAR1",null,"Fresno Solar South",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["KERMAN_6_SOLAR2",null,"Fresno Solar West",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["KERNFT_1_UNITS",null,"KERN FRONT LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",1,52.4,null,"FC","","",null," "," "," "," ",1,24,24,52.4,52.4,52.4,52.4,52.4,52.4,52.4,52.4,52.4,52.4,52.4,52.4]
["KERNRG_1_UNITS",null,"South Belridge Cogen Facility",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,null,55.2,null,"FC","","",null," "," "," "," ",1,24,24,0.87,0.44,0.21,0.87,0.79,0.79,0.68,0.62,0.46,0.46,0.84,0.98]
["KERRGN_1_UNIT 1",null,"KERN RIVER HYDRO UNITS 1-4 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","CAISO System",null,null,25.6,null,"FC","","",null," "," "," "," ",1,24,24,10,11.97,16.940000000000001,24.01,24,23.81,21.4,15.54,8.0299999999999994,8.06,8.7200000000000006,9.66]
["KINGCO_1_KINGBR",null,"Kingsburg Cogen",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon, Hanford",1,34.5,null,"FC","","",null," "," "," "," ",1,24,24,34.5,34.5,34.5,34.5,34.5,34.5,34.5,34.5,34.5,34.5,34.5,34.5]
["KINGRV_7_UNIT 1",null,"KINGS RIVER HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon, Reedley",1,51.2,null,"FC","","",null," "," "," "," ",1,24,24,38.979999999999997,32,11.2,32,11.2,40.96,39.03,40.799999999999997,42.96,40.96,40.96,40.96]
["KIRKER_7_KELCYN",null,"KELLER CANYON LANDFILL GEN FACILICITY",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Pittsburg",null,3.56,null,"FC","","",null," "," "," "," ",1,24,24,3.48,3.51,3.56,3.42,3.56,3.56,3.55,3.41,3.55,3.56,3.56,3.56]
["KNGBRD_2_SOLAR1",null,"Kingbird Solar A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["KNGBRD_2_SOLAR2",null,"Kingbird Solar B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["KNGBRG_1_KBSLR1",null,"Kingsburg1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["KNGBRG_1_KBSLR2",null,"Kingsburg2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["KNGCTY_6_UNITA1",null,"King City Energy Center, Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,44.6,null,"FC","","",null," "," "," "," ",1,24,24,44.6,44.6,44.6,44.6,44.6,44.6,44.6,44.6,44.6,44.6,44.6,44.6]
["KNTSTH_6_SOLAR",null,"Kent South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["KRAMER_1_R1BX3",null,"Resurgence 1 BESS","KRAMER_1_R1PX3","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,75,90,"FC","","",false,1,0.8,300,300,1,24,4,75,75,75,75,75,75,75,75,75,75,75,75]
["KRAMER_1_R1PX3",null,"Resurgence 1 PV","KRAMER_1_R1BX3","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,90,90,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.52,0.27,29.55,38.200000000000003,59.22,51.11,2.74,0.1,0.1,0.1]
["KRAMER_1_R2BX2",null,"Resurgence 2 BESS","KRAMER_1_R2PX2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,null,40,48,"FC","","",null,1,0.8,160,160,1,24,4,40,40,40,40,40,40,40,40,40,40,40,40]
["KRAMER_1_R2PX2",null,"Resurgence 2 PV","KRAMER_1_R2BX2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,48,48,"FC","","",null,null,null,null,null,1,24,24,0.1,0.1,1.35,0.14000000000000001,15.76,20.37,31.58,27.26,1.46,0.1,0.1,0.1]
["KRAMER_2_SEGS 9",null,"Kramer Junction 9",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,80,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.59,1.81,29.02,32.99,32.840000000000003,34.72,7.82,1.24,0.1,0.1]
["KRNCNY_6_UNIT",null,"KERN CANYON POWERHOUSE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,10.6,null,"FC","","",null," "," "," "," ",1,24,24,3.38,3.56,4.1399999999999997,7.52,6.88,6.16,5.47,3.36,2.21,1.51,1.61,1.55]
["KYCORA_6_KMSBT1",null,"Kearny Mesa Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,1,null,"EO","","",null,1,0.8,4,4,1,24,4,0,0,0,0,0,0,0,0,0,0,0,0]
["LACIEN_2_VENICE",null,"MWD Venice Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western, El Nido",null,9.9499999999999993,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["LAKHDG_6_UNIT 1",null,"Lake Hodges Pumped Storage-Unit1",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","South","San Diego-IV","San Diego",1,20,null,"FC","","",null," "," "," "," ",1,24,24,20,20,20,20,20,20,20,20,20,20,20,20]
["LAKHDG_6_UNIT 2",null,"Lake Hodges Pumped Storage-Unit2",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","South","San Diego-IV","San Diego",1,20,null,"FC","","",null," "," "," "," ",1,24,24,20,20,20,20,20,20,20,20,20,20,20,20]
["LAMONT_1_SOLAR1",null,"Regulus Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,60,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.83,0.62,26.22,32.869999999999997,44.8,37.619999999999997,3.13,0.1,0.1,0.1]
["LAMONT_1_SOLAR2",null,"Redwood Solar Farm 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["LAMONT_1_SOLAR3",null,"Woodmere Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,14.99,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.46,0.16,6.55,8.2100000000000009,11.19,9.4,0.78,0.1,0.1,0.1]
["LAMONT_1_SOLAR4",null,"Hayworth Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,26.66,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.81,0.28000000000000003,11.65,14.6,19.91,16.72,1.39,0.1,0.1,0.1]
["LAMONT_1_SOLAR5",null,"Redcrest Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern PWR-Tevis",null,16.66,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.51,0.17,7.28,9.1300000000000008,12.44,10.45,0.87,0.1,0.1,0.1]
["LAPLMA_2_UNIT 1",null,"La Paloma Generating Plant Unit #1",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,267,null,"FC","","",null," "," "," "," ",1,24,24,267,267,267,267,267,267,267,267,267,267,267,267]
["LAPLMA_2_UNIT 2",null,"La Paloma Generating Plant Unit #2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,266,null,"FC","","",null," "," "," "," ",1,24,24,266,266,266,266,266,266,266,266,266,266,266,266]
["LAPLMA_2_UNIT 3",null,"La Paloma Generating Plant Unit #3",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,266,null,"FC","","",null," "," "," "," ",1,24,24,266,266,266,266,266,266,266,266,266,266,266,266]
["LAPLMA_2_UNIT 4",null,"LA PALOMA GENERATING PLANT, UNIT #4",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,267,null,"FC","","",null," "," "," "," ",1,24,24,267,267,267,267,267,267,267,267,267,267,267,267]
["LARKSP_6_UNIT 1",null,"LARKSPUR PEAKER UNIT 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, Border",1,49,null,"FC","","",null," "," "," "," ",1,24,24,49,49,49,49,49,49,49,49,49,49,49,49]
["LARKSP_6_UNIT 2",null,"LARKSPUR PEAKER UNIT 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego, Border",1,49,null,"FC","","",null," "," "," "," ",1,24,24,49,49,49,49,49,49,49,49,49,49,49,49]
["LAROA2_2_UNITA1",null,"LR2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV",null,1,322,null,"FC","","",null," "," "," "," ",1,24,24,322,322,322,322,322,322,322,322,322,322,322,322]
["LASSEN_6_UNITS",null,"Honey Lake Power",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,1,30,null,"FC","","",null," "," "," "," ",1,24,24,30,30,30,30,30,30,30,30,30,30,30,30]
["LAWRNC_7_SUNYVL",null,"City of Sunnyvale Unit 1 and 2",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area",null,null,0.3,null,"FC","","",null," "," "," "," ",1,24,24,0.11,0.04,7.0000000000000007E-2,0.14000000000000001,0.16,0.13,0.12,0.15,0.13,7.0000000000000007E-2,0.09,0.18]
["LCKHT1_2_LH1SR1",null,"Lockhart Solar 1 PV",null,"PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,85,null,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,2.38,0.25,27.91,36.08,55.93,48.27,2.59,0.1,0.1,0.1]
["LCKHT1_2_LH1SR2",null,"Lockhart Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,75,null,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,2.1,0.22,24.62,31.83,49.35,42.59,2.2799999999999998,0.1,0.1,0.1]
["LEBECS_2_UNITS",null,"Pastoria Energy Facility",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,799.47,null,"FC","","",null," "," "," "," ",1,24,24,799.47,799.47,795,785,775,775,775,775,775,785,799.47,799.47]
["LECEF_1_UNITS",null,"LOS ESTEROS ENERGY FACILITY AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",1,309.83999999999997,null,"FC","","",null," "," "," "," ",1,24,24,304,304,304,303,303,302,302,299,302,303,303,303]
["LECONT_2_LESBT1",null,"LeConte Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV",null,1,125,null,"PD","",40.4,null,1,0.8,250,250,1,24,4,40,40,40,40,40,40,40,40,40,40,40,40]
["LEPRFD_1_KANSAS",null,"Kansas",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Hanford",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["LGHTHP_6_ICEGEN",null,"CARSON COGENERATION",null,"COMBINED CYCLE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,48,null,"FC","","",null," "," "," "," ",1,24,24,48,48,48,48,48,48,48,48,48,48,48,48]
["LHILLS_6_SOLAR1",null,"Lost Hills Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["LILIAC_6_SOLAR",null,"Mesa Crest",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV","San Diego",null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["LITLRK_6_GBCSR1",null,"Green Beanworks C",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["LITLRK_6_SEPV01",null,"Gestamp Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,2,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["LITLRK_6_SOLAR1",null,"Lancaster Little Rock C ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,1.64,2.12,3.29,2.84,0.15,0.1,0.1,0.1]
["LITLRK_6_SOLAR2",null,"Palmdale 18",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.66,0.85,1.32,1.1399999999999999,0.1,0.1,0.1,0.1]
["LITLRK_6_SOLAR3",null,"One Ten Partners",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.66,0.85,1.32,1.1399999999999999,0.1,0.1,0.1,0.1]
["LITLRK_6_SOLAR4",null,"Little Rock Pham Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["LIVEOK_6_SOLAR",null,"Harris",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Sierra","Pease",null,1.25,null,"PD",0.4,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.15,0.18,0.3,0.26,0.1,0.1,0.1,0.1]
["LIVOAK_1_UNIT 1",null,"LIVE OAK LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",1,49.7,null,"FC","","",null," "," "," "," ",1,24,24,49.7,49.7,49.7,49.7,49.7,49.7,49.7,49.7,49.7,49.7,49.7,49.7]
["LMBEPK_2_UNITA1",null,"Lambie Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,47.5,null,"FC","","",null," "," "," "," ",1,24,24,47.5,47.5,47.5,47.5,47.5,47.5,47.5,47.5,47.5,47.5,47.5,47.5]
["LMBEPK_2_UNITA2",null,"Creed Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,47.6,null,"FC","","",null," "," "," "," ",1,24,24,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6]
["LMBEPK_2_UNITA3",null,"Goose Haven Energy Center, Unit #1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,47.75,null,"FC","","",null," "," "," "," ",1,24,24,47.75,47.75,47.75,47.75,47.75,47.75,47.75,47.75,47.75,47.75,47.75,47.75]
["LMEC_1_PL1X3",null,"Los Medanos Energy Center AGGREGATE",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Pittsburg",1,580,null,"FC","","",null," "," "," "," ",1,24,24,580,580,580,580,580,580,580,580,580,580,580,580]
["LNCSTR_6_CREST",null,"Lanacaster Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,5.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_SUN","SEPV Sierra NGR",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","Big Creek-Ventura",null,2,3,8.25,"PD","",6.9,null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["LNCSTR_6_SOLAR2","LNCSTR_6_SOLAR2_LESR","SEPV Sierra NGR",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","Big Creek-Ventura",null,2,7,8.25,"PD","",6.9,true,1,0.8,28,28,1,24,4,6.9,6.9,6.9,6.9,6.9,6.9,6.9,6.9,6.9,6.9,6.9,6.9]
["LOCKFD_1_BEARCK",null,"Bear Creek Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Stockton","Tesla-Bellota",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["LOCKFD_1_KSOLAR",null,"Kettleman Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Stockton","Tesla-Bellota",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.3,0.36,0.6,0.52,0.1,0.1,0.1,0.1]
["LODI25_2_UNIT 1",null,"LODI GAS TURBINE",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Stockton","Lockeford",1,25,null,"FC","","",null," "," "," "," ",1,24,24,23.8,23.8,23.8,23.8,23.8,23.8,23.8,23.8,23.8,23.8,23.8,23.8]
["LODIEC_2_PL1X2",null,"Lodi Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Sierra","South of Rio Oso, South of Palermo",1,302.58,null,"FC","","",null," "," "," "," ",1,24,24,302.58,302.58,302.58,302.58,302.58,302.58,302.58,302.58,302.58,302.58,302.58,302.58]
["LOTUS_6_LSFSR1",null,"Lotus Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Borden",null,50,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.52,0.52,21.85,27.39,37.33,31.35,2.61,0.1,0.1,0.1]
["LOWGAP_1_SUPHR",null,"Mill & Sulphur Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.99,null,"FC","","",null," "," "," "," ",1,24,24,0.4,0.33,0.13,0.24,0.19,0,0,0,0,0.05,0.04,0.1]
["LOWGAP_7_QFUNTS",null,"Matthews Dam Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1.35,null,"FC","","",null," "," "," "," ",1,24,24,0.66,0.77,0.59,0.67,0.67,0.33,0.19,0.14000000000000001,0.3,0.27,0.71,0.49]
["LTBEAR_1_LB3SR3",null,"Little Bear 3 Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["LTBEAR_1_LB4SR4",null,"Little Bear 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,50,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.52,0.52,21.85,27.39,37.33,31.35,2.61,0.1,0.1,0.1]
["LTBEAR_1_LB4SR5",null,"Little Bear 4 Solar 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,50,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.52,0.52,21.85,27.39,37.33,31.35,2.61,0.1,0.1,0.1]
["LTBERA_1_LB1SR1",null,"Little Bear Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,40,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.22,0.41,17.48,21.91,29.87,25.08,2.09,0.1,0.1,0.1]
["MAGNLA_6_ANAHEIM",null,"Magnolia Power Plant Anaheim",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP","South",null,null,1,109,null,"FC","","",null," "," "," "," ",1,24,24,109,109,109,109,109,109,109,109,109,109,109,109]
["MAGNLA_6_CERRITOS",null,"Magnolia Power Plant Cerritos",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP","South",null,null,null,12,null,"FC","","",null," "," "," "," ",1,24,24,12,12,12,12,12,12,12,12,12,12,12,12]
["MAGNLA_6_COLTON",null,"Magnolia Power Project",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP","South",null,null,null,12,null,"FC","","",null," "," "," "," ",1,24,24,12,12,12,12,12,12,12,12,12,12,12,12]
["MAGNLA_6_PASADENA",null,"Magnolia Power Plant - PASADENA",null,"COMBINED CYCLE","CCGT","NATURAL GAS","LADWP","South",null,null,null,18,null,"FC","","",null," "," "," "," ",1,24,24,18,18,18,18,18,18,18,18,18,18,18,18]
["MAGUND_1_BKISR1",null,"Bakersfield Industrial 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern Oil",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.44,0.55000000000000004,0.75,0.63,0.1,0.1,0.1,0.1]
["MAGUND_1_BKSSR2",null,"Bakersfield Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern Oil",null,5.25,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.16,0.1,2.29,2.88,3.92,3.29,0.27,0.1,0.1,0.1]
["MALAGA_1_PL1X2",null,"Malaga Power Aggregate",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon",1,96.61,null,"FC","","",null," "," "," "," ",1,24,24,96.61,96.61,96.61,96.61,96.61,96.61,96.61,96.61,96.61,96.61,96.61,96.61]
["MALCHQ_7_UNIT 1",null,"MALACHA HYDRO L.P.",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,32.5,null,"FC","","",null," "," "," "," ",1,24,24,10,10.57,3.98,4.18,0.62,0.09,0.17,0,0,0.26,0.67,2.19]
["MALIN_5_BPADYN",null,"MALIN_5_BPADYN",null,"HYDRO","Hydro","WATER","BPAT","North",null,null,null,700,null,"FC","","",null," "," "," "," ",1,24,24,700,700,700,700,700,700,700,700,700,700,700,700]
["MALIN_5_GCPDDYN",null,"Grant County Hydro Facilities",null,"HYDRO","Hydro","WATER","BPAT","North",null,null,null,125,null,"FC","","",null," "," "," "," ",1,24,24,125,125,125,125,125,125,125,125,125,125,125,125]
["MALIN_5_HERMDYN",null,"MALIN_5_HERMDYN",null,"COMBINED CYCLE","CCGT","NATURAL GAS","BPAT","North",null,null,null,308,null,"FC","","",null," "," "," "," ",1,24,24,308,308,308,308,308,308,308,308,308,308,308,308]
["MALIN_5_IBERDR",null,"Iberdrola Centroid Sytem Resource",null,"WIND","Wind","WIND","BPAT","North",null,null,1,100,null,"FC","","",null," "," "," "," ",1,24,24,20.059999999999999,21.23,20.059999999999999,29.3,22,16.55,10,6,11.64,6.78,10.3,15.06]
["MALIN_5_INHRED",null,"CSF Columbia Gorge",null,"WIND","Wind","WIND","BPAT","North",null,null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,10.029999999999999,10.61,10.029999999999999,14.65,11,8.27,5,3,5.82,3.39,5.15,7.53]
["MALIN_5_INHRPG",null,"BIGLOW CANYON",null,"WIND","Wind","WIND","BPAT","North",null,null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,10.029999999999999,10.61,10.029999999999999,14.65,11,8.27,5,3,5.82,3.39,5.15,7.53]
["MANTEC_1_ML1SR1",null,"Manteca  Land 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Stockton","Tesla-Bellota",null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["MANZNA_2_WIND",null,"Manzana Wind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,189,null,"FC","","",null," "," "," "," ",1,24,24,10.3,22.23,24.02,76.260000000000005,81.28,71.66,62.98,55.15,37.81,17.690000000000001,8.18,8.68]
["MARCPW_6_SOLAR1",null,"Maricopa West Solar PV",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["MARTIN_1_SUNSET",null,"Sunset Reservoir - North Basin",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Bay Area",null,null,4.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.15,0.1,1.35,1.64,2.72,2.34,0.24,0.1,0.1,0.1]
["MARVEL_2_MARBT3",null,"Marvel 2",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin",null,1,74.94,null,"ID",1,"",null,1,0.8,300,300,1,24,4,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007,74.930000000000007]
["MARVEL_2_MARBX2",null,"Marvel",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin",null,1,325,null,"ID",1,"",null,1,0.8,1300,1300,1,24,4,324.99,324.99,324.99,324.99,324.99,324.99,324.99,324.99,324.99,324.99,324.99,324.99]
["MCARTH_6_FRIVRB",null,"Fall River Mills Project B",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,1.5,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["MCCALL_1_QF",null,"Fish Water",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,0.52,null,"FC","","",null," "," "," "," ",1,24,24,0.3,0.39,0.27,0.28999999999999998,0.33,0.32,0.3,0.2,0.24,0.35,0.32,0.23]
["MCFLND_5_MFSBT1",null,"McFarland Solar A BESS","MCFLND_5_MFSSR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,100,200,"FC","","",null,null,0.8,null,null,1,24,24,null,100,100,100,100,100,100,100,100,100,100,100]
["MCFLND_5_MFSSR1",null,"Daggett Solar 3 cd BESS","MCFLND_5_MFSBT1","OTHER","Solar_1Axis","LESR","CISO","South","CAISO System",null,null,12.5,200,"FC","","",null,null,null,null,null,1,24,24,null,null,null,null,65.66,84.89,131.59,113.59,6.09,0.1,0.1,0.1]
["MCSWAN_6_UNITS",null,"MC SWAIN HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",1,9,null,"FC",0,"",null," "," "," "," ",1,24,24,9,9,9,9,9,9,9,9,9,9,9,9]
["MDFKRL_2_PROJCT",null,"MIDDLE FORK AND RALSTON PSP",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",1,210,null,"FC","","",null," "," "," "," ",1,24,24,210,210,210,210,210,210,210,210,210,210,210,210]
["MELRSE_6_MELBT1",null,"Point Wind 1",null,"WIND","Battery Storage","WIND","CISO","South","San Diego-IV",null,null,47.49,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,10,30.7,10,10,10,10,10,10,10]
["MELRSE_6_MELBT2",null,"Point Wind 2",null,"WIND","Battery Storage","WIND","CISO","South","San Diego-IV",null,null,14.4,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,10,30.7,10,10,10,10,10,10,10]
["MENBIO_6_RENEW1",null,"CalRENEW - 1(A)",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Panoche 115 kV, Wilson 115 kV",null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.16,0.1,1.5,1.82,3.02,2.6,0.27,0.1,0.1,0.1]
["MERCED_1_SOLAR1",null,"Mission Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["MERCED_1_SOLAR2",null,"Merced Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["MERCFL_6_UNIT",null,"Merced Falls Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",1,3.5,null,"FC",0,"",null," "," "," "," ",1,24,24,3.5,3.5,3.5,3.5,3.5,3.5,3.5,3.5,3.5,3.5,3.5,3.5]
["MESAP_1_QF",null,"SMALL QF AGGREGATION - SAN LUIS OBISPO",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,1,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["METEC_2_PL1X3",null,"Metcalf Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","South Bay-Moss Landing",1,597.04999999999995,null,"FC","","",null," "," "," "," ",1,24,24,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995,597.04999999999995]
["MIDWD_2_WIND2",null,"Coram Energy",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.16,0.35,0.38,1.21,1.29,1.1399999999999999,1,0.88,0.6,0.28000000000000003,0.13,0.14000000000000001]
["MIDWD_7_CORAMB",null,"CELLC 7.5 MW Tehachapi Project",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,7.5,null,"FC","","",null," "," "," "," ",1,24,24,0.41,0.88,0.95,3.03,3.23,2.84,2.5,2.19,1.5,0.7,0.32,0.34]
["MIDWY3_2_MDSSR1",null,"Midway South Solar Farm",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID","South",null,null,1,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.54,0.1,3.79,5.18,10.09,8.67,0.46,0.1,0.1,0.1]
["MIDWYS_2_MIDSL1",null,"Midway Solar Farm",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID","South",null,null,1,49.9,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.35,0.1,9.4499999999999993,12.91,25.18,21.64,1.1499999999999999,0.1,0.1,0.1]
["MILFRD_7_PASADENA",null,"Milford I",null,"WIND","Wind","WIND","LADWP","South",null,null,null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.27,0.59,0.64,2.02,2.15,1.9,1.67,1.46,1,0.47,0.22,0.23]
["MIRLOM_2_CORONA",null,"MWD Corona Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,2.85,null,"FC","","",null," "," "," "," ",1,24,24,1.5,0.98,0.86,0.93,1.85,1.51,0.33,0.64,0.53,0.78,0.82,1.24]
["MIRLOM_2_CREST",null,"Temescal Canyon RV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Eastern",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["MIRLOM_2_LNDFL",null,"Milliken Landfill Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["MIRLOM_2_MLBBTA",null,"Mira Loma BESS A",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern",1,10,null,"FC","","",null,2.7914438502673793,0.87,40,111.65775401069517,1,24,11.165775401069517,10,10,10,10,10,10,10,10,10,10,10,10]
["MIRLOM_2_MLBBTB",null,"Mira Loma BESS B",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Eastern",1,10,null,"FC","","",null,2.7914438502673793,0.87,40,111.65775401069517,1,24,11.165775401069517,10,10,10,10,10,10,10,10,10,10,10,10]
["MIRLOM_2_TEMESC",null,"MWD Temescal Hydroelectric Recovery Plan",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,2.85,null,"FC","","",null," "," "," "," ",1,24,24,1.33,0.57999999999999996,1.07,1.65,1.71,1.01,0.06,0.77,0.92,0.73,0.85,1.43]
["MIRLOM_6_PEAKER",null,"Mira Loma Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,47.18,null,"FC","","",null," "," "," ",423.06,1,24,8.9669351420093264,47.18,47.18,47.18,47.18,47.18,47.18,47.18,47.18,47.18,47.18,47.18,47.18]
["MIRLOM_7_MWDLKM",null,"Lake Mathews Hydroelectric Recovery Plan",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",1,5,null,"FC","","",null," "," "," "," ",1,24,24,2.4,2.4,1.6,2.4,2.4,3.2,3.2,3.6,2.8,2.4,2.4,1.6]
["MISSIX_1_QF",null,"SMALL QF AGGREGATION - SAB FRABCUSCI",null,"FTUR","CHP","NATURAL GAS","CISO","North","Bay Area","Ames",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01]
["MKTRCK_1_UNIT 1",null,"MCKITTRICK LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,47.72,null,"FC","","",null," "," "," "," ",1,24,24,47.72,47.72,47.72,47.72,47.72,47.72,47.72,47.72,47.72,47.72,47.72,47.72]
["MLPTAS_7_QFUNTS",null,"MLPTAS_7_QFUNTS",null,"OTHER","CHP","OTHER","CISO","North","Bay Area","San Jose, South Bay-Moss Landing",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["MNDALY_6_MCGRTH",null,"McGrath Beach Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",1,48.56,null,"FC","","",null," "," "," ",1165.44,1,24,24,48.56,48.56,48.56,48.56,48.56,48.56,48.56,48.56,48.56,48.56,48.56,48.56]
["MNDOTA_1_SOLAR1",null,"North Star Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV, Wilson 115 kV",null,60,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.83,0.62,26.22,32.869999999999997,44.8,37.619999999999997,3.13,0.1,0.1,0.1]
["MNDOTA_1_SOLAR2",null,"Citizen Solar B ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["MOJAVE_1_SIPHON",null,"MOJAVE SIPHON POWER PLANT",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",2,14.36,null,"FC","","",null," "," "," "," ",1,24,24,10.52,5.92,7.78,10.32,10.119999999999999,10.96,10.38,9.85,10.98,9.68,11.13,10.06]
["MOJAVW_2_SOLAR",null,"Mojave West",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["MONTPH_7_UNITS",null,"MONTICELLO HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Fulton",null,12.5,null,"FC","","",null," "," "," "," ",1,24,24,0.28000000000000003,0.47,2.27,4.03,5.12,7.93,8.52,6.81,5.5,2.5,0.73,0.48]
["MOORPK_2_ACOBT1",null,"Acorn I BESS",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","Moorpark",3,1.95,null,"FC","","",null,1,0.8,4,4,1,24,2,1,1,1,1,1,1,1,1,1,1,1,1]
["MOORPK_2_CALABS",null,"Calabasas Gas-to-Energy Facility",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura","Moorpark",null,6.96,null,"FC","","",null," "," "," "," ",1,24,24,4.4000000000000004,4.26,3.84,3.98,4.21,4.16,4.04,3.44,3.76,4.21,4.0999999999999996,4.1100000000000003]
["MOORPK_6_QF",null,"MOORPARK QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","Moorpark",null,0.8,null,"FC","","",null," "," "," "," ",1,24,24,0.01,0.06,0.02,0,0,0.04,0.04,0.28000000000000003,0.4,0.4,0.4,0.39]
["MORWD_6_QF",null,"Morwind",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,38.159999999999997,null,"FC","","",null," "," "," "," ",1,24,24,2.08,4.49,4.8499999999999996,15.4,16.41,14.47,12.72,11.14,7.63,3.57,1.65,1.75]
["MOSSLD_2_PSP1",null,"MOSS LANDING POWER BLOCK 1",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","South Bay-Moss Landing",1,510,null,"FC","","",null," "," "," "," ",1,24,24,510,510,510,510,510,510,510,510,510,510,510,510]
["MOSSLD_2_PSP2",null,"MOSS LANDING POWER BLOCK 2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","South Bay-Moss Landing",1,510,null,"FC","","",null," "," "," "," ",1,24,24,510,510,510,510,510,510,510,510,510,510,510,510]
["MRCHNT_2_PL1X3",null,"Desert Star Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","CAISO System",null,1,494.58,null,"PD","",419.25,null," "," "," "," ",1,24,24,419.25,419.25,419.25,419.25,419.25,419.25,419.25,419.25,419.25,419.25,419.25,419.25]
["MRGT_6_MEF2",null,"Miramar Energy Facility II",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,44,null,"FC","","",null," "," "," "," ",1,24,24,44,44,44,44,44,44,44,44,44,44,44,44]
["MRGT_6_MMAREF",null,"Miramar Energy Facility",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,45,null,"FC","","",null," "," "," "," ",1,24,24,45,45,45,45,45,45,45,45,45,45,45,45]
["MRGT_6_TGEBT1",null," Top Gun Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,30,null,"FC","","",null,1,0.8,120,120,1,24,4,30,30,30,30,30,30,30,30,30,30,30,30]
["MRLSDS_6_SOLAR1",null,"Morelos Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,15,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.46,0.16,6.56,8.2200000000000006,11.2,9.4,0.78,0.1,0.1,0.1]
["MSHGTS_6_MMARLF",null,"MIRAMAR LANDFILL",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,5,null,"FC","","",null," "," "," "," ",1,24,24,3.63,3.82,3.75,4.0999999999999996,4.1900000000000004,4.1500000000000004,4.16,4.08,4.3099999999999996,4.01,3.9,3.6]
["MSOLAR_2_SOLAR1",null,"Mesquite Solar 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,165,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.46,0.24,31.25,42.7,83.27,71.569999999999993,3.79,0.1,0.1,0.1]
["MSOLAR_2_SOLAR2",null,"Mesquite Solar 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,100.81,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.73,0.14000000000000001,19.09,26.09,50.87,43.72,2.3199999999999998,0.1,0.1,0.1]
["MSOLAR_2_SOLAR3",null,"Mesquite Solar 3, LLC",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,152,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.1100000000000003,0.22,28.78,39.340000000000003,76.709999999999994,65.930000000000007,3.49,0.1,0.1,0.1]
["MSQUIT_5_SERDYN",null,"MSQUIT_5_SERDYN",null,"COMBINED CYCLE","CCGT","NATURAL GAS","SRP","South",null,null,null,625,null,"FC","","",null," "," "," "," ",1,24,24,625,625,625,625,625,625,625,625,625,625,625,625]
["MSSION_2_QF",null,"SMALL QF AGGREGATION - SAN DIEGO",null,"OTHER","CHP","OTHER","CISO","South","San Diego-IV","San Diego",null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.15,0.15,0.15,0.19,0.28999999999999998,0.33,0.3,0.32,0.32,0.28000000000000003,0.26,0.16]
["MSTANG_2_MTGBT1",null,"Mustang 1 BESS","MSTANG_2_SOLAR, MSTANG_2_SOLAR3, MSTANG_2_SOLAR4","OTHER","Paired_BattStorage","LESR","CISO","North","Fresno",null,1,75,100,"FC","","",true,1,0.8,300,300,1,24,4,75,75,75,75,75,75,75,75,75,75,75,75]
["MSTANG_2_SOLAR",null,"Mustang","MSTANG_2_MTGBT1, MSTANG_2_SOLAR3, MSTANG_2_SOLAR4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","Fresno",null,null,30,100,"EO","","",null," "," "," "," ",1,24,24,0.1,0.1,0.91,0.31,13.11,16.43,22.4,18.809999999999999,1.57,0.03,0.1,0.1]
["MSTANG_2_SOLAR3",null,"Mustang 3","MSTANG_2_SOLAR, MSTANG_2_MTGBT1, MSTANG_2_SOLAR4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","Fresno",null,null,40,100,"PD",0.37369999999999998,"",null," "," "," "," ",1,24,24,0.1,0.1,1.22,0.41,17.48,21.91,29.87,25.08,2.09,0.1,0.1,0.1]
["MSTANG_2_SOLAR4",null,"Mustang 4","MSTANG_2_SOLAR, MSTANG_2_MTGBT1, MSTANG_2_SOLAR3","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","Fresno",null,null,30,100,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.91,0.31,13.11,16.43,22.4,18.809999999999999,1.57,0.1,0.1,0.1]
["MTNPOS_1_UNIT",null,"MT.POSO COGENERATION CO.",null,"STEAM","CHP","BIOMASS","CISO","North","Kern","South Kern PP, Kern Oil",null,46.64,null,"FC","","",null," "," "," "," ",1,24,24,29.05,28.4,17.440000000000001,28.88,31.82,39.72,41.67,40.549999999999997,39.56,39.299999999999997,38.79,27.09]
["MTWIND_1_MVPWD1",null,"Mountain View Power Project I Repower",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,66.599999999999994,null,"FC","","",null," "," "," "," ",1,24,24,3.63,7.83,8.4600000000000009,26.87,28.64,25.25,22.19,19.43,13.32,6.23,2.88,3.06]
["MTWIND_1_UNIT 3",null,"Mountain View Power Project III",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,22.44,null,"FC","","",null," "," "," "," ",1,24,24,1.22,2.64,2.85,9.0500000000000007,9.65,8.51,7.48,6.55,4.49,2.1,0.97,1.03]
["MURRAY_6_UNIT",null,"Grossmont Hospital",null,"FTUR","CHP","NATURAL GAS","CISO","South","San Diego-IV","San Diego",null,4.12,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["NAROW1_2_UNIT",null,"NARROWS PH 1 UNIT",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,1,12,null,"FC","","",null," "," "," "," ",1,24,24,12,12,12,12,12,12,12,12,12,12,12,12]
["NAROW2_2_UNIT",null,"Narrows Powerhouse Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra",null,2,55,null,"FC","","",null," "," "," "," ",1,24,24,55,55,55,55,55,55,55,55,55,55,55,55]
["NAVYII_2_UNITS",null,"COSO POWER DEVELOPER (NAVY II) AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","South","CAISO System",null,1,90,null,"PD","",55,null," "," "," "," ",1,24,24,55,55,55,55,55,55,55,55,55,55,55,55]
["NCPA_7_GP1UN1",null,"NCPA GEO PLANT 1 UNIT 1",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,38.85,null,"FC","","",null," "," "," "," ",1,24,24,38.85,38.85,38.85,38.85,38.85,38.85,38.85,38.85,38.85,38.85,38.85,38.85]
["NCPA_7_GP1UN2",null,"NCPA GEO PLANT 1 UNIT 2",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,39.94,null,"FC","","",null," "," "," "," ",1,24,24,39.94,39.94,39.94,39.94,39.94,39.94,39.94,39.94,39.94,39.94,39.94,39.94]
["NCPA_7_GP2UN3",null,"NCPA GEO PLANT 2 UNIT 3",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",1,42.42,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["NCPA_7_GP2UN4",null,"NCPA GEO PLANT 2 UNIT 4",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB","Fulton",1,52.73,null,"FC","","",null," "," "," "," ",1,24,24,52.73,52.73,52.73,52.73,52.73,52.73,52.73,52.73,52.73,52.73,52.73,52.73]
["NEENCH_6_SOLAR",null,"Alpine Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,66,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.78,0.1,12.5,17.079999999999998,33.31,28.63,1.52,0.1,0.1,0.1]
["NEWARK_1_QF",null,"NEWARK 1 QF",null,"OTHER","CHP","OTHER","CISO","North","Bay Area",null,null,0.1,null,"FC","","",null," "," "," "," ",1,24,24,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03]
["NGILAA_5_SDGDYN",null,"NGILAA_5_SDGDYN",null,"COMBINED CYCLE","CCGT","NATURAL GAS","AZPS","South",null,null,null,55,null,"FC","","",null," "," "," "," ",1,24,24,55,55,55,55,55,55,55,55,55,55,55,55]
["NHOGAN_6_UNITS",null,"NEW HOGAN PH AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,4,null,"FC","","",null," "," "," "," ",1,24,24,0.13,0.02,0.09,0.52,1.1499999999999999,0.96,1.53,1.17,0.98,0.02,0,0]
["NORCNV_1_NCVBT1",null,"North Central Valley ",null,"OTHER","Battery Storage","LESR","CISO","North","Stockton",null,1,132,null,"ID",1,"",null,1,0.8,528,528,1,24,4,132,132,132,132,132,132,132,132,132,132,132,132]
["NOVATO_6_LNDFL",null,"Redwood Renewable Energy",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","NCNB",null,null,3.9,null,"FC","","",null," "," "," "," ",1,24,24,3.64,3.67,3.64,3.62,3.58,3.26,2.83,2.87,3.03,2.78,3.24,3.29]
["NWCSTL_7_UNIT 1",null,"NEWCASTLE HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",null,12,null,"FC","","",null," "," "," "," ",1,24,24,0.95,2.4700000000000002,3.29,1.43,0.3,0,0.33,0,0,0.52,0,1.19]
["NZWIND_2_WDSTR5",null,"Windstream 6111",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,6.31,null,"FC","","",null," "," "," "," ",1,24,24,0.34,0.74,0.8,2.5499999999999998,2.71,2.39,2.1,1.84,1.26,0.59,0.27,0.28999999999999998]
["NZWIND_6_CALWND",null,"Wind Resource I",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,9,null,"FC","","",null," "," "," "," ",1,24,24,0.49,1.06,1.1399999999999999,3.63,3.87,3.41,3,2.63,1.8,0.84,0.39,0.41]
["NZWIND_6_WDSTR",null,"Windstream 39",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,3.35,null,"FC","","",null," "," "," "," ",1,24,24,0.18,0.39,0.43,1.35,1.44,1.27,1.1200000000000001,0.98,0.67,0.31,0.14000000000000001,0.15]
["NZWIND_6_WDSTR2",null,"Windstream 6040",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,4.07,null,"FC","","",null," "," "," "," ",1,24,24,0.22,0.48,0.52,1.64,1.75,1.54,1.36,1.19,0.81,0.38,0.18,0.19]
["NZWIND_6_WDSTR3",null,"Windstream 6041",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,3.86,null,"FC","","",null," "," "," "," ",1,24,24,0.21,0.45,0.49,1.56,1.66,1.46,1.29,1.1299999999999999,0.77,0.36,0.17,0.18]
["NZWIND_6_WDSTR4",null,"Windstream 6042",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,6.77,null,"FC","","",null," "," "," "," ",1,24,24,0.37,0.8,0.86,2.73,2.91,2.57,2.2599999999999998,1.98,1.35,0.63,0.28999999999999998,0.31]
["OAK C_1_EBMUD",null,"MWWTP PGS 1 - ENGINES",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Oakland",null,6.9,null,"FC","","",null," "," "," "," ",1,24,24,1.67,1.56,1.51,1.68,1.23,1.46,1.39,1.7,1.89,1.67,1.6,1.96]
["OAK C_7_UNIT 1",null,"OAKLAND STATION C GT UNIT 1",null,"COMBUSTION TURBINE","Peaker","DISTILLATE","CISO","North","Bay Area","Oakland",1,55,null,"FC","","",null," "," "," "," ",1,24,24,55,55,55,55,55,55,55,55,55,55,55,55]
["OAK C_7_UNIT 3",null,"OAKLAND STATION C GT UNIT 3",null,"COMBUSTION TURBINE","Peaker","DISTILLATE","CISO","North","Bay Area","Oakland",1,55,null,"FC","","",null," "," "," "," ",1,24,24,55,55,55,55,55,55,55,55,55,55,55,55]
["OAK L_1_GTG1",null,"MWWTP PGS 2 - Turbine",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","North","Bay Area","Oakland",null,4.5999999999999996,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["OAKWD_6_QF",null,"Oak Creek",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,27.87,null,"FC","","",null," "," "," "," ",1,24,24,1.52,3.28,3.54,11.25,11.99,10.57,9.2899999999999991,8.1300000000000008,5.58,2.61,1.21,1.28]
["OAKWD_6_ZEPHWD",null,"Zephyr Park",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,3.5,null,"FC","","",null," "," "," "," ",1,24,24,0.19,0.41,0.44,1.41,1.51,1.33,1.17,1.02,0.7,0.33,0.15,0.16]
["OASIS_6_CREST",null,"CREST Contracts",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,10.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["OASIS_6_GBDSR4",null,"Green Beanworks D",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["OASIS_6_SOLAR1",null,"Morgan Lancaster I",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","South","Big Creek-Ventura",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["OASIS_6_SOLAR2",null,"Oasis Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["OASIS_6_SOLAR3",null,"Soccer Center",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["OBERON_5_O1BBX2",null,"Oberon 1 BESS","OBERON_5_O1SSR3, OBERON_5_O1SSX2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,125,250,"ID",1,"",false,1,0.8,500,500,1,24,4,125,125,125,125,125,125,125,125,125,125,125,125]
["OBERON_5_O1SSR3",null,"Oberon 1B Solar","OBERON_5_O1BBX2, OBERON_5_O1SSX2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,250,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["OBERON_5_O1SSX2",null,"Oberon 1A Solar","OBERON_5_O1SSR3, OBERON_5_O1BBX2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,150,250,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,4.21,0.44,49.25,63.66,98.7,85.19,4.57,0.1,0.1,0.1]
["OBERON_5_O2BBX2",null,"Oberon 2 BESS","OBERON_5_O2SSR4, OBERON_5_O2SSR5","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,125,250,"ID",1,"",null,1,0.8,500,500,1,24,4,125,125,125,125,125,125,125,125,125,125,125,125]
["OBERON_5_O2SSR4",null,"Oberon 2A Solar","OBERON_5_O2BBX2, OBERON_5_O2SSR5","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,125,250,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.51,0.37,41.04,53.05,82.25,70.989999999999995,3.81,0.1,0.1,0.1]
["OBERON_5_O2SSR5",null,"Oberon 2B Solar","OBERON_5_O2BBX2, OBERON_5_O2SSR4","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,125,250,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.51,0.37,41.04,53.05,82.25,70.989999999999995,3.81,0.1,0.1,0.1]
["OCOTLO_6_OCWSB1","OCOTLO_6_OCWSB1_SUN","Ocotillo Wells Solar and BESS",null,"OTHER","Hybrid_Solar1Axis","HYBD","IID","South",null,null,2,50,50,"FC","","",null,null,null,null,null,1,24,24,0.1,0.1,1.4,0.15,16.420000000000002,21.22,32.9,28.4,1.52,0.1,0.1,0.1]
["OCOTLO_6_OCWSB1","OCOTLO_6_OCWSB1_LESR","Ocotillo Wells Solar and BESS",null,"OTHER","Hybrid_Storage","HYBD","IID","South",null,null,2,50,50,"FC","","",null,1,0.8,200,200,1,24,4,50,50,50,50,50,50,50,50,50,50,50,50]
["OCTILO_5_WIND",null,"Ocotillo Wind Energy Facility",null,"WIND","Wind","WIND","CISO","South","San Diego-IV",null,null,265,null,"FC","","",null," "," "," "," ",1,24,24,14.45,31.17,33.68,106.92,113.96,100.47,88.3,77.33,53.02,24.81,11.47,12.17]
["OGROVE_6_PL1X2",null,"Orange Grove Energy Center",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,96,null,"FC","","",null," "," "," "," ",1,24,24,96,96,96,96,96,96,96,96,96,96,96,96]
["OILFLD_7_QFUNTS",null,"Nacimiento Hydroelectric Plant",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,3.8,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.11,0.69,1.88,1.41,0.99,0.95,0.81,0.37,0.05,0.04,0]
["OLDRIV_6_BIOGAS",null,"Bidart Old River 1",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Kern","South Kern PP, Kern 70 kV",null,2,null,"FC","","",null," "," "," "," ",1,24,24,1.76,1.83,1.84,1.68,1.79,1.74,1.71,1.75,1.76,1.77,1.77,1.66]
["OLDRIV_6_CESDBM",null,"Ces Dairy Biogas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Kern","South Kern PP, Kern 70 kV",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.95,0.97,0.94,0.93,0.95,0.91,0.92,0.93,0.94,0.96,0.96,0.97]
["OLDRIV_6_LKVBM1",null,"Lakeview Dairy Biogas",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Kern","South Kern PP, Kern 70 kV",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.97,0.96,0.94,0.95,0.94,0.94,0.93,0.93,0.94,0.95,0.97,0.97]
["OLDRV1_6_SOLAR",null,"Old River One",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Kern","South Kern PP, Kern 70 kV",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["OLINDA_2_COYCRK",null,"MWD Coyote Creek Hydroelectric Recovery ",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",1,3.13,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0.8,0,0,0]
["OLINDA_2_LNDFL2",null,"Brea Power II",null,"COMBINED CYCLE","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,28.1,null,"FC","","",null," "," "," "," ",1,24,24,25.9,26.23,26.22,24.03,26.31,25.12,25.3,24.99,25.06,25.49,25.94,25.99]
["OLINDA_7_BLKSND",null,"BlackSand Generating Facility",null,"COMBUSTION TURBINE","Biomass","WASTE TO POWER","CISO","South","LA Basin","Western",null,8,null,"FC","","",null," "," "," "," ",1,24,24,0.11,0.1,0.15,0.22,0.28999999999999998,0.38,0.36,0.25,0.98,1.28,1.04,1.48]
["OLIVEP_1_SOLAR",null,"White River Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["OLIVEP_1_SOLAR2",null,"White River West",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,19.75,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.92,7.2,11.92,10.25,1.05,0.1,0.1,0.1]
["OLSEN_2_UNIT",null,"OLSEN POWER PARTNERS",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,5.5,null,"FC","","",null," "," "," "," ",1,24,24,1.1599999999999999,0.88,0.97,2.2999999999999998,2.06,0.56999999999999995,0.02,0,0,0.11,0.09,0.35]
["OMAR_2_UNIT 1",null,"KERN RIVER COGENERATION CO. UNIT 1",null,"FTUR","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,75,null,"FC","","",null," "," "," "," ",1,24,24,75,75,75,75,74.67,73.67,73,72.67,73.67,74.33,75,75]
["OMAR_2_UNIT 2",null,"KERN RIVER COGENERATION CO. UNIT 2",null,"FTUR","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,75,null,"FC","","",null," "," "," "," ",1,24,24,75,75,75,75,74.67,73.67,73.33,73,73.67,74.67,75,75]
["OMAR_2_UNIT 3",null,"KERN RIVER COGENERATION CO. UNIT 3",null,"FTUR","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,75,null,"FC","","",null," "," "," "," ",1,24,24,75,75,75,75,73.67,73.67,73.33,73,73.67,75,75,75]
["OMAR_2_UNIT 4",null,"KERN RIVER COGENERATION CO. UNIT 4",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,75,null,"FC","","",null," "," "," "," ",1,24,24,75,75,75,75,74,73.33,73.67,73.67,74.33,75,75,75]
["ONLLPP_6_UNITS",null,"O'NEILL PUMP-GEN (AGGREGATE)",null,"HYDRO","Pumped Hydro","WATER","CISO","North","Fresno",null,null,25.2,null,"FC","","",null," "," "," "," ",1,24,24,0,0.74,7.0000000000000007E-2,0.18,12.91,1.8,1.49,0.63,0.05,0.71,0.15,0]
["ORLND_6_HIGHLI",null,"High Line Canal Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.5,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0.04,0.03,0,0,0,0,0,0,0]
["ORLND_6_SOLAR1",null,"Enerparc California 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.66,0.82,1.1200000000000001,0.94,0.1,0.1,0.1,0.1]
["ORMOND_7_UNIT 1",null,"ORMOND BEACH GEN STA. UNIT 1",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","Big Creek-Ventura","Moorpark",1,741.27,null,"FC","","",null," "," "," "," ",1,24,24,741.27,741.27,741.27,741.27,741.27,741.27,741.27,741.27,741.27,741.27,741.27,741.27]
["ORMOND_7_UNIT 2",null,"ORMOND BEACH GEN STA. UNIT 2",null,"STEAM","Steam Turbine","NATURAL GAS","CISO","South","Big Creek-Ventura","Moorpark",1,750,null,"FC","","",null," "," "," "," ",1,24,24,750,750,750,750,750,750,750,750,750,750,750,750]
["OROLOM_1_SOLAR1",null,"Oro Loma Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV",null,10,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["OROLOM_1_SOLAR2",null,"Oro Loma Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Panoche 115 kV",null,10,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["OROVIL_6_UNIT",null,"Oroville Cogeneration, LP",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","North","Sierra","Drum-Rio Oso",1,7.5,null,"FC","","",null," "," "," "," ",1,24,24,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5]
["ORTGA_6_ME1SL1",null,"Merced 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,1.31,1.64,2.2400000000000002,1.88,0.16,0.1,0.1,0.1]
["OSO_6_NSPIN",null,"OSO_6_NSPIN",null,"PUMP","Pump","WATER","CISO","South","Big Creek-Ventura",null,1,70,null,"FC","","",null," "," "," "," ",1,24,24,18,18,18,18,18,18,18,18,18,18,18,18]
["OTAY_6_PL1X2",null,"Chula Vista Energy Center, LLC",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,39.57,null,"PD","",37.200000000000003,null," "," "," "," ",1,24,24,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003,37.200000000000003]
["OTMESA_2_PL1X3",null,"OTAY MESA ENERGY CENTER",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,603.67999999999995,null,"FC","","",null," "," "," "," ",1,24,24,603.6,603.6,603.6,603.6,603.6,603.6,603.6,603.6,603.6,603.6,603.6,603.6]
["OXBOW_6_DRUM",null,"OXBOW HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,5.8,null,"FC","","",null," "," "," "," ",1,24,24,2.1,1.45,1.51,2.92,1.54,1.24,1.83,2.41,1.64,0.02,0.97,1.18]
["OXMTN_6_LNDFIL",null,"Ox Mountain Landfill Generating Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area","Ames",null,10.62,null,"FC","","",null," "," "," "," ",1,24,24,10.62,10.62,10.62,10.62,10.5,10.38,10.57,10.29,10.38,10.3,10.46,10.62]
["PACLUM_6_UNIT",null,"Humboldt Redwood",null,"STEAM","Biomass","BIOMASS","CISO","North","Humboldt",null,null,28.8,null,"FC","","",null," "," "," "," ",1,24,24,14.62,12.54,11.91,11.66,14.79,15.29,14.72,12.65,14.37,15.23,13.29,14.04]
["PADUA_2_ONTARO",null,"ONTARIO/SIERRA HYDRO PSP",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",null,1.92,null,"FC","","",null," "," "," "," ",1,24,24,0.89,0.92,0.83,0.82,0.86,0.75,0.75,0.64,0.53,0.44,0.4,0.48]
["PADUA_2_SOLAR1",null,"Kona Solar - Rancho DC #1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,1.75,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PADUA_6_MWDSDM",null,"San Dimas Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",1,9.9,null,"FC","","",null," "," "," "," ",1,24,24,0,0.8,3.6,0.8,0.8,0.8,0.8,0.8,1.6,1.6,6.4,4.8]
["PADUA_6_QF",null,"PADUA QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Eastern",null,1.82,null,"FC","","",null," "," "," "," ",1,24,24,0.17,0.28999999999999998,0.24,0.28000000000000003,0.35,0.39,0.4,0.34,0.36,0.32,0.32,0.22]
["PADUA_7_SDIMAS",null,"San Dimas Wash Hydro",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern",1,1.05,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,1.05,1.05,1.05,1.05,1.05,1.05,1.05,1.05]
["PAIGES_6_SOLAR",null,"Paige Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PALA_6_PGCBT1",null,"Wind Wall Monolith 1",null,"WIND","Battery Storage","WIND","CISO","South","San Diego-IV",null,null,19.850000000000001,null,"EO","","",null,null,0.8,null,null,1,24,24,null,null,null,0,0,0,0,0,0,0,0,0]
["PALALT_7_COBUG",null,"Cooperatively Owned Back Up Generator",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area",null,null,4.5,null,"FC","","",null," "," "," "," ",1,24,24,4.5,4.5,4.5,4.5,4.5,4.5,4.5,4.5,4.5,4.5,4.5,4.5]
["PALOMR_2_PL1X3",null,"Palomar Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,588.21,null,"FC","","",null," "," "," "," ",1,24,24,588.21,588.21,588.21,588.21,588.21,588.21,588.21,588.21,588.21,588.21,588.21,588.21]
["PARDEB_6_UNITS",null,"Pardee Power House",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,30,null,"FC","","",null," "," "," "," ",1,24,24,15.76,14.96,15.76,23.6,24,24,14.96,14.96,14.96,14.96,14.16,15.76]
["PARDSE_6_PESBT1",null,"Wind Wall Monolith 2",null,"WIND","Battery Storage","WIND","CISO","South","San Diego-IV",null,null,23.66,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,9.75,9.75,9.75,9.75,9.75,9.75,9.75,9.75,9.75]
["PBLOSM_2_SOLAR",null,"PearBlossom",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,9.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.27,0.1,3.12,4.03,6.25,5.4,0.28999999999999998,0.1,0.1,0.1]
["PEABDY_2_LNDFIL",null,"G2 Energy Hay Road Power Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,1.6,null,"FC","","",null," "," "," "," ",1,24,24,1.54,1.54,1.49,1.53,1.52,1.51,1.51,1.51,1.51,1.52,1.53,1.52]
["PEABDY_2_LNDFL1",null,"Potrero Hills Energy Producers",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,8,null,"FC","","",null," "," "," "," ",1,24,24,7.7,7.67,7.54,7.57,7.03,7.39,7.56,7.54,7.52,7.41,7.47,7.22]
["PEARBL_2_NSPIN",null,"PEARBL_2_NSPIN",null,"PUMP","Pump","WATER","CISO","South","CAISO System",null,1,118,null,"FC","","",null," "," "," "," ",1,24,24,46,46,46,46,46,46,46,46,46,46,46,46]
["PEASE_1_TBEBT1",null,"Tierra Buena Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Sierra","Pease, Drum-Rio Oso",3,6,null,"ID",1,"",null,1,0.8,24,24,1,24,4,5,5,5,5,5,5,5,5,5,5,5,5]
["PEORIA_1_SOLAR",null,"Sonora 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["PHOENX_1_UNIT",null,"PHOENIX PH",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.62,0.51,0.71,0.87,0.77,0.79,0.96,1.02,1.06,0.59,0.19,0]
["PINFLT_7_UNITS",null,"PINE FLAT HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",1,198.51,null,"FC","","",null," "," "," "," ",1,24,24,0,24.35,36.6,65.5,104,165.54,176.65,120.84,36.57,11.5,0,0]
["PIOPIC_2_CTG1",null,"Pio Pico Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,111.3,null,"FC","","",null," "," "," "," ",1,24,24,111.3,111.3,111.3,111.3,111.3,111.3,111.3,111.3,111.3,111.3,111.3,111.3]
["PIOPIC_2_CTG2",null,"Pio Pico Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,112.7,null,"FC","","",null," "," "," "," ",1,24,24,112.7,112.7,112.7,112.7,112.7,112.7,112.7,112.7,112.7,112.7,112.7,112.7]
["PIOPIC_2_CTG3",null,"Pio Pico Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","San Diego-IV","San Diego",1,112,null,"FC","","",null," "," "," "," ",1,24,24,112,112,112,112,112,112,112,112,112,112,112,112]
["PIT1_6_FRIVRA",null,"Fall River Mills Project A",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,1.5,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["PIT1_7_UNIT 1",null,"PIT PH 1 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,32,null,"FC","","",null," "," "," "," ",1,24,24,21.2,18.399999999999999,19,16,16.8,10.83,10.8,9.51,9.1999999999999993,8,14.4,15.68]
["PIT1_7_UNIT 2",null,"PIT PH 1 UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,32,null,"FC","","",null," "," "," "," ",1,24,24,14.4,14.4,15.68,14.4,15.68,10.8,8.6,9.1999999999999993,9.1999999999999993,4.8,14.4,15.68]
["PIT3_7_PL1X3",null,"PIT PH 3 UNITS 1, 2 & 3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,70.599999999999994,null,"FC","","",null," "," "," "," ",1,24,24,36,35.68,28.8,34.4,42.4,46,52.4,47.6,26.4,28,29.6,36.6]
["PIT4_7_PL1X2",null,"PIT PH 4 UNITS 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,95,null,"FC","","",null," "," "," "," ",1,24,24,50.2,40.799999999999997,44,44.8,40.799999999999997,55.2,60.6,55.6,36.4,40.799999999999997,44.6,48.8]
["PIT5_7_PL1X2",null,"PIT PH 5 UNITS 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,82,null,"FC","","",null," "," "," "," ",1,24,24,36,31.2,32,31.2,32,32,34.4,32.799999999999997,28,18.399999999999999,44,40]
["PIT5_7_PL3X4",null,"PIT PH 5 UNITS 3 & 4 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,82,null,"FC","","",null," "," "," "," ",1,24,24,32,36.799999999999997,28.8,32,32,32.799999999999997,36.799999999999997,39.200000000000003,34.4,43,28.8,32]
["PIT5_7_QFUNTS",null,"GRASSHOPPER FLAT HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1.1000000000000001,null,"FC","","",null," "," "," "," ",1,24,24,0.26,0.28999999999999998,0.15,0.3,0.08,0,0,0,0,0.01,0.05,0.03]
["PIT6_7_UNIT 1",null,"PIT PH 6 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,39,null,"FC","","",null," "," "," "," ",1,24,24,30.85,30.62,31.14,37.78,38,37.159999999999997,37.520000000000003,37.619999999999997,30.62,30.71,37.06,38.119999999999997]
["PIT6_7_UNIT 2",null,"PIT PH 6 UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,40,null,"FC","","",null," "," "," "," ",1,24,24,36.97,37.74,38.4,38.03,31.1,37.58,37.450000000000003,37.700000000000003,37.44,30.42,37.130000000000003,38.18]
["PIT7_7_UNIT 1",null,"PIT PH 7 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,55.7,null,"FC","","",null," "," "," "," ",1,24,24,53,51.72,52.76,52.21,51.56,52.34,53.04,53.55,53.4,51.38,42.4,53.08]
["PIT7_7_UNIT 2",null,"PIT PH 7 UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,54.6,null,"FC","","",null," "," "," "," ",1,24,24,51.36,49.56,51.76,51.96,41.76,51.36,52.32,53.43,53.38,52.89,53.18,42.41]
["PIUTE_6_GNBSR1",null,"Green Beanworks B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["PLACVL_1_CHILIB",null,"Chili Bar Powerhouse",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Gold Hill-Drum, South of Rio Oso, South of Palermo",null,8.34,null,"FC","","",null," "," "," "," ",1,24,24,1.1399999999999999,0.95,1.63,3.8,3.72,1.35,0.79,1.89,1.55,1.04,0.78,1.54]
["PLACVL_1_RCKCRE",null,"Rock Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Rio Oso, South of Palermo",null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.16,0.04,0.12,0.19,0.02,0,0,0,0,0,0.01,0.04]
["PLAINV_6_BSOLAR",null,"Western Antelope Blue Sky Ranch A ",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PLAINV_6_DSOLAR",null,"Western Antelope Dry Ranch ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.28000000000000003,0.1,3.28,4.24,6.58,5.68,0.3,0.1,0.1,0.1]
["PLAINV_6_NLRSR1",null,"North Lancaster Ranch ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PLAINV_6_SOLAR3",null,"Sierra Solar Greenworks LLC",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PLAINV_6_SOLARC",null,"Central Antelope Dry Ranch C",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PLMSSR_6_HISIER",null,"High Sierra Cogeneration Aggregate",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,1,6,null,"FC","","",null," "," "," "," ",1,24,24,6,6,6,6,6,6,6,6,6,6,6,6]
["PLSNTG_7_LNCLND",null,"Lincoln Landfill Power Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,4.9800000000000004,null,"FC","","",null," "," "," "," ",1,24,24,3.68,3.75,3.84,3.86,3.97,4,3.96,3.78,3.68,3.73,3.52,3.71]
["PMDLET_6_SOLAR1",null,"SEPV Palmdale East, LLC",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.28000000000000003,0.1,3.28,4.24,6.58,5.68,0.3,0.1,0.1,0.1]
["PMPJCK_1_RB2SLR",null,"Rio Bravo Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["PMPJCK_1_SOLAR1",null,"Pumpjack Solar I",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["PMPJCK_1_SOLAR2",null,"Rio Bravo Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["PNCHEG_2_PL1X4",null,"PANOCHE ENERGY CENTER (Aggregated)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,417,null,"ID",1,"",null," "," "," "," ",1,24,24,417,417,417,417,416,412,403,403,408,416,417,417]
["PNCHPP_1_PL1X2",null,"Midway Peaking Aggregate",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Panoche 115 kV",1,119.91,null,"FC","","",null," "," "," "," ",1,24,24,119.91,119.91,119,117.54,119.91,119.91,119.91,119.91,119.91,119.91,119.91,119.91]
["PNCHVS_2_SOLAR",null,"Panoche Valley Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,140,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.26,1.45,61.19,76.69,104.53,87.78,7.31,0.13,0.1,0.1]
["PNOCHE_1_PL1X2",null,"Panoche Peaker",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Herndon, Panoche 115 kV",1,49.97,null,"FC","","",null," "," "," "," ",1,24,24,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97]
["PNOCHE_1_UNITA1",null,"CalPeak Power Panoche Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Fresno","Panoche 115 kV",1,52.3,null,"PD","",52.01,null," "," "," "," ",1,24,24,52.01,52.01,52.01,52.01,52.01,52.01,52.01,52.01,52.01,52.01,52.01,52.01]
["POEPH_7_UNIT 1",null,"POE HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,68,null,"FC","",21,null," "," "," "," ",1,24,24,21,21,21,21,21,21,21,21,21,21,9.6,9.81]
["POEPH_7_UNIT 2",null,"POE HYDRO UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,68.5,null,"FC","",20.82,null," "," "," "," ",1,24,24,20.82,20.82,20.82,20.82,20.82,20,20.82,20.82,20.82,20.399999999999999,16.34,15.3]
["POLRIS_2_ASEBT1",null,"Antelope Solar 2 Estrella BESS","POLRIS_2_ASESR1","OTHER","Paired_BattStorage","LESR","CISO","South","Big Creek-Ventura",null,null,28,56,"ID","","",null,null,0.8,null,null,1,24,24,null,28,28,28,28,28,28,28,28,28,28,28]
["POLRIS_2_ASESR1",null,"Antelope Solar 2 Estrella","POLRIS_2_ASEBT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,56,56,"ID","","",null,null,null,null,null,1,24,24,null,0.1,1.57,0.17,18.39,23.77,36.85,31.8,1.71,0.1,0.1,0.1]
["POLRIS_2_ASRBT1",null,"Bailey Creek Ranch","POLRIS_2_ASRSR1","HYDRO","Paired_BattStorage","WATER","CISO","South","Big Creek-Ventura",null,2,0.63,125,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,79.3,79.3,79.3,79.3,79.3,79.3,79.3,79.3]
["POLRIS_2_ASRSR1",null,"Digger Creek Ranch Hydro","POLRIS_2_ASRBT1","HYDRO","Paired_Solar_1Axis","WATER","CISO","South","Big Creek-Ventura",null,null,0.6,125,"FC","","",null,null,null,null,null,1,24,24,null,null,null,null,41.04,53.05,0.39,0.34,0.02,0,0.1,0.1]
["POTTER_7_VECINO",null,"Vecino Vineyards LLC",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",null,1.25,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PRCTVY_1_MIGBT1",null,"Miguel BESS",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",null,2,null,"EO","","",null,1,0.8,8,8,1,24,4,0,0,0,0,0,0,0,0,0,0,0,0]
["PRIMM_2_SOLAR1",null,"Silver State South",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,250,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,6.76,0.36,47.34,64.7,126.16,108.43,5.75,0.1,0.1,0.1]
["PROXSR_2_PS1BT1",null,"Ponderosa Bailey Hydroelectric",null,"HYDRO","Battery Storage","WATER","CISO","North","CAISO System",null,1,1.25,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,40,40,40,40,40,40,40,40]
["PROXSR_2_PS2BT3",null,"VOLTA_7_QFUNTS",null,"HYDRO","Battery Storage","WATER","CISO","North","CAISO System",null,2,0.15,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,90,90,90,90,90,90,90,90]
["PSWEET_1_STCRUZ",null,"Santa Cruz Energy LLC",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,1,1.6,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["PUTHCR_1_PCNSB1","PUTHCR_1_PCNSB1_SUN","Putah Creek Solar Farm North",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","North","CAISO System",null,1,3,5.25,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,1.31,1.64,2.2400000000000002,1.88,0.16,0.1,0.1,0.1]
["PUTHCR_1_PCNSB1","PUTHCR_1_PCNSB1_LESR","Putah Creek Solar Farm North",null,"OTHER","Hybrid_Storage","HYBD","CISO","North","CAISO System",null,1,5.25,5.25,"ID",1,"",false,1,0.86899999999999999,21,21,1,24,4,3,3,3,3,3,3,3,3,3,3,3,3]
["PUTHCR_1_SOLAR1",null,"Putah Creek Solar Farm",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,1.98,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.59,0.72,1.2,1.03,0.11,0.1,0.1,0.1]
["PVERDE_5_SCEDYN",null,"PVERDE_5_SCEDYN",null,null,"Nuclear","URANIUM","SRP","South",null,null,null,635,null,"FC","","",null," "," "," "," ",1,24,24,635,635,635,635,635,635,635,635,635,635,635,635]
["PWEST_1_UNIT",null,"PACIFIC WEST 1 WIND GENERATION",null,"WIND","Wind","WIND","CISO","South","LA Basin","Western",null,2.1,null,"FC","","",null," "," "," "," ",1,24,24,0.11,0.25,0.27,0.85,0.9,0.8,0.7,0.61,0.42,0.2,0.09,0.1]
["RAMON_2_SCEDYN",null,"RAMON_2_SCEDYN",null,"OTHER","Geothermal","GEOTHERMAL","IID","South",null,null,null,106.18,null,"FC","","",null," "," "," "," ",1,24,24,106.18,106.18,106.18,106.18,106.18,106.18,106.18,106.18,106.18,106.18,106.18,106.18]
["RATSKE_2_NROSR1",null,"North Rosamond Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.21,0.44,49.25,63.66,98.7,85.19,4.57,0.1,0.1,0.1]
["RATSKE_2_RBSSB1","RATSKE_2_RBSSB1_SUN","Rabbitbrush Solar 1",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,2,60,60,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.68,0.18,19.7,25.47,39.479999999999997,34.08,1.83,0.1,0.1,0.1]
["RATSKE_2_RBSSB1","RATSKE_2_RBSSB1_LESR","Rabbitbrush Solar 1",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,7.5,60,"ID",1,"",false,1,0.8,30,30,1,24,4,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5,7.5]
["RATSKE_2_RBSSB2","RATSKE_2_RBSSB2_SUN","Rabbitbrush Solar 2",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,2,40,40,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.1200000000000001,0.12,13.13,16.98,26.32,22.72,1.22,0.1,0.1,0.1]
["RATSKE_2_RBSSB2","RATSKE_2_RBSSB2_LESR","Rabbitbrush Solar 2",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,8,40,"ID",1,"",false,2,0.87,32,64,1,24,4,5,5,5,5,5,5,5,5,5,5,5,5]
["RCKCRK_7_UNIT 1",null,"ROCK CREEK HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,57,null,"FC","",13.9,null," "," "," "," ",1,24,24,13.9,13.9,13.9,13.9,10.72,13.9,13.9,13.9,13.9,0,5.6,13.43]
["RCKCRK_7_UNIT 2",null,"ROCK CREEK HYDRO UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","South of Palermo",1,56.9,null,"FC","",17.329999999999998,null," "," "," "," ",1,24,24,17.329999999999998,17.329999999999998,17.329999999999998,17.329999999999998,17.329999999999998,17.329999999999998,17.329999999999998,17.329999999999998,17.329999999999998,0,0,17.329999999999998]
["RDWAY_1_CREST",null,"CREST Contracts",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,6.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["RECTOR_2_CREST",null,"Rector Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,10.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["RECTOR_2_IVANPV",null,"Ivanhoe Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,3.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["RECTOR_2_KAWEAH",null,"KAWEAH PH 2 & 3 PSP AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,6.55,null,"FC","","",null," "," "," "," ",1,24,24,0.85,1.1100000000000001,1.6,1.93,1.98,1.83,0.39,0.03,0,0,0,0]
["RECTOR_2_KAWH 1",null,"KAWEAH PH 1 UNIT 1",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,2.25,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0.1,0.04,0.03,0,0,0,0]
["RECTOR_2_QF",null,"Kaweah Unit 1",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",1,20.09,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,8.4,6.7,0,0,0,0,1.2]
["RECTOR_2_TFDBM1",null,"Two Fiets Dairy Digester",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura","Rector, Vestal",null,0.8,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["RECTOR_7_TULARE",null,"MM Tulare ",null,"RECIPROCATING ENGINE","Biomass","BIOMASS","CISO","South","Big Creek-Ventura","Rector, Vestal",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["REDBLF_6_UNIT",null,"RED BLUFF PEAKER PLANT",null,"RECIPROCATING ENGINE","Reciprocating Engine","NATURAL GAS","CISO","North","CAISO System",null,1,44,null,"FC","","",null," "," "," "," ",1,24,24,44,44,44,44,44,44,44,44,44,44,44,44]
["REDMAN_2_SOLAR",null,"Lancaster East Avenue F",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3.75,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.11,0.1,1.23,1.59,2.4700000000000002,2.13,0.11,0.1,0.1,0.1]
["REDMAN_6_AVSSR1",null,"Antelope Valley Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["REEDLY_6_SOLAR",null,"Terzian",null,"PHOTO VOLTAIC","Solar_2Axis","SUN","CISO","North","Fresno","Herndon, Reedley",null,1.23,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["RENWD_1_QF",null,"Renwind re-powering project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.55000000000000004,1.18,1.27,4.03,4.3,3.79,3.33,2.92,2,0.94,0.43,0.46]
["RICHMN_1_CHVSR2",null,"Chevron 8.5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Bay Area",null,null,8.5,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.26,0.1,3.72,4.66,6.35,5.33,0.44,0.1,0.1,0.1]
["RICHMN_1_SOLAR",null,"Chevron 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Bay Area",null,null,2,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.87,1.1000000000000001,1.49,1.25,0.1,0.1,0.1,0.1]
["RICHMN_7_BAYENV",null,"BAY ENVIRONMENTAL (NOVE POWER)",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Bay Area",null,null,2.5,null,"FC","","",null," "," "," "," ",1,24,24,0.64,0.63,0.4,0.38,0.35,0.37,0.35,0.37,7.0000000000000007E-2,0.25,0.35,0.18]
["RIOBRV_6_UNIT 1",null,"RIO BRAVO HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,14,null,"FC","","",null," "," "," "," ",1,24,24,0.14000000000000001,0.19,0,1.51,2.42,4.12,3.39,1.31,0,0,0,0]
["RIOOSO_1_QF",null,"SMALL QF AGGREGATION - GRASS VALLEY",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,1.1100000000000001,null,"FC","","",null," "," "," "," ",1,24,24,0.04,7.0000000000000007E-2,0.08,0.28999999999999998,0.53,0.3,0.23,0.3,0.25,0.03,0.01,0.02]
["RNDMTN_2_SLSPHY1",null,"Silver Springs",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.6,null,"FC","","",null," "," "," "," ",1,24,24,0.2,0.21,0.19,0.18,0.18,0.17,0.15,0.15,0.14000000000000001,0.15,0.14000000000000001,0.14000000000000001]
["RNDSBG_1_HZASR1",null,"Hazel A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,2.99,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["ROLLIN_6_UNIT",null,"ROLLINS HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",2,13.5,null,"FC","","",null," "," "," "," ",1,24,24,7.78,5.81,5.23,8.3000000000000007,7.56,5.64,6.46,6.2,4.62,2.38,1.18,6.6]
["ROSMDW_2_WIND1",null,"Pacific Wind - Phase 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,140,null,"FC","","",null," "," "," "," ",1,24,24,7.63,16.47,17.79,56.49,60.21,53.08,46.65,40.85,28.01,13.1,6.06,6.43]
["ROSMND_6_SOLAR",null,"Lancaster B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.98,1.27,1.97,1.7,0.1,0.1,0.1,0.1]
["RSMSLR_6_SOLAR1",null,"Rosamond One",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.54,0.1,3.79,5.18,10.09,8.67,0.46,0.1,0.1,0.1]
["RSMSLR_6_SOLAR2",null,"Rosamond Two",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["RTEDDY_2_RWSBT1",null,"Wishon/San Joaquin  #1-A AGGREGATE",null,"HYDRO","Battery Storage","WATER","CISO","South","CAISO System",null,null,18.399999999999999,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,null,30,30,30,30,30,30,30]
["RTEDDY_2_RWSBT2",null,null,null,"PHOTO VOLTAIC","Battery Storage","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,null,30,30,30,30,30,30,30]
["RTEDDY_2_RWSBT3",null,"Wistaria Ranch Solar",null,"PHOTO VOLTAIC","Battery Storage","SUN","CISO","South","CAISO System",null,null,100,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,null,45,45,45,45,45,45,45]
["RTEDDY_2_RWSBT4",null,"Wildwood Solar I",null,"PHOTO VOLTAIC","Battery Storage","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,null,30,30,30,30,30,30,30]
["RTEDDY_2_RWSBT5",null,"Wildwood Solar 2",null,"PHOTO VOLTAIC","Battery Storage","SUN","CISO","South","CAISO System",null,null,15,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,null,12,12,12,12,12,12,12]
["RTEDDY_2_SC1SR3",null,"Rosamond West Solar Clean",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,40,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.1200000000000001,0.12,13.13,16.98,26.32,22.72,1.22,0.1,0.1,0.1]
["RTEDDY_2_SEBSR3",null,"Rosamond West Solar East Bay 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,56,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.57,0.17,18.39,23.77,36.85,31.8,1.71,0.1,0.1,0.1]
["RTEDDY_2_SEBSR4",null,"Rosamond West Solar East Bay 4",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,56,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.57,0.17,18.39,23.77,36.85,31.8,1.71,0.1,0.1,0.1]
["RTEDDY_2_SOLAR1",null,"Rosamond West Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,54,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.51,0.16,17.73,22.92,35.53,30.67,1.64,0.1,0.1,0.1]
["RTEDDY_2_SOLAR2",null,"Rosamond West Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,54,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.51,0.16,17.73,22.92,35.53,30.67,1.64,0.1,0.1,0.1]
["RTEDDY_2_SPASR4",null,"Rosamond West Solar Palo Alto",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,26,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.73,0.1,8.5399999999999991,11.04,17.11,14.77,0.79,0.1,0.1,0.1]
["RTEDDY_2_SRXSR4",null,"Rosamond West Solar Rosie X",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,13.6,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.38,0.1,4.46,5.77,8.9499999999999993,7.72,0.41,0.1,0.1,0.1]
["RTREE_2_WIND1",null,"Rising Tree 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,79.2,null,"FC","","",null," "," "," "," ",1,24,24,4.32,9.32,10.06,31.96,34.06,30.03,26.39,23.11,15.85,7.41,3.43,3.64]
["RTREE_2_WIND2",null,"Rising Tree 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,19.8,null,"FC","","",null," "," "," "," ",1,24,24,1.08,2.33,2.52,7.99,8.51,7.51,6.6,5.78,3.96,1.85,0.86,0.91]
["RTREE_2_WIND3",null,"Rising Tree 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,99,null,"FC","","",null," "," "," "," ",1,24,24,5.4,11.65,12.58,39.94,42.57,37.53,32.99,28.89,19.809999999999999,9.27,4.28,4.55]
["RUSCTY_2_UNITS",null,"Russell City Energy Center",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Bay Area","Ames",1,615.17999999999995,null,"FC","","",null," "," "," "," ",1,24,24,615.17999999999995,615.17999999999995,615.17999999999995,612.70000000000005,607.70000000000005,601,597.4,597.4,600.9,606.1,615.17999999999995,615.17999999999995]
["RVRVEW_1_UNITA1",null,"Riverview Energy Center (GP Antioch)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Bay Area","Contra Costa",1,48.7,null,"FC","","",null," "," "," "," ",1,24,24,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6,47.6]
["RVSIDE_2_RERCU3",null,"Riverside Energy Res. Ctr Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,49,null,"FC","","",null," "," "," "," ",1,24,24,49,49,49,49,49,49,49,49,49,49,49,49]
["RVSIDE_2_RERCU4",null,"Riverside Energy Res. Ctr Unit 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,49,null,"FC","","",null," "," "," "," ",1,24,24,49,49,49,49,49,49,49,49,49,49,49,49]
["RVSIDE_6_RERCU1",null,"Riverside Energy Res. Ctr Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,48.35,null,"FC","","",null," "," "," "," ",1,24,24,48.35,48.35,48.35,48.35,48.35,48.35,48.35,48.35,48.35,48.35,48.35,48.35]
["RVSIDE_6_RERCU2",null,"Riverside Energy Res. Ctr Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,48.5,null,"FC","","",null," "," "," "," ",1,24,24,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5,48.5]
["RVSIDE_6_SOLAR1",null,"Tequesquite Landfill Solar Project",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern",null,7.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.21,0.1,2.46,3.18,4.93,4.26,0.23,0.1,0.1,0.1]
["RVSIDE_6_SPRING",null,"SPRINGS GENERATION PROJECT AGGREGATE",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern",1,36,null,"FC","","",null," "," "," "," ",1,24,24,36,36,36,36,36,36,36,36,36,36,36,36]
["S_RITA_6_SOLAR1",null,"Sun Harvest Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SALIRV_2_UNIT",null,"Salinas River Cogeneration",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,39,null,"FC","","",null," "," "," "," ",1,24,24,23.11,22,23.11,21.52,17.170000000000002,19.170000000000002,17.55,19.23,19.61,19.48,21.65,23.33]
["SALTSP_7_UNITS",null,"SALT SPRINGS HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,46,null,"FC","","",null," "," "," "," ",1,24,24,1.6,4.72,12.8,0.4,17.46,16.93,18.559999999999999,24.1,6.32,4.24,2.8,20.7]
["SAMPSN_6_KELCO1",null,"KELCO QUALIFYING FACILITY",null,"COMBUSTION TURBINE","CHP","OTHER","CISO","South","San Diego-IV","San Diego",null,25,null,"FC","","",null," "," "," "," ",1,24,24,1.03,1.05,2.1800000000000002,2.77,3.33,3.81,2.44,1.59,3.62,1.85,1.24,2.21]
["SANBRN_2_EESSB2",null,"Edsan 2 Edwards Sanborn E1B",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,2,166,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,4.66,0.49,54.5,70.459999999999994,109.22,94.28,5.05,0.1,0.1,0.1]
["SANBRN_2_ES1BT3","SANBRN_2_ES1BT3_SUN","EdSan 1 Edwards 1",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","South","CAISO System",null,2,40,50.43,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.1200000000000001,0.12,13.13,16.98,26.32,22.72,1.22,0.1,0.1,0.1]
["SANBRN_2_ES1BT3","SANBRN_2_ES1BT3_LESR","EdSan 1 Edwards 1",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,22,50.43,"ID",1,"",false,1,0.8,88,88,1,24,4,22,22,22,22,22,22,22,22,22,22,22,22]
["SANBRN_2_ES2SB3","SANBRN_2_ES2SB3_SUN","EdSan 2 Sanborn 3",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,2,33,42,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.93,0.1,10.83,14.01,21.71,18.739999999999998,1,0.1,0.1,0.1]
["SANBRN_2_ES2SB3","SANBRN_2_ES2SB3_LESR","EdSan 2 Sanborn 3",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,2,18,42,"ID",1,"",false,1,0.8,72,72,1,24,4,18,18,18,18,18,18,18,18,18,18,18,18]
["SANBRN_2_ESABT1",null,"EdSan 1A",null,"OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,100,null,"ID",1,"",null,1,0.8,400,400,1,24,4,50,50,50,50,50,50,50,50,50,50,50,50]
["SANBRN_2_ESBBT1",null,"EdSan 1B",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,2,100,null,"ID",1,"",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["SANBRN_2_SS2BT3",null,"Sanborn Solar 2 SBESS 3",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,2,169,null,"ID",1,"",null,1,0.8,676,676,1,24,4,169,169,169,169,169,169,169,169,169,169,169,169]
["SANBRN_2_SS2BT4",null,"Sanborn Solar 2 SBESS 4",null,"OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,47,null,"ID","","",null,null,0.8,null,null,1,24,24,47,47,47,47,47,47,47,47,47,47,47,47]
["SANBRN_2_SS2SB4","SANBRN_2_SS2SB4_SUN","Sanborn Solar 2 Edwards Sanborn S4",null,"OTHER","Solar_1Axis","HYBD","CISO","South","CAISO System",null,1,36,36,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.01,0.11,11.82,15.28,23.69,20.45,1.1000000000000001,0.1,0.1,0.1]
["SANBRN_2_SS2SB4","SANBRN_2_SS2SB4_LESR","Sanborn Solar 2 Edwards Sanborn S5",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,1,18,36,"ID",1,"",null,1,0.8,72,72,1,24,4,72,72,72,72,72,72,72,72,72,72,72,72]
["SANDLT_2_SUNITS",null,"Mojave Solar",null,"STEAM","Solar_Thermal","SUN","CISO","South","CAISO System",null,null,275,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.0299999999999998,6.21,99.74,113.4,112.88,119.35,26.89,4.2699999999999996,0.1,0.1]
["SANITR_6_UNITS",null,"LACSD CARSON WATER POLLUTION AGGREGATE",null,"COMBINED CYCLE","Biogas","NATURAL GAS","CISO","South","LA Basin","Eastern",null,8,null,"FC","","",null," "," "," "," ",1,24,24,1.05,1.1000000000000001,0.2,0.18,0.66,0.65,0.84,1.1100000000000001,1.0900000000000001,0.78,0.66,0.52]
["SANLOB_1_LNDFIL",null,"Cold Canyon",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SANLOB_1_OSFBM1",null,"Old Santa Fe Road",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,1,0.85,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SANTFG_7_UNITS",null,"GEYSERS CALISTOGA AGGREGATE",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,72,null,"FC","","",null," "," "," "," ",1,24,24,72,72,72,72,72,72,72,72,72,72,72,72]
["SANTGO_2_LNDFL1",null,"Bowerman Power",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,19.600000000000001,null,"FC","","",null," "," "," "," ",1,24,24,18.54,18.97,17.899999999999999,18.82,18.12,19.53,18.66,18.64,18.5,17.79,18.48,19.600000000000001]
["SANTGO_2_MABBT1",null,"Millikan Avenue BESS",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin","Western",3,2,null,"FC","","",null,1,0.8,8,8,1,24,4,2,2,2,2,2,2,2,2,2,2,2,2]
["SANWD_1_QF",null,"San Gorgonio Farms Wind Farm",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,31,null,"FC","","",null," "," "," "," ",1,24,24,1.69,3.65,3.94,12.51,13.33,11.75,10.33,9.0500000000000007,6.2,2.9,1.34,1.42]
["SAUGUS_2_SPESBT1",null,"Voyager Wind Oasis Alta",null,"WIND","Battery Storage","WIND","CISO","South","Big Creek-Ventura",null,3,13.98,null,"FC","","",null,null,0.8,null,null,1,24,24,null,null,null,null,15,15,15,15,15,15,15,15]
["SAUGUS_6_CREST",null,"East Portal Hydro",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,null,1,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SAUGUS_6_MWDFTH",null,"Foothill Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,1,9.1,null,"FC","","",null," "," "," "," ",1,24,24,2.4,2.4,1.6,3.2,4.8,4,4.8,4,4,4.8,4,2.4]
["SAUGUS_6_QF",null,"SAUGUS QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura",null,null,2.19,null,"FC","","",null," "," "," "," ",1,24,24,7.0000000000000007E-2,0.2,0.14000000000000001,0.4,0.23,0.19,0.27,0.59,1,1,1,0.97]
["SAUGUS_7_CHIQCN",null,"Chiquita Canyon Landfill Fac",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura",null,null,8,null,"FC","","",null," "," "," "," ",1,24,24,5.55,5.28,5.34,5.43,5.63,5.37,5.14,5.34,4.8099999999999996,5.25,5.46,5.45]
["SBERDO_2_PSP3",null,"Mountainview Gen Sta. Unit 3",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Eastern, West of Devers",1,555,null,"FC","","",null," "," "," "," ",1,24,24,555,555,555,555,555,555,555,555,555,555,555,555]
["SBERDO_2_PSP4",null,"Mountainview Gen Sta. Unit 4",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Eastern, West of Devers",1,555,null,"FC","","",null," "," "," "," ",1,24,24,555,555,555,555,555,555,555,555,555,555,555,555]
["SBERDO_2_SNTANA",null,"SANTA ANA PSP",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, West of Devers",null,6.95,null,"FC","","",null," "," "," "," ",1,24,24,0.46,0.53,0.52,0.34,0.27,0,0,0,0,0,0,0]
["SBERDO_6_MILLCK",null,"MILL CREEK PSP",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, West of Devers",null,3.93,null,"FC","","",null," "," "," "," ",1,24,24,1.33,1.4,1.46,1.61,1.04,0.95,0.87,0.56999999999999995,0.62,0.54,0.78,0.89]
["SCARLT_2_SSABT1",null,"BUENA VISTA ENERGY, LLC",null,"WIND","Paired_BattStorage","WIND","CISO","North","Fresno",null,null,38,null,"ID",1,"",null,null,0.8,null,null,1,24,24,null,null,null,null,null,10,10,10,10,10,10,10]
["SCARLT_2_SSASR1",null,"Windstar",null,"WIND","Paired_Solar_1Axis","WIND","CISO","North","Fresno",null,null,120,null,"ID",1,"",null,null,null,null,null,1,24,24,null,null,null,null,null,12.55,13.78,11.83,10.54,6.97,5.29,3.16]
["SCARLT_2_SSBBT1",null,"Wolfskill Energy Center",null,"COMBUSTION TURBINE","Paired_BattStorage","NATURAL GAS","CISO","North","Fresno",null,null,48.68,null,"ID",1,"",null,null,0.8,null,null,1,24,24,null,null,null,null,null,30,30,30,30,30,30,30]
["SCARLT_2_SSBSR1",null,"Quinten Luallen",null,"HYDRO","Paired_Solar_1Axis","WATER","CISO","North","Fresno",null,null,7.3,null,"ID",1,"",null,null,null,null,null,1,24,24,null,null,null,null,null,11.45,12.53,10.69,9.41,6.11,4.4800000000000004,2.4700000000000002]
["SCHLTE_1_PL1X3",null,"Tracy Combined Cycle Power Plant",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Stockton","Tesla-Bellota",1,336.04,null,"FC","","",null," "," "," "," ",1,24,24,336.04,336.04,336.04,336.04,336.04,336.04,336.04,336.04,336.04,336.04,336.04,336.04]
["SCHNDR_1_FIVPTS",null,"Five Points Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,15,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.48,0.13,4.5,5.46,9.0500000000000007,7.79,0.8,0.1,0.1,0.1]
["SCHNDR_1_WSTSDE",null,"Westside Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,15,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.48,0.13,4.5,5.46,9.0500000000000007,7.79,0.8,0.1,0.1,0.1]
["SEARLS_7_ARGUS",null,"Argus Cogeneration",null,"OTHER","CHP","OTHER","CISO","South","CAISO System",null,null,19,null,"FC","","",null," "," "," "," ",1,24,24,4.75,5.75,4.49,4.47,3.15,2.06,1.1399999999999999,1.48,3.39,4.18,3.73,4.6100000000000003]
["SEGS_1_SR2SL2",null,"Sunray 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["SENTNL_2_CTG1",null,"Sentinel Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,107.68,null,"FC","","",null," "," "," "," ",1,24,24,107.68,107.68,107.68,107.68,107.68,107.68,107.68,107.68,107.68,107.68,107.68,107.68]
["SENTNL_2_CTG2",null,"Sentinel Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,104.19,null,"FC","","",null," "," "," "," ",1,24,24,103.98,103.98,103.98,103.98,103.98,103.98,103.98,103.98,103.98,103.98,103.98,103.98]
["SENTNL_2_CTG3",null,"Sentinel Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,105.69,null,"FC","","",null," "," "," "," ",1,24,24,105.69,105.69,105.69,105.69,105.69,105.69,105.69,105.69,105.69,105.69,105.69,105.69]
["SENTNL_2_CTG4",null,"Sentinel Unit 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,106.55,null,"FC","","",null," "," "," "," ",1,24,24,106.55,106.55,106.55,106.55,106.55,106.55,106.55,106.55,106.55,106.55,106.55,106.55]
["SENTNL_2_CTG5",null,"Sentinel Unit 5",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,107.52,null,"FC","","",null," "," "," "," ",1,24,24,107.52,107.52,107.52,107.52,107.52,107.52,107.52,107.52,107.52,107.52,107.52,107.52]
["SENTNL_2_CTG6",null,"Sentinel Unit 6",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,105,null,"FC","","",null," "," "," "," ",1,24,24,105,105,105,105,105,105,105,105,105,105,105,105]
["SENTNL_2_CTG7",null,"Sentinel Unit 7",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,106.73,null,"FC","","",null," "," "," "," ",1,24,24,106.73,106.73,106.73,106.73,106.73,106.73,106.73,106.73,106.73,106.73,106.73,106.73]
["SENTNL_2_CTG8",null,"Sentinel Unit 8",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Eastern, Valley-Devers",1,106.85,null,"FC","","",null," "," "," "," ",1,24,24,106.85,106.85,106.85,106.85,106.85,106.85,106.85,106.85,106.85,106.85,106.85,106.85]
["SGREGY_6_SANGER",null,"Algonquin Power Sanger 2",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","Fresno","Herndon",1,48.3,null,"FC","","",null," "," "," "," ",1,24,24,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08,48.08]
["SHELRF_1_UNITS",null,"SHELL OIL REFINERY AGGREGATE",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,100,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,33.33,0,0]
["SHUTLE_6_CREST",null,"CREST Contracts",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura",null,null,4,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SIERRA_1_UNITS",null,"HIGH SIERRA LIMITED",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Kern","South Kern PP",1,52.43,null,"FC","","",null," "," "," "," ",1,24,24,52.43,52.43,52.43,52.43,52.43,52.43,52.43,52.43,52.43,52.43,52.43,52.43]
["SIGHEB_6_HE2SCEDYN",null,"Heber 2",null,"COMBUSTION TURBINE","Geothermal","GEOTHERMAL","IID","South",null,null,null,28,null,"FC","","",null," "," "," "," ",1,24,24,28,28,28,28,28,28,28,28,28,28,28,28]
["SIGHEB_6_MIRDYN",null,"Heber South",null,"COMBUSTION TURBINE","Geothermal","GEOTHERMAL","IID","South",null,null,null,17,null,"FC","","",null," "," "," "," ",1,24,24,17,17,17,17,17,17,17,17,17,17,17,17]
["SISPRG_2_DS3BT1",null,"Daggett Solar 3 a BESS","SISPRG_2_DS3SR1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,null,61.16,123,"ID",1,"",null,1,0.8,246,246,1,24,4,61.5,61.5,61.5,61.5,61.5,61.5,61.5,61.5,61.5,61.5,61.5,61.5]
["SISPRG_2_DS3BT2",null,"Daggett 3 B BESS","SISPRG_2_DS3SR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,60,110,"ID",1,"",false,1,0.8,240,240,1,24,4,60,60,60,60,60,60,60,60,60,60,60,60]
["SISPRG_2_DS3BT3",null,"Daggett Solar 3 cd BESS","SISPRG_2_DS3SR3","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,12.5,50,"ID",1,"",null,1,0.8,50,50,1,24,4,12.5,12.5,12.5,12.5,12.5,12.5,12.5,12.5,12.5,12.5,12.5,12.5]
["SISPRG_2_DS3BT4",null,"Daggett Solar 3 e BESS","SISPRG_2_DS3SR4","OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,1,15,17,"ID",1,"",null,1,0.8,60,60,1,24,4,15,15,15,15,15,15,15,15,15,15,15,15]
["SISPRG_2_DS3SR1",null,"Daggett Solar 3 a PV","SISPRG_2_DS3BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,123,123,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.45,0.36,40.380000000000003,52.2,80.930000000000007,69.849999999999994,3.75,0.1,0.1,0.1]
["SISPRG_2_DS3SR2",null,"Daggett 3 B PV","SISPRG_2_DS3BT2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,110,110,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.09,0.32,36.11,46.69,72.38,62.47,3.35,0.1,0.1,0.1]
["SISPRG_2_DS3SR3",null,"Daggett Solar 3 cd PV","SISPRG_2_DS3BT3","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,50,50,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,1.4,0.15,16.420000000000002,21.22,32.9,28.4,1.52,0.1,0.1,0.1]
["SISPRG_2_DS3SR4",null,"Sutter Power Plant Pseudo-CISO","SISPRG_2_DS3BT4","COMBINED CYCLE","Solar_1Axis","NATURAL GAS","CISO","South","CAISO System",null,null,275,17,"ID",1,"",15,null,null,null,null,1,24,24,null,null,0.48,0.05,5.58,7.22,11.19,9.65,0.52,0.1,0.1,0.1]
["SISQUC_1_SMARIA",null,"Santa Maria II LFG Power Plant",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,1.42,null,"FC","","",null," "," "," "," ",1,24,24,0.99,1.01,1,1.01,1.01,1.03,1.02,1.03,0.69,0.69,1.02,1.03]
["SKERN_6_SOLAR1",null,"South Kern Solar PV Plant",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern 70 kV",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["SKERN_6_SOLAR2",null,"SKIC Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Kern","South Kern PP, Kern 70 kV",null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.3,0.1,4.37,5.48,7.47,6.27,0.52,0.1,0.1,0.1]
["SLATE_2_SLASR1",null,"Slate",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,50.5,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.54,0.52,22.07,27.66,37.71,31.66,2.64,0.1,0.1,0.1]
["SLATE_2_SLASR2","SLATE_2_SLASR2_SUN","SLATE_2",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,2,93,93,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3,0.78,27.87,33.880000000000003,56.13,48.28,4.95,0.11,0.1,0.1]
["SLATE_2_SLASR2","SLATE_2_SLASR2_LESR","SLATE_2",null,"OTHER","Hybrid_Storage","HYBD","CISO","North","Fresno",null,2,46.5,93,"ID",1,"",false,1,0.88,186,186,1,24,4,46.5,46.5,46.5,46.5,46.5,46.5,46.5,46.5,46.5,46.5,46.5,46.5]
["SLATE_2_SLASR3","SLATE_2_SLASR3_SUN","SLATE_3",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,2,67.5,67.5,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,2.1800000000000002,0.56999999999999995,20.23,24.59,40.74,35.04,3.59,0.1,0.1,0.1]
["SLATE_2_SLASR3","SLATE_2_SLASR3_LESR","SLATE_3",null,"OTHER","Hybrid_Storage","HYBD","CISO","North","Fresno",null,2,33.75,67.5,"ID",1,"",false,1,0.8,135,135,1,24,4,33.75,33.75,33.75,33.75,33.75,33.75,33.75,33.75,33.75,33.75,33.75,33.75]
["SLATE_2_SLASR4","SLATE_2_SLASR4_SUN","SLATE_4",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,3,63,63,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,2.0299999999999998,0.53,18.88,22.95,38.020000000000003,32.71,3.35,0.1,0.1,0.1]
["SLATE_2_SLASR4","SLATE_2_SLASR4_LESR","SLATE_4",null,"OTHER","Hybrid_Storage","HYBD","CISO","North","Fresno",null,3,50,63,"ID",1,"",false,1,0.8,200,200,1,24,4,50,50,50,50,50,50,50,50,50,50,50,50]
["SLATE_2_SLASR5","SLATE_2_SLASR5_SUN","Slate 5",null,"OTHER","Hybrid_SolarFixed","HYBD","CISO","North","Fresno",null,2,26,26,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.84,0.22,7.79,9.4700000000000006,15.69,13.5,1.38,0.1,0.1,0.1]
["SLATE_2_SLASR5","SLATE_2_SLASR5_LESR","Slate 5",null,"OTHER","Hybrid_Storage","HYBD","CISO","North","Fresno",null,2,10,26,"ID",1,"",false,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["SLRMS3_2_SRMSR1",null,"SILVER RIDGE MOUNT SIGNAL 3",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,250,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,7.01,0.74,82.08,106.11,164.49,141.97999999999999,7.61,0.1,0.1,0.1]
["SLST13_2_SOLAR1",null,"Quinto Solar PV Project",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,107.6,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,3.28,1.1100000000000001,47.03,58.94,80.34,67.459999999999994,5.62,0.1,0.1,0.1]
["SLSTR1_2_SOLAR1",null,"Solar Star 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,310,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,8.6999999999999993,0.91,101.78,131.57,203.97,176.06,9.44,0.1,0.1,0.1]
["SLSTR2_2_SOLAR2",null,"Solar Star 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,276,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,7.74,0.81,90.61,117.14,181.6,156.75,8.4,0.1,0.1,0.1]
["SLUISP_2_UNITS",null,"SAN LUIS (GIANELLI) PUMP-GEN (AGGREGATE)",null,"PUMPED STORAGE","Pumped Hydro","WATER","CISO","North","CAISO System",null,null,374.43,null,"FC","","",null," "," "," "," ",1,24,24,0,46.13,42.68,99.91,83.47,66.459999999999994,0,0,0,0,0,0]
["SLYCRK_1_UNIT 1",null,"SLY CREEK HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",1,13,null,"FC","","",null," "," "," "," ",1,24,24,6.03,7.07,7.2,8,8.8000000000000007,8.8000000000000007,8,9.77,7.18,7.2,6.4,6.74]
["SMPRIP_1_SMPSON",null,"Ripon Cogeneration Unit 1",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","CAISO System",null,1,46.05,null,"FC","","",null," "," "," "," ",1,24,24,46.05,46.05,46.05,46.05,46.05,46.05,46.05,46.05,46.05,46.05,46.05,46.05]
["SMRCOS_6_LNDFIL",null,"San Marcos Energy",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","South","San Diego-IV","San Diego",null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,1.5,1.5,1.5,1.5,1.49,1.48,1.5,1.5,1.5,1.5,1.5,1.5]
["SMUDGO_7_UNIT 1",null,"SONOMA POWER PLANT",null,"STEAM","Geothermal","GEOTHERMAL","CISO","North","NCNB",null,1,64.8,null,"FC","","",null," "," "," "," ",1,24,24,47,47,47,47,47,47,47,47,47,47,47,47]
["SMYRNA_1_DL1SR1",null,"Delano Land 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.44,0.55000000000000004,0.75,0.63,0.1,0.1,0.1,0.1]
["SNCLRA_2_HOWLNG",null,"Houwelings Nurseries Oxnard, Inc",null,"RECIPROCATING ENGINE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,12.71,null,"FC","","",null," "," "," "," ",1,24,24,6.1,6.85,6.43,5.62,4.4400000000000004,6.64,5.0199999999999996,5.03,5.48,2.97,3.65,2.82]
["SNCLRA_2_SILBT1",null,"Silverstrand BESS",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",3,11,null,"FC","","",null,1,0.8,44,44,1,24,4,11,11,11,11,11,11,11,11,11,11,11,11]
["SNCLRA_2_SPRHYD",null,"Springville Hydroelectric Generator",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.05,0.03,0.11,0.06,0.06,0.13,0.15,0.16,0.1,0.04,0.03,0.03]
["SNCLRA_2_UNIT",null,"Channel Islands Power",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",1,27.5,null,"FC","","",null," "," "," "," ",1,24,24,27.5,27.5,27.5,27.5,27.5,27.5,27.5,27.5,27.5,27.5,27.5,27.5]
["SNCLRA_2_UNIT1",null,"New Indy Oxnard",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",1,27.8,null,"FC","","",null," "," "," "," ",1,24,24,27.8,27.8,27.8,27.8,27.8,27.8,27.8,27.8,27.8,27.8,27.8,27.8]
["SNCLRA_2_VESBT1",null,"Ventura Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",3,100,null,"FC","","",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["SNCLRA_6_OXGEN",null,"OXGEN",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",2,47.7,null,"FC","","",null," "," "," "," ",1,24,24,47.7,47.7,47.7,47.7,47.7,47.7,47.7,47.7,47.7,47.7,47.7,47.7]
["SNCLRA_6_PROCGN",null,"Procter and Gamble Oxnard 2",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,47.9,null,"FC","","",null," "," "," "," ",1,24,24,28.35,22.46,28.38,28.33,28.21,28.06,27.46,19.41,19.22,19.2,19.239999999999998,19.440000000000001]
["SNCLRA_6_QF",null,"SANTA CLARA QFS",null,"OTHER","CHP","OTHER","CISO","South","Big Creek-Ventura","S.Clara, Moorpark",null,1.65,null,"FC","","",null," "," "," "," ",1,24,24,0.22,0.22,0.18,0.24,0.23,0.25,0.24,0.31,0.3,0.26,0.34,0.46]
["SNDBAR_7_UNIT 1",null,"SANDBAR",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,16.2,null,"FC","","",null," "," "," "," ",1,24,24,8.92,4.25,0.68,6.47,6.64,6.6,5.42,3.57,3.19,0.7,5.81,12.69]
["SNMALF_6_UNITS",null,"Sonoma County Landfill",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","NCNB","Fulton",null,5,null,"FC","","",null," "," "," "," ",1,24,24,3.07,2.54,3.24,3.21,2.87,2.61,3.15,3.05,3.02,3.02,3.13,2.87]
["SNORA_2_SNRSLR",null,"Sonora (Solar Gen 2)",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","IID","South",null,null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.35,0.1,9.4700000000000006,12.94,25.23,21.69,1.1499999999999999,0.1,0.1,0.1]
["SOLBLU_2_WSBBX2",null,"Westlands Solar Blue BESS","SOLBLU_2_WSBSX2","OTHER","Paired_BattStorage","LESR","CISO","North","CAISO System",null,2,225,250,"ID","","",null,null,0.8,null,null,1,24,24,225,225,225,225,225,225,225,225,225,225,225,225]
["SOLBLU_2_WSBSX2",null,"Westlands Solar Blue","SOLBLU_2_WSBBX2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","North","CAISO System",null,null,250,250,"ID","","",null,null,null,null,null,1,24,24,0.1,0.1,7.61,2.59,109.27,136.94999999999999,186.66,156.75,13.05,0.22,0.1,0.1]
["SOUTH_2_UNIT",null,"SOUTH HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,7.1,null,"FC","","",null," "," "," "," ",1,24,24,2.73,3.12,2.46,1.1499999999999999,2.3199999999999998,1.45,1.26,1.07,1.04,1.1100000000000001,1.36,1.35]
["SPAULD_6_UNIT 3",null,"SPAULDING HYDRO PH 3 UNIT",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",null,6.5,null,"FC","","",null," "," "," "," ",1,24,24,0.8,0.79,0.79,1.0900000000000001,3.42,0.73,1.68,3.53,2.96,1.93,0.62,0.82]
["SPAULD_6_UNIT12",null,"SPAULDING HYDRO PH 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso, South of Palermo",1,11.4,null,"FC","","",null," "," "," "," ",1,24,24,2.98,1.65,1.8,1.92,4.4400000000000004,4.4000000000000004,3.41,3.62,1.2,1.2,1.6,2.58]
["SPBURN_2_UNIT 1",null,"Burney Biomass",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,22,null,"FC","","",null," "," "," "," ",1,24,24,9.91,10.64,10.78,10.62,10.63,12.14,12.75,12.66,12.76,11.94,10.89,9.33]
["SPBURN_7_SNOWMT",null,"Burney Creek Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,3,null,"FC","","",null," "," "," "," ",1,24,24,0.2,0.02,0.19,0.92,0.44,0,0,0,0,0.01,0.01,0.06]
["SPI LI_2_UNIT 1",null,"Lincoln Biomass",null,"STEAM","Biomass","BIOMASS","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,17.2,null,"FC","","",null," "," "," "," ",1,24,24,7.56,6.64,6.38,6.26,8.39,9.34,9.43,9.5500000000000007,9.43,8.52,6.71,7.03]
["SPIAND_1_ANDSN2",null,"SPI Anderson 2",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,27.15,null,"FC","","",null," "," "," "," ",1,24,24,12.23,13.3,14.75,14.47,16.25,17.899999999999999,17.77,18.420000000000002,18.34,15.65,14.85,14.87]
["SPICER_1_UNITS",null,"SPICER HYDRO UNITS 1-3 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,6,null,"FC","","",null," "," "," "," ",1,24,24,0.36,0.36,0.33,0.19,0.23,1.63,2.15,2.3199999999999998,1.85,1.58,1.06,1]
["SPIFBD_1_PL1X2",null,"SIERRA PACIFIC IND. (SONORA)",null,"STEAM","CHP","BIOMASS","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,7.5,null,"FC","","",null," "," "," "," ",1,24,24,2.62,2.61,2.72,2.58,3.03,3.29,3.55,3.78,3.72,3.12,2.78,2.54]
["SPQUIN_6_SRPCQU",null,"Quincy Biomass",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,24,null,"FC","","",null," "," "," "," ",1,24,24,18.25,16.86,16.760000000000002,14.42,19.079999999999998,21.09,19.62,14.76,13.92,10.5,9.59,15.22]
["SPRGAP_1_UNIT 1",null,"SPRING GAP HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,7,null,"FC","","",null," "," "," "," ",1,24,24,2.19,1.89,3.03,4.8899999999999997,4.9000000000000004,1.63,0,0,3.1,3.9,2.5299999999999998,3.22]
["SPRGVL_2_CREST",null,"Springerville Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,3,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SPRGVL_2_EXETPV",null,"Exeter Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,3.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SPRGVL_2_LINDPV",null,"Lindsay Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,4,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SPRGVL_2_PORTPV",null,"Porterville Tulare PV",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Rector, Vestal",null,3.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SPRGVL_2_TULESC",null,"TULE RIVER HYDRO PLANT (SCE)",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Rector, Vestal",null,2.5,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SRINTL_6_UNIT",null,"SRI INTERNATIONAL",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","North","Bay Area",null,null,6.9,null,"FC","","",null," "," "," "," ",1,24,24,1.32,1.24,1.36,1.39,1.32,1.0900000000000001,1,0.96,0.9,0.98,1.23,1.27]
["STANIS_7_UNIT 1",null,"STANISLAUS HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",1,91,null,"FC","","",null," "," "," "," ",1,24,24,66.66,56.75,54.07,40,28,59,61.99,70.02,56.65,20.88,0,65.849999999999994]
["STANTN_2_SBEBX2",null,"Stanton Battery Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","LA Basin",null,1,68.8,null,"FC",0,"",null,1,0.8,275.2,275.2,1,24,4,68.8,68.8,68.8,68.8,68.8,68.8,68.8,68.8,68.8,68.8,68.8,68.8]
["STANTN_2_STAGT1",null,"Stanton 1",null,"OTHER","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,49.65,null,"FC","","",null," "," "," "," ",1,24,24,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65]
["STANTN_2_STAGT2",null,"Stanton 2",null,"OTHER","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,49.65,null,"FC","","",null," "," "," "," ",1,24,24,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65,49.65]
["STIGCT_2_LODI",null,"LODI STIG UNIT",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","South of Rio Oso, South of Palermo",1,49.9,null,"FC","","",null," "," "," "," ",1,24,24,49.5,49.5,49.5,49.5,49.5,49.5,49.5,49.5,49.5,49.5,49.5,49.5]
["STNRES_1_UNIT",null,"Covanta Stanislaus",null,"STEAM","Biomass","WASTE TO POWER","CISO","North","Stockton","Tesla-Bellota",null,19.899999999999999,null,"FC","","",null," "," "," "," ",1,24,24,15.91,19.309999999999999,19.02,15.14,13.88,17.579999999999998,19.43,19.79,19.32,18.87,19.39,18.170000000000002]
["STOILS_1_UNITS",null,"Chevron Richmond Refinery",null,"COMBINED CYCLE","CHP","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,56.2,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,5.33,9.44,0,11.34,16.559999999999999,0]
["STOREY_2_MDRCH2",null,"Madera Chowchilla 2",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,0.56000000000000005,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0.04,0.19,0.32,0.04,0,0,0,0]
["STOREY_2_MDRCH3",null,"Madera Chowchilla 3",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,0.42,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0.01,0.11,0.22,0.02,0,0,0,0]
["STOREY_2_MDRCH4",null,"Madera Chowchilla 4",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,0.92,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0.01,0.1,0.31,0.01,0,0,0,0]
["STOREY_7_MDRCHW",null,"Madera Canal Site 980",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,null,1.84,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0.45,0.82,0.06,0,0,0,0]
["STRAUS_1_STRWD1",null,"Strauss Wind, LLC",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,95.25,null,"FC","","",null,null,null,null,null,1,24,24,5.19,11.2,12.1,38.43,40.96,36.11,31.74,27.79,19.059999999999999,8.92,4.12,4.37]
["STROUD_6_SOLAR",null,"Stroud Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["STROUD_6_WWHSR1",null,"Winter Wheat Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["SUMWHT_6_SWSSR1",null,"Summer Wheat Solar Farm",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,18.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.19,8.09,10.130000000000001,13.81,11.6,0.97,0.1,0.1,0.1]
["SUNCAT_2_A1ABT1",null,"Arlington Solar Unit 1A BESS ","ARLNTN_2_ASUSR1, SUNCAT_2_A1BBT1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,47,131,"ID",1,"",false,1,0.8,188,188,1,24,4,47,47,47,47,47,47,47,47,47,47,47,47]
["SUNCAT_2_A1BBT1",null,"Arlington Solar Unit 1B BESS ","ARLNTN_2_ASUSR1, SUNCAT_2_A1ABT1","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,63,131,"ID",1,"",false,1,0.8,252,252,1,24,4,63,63,63,63,63,63,63,63,63,63,63,63]
["SUNCAT_2_A2ABT2",null,"Arlington Solar Unit 2A BESS ","ARLNTN_2_AR1SR1, SUNCAT_2_A2BSR2","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,2,132,269,"ID",1,"",false,1,0.8,528,528,1,24,4,132,132,132,132,132,132,132,132,132,132,132,132]
["SUNCAT_2_A2BSR2",null,"Arlington Solar Unit 2B","ARLNTN_2_AR1SR1, SUNCAT_2_A2ABT2","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,133,269,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3.73,0.39,43.67,56.45,87.51,75.53,4.05,0.1,0.1,0.1]
["SUNRIS_2_PL1X3",null,"Sunrise Power Project AGGREGATE II",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","North","CAISO System",null,1,586.02,null,"FC","","",null," "," "," "," ",1,24,24,586.02,586.02,586.02,586.02,586.02,586.02,586.02,586.02,586.02,586.02,586.02,586.02]
["SUNSET_2_UNITS",null,"MIDWAY SUNSET COGENERATION PLANT",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,1,248,null,"FC","","",null," "," "," "," ",1,24,24,248,248,248,245,240,234,229,229,231,243,246,248]
["SUNSHN_2_LNDFL",null,"Sunshine Gas Producers",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","South","Big Creek-Ventura",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,17.489999999999998,16.89,17.350000000000001,16.579999999999998,17.14,16.97,16.399999999999999,15.75,15.88,15.59,16.8,15.43]
["SUNSLR_1_SSVSR1",null,"Sunshine Valley Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["SUNSPT_2_WNASR1",null,"Windhub Solar A",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["SUNST2_5_SS2SR1",null,"Sun Streams Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,150,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.21,0.44,49.25,63.66,98.7,85.19,4.57,0.1,0.1,0.1]
["SUNSTR_5_SS1SCEDYN",null,"Sunstream Solar 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","AZPS","South",null,null,1,150,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,4.0599999999999996,0.21,28.4,38.82,75.7,65.06,3.45,0.1,0.1,0.1]
["SUTTER_2_CISO",null,"Sutter Power Plant Pseudo-CISO",null,"COMBINED CYCLE","CCGT","NATURAL GAS","BANC","North",null,null,1,275,null,"FC","","",null," "," "," "," ",1,24,24,275,275,275,275,275,275,275,275,275,275,275,275]
["SYCAMR_2_UNIT 1",null,"Sycamore Cogeneration Unit 1",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,null,74,null,"FC","","",null," "," "," "," ",1,24,24,74,74,74,74,74,74,74,74,74,74,74,74]
["SYCAMR_2_UNIT 2",null,"Sycamore Cogeneration Unit 2",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,76,null,"FC","","",null," "," "," "," ",1,24,24,76,76,76,76,76,76,76,76,76,76,76,76]
["SYCAMR_2_UNIT 3",null,"Sycamore Cogeneration Unit 3",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,74,null,"FC","","",null," "," "," "," ",1,24,24,74,74,74,74,74,74,74,74,74,74,74,74]
["SYCAMR_2_UNIT 4",null,"Sycamore Cogeneration Unit 4",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,76,null,"FC","","",null," "," "," "," ",1,24,24,76,76,76,76,76,76,76,76,76,76,76,76]
["TANHIL_6_SOLART",null,"Berry Cogen 18",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,17,null,"FC","","",null," "," "," "," ",1,24,24,12.04,12.08,11.77,12.17,12.38,11.78,11.36,11.05,11.1,12.04,11.36,11.07]
["TBLMTN_6_QF",null,"SMALL QF AGGREGATION - PARADISE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1.7,null,"FC","","",null," "," "," "," ",1,24,24,0.19,0.24,0.22,0.21,0.22,0.18,0.2,0.19,0.19,0.16,0.16,0.18]
["TECOLOTE_3_WBDYN",null,"TECOLOTE WIND",null,"WIND","Wind","WIND","PNM","South",null,null,1,271.68,null,"FC","","",null," "," "," "," ",1,24,24,130.76,112.81,92.3,110.24,102.55,82.04,56.31,53.84,61.53,64.099999999999994,102.55,143.57]
["TEHAPI_2_PW1WD1",null,"Point Wind 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,47.49,null,"FC","","",null," "," "," "," ",1,24,24,2.59,5.59,6.04,19.16,20.420000000000002,18.010000000000002,15.82,13.86,9.5,4.45,2.0499999999999998,2.1800000000000002]
["TEHAPI_2_PW2WD2",null,"Point Wind 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,14.4,null,"FC","","",null," "," "," "," ",1,24,24,0.79,1.69,1.83,5.81,6.19,5.46,4.8,4.2,2.88,1.35,0.62,0.66]
["TEHAPI_2_WIND1",null,"Wind Wall Monolith 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,19.850000000000001,null,"FC",0,"",null," "," "," "," ",1,24,24,1.08,2.33,2.52,8.01,8.5399999999999991,7.53,6.61,5.79,3.97,1.86,0.86,0.91]
["TEHAPI_2_WIND2",null,"Wind Wall Monolith 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,23.66,null,"FC",0,"",null," "," "," "," ",1,24,24,1.29,2.78,3.01,9.5500000000000007,10.17,8.9700000000000006,7.88,6.9,4.7300000000000004,2.21,1.02,1.0900000000000001]
["TENGEN_2_PL1X2",null,"Placerita Canyon Cogen",null,"COMBUSTION TURBINE","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura",null,1,37.700000000000003,null,"FC","","",null," "," "," "," ",1,24,24,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003,37.700000000000003]
["TERMEX_2_PL1X3",null,"TDM",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","San Diego-IV",null,1,625,null,"FC","","",null," "," "," "," ",1,24,24,605,605,605,605,601,593,591,593,596,605,605,605]
["TESLA_1_QF",null,"SMALL QF AGGREGATION - STOCKTON",null,"OTHER","CHP","OTHER","CISO","North","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.09,7.0000000000000007E-2,0.1,0.13,0.17,0.32,0.23,0.2,0.17,7.0000000000000007E-2,0.04,7.0000000000000007E-2]
["TIDWTR_2_UNITS",null,"MARTINEZ COGEN LIMITED PARTNERSHIP",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,114.8,null,"FC","","",null," "," "," "," ",1,24,24,33.06,37.659999999999997,30.76,37.11,52.09,49.61,52.59,81.900000000000006,88.36,88.04,43.35,40.43]
["TIFFNY_1_DILLON",null,"TIFFNY_1_DILLON",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,45,null,"FC","","",null," "," "," "," ",1,24,24,2.4500000000000002,5.29,5.72,18.16,19.350000000000001,17.059999999999999,15,13.13,9,4.21,1.95,2.0699999999999998]
["TIGRCK_7_UNITS",null,"TIGER CREEK HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,62,null,"FC","","",null," "," "," "," ",1,24,24,26,16.8,14.17,0,16.66,36.799999999999997,33.909999999999997,40.4,36.08,30.37,30.43,28.38]
["TITANS_2_TTSSR1",null,"Titan Solar 1 Pseudo",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","IID","South",null,null,null,70,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.96,0.21,22.98,29.71,46.06,39.75,2.13,0.1,0.1,0.1]
["TKOPWR_6_HYDRO",null,"Bear Creek Hydroelectric Project",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,2.83,null,"FC","","",null," "," "," "," ",1,24,24,0.35,0.27,0,0.16,0,0,0,0,0,0.04,0.04,0.12]
["TMPLTN_2_SOLAR",null,"Vintner Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["TOADTW_6_UNIT",null,"TOAD TOWN",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.38,0.59,0.37,0.26,0.39,0.28000000000000003,0.2,0.18,0.03,0.03,0.11,0.06]
["TOPAZ_2_SOLAR",null,"Topaz Solar Farms",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,550,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,17.72,4.62,164.83,200.38,331.96,285.54000000000002,29.27,0.64,0.1,0.1]
["TORTLA_1_SOLAR",null,"Longboat Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["TOWNSITE_2_MEADDYN","TOWNSITE_2_MEADDYN_SUN","Townsite Solar BESS",null,"OTHER","Hybrid_Solar1Axis","HYBD","WALC","South",null,null,2,180,180,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,5.05,0.53,59.1,76.400000000000006,118.44,102.23,5.48,0.1,0.1,0.1]
["TOWNSITE_2_MEADDYN","TOWNSITE_2_MEADDYN_LESR","Townsite Solar BESS",null,"OTHER","Hybrid_Storage","HYBD","WALC","South",null,null,2,90,180,"FC","","",false,1,0.8,720,720,1,24,4,20,20,20,20,20,20,20,20,20,20,20,20]
["TRNQL8_2_AMASR1",null,"Tranquillity 8 Amarillo",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["TRNQL8_2_AZUSR1",null,"Tranquillity 8 Azul",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,20,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["TRNQL8_2_ROJSR1",null,"Tranquillity 8 Rojo",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,100,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,3.05,1.04,43.71,54.78,74.66,62.7,5.22,0.1,0.1,0.1]
["TRNQL8_2_VERSR1",null,"Tranquillity 8 Verde",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,60,null,"ID",1,"",null," "," "," "," ",1,24,24,0.1,0.1,1.83,0.62,26.22,32.869999999999997,44.8,37.619999999999997,3.13,0.1,0.1,0.1]
["TRNQLT_2_RETBT1",null,"RE Tranquillity BESS","TRNQLT_2_SOLAR","OTHER","Paired_BattStorage","LESR","CISO","North","Fresno",null,1,72,200,"FC","","",false,2.801535263073724,0.87590000000000001,288,806.84215576523252,1,24,11.206141052294896,72,72,72,72,72,72,72,72,72,72,72,72]
["TRNQLT_2_SOLAR",null,"Tranquillity","TRNQLT_2_RETBT1","PHOTO VOLTAIC","Paired_Solar_Fixed","SUN","CISO","North","Fresno",null,null,200,200,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,6.45,1.68,59.94,72.87,120.71,103.83,10.64,0.23,0.1,0.1]
["TRNSWD_1_QF",null,"FPL Energy C Wind",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,38.97,null,"FC","","",null," "," "," "," ",1,24,24,2.12,4.58,4.95,15.72,16.760000000000002,14.77,12.99,11.37,7.8,3.65,1.69,1.79]
["TULARE_2_TULBM1",null,"Tulare BioMAT Fuel Cell",null,"OTHER","Biogas","BIOGAS","CISO","South","Big Creek-Ventura",null,null,2.8,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["TULEWD_1_TULWD1",null,"Tule Wind",null,"WIND","Wind","WIND","CISO","South","San Diego-IV","Eastern, Valley-Devers",null,130.5,null,"FC","","",null," "," "," "," ",1,24,24,7.11,15.35,16.579999999999998,52.65,56.12,49.48,43.49,38.08,26.11,12.22,5.65,5.99]
["TULLCK_7_UNITS",null,"Tullock Hydro",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota",null,25.9,null,"FC","","",null," "," "," "," ",1,24,24,3.87,7.97,12.42,16.579999999999998,20.51,23.23,20.55,18.149999999999999,12.68,8.82,1.58,2.4700000000000002]
["TUPMAN_1_BIOGAS",null,"ABEC Bidart-Stockale #1",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,0.6,null,"FC","","",null," "," "," "," ",1,24,24,0.32,0.32,0.32,0.33,0.33,0.35,0.34,0.33,0.35,0.32,0.3,0.3]
["TVYVLY_6_KRSHY1",null,"Kings River Syphon",null,"HYDRO","Hydro","WATER","CISO","North","Fresno",null,1,1.3,null,"FC","","",null," "," "," "," ",1,24,24,0.25,0.36,0,0,0,0.2,0.25,0.32,0.25,0.19,0,0.32]
["TWISSL_6_SOLAR",null,"Nickel 1 (\"NLH1\")",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,1.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.45,0.55000000000000004,0.91,0.78,0.1,0.1,0.1,0.1]
["TWISSL_6_SOLAR1",null,"Coronal Lost Hills",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["TX-ELK_6_ECKSR2",null,"Eagle Creek",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,3,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["TX-ELK_6_SOLAR1",null,"Castor",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["TXMCKT_6_UNIT",null,"McKittrick Cogen",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,11.2,null,"FC","","",null," "," "," "," ",1,24,24,4.1399999999999997,3.98,3.48,4.26,3.99,4.0599999999999996,3.85,3.93,3.96,3.82,3.83,4.0999999999999996]
["UKIAH_7_LAKEMN",null,"UKIAH LAKE MENDOCINO HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","NCNB","Eagle Rock, Fulton",1,3.5,null,"FC","","",null," "," "," "," ",1,24,24,0.28999999999999998,0.22,0.57999999999999996,0.48,0.48,0.71,0.87,0.87,0.72,0.63,0.35,0.38]
["ULTPCH_1_UNIT 1",null,"Pacific Ultrapower Chinese Station",null,"STEAM","Biomass","BIOMASS","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,18,null,"FC","","",null," "," "," "," ",1,24,24,17.989999999999998,17.36,15.48,15.96,17.809999999999999,11.8,17.37,17.809999999999999,17,16.510000000000002,14.92,17.62]
["ULTPFR_1_UNIT 1",null,"Rio Bravo Fresno",null,"STEAM","Biomass","BIOMASS","CISO","North","Fresno","Herndon",null,24.3,null,"FC","","",null," "," "," "," ",1,24,24,22.81,23.17,23.93,18.63,23.2,22.81,22.94,16.100000000000001,14.8,14.6,18.88,21.77]
["ULTRCK_2_UNIT",null,"Rio Bravo Rocklin",null,"STEAM","Biomass","BIOMASS","CISO","North","Sierra","Drum-Rio Oso, South of Rio Oso, South of Palermo",null,24.4,null,"FC","","",null," "," "," "," ",1,24,24,15.73,20.84,23.09,21.71,21.8,23.36,21.68,23.38,19.510000000000002,22.69,23.36,22.6]
["UNOCAL_1_UNITS",null,"TOSCO (RODEO PLANT)",null,"FTUR","Peaker","NATURAL GAS","CISO","North","Bay Area","Pittsburg",null,49.85,null,"FC","","",null," "," "," "," ",1,24,24,4.22,5.24,4.8600000000000003,3.83,2.59,4.47,2.87,2.19,2.63,4.34,2.75,3.17]
["UNVRSY_1_UNIT 1",null,"Berry Cogen 38 - Unit 1",null,"FTUR","CHP","NATURAL GAS","CISO","North","CAISO System",null,null,38,null,"FC","","",null," "," "," "," ",1,24,24,35.76,31.33,35.270000000000003,30.82,34.6,33.479999999999997,33.01,32.07,31.52,28.94,34.85,34.729999999999997]
["USWND2_1_WIND1",null,"Golden Hills A",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,42.96,null,"FC","","",null," "," "," "," ",1,24,24,1.82,3.15,4.24,13.13,20.66,13.2,16.920000000000002,9.24,3.19,0.77,1.22,1.84]
["USWND2_1_WIND2",null,"Golden Hills B",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,42.96,null,"FC","","",null," "," "," "," ",1,24,24,1.82,3.15,4.24,13.13,20.66,13.2,16.920000000000002,9.24,3.19,0.77,1.22,1.84]
["USWND2_1_WIND3",null,"Golden Hills C",null,"WIND","Wind","WIND","CISO","North","CAISO System",null,null,46,null,"FC","","",null," "," "," "," ",1,24,24,1.95,3.37,4.54,14.06,22.12,14.13,18.12,9.89,3.41,0.83,1.3,1.97]
["USWND4_2_UNIT2",null,"Altamont Landfill Gas to Energy",null,"COMBUSTION TURBINE","Biogas","BIOGAS","CISO","North","CAISO System",null,1,7.4,null,"FC","","",null," "," "," "," ",1,24,24,7.4,7.4,7.35,6.41,7.4,7.4,7.4,7.4,7.4,7.23,7.4,7.4]
["USWNDR_2_LABWD1",null,"LaBrisa Wind Project",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,9,null,"FC","","",null," "," "," "," ",1,24,24,0.38,0.66,0.89,2.75,4.33,2.76,3.54,1.94,0.67,0.16,0.25,0.39]
["USWNDR_2_SMUD",null,"SOLANO WIND FARM",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,102.18,null,"FC","","",null," "," "," "," ",1,24,24,4.33,7.49,10.07,31.23,49.13,31.39,40.24,21.98,7.58,1.84,2.89,4.38]
["USWNDR_2_SMUD2",null,"Solano Wind Project Phase 3",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,127.8,null,"FC","","",null," "," "," "," ",1,24,24,5.42,9.3699999999999992,12.6,39.06,61.45,39.26,50.33,27.49,9.48,2.2999999999999998,3.62,5.47]
["USWPFK_6_FRICK",null,"Frick Summit Wind Repower",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,10,null,"FC","","",null," "," "," "," ",1,24,24,0.42,0.73,0.99,3.06,4.8099999999999996,3.07,3.94,2.15,0.74,0.18,0.28000000000000003,0.43]
["USWPJR_2_UNITS",null,"Vasco Wind",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,78.2,null,"FC","","",null," "," "," "," ",1,24,24,3.31,5.73,7.71,23.9,37.6,24.02,30.8,16.82,5.8,1.41,2.21,3.35]
["VACADX_1_SOLAR",null,"Vaca-Dixon Solar Station",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,2.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.75,0.91,1.51,1.3,0.13,0.1,0.1,0.1]
["VACADX_1_UNITA1",null,"CalPeak Power Vaca Dixon Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,51.91,null,"PD","",50.61,null," "," "," "," ",1,24,24,50.61,50.61,50.61,50.61,50.61,50.61,50.61,50.61,50.61,50.61,50.61,50.61]
["VALLEY_5_PERRIS",null,"MWD Perris Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",1,7.94,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,2.4,2.4,0,0,0,0]
["VALLEY_5_REDMTN",null,"MWD Red Mountain Hydroelectric Recovery ",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,5.9,null,"FC","","",null," "," "," "," ",1,24,24,1.49,1.39,0.46,1.37,1.35,1.26,0.8,1.21,1.59,1.6,1.31,1.01]
["VALLEY_5_SOLAR1",null,"Kona Solar - Meridian #1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,1.49,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VALLEY_5_SOLAR2",null,"AP North Lake Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","LA Basin","Eastern, Valley, Valley-Devers",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["VALTNE_2_AVASR1",null,"Valentine Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["VALTNE_2_TBBBT1","VALTNE_2_TBBBT1_SUN","Tropico Solar Big Beau",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,1,58,58,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,1.63,0.17,19.04,24.62,38.159999999999997,32.94,1.77,0.1,0.1,0.1]
["VALTNE_2_TBBBT1","VALTNE_2_TBBBT1_LESR","Tropico Solar Big Beau",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,1,18,58,"ID",1,"",false,1,0.8,72,72,1,24,4,18,18,18,18,18,18,18,18,18,18,18,18]
["VALTNE_2_TRSBT1","VALTNE_2_TRSBT1_SUN","Tropico Solar",null,"OTHER","Hybrid_Solar1Axis","HYBD","CISO","South","CAISO System",null,1,70,70,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,1.96,0.21,22.98,29.71,46.06,39.75,2.13,0.1,0.1,0.1]
["VALTNE_2_TRSBT1","VALTNE_2_TRSBT1_LESR","Tropico Solar",null,"OTHER","Hybrid_Storage","HYBD","CISO","South","CAISO System",null,1,22,70,"ID",1,"",false,1,0.8,88,88,1,24,4,22,22,22,22,22,22,22,22,22,22,22,22]
["VEAVST_1_SOLAR",null,"Community Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,14.4,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VEDDER_1_SEKERN",null,"TEXACO EXPLORATION & PROD (SE KERN RIVER",null,"FTUR","CHP","NATURAL GAS","CISO","North","Kern","South Kern PP, Kern Oil",null,34.47,null,"FC","","",null," "," "," "," ",1,24,24,1.82,2.98,3.11,2.66,2.62,2.06,2.69,3.04,2.58,4.17,3.04,2.4700000000000002]
["VEGA_6_SOLAR1",null,"Vega Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VENWD_1_WIND3",null,"Painted Hills",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,44.53,null,"FC","","",null," "," "," "," ",1,24,24,2.4300000000000002,5.24,5.66,17.97,19.149999999999999,16.88,14.84,12.99,8.91,4.17,1.93,2.04]
["VERNON_6_GONZL1",null,"H. Gonzales Unit #1",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,5.75,null,"FC","","",null," "," "," "," ",1,24,24,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75]
["VERNON_6_GONZL2",null,"H. Gonzales Unit #2",null,"FTUR","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,5.75,null,"FC","","",null," "," "," "," ",1,24,24,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75,5.75]
["VERNON_6_MALBRG",null,"Malburg Generating Station",null,"COMBINED CYCLE","CCGT","NATURAL GAS","CISO","South","LA Basin","Western",1,139,null,"FC","","",null," "," "," "," ",1,24,24,139,139,139,139,139,139,139,139,139,139,139,139]
["VESTAL_2_KERN",null,"KERN RIVER PH 3 UNITS 1 & 2 AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Vestal",null,36.799999999999997,null,"FC","","",null," "," "," "," ",1,24,24,9.0500000000000007,10.039999999999999,8.61,20.79,26.24,14.06,2.25,0.3,0.26,0.28000000000000003,3.88,7.04]
["VESTAL_2_RTS042",null,"SPVP042 Porterville Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","Big Creek-Ventura","Vestal",null,5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VESTAL_2_SOLAR1",null,"NICOLIS",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.56000000000000005,0.1,6.57,8.49,13.16,11.36,0.61,0.1,0.1,0.1]
["VESTAL_2_SOLAR2",null,"TROPICO",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,14,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.39,0.1,4.5999999999999996,5.94,9.2100000000000009,7.95,0.43,0.1,0.1,0.1]
["VESTAL_2_TS5SR1",null,"Tulare Solar 5",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","Big Creek-Ventura","Vestal",null,55.83,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,1.57,0.16,18.329999999999998,23.7,36.729999999999997,31.71,1.7,0.1,0.1,0.1]
["VESTAL_2_UNIT1",null,"CALGREN-PIXLEY",null,"FTUR","CHP","NATURAL GAS","CISO","South","Big Creek-Ventura","Vestal",null,5,null,"FC","","",null," "," "," "," ",1,24,24,2.38,2.46,2.16,1.86,1.89,2,2.06,2.69,3,3.17,3.27,3.29]
["VESTAL_2_WELLHD",null,"Wellhead Power Delano",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","Big Creek-Ventura","Vestal",1,49,null,"FC","","",null," "," "," "," ",1,24,24,49,49,49,49,49,49,49,49,49,49,49,49]
["VESTAL_6_QF",null,"Isabella Hydro Dam 1",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura","Vestal",null,11.95,null,"FC","","",null," "," "," "," ",1,24,24,3.81,2.0099999999999998,1.96,2.92,2.5099999999999998,3.82,3.24,2.4900000000000002,2.27,1.7,1.82,1.75]
["VICPAS_2_SLOBT1",null,"Whitney Point Solar",null,"PHOTO VOLTAIC","Paired_BattStorage","SUN","CISO","South","CAISO System",null,1,20,null,"ID",1,"",null,null,0.8,null,null,1,24,24,null,null,null,null,null,15,15,15,15,15,15,15]
["VICPAS_2_SOCBT1",null,"Sycamore Cogeneration Unit 1",null,"FTUR","Battery Storage","NATURAL GAS","CISO",null,"CAISO System",null,1,74,null,null,"","",null,null,0.8,null,null,1,24,24,null,null,null,50,50,50,50,50,50,50,50,50]
["VICPAS_2_SOCBT2",null,"Whitewater Hill Wind Project","VICPAS_2_SOCSR2","WIND","Paired_BattStorage","WIND","CISO","South","CAISO System",null,null,61.5,100,"ID",1,"",null,null,0.8,null,null,1,24,24,null,null,null,71,71,71,71,71,71,71,71,71]
["VICPAS_2_SOCSR2",null,"Wise Hydro Unit 1","VICPAS_2_SOCBT2","HYDRO","Paired_Solar_1Axis","WATER","CISO","South","CAISO System",null,null,14.5,105,"EO","","",null,null,null,null,null,1,24,24,null,null,null,null,65.56,82.17,9.5399999999999991,8.23,0.44,0,0.1,0.1]
["VICPAS_2_VPSBT1",null,"WISE HYDRO UNIT 2",null,"HYDRO","Paired_BattStorage","WATER","CISO","South","CAISO System",null,2,3.2,null,"ID",1,"",null,null,0.8,null,null,1,24,24,null,null,null,50,50,50,50,50,50,50,50,50]
["VICTOR_1_CREST",null,"Victor Aggregate Solar Resources",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,24.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_EXSLRA",null,"Expressway Solar A",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.38,0.52,1.01,0.87,0.1,0.1,0.1,0.1]
["VICTOR_1_EXSLRB",null,"Expressway Solar B",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,2,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.38,0.52,1.01,0.87,0.1,0.1,0.1,0.1]
["VICTOR_1_LVSLR1",null,"Lone Valley Solar Park 1",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,10,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_LVSLR2",null,"Lone Valley Solar Park 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_SLRHES",null,"Sunedison - Hesperia",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","CAISO System",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_SOLAR1",null,"Victor Phelan Solar One",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,17.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_SOLAR2",null,"Alamo Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_SOLAR3",null,"Adelanto Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,7,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.2,0.1,2.2999999999999998,2.97,4.6100000000000003,3.98,0.21,0.1,0.1,0.1]
["VICTOR_1_SOLAR4",null,"Adelanto Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VICTOR_1_VDRYFA",null,"Victor Dry Farm Ranch A ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,1.64,2.12,3.29,2.84,0.15,0.1,0.1,0.1]
["VICTOR_1_VDRYFB",null,"Victor Dry Farm Ranch B ",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","CAISO System",null,null,5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VILLPK_2_VALLYV",null,"MWD Valley View Hydroelectric Recovery P",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",1,4.0999999999999996,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,1.44,1.2,1.2,1.2,1.2,0,0.8,1.2,0]
["VILLPK_6_MWDYOR",null,"Yorba Linda Hydroelectric Recovery Plant",null,"HYDRO","Hydro","WATER","CISO","South","LA Basin","Western",1,5.0999999999999996,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,1.6,2.4,3.2,2.4,2.4,0]
["VISTA_6_QF",null,"VISTA QFS",null,"OTHER","CHP","OTHER","CISO","South","LA Basin","Eastern",null,0.18,null,"FC","","",null," "," "," "," ",1,24,24,0.01,0.01,0.01,0.01,0.04,0.06,0.08,0.1,7.0000000000000007E-2,0.05,0.03,0.02]
["VISTRA_5_DALBT1",null,"Dallas Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",1,100,null,"FC","","",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["VISTRA_5_DALBT2",null,"Dallas Energy Storage 2",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",1,100,null,"FC","","",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["VISTRA_5_DALBT3",null,"Dallas Energy Storage 3",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",1,100,null,"FC","","",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["VISTRA_5_DALBT4",null,"Dallas Energy Storage 4",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area","South Bay-Moss Landing",1,100,null,"FC","","",null,1,0.8,400,400,1,24,4,100,100,100,100,100,100,100,100,100,100,100,100]
["VISTRA_5_PLABT1",null,"Plano Storage 1",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area",null,1,100.4,null,"FC","","",null,1,0.8,401.6,401.6,1,24,4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4]
["VISTRA_5_PLABT2",null,"Plano Storage 2",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area",null,1,100.4,null,"FC","","",null,1,0.8,401.6,401.6,1,24,4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4,100.4]
["VISTRA_5_PLABT3",null,"Plano Storage 3",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area",null,1,74.599999999999994,null,"FC","","",null,1,0.8,298.39999999999998,298.39999999999998,1,24,4,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994]
["VISTRA_5_PLABT4",null,"Plano Storage 4",null,"OTHER","Battery Storage","LESR","CISO","North","Bay Area",null,1,74.599999999999994,null,"FC","","",null,1,0.8,298.39999999999998,298.39999999999998,1,24,4,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994,74.599999999999994]
["VLCNTR_6_VCEBT1",null,"Valley Center Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,54,null,"PD","",54,null,1,0.8,216,216,1,24,4,54,54,54,54,54,54,54,54,54,54,54,54]
["VLCNTR_6_VCEBT2",null,"Valley Center Energy Storage B",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",2,85,null,"PD","",50,null,1,0.8,340,340,1,24,4,50,50,50,50,50,50,50,50,50,50,50,50]
["VLCNTR_6_VCSLR",null,"Cole Grade",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV","San Diego",null,2.33,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.76,0.99,1.53,1.32,0.1,0.1,0.1,0.1]
["VLCNTR_6_VCSLR1",null,"Valley Center 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,2.5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.1,0.1,0.47,0.65,1.26,1.08,0.1,0.1,0.1,0.1]
["VLCNTR_6_VCSLR2",null,"Valley Center 2",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","San Diego-IV","San Diego",null,5,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.14000000000000001,0.1,0.95,1.29,2.52,2.17,0.11,0.1,0.1,0.1]
["VLYHOM_7_SSJID",null,"Woodward Power Plant",null,"HYDRO","Hydro","WATER","CISO","North","Stockton","Tesla-Bellota, Stanislaus",null,3,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0.4,0,0.1,0.44,0.28999999999999998,0.02,0,0,0]
["VOLTA_2_UNIT 1",null,"VOLTA HYDRO UNIT 1",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,9.1,null,"FC","","",null," "," "," "," ",1,24,24,4.1500000000000004,4.25,1.19,0.46,2.0499999999999998,1.26,0.73,0.75,1.33,1.33,1.71,2.06]
["VOLTA_2_UNIT 2",null,"Volta Hydro Unit 2",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1,null,"FC","","",null," "," "," "," ",1,24,24,0.28999999999999998,0.4,0.3,0.2,0.37,0.24,0.16,0.09,0.21,0.17,0.23,0.26]
["VOLTA_6_BAILCK",null,"Bailey Creek Ranch",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.63,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["VOLTA_6_DIGHYD",null,"Digger Creek Ranch Hydro",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.6,null,"FC","","",null," "," "," "," ",1,24,24,0.3,0.31,0.3,0.38,0.33,0.28999999999999998,0.25,0.22,0.22,0.23,0.22,0.25]
["VOLTA_7_PONHY1",null,"Ponderosa Bailey Hydroelectric",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,1.25,null,"FC","","",null," "," "," "," ",1,24,24,0.22,0.21,0.2,0.11,0.2,0.15,0,0,0,0.03,0.01,0.04]
["VOLTA_7_QFUNTS",null,"VOLTA_7_QFUNTS",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,null,0.15,null,"FC","","",null," "," "," "," ",1,24,24,0.08,7.0000000000000007E-2,0.06,0.05,0.05,0.04,0.04,0.02,0.01,0.01,0.03,0.04]
["VOYAGR_2_VOAWD5",null,"Voyager Wind Oasis Alta",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,13.98,null,"FC","","",null," "," "," "," ",1,24,24,0.76,1.64,1.78,5.64,6.01,5.3,4.66,4.08,2.8,1.31,0.6,0.64]
["VOYAGR_2_VOYWD1",null,"Voyager 1",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,128.91,null,"FC","","",null," "," "," "," ",1,24,24,7.03,15.16,16.38,52.01,55.44,48.87,42.96,37.619999999999997,25.79,12.07,5.58,5.92]
["VOYAGR_2_VOYWD2",null,"Voyager Wind 2",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,126.35,null,"FC","","",null," "," "," "," ",1,24,24,6.89,14.86,16.059999999999999,50.98,54.34,47.9,42.1,36.869999999999997,25.28,11.83,5.47,5.8]
["VOYAGR_2_VOYWD3",null,"Voyager Wind 3",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,42.45,null,"FC","","",null," "," "," "," ",1,24,24,2.31,4.99,5.39,17.13,18.260000000000002,16.09,14.15,12.39,8.49,3.97,1.84,1.95]
["VOYAGR_2_VOYWD4",null,"Voyager Wind 4",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,21.01,null,"FC","","",null," "," "," "," ",1,24,24,1.1499999999999999,2.4700000000000002,2.67,8.48,9.0399999999999991,7.97,7,6.13,4.2,1.97,0.91,0.96]
["VSTAES_6_VESBT1",null,"Vista Energy Storage",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV","San Diego",1,40,null,"PD","",30,null,1,0.8,40,40,1,24,4,10,10,10,10,10,10,10,10,10,10,10,10]
["WADHAM_6_UNIT",null,"Wadham Energy LP",null,"STEAM","Biomass","WASTE TO POWER","CISO","North","CAISO System",null,null,29.07,null,"FC","","",null," "," "," "," ",1,24,24,25,24.83,24.03,22.2,16.53,24.4,23.93,23.44,24.37,23.6,13.83,24.61]
["WALCRK_2_CTG1",null,"Walnut Creek Energy Park Unit 1",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,97.32,null,"FC","","",null," "," "," "," ",1,24,24,96.43,96.43,96.43,96.43,96.43,96.43,96.43,96.43,96.43,96.43,96.43,96.43]
["WALCRK_2_CTG2",null,"Walnut Creek Energy Park Unit 2",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,96.91,null,"FC","","",null," "," "," "," ",1,24,24,96.91,96.91,96.91,96.91,96.91,96.91,96.91,96.91,96.91,96.91,96.91,96.91]
["WALCRK_2_CTG3",null,"Walnut Creek Energy Park Unit 3",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,96.65,null,"FC","","",null," "," "," "," ",1,24,24,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65]
["WALCRK_2_CTG4",null,"Walnut Creek Energy Park Unit 4",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,96.6,null,"FC","","",null," "," "," "," ",1,24,24,96.49,96.49,96.49,96.49,96.49,96.49,96.49,96.49,96.49,96.49,96.49,96.49]
["WALCRK_2_CTG5",null,"Walnut Creek Energy Park Unit 5",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","South","LA Basin","Western",1,96.65,null,"FC","","",null," "," "," "," ",1,24,24,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65]
["WALNUT_2_SOLAR",null,"Industry MetroLink PV 1",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","South","LA Basin","Western",null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["WALNUT_6_HILLGEN",null,"Puente Hills",null,"OTHER","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,47,null,"FC","","",null," "," "," "," ",1,24,24,22.26,22.75,22.47,21.68,21.05,21.96,22,21.88,21.69,21.18,20.96,20.91]
["WALNUT_7_WCOVST",null,"MM West Covina - ST Unit",null,"STEAM","Biogas","BIOGAS","CISO","South","LA Basin","Western",null,6.5,null,"FC","","",null," "," "," "," ",1,24,24,4.88,4.87,4.87,5.22,5.16,5.12,5.07,5.0199999999999996,4.99,4.7699999999999996,4.9400000000000004,4.9400000000000004]
["WARNE_2_UNIT",null,"WARNE HYDRO AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","South","Big Creek-Ventura",null,1,76,null,"FC","","",null," "," "," "," ",1,24,24,36.6,43.28,40.96,41.95,41.04,42.33,41.36,41.31,42.75,40.96,42.17,37.590000000000003]
["WAUKNA_1_SOLAR",null,"Corcoran Solar",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno","Herndon, Hanford",null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.64,0.17,5.99,7.29,12.07,10.38,1.06,0.1,0.1,0.1]
["WAUKNA_1_SOLAR2",null,"Corcoran 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Herndon, Hanford",null,19.75,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.6,0.2,8.6300000000000008,10.82,14.75,12.38,1.03,0.1,0.1,0.1]
["WDLEAF_7_UNIT 1",null,"WOODLEAF HYDRO",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Drum-Rio Oso",1,60,null,"FC","","",null," "," "," "," ",1,24,24,48,48,49.2,55,56,48,48,59.9,48,50.37,48,48.4]
["WEBER_6_FORWRD",null,"Forward",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","CAISO System",null,null,4.2,null,"FC","","",null," "," "," "," ",1,24,24,4.0199999999999996,4.04,3.76,3.4,4.0199999999999996,3.98,4.01,3.88,3.96,4.05,4.05,4.01]
["WESCAN_2_BDSBT1",null,"Bateria Del Sur",null,"OTHER","Battery Storage","LESR","CISO","South","San Diego-IV",null,1,131,null,"PD","",131,null,1,0.8,524,524,1,24,4,131,131,131,131,131,131,131,131,131,131,131,131]
["WESTPT_2_UNIT",null,"West Point Hydro Plant",null,"HYDRO","Hydro","WATER","CISO","North","CAISO System",null,1,14,null,"FC","","",null," "," "," "," ",1,24,24,9.5500000000000007,6.79,8.1999999999999993,4.5199999999999996,2.2999999999999998,10.8,10.54,11.4,10.34,9.94,10.72,10.16]
["WFRESN_1_SOLAR",null,"Joya Del Sol",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","Fresno",null,null,1.5,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["WHEATL_6_LNDFIL",null,"G2 ENERGY, OSTROM ROAD LLC",null,"RECIPROCATING ENGINE","Biogas","BIOGAS","CISO","North","Sierra",null,null,3.55,null,"FC","","",null," "," "," "," ",1,24,24,3.41,3.19,3.38,3.25,3.25,3.02,3.23,3.11,3.29,3.36,3.29,2.84]
["WHITEH_2_MEADDYN1",null,"White Hills A",null,"WIND","Wind","WIND","WALC","South",null,null,1,50,null,"FC","","",null," "," "," "," ",1,24,24,10.029999999999999,10.61,10.029999999999999,14.65,11,8.27,5,3,5.82,3.39,5.15,7.53]
["WHITEH_2_MEADDYN2",null,"White Hills B",null,"WIND","Wind","WIND","WALC","South",null,null,1,300,null,"FC","","",null," "," "," "," ",1,24,24,60.18,63.68,60.18,87.91,66,49.64,30,18,34.93,20.329999999999998,30.91,45.18]
["WHITNY_6_SOLAR",null,"Whitney Point Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","Fresno","Coalinga, Panoche 115 kV",null,20,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["WHTWTR_1_WINDA1",null,"Whitewater Hill Wind Project",null,"WIND","Wind","WIND","CISO","South","LA Basin","Eastern, Valley-Devers",null,61.5,null,"FC","","",null," "," "," "," ",1,24,24,3.35,7.23,7.82,24.81,26.45,23.32,20.49,17.95,12.3,5.76,2.66,2.82]
["WISE_1_UNIT 1",null,"Wise Hydro Unit 1",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",1,14.5,null,"FC","","",null," "," "," "," ",1,24,24,3.77,4.97,5.2,6.76,8.1999999999999993,7.46,8.34,8.85,7.34,4,0,4.08]
["WISE_1_UNIT 2",null,"WISE HYDRO UNIT 2",null,"HYDRO","Hydro","WATER","CISO","North","Sierra","Placer, Gold Hill-Drum, Drum-Rio Oso, South of Rio Oso, South of Palermo",1,3.2,null,"FC","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["WISHON_6_UNITS",null,"Wishon/San Joaquin  #1-A AGGREGATE",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Borden",2,18.399999999999999,null,"FC","","",null," "," "," "," ",1,24,24,1.61,1.76,2.5,2.16,0.8,0.43,0,0,0,6.72,5.1100000000000003,1.5]
["WISTER_2_WISSR1",null,"Wister Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","IID","South",null,null,1,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.54,0.1,3.79,5.18,10.09,8.67,0.46,0.1,0.1,0.1]
["WISTRA_2_WRSSR1",null,"Wistaria Ranch Solar",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","South","San Diego-IV",null,null,100,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,2.81,0.28999999999999998,32.83,42.44,65.8,56.79,3.05,0.1,0.1,0.1]
["WLDWD_1_SOLAR1",null,"Wildwood Solar I",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,20,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.61,0.21,8.74,10.96,14.93,12.54,1.04,0.1,0.1,0.1]
["WLDWD_1_SOLAR2",null,"Wildwood Solar 2",null,"PHOTO VOLTAIC","Solar_1Axis","SUN","CISO","North","CAISO System",null,null,15,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,0.46,0.16,6.56,8.2200000000000006,11.2,9.4,0.78,0.1,0.1,0.1]
["WNDMAS_2_UNIT 1",null,"BUENA VISTA ENERGY, LLC",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,38,null,"FC","","",null," "," "," "," ",1,24,24,1.61,2.78,3.75,11.61,18.27,11.67,14.97,8.17,2.82,0.68,1.08,1.63]
["WNDSTR_2_WIND",null,"Windstar",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,120,null,"FC","","",null," "," "," "," ",1,24,24,6.54,14.12,15.25,48.42,51.61,45.5,39.99,35.020000000000003,24.01,11.23,5.19,5.51]
["WOLFSK_1_UNITA1",null,"Wolfskill Energy Center",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","CAISO System",null,1,48.68,null,"FC","","",null," "," "," "," ",1,24,24,46.9,46.9,46.9,46.9,46.9,46.9,46.9,46.9,46.9,46.9,46.9,46.9]
["WOODWR_1_HYDRO",null,"Quinten Luallen",null,"HYDRO","Hydro","WATER","CISO","North","Fresno","Herndon",null,7.3,null,"EO","","",null," "," "," "," ",1,24,24,0,0,0,0,0,0,0,0,0,0,0,0]
["WRGTSR_2_WSFSR1",null,"Wright Solar Freeman",null,"PHOTO VOLTAIC","Solar_Fixed","SUN","CISO","North","CAISO System",null,null,200,null,"FC","","",null," "," "," "," ",1,24,24,0.1,0.1,6.45,1.68,59.94,72.87,120.71,103.83,10.64,0.23,0.1,0.1]
["WSENGY_1_UNIT 1",null,"Wheelabrator Shasta",null,"STEAM","Biomass","BIOMASS","CISO","North","CAISO System",null,null,50,null,"FC","","",null," "," "," "," ",1,24,24,34.04,34.049999999999997,34.049999999999997,32.979999999999997,34.04,34.04,34.200000000000003,37.119999999999997,36.18,33.92,32.97,34.06]
["WSNR_2_CVPDYN",null,"Central Valley 1",null,"HYDRO","Hydro","WATER","BANC","North",null,null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,10,10,10,10,10,10,10,10,10,10,10,10]
["WSNR_2_TESLADYN",null,"Central Valley Tesla",null,"HYDRO","Hydro","WATER","BANC","North",null,null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,10,10,10,10,10,10,10,10,10,10,10,10]
["WSNR_5_TRCYDYN",null,"Central Valley Tracy",null,"HYDRO","Hydro","WATER","BANC","North",null,null,null,10,null,"FC","","",null," "," "," "," ",1,24,24,10,10,10,10,10,10,10,10,10,10,10,10]
["WSTWND_2_M89BT2",null,"Mojave 89 BESS 2B","WSTWND_2_M89WD2","OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,1,70.599999999999994,82.7,"EO","","",null,1,0.8,282.39999999999998,282.39999999999998,1,24,4,0,0,0,0,0,0,0,0,0,0,0,0]
["WSTWND_2_M89WD2",null,"Mojave 89 Wind","WSTWND_2_M89BT2","WIND","Wind","WIND","CISO","South","CAISO System",null,null,82.65,82.7,"FC","","",null," "," "," "," ",1,24,24,4.51,9.7200000000000006,10.5,33.35,35.54,31.34,27.54,24.12,16.54,7.74,3.58,3.79]
["WSTWND_2_M90WD2",null,"Mojave 90",null,"WIND","Wind","WIND","CISO","South","CAISO System",null,null,64.819999999999993,null,"FC","","",null," "," "," "," ",1,24,24,3.53,7.62,8.24,26.15,27.88,24.58,21.6,18.91,12.97,6.07,2.8,2.98]
["WSTWND_2_SBSBT1",null,"Sagebrush Solar 2",null,"OTHER","Battery Storage","LESR","CISO","South","CAISO System",null,1,80,null,"ID",1,"",null,1,0.8,320,320,1,24,4,80,80,80,80,80,80,80,80,80,80,80,80]
["YELPIN_2_YP2BT1",null,"Yellow Pine 2 BESS","YELPIN_2_YP2SR1 ","OTHER","Paired_BattStorage","LESR","CISO","South","CAISO System",null,1,65,125,"ID","",65,false,1,0.86499999999999999,260,260,1,24,4,65,65,65,65,65,65,65,65,65,65,65,65]
["YELPIN_2_YP2SR1",null,"Yellow Pine 2","YELPIN_2_YP2BT1","PHOTO VOLTAIC","Paired_Solar_1Axis","SUN","CISO","South","CAISO System",null,null,125,125,"ID",1,"",null,null,null,null,null,1,24,24,0.1,0.1,3.51,0.37,41.04,53.05,82.25,70.989999999999995,3.81,0.1,0.1,0.1]
["YUBACT_1_SUNSWT",null,"YUBA CITY COGEN",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","Pease, Drum-Rio Oso",1,49.97,null,"FC","","",null," "," "," "," ",1,24,24,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97,49.97]
["YUBACT_6_UNITA1",null,"Yuba City Energy Center (Calpine)",null,"COMBUSTION TURBINE","Peaker","NATURAL GAS","CISO","North","Sierra","Pease, Drum-Rio Oso",1,47.16,null,"FC","","",null," "," "," "," ",1,24,24,47.16,47.16,47.16,47.16,47.16,47.16,47.16,47.16,47.16,47.16,47.16,47.16]
["ZOND_6_UNIT",null,"ZOND WINDSYSTEMS INC.",null,"WIND","Wind","WIND","CISO","North","Bay Area","Contra Costa",null,17.100000000000001,null,"FC","","",null," "," "," "," ",1,24,24,0.72,1.25,1.69,5.23,8.2200000000000006,5.25,6.73,3.68,1.27,0.31,0.48,0.73]
["PGCC_1_PDRP02",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.5,0.8,0.2,0.35,1.6,1.6,0,0,0,0,0,0]
["PGCC_1_PDRP17",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.3,0.16,0,0.12,0.69,0.38,0,0,0,0,0,0]
["PGCC_1_PDRP22",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0,0,0,0,0,0,0,0,0]
["PGCC_1_PDRP24",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.95,0.91,0.91,0.91,0.91,0.85,0,0,0,0,0,0]
["PGCC_1_PDRP34",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.37,0,0,0,0.25,0.22,0,0,0,0,0,0]
["PGEB_2_PDRP08",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.5,0.8,0.2,0,1.75,1.9,0,0,0,0,0,0]
["PGEB_2_PDRP09",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.22,0.15,0.2,0.2,0.2,0,0,0,0,0,0]
["PGEB_2_PDRP10",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.21,0.15,0.2,0.17,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP107",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0.21,0.21,0.21,0.37,0.35,0,0,0,0,0,0]
["PGEB_2_PDRP111",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.16,0.16,0.16,0.16,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP21",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.22,0.15,0.2,0.2,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP22",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.21,0.15,0.2,0.17,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP23",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.22,0.15,0.2,0.2,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP24",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.21,0.16,0.2,0.17,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP57",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.1000000000000001,1.1000000000000001,1.1000000000000001,1.3,1.3,1.5,0,0,0,0,0,0]
["PGEB_2_PDRP70",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.99,0.6,0.99,0,0.49,0,0,0,0,0,0,0]
["PGEB_2_PDRP73",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.16,0.11,0.99,0,0.62,0.56000000000000005,0,0,0,0,0,0]
["PGEB_2_PDRP76",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.69,0.32,0.99,0,0,0,0,0,0,0,0,0]
["PGEB_2_PDRP77",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.44,0.45,0.23,0,0,0,0,0,0,0,0,0]
["PGEB_2_PDRP78",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.44,0.1,0,0.75,0.92,0,0,0,0,0,0]
["PGEB_2_PDRP81",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.18,0.68,0,0.19,0.21,0,0,0,0,0,0]
["PGEB_2_PDRP82",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0,0,0,0.1,0.99,0,0,0,0,0,0]
["PGF1_2_PDRP108",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,2.67,2.13,2.13,2.13,2.13,2,0,0,0,0,0,0]
["PGF1_2_PDRP109",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.59,0.24,0.99,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP11",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.6,0.8,0.3,0.92,1.8,1.9,0,0,0,0,0,0]
["PGF1_2_PDRP110",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.11,0,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP111",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,3.2,3.2,3.2,3.2,3.2,3,0,0,0,0,0,0]
["PGF1_2_PDRP16",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.13,0.17,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP17",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.14000000000000001,0.2,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP18",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.15,0.13,0.17,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP19",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.14000000000000001,0.2,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP20",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP21",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.14000000000000001,0.2,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP24",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP25",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.14000000000000001,0.2,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP26",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP27",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.14000000000000001,0.2,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP29",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.14000000000000001,0.2,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP60",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,2.5099999999999998,1.41,5.01,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP62",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.11,0,0,0,0.99,0,0,0,0,0,0]
["PGF1_2_PDRP64",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.32,0,0,0.99,0.63,0.99,0,0,0,0,0,0]
["PGF1_2_PDRP68",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.18,0.12,0.22,0,0.12,0.13,0,0,0,0,0,0]
["PGF1_2_PDRP77",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.61,0.51,0.99,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP78",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.21,0.26,0.24,0,0.12,0.12,0,0,0,0,0,0]
["PGF1_2_PDRP81",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.2,0.16,0.14000000000000001,0,0.1,0.99,0,0,0,0,0,0]
["PGF1_2_PDRP83",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.57999999999999996,0.67,0.99,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP84",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.99,0.18,0.99,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP92",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,2.34,1.28,1.28,1.28,1.28,1.2,0,0,0,0,0,0]
["PGFG_1_PDRP21",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0.2,0.18,0,0.22,0.37,0,0,0,0,0,0]
["PGFG_1_PDRP35",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.43,0.43,0.48,0.46,1,1,0,0,0,0,0,0]
["PGFG_1_PDRP37",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.11,0.11,0.11,0.1,0,0,0,0,0,0]
["PGHB_6_PDRP02",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0,0,0,0,0,0,0]
["PGKN_2_PDRP02",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.15,0.16,0,0.17,0.15,0,0,0,0,0,0]
["PGKN_2_PDRP07",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.15,0.16,0,0.2,0.2,0,0,0,0,0,0]
["PGKN_2_PDRP32",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.17,1.39,1.39,0.53,0.53,0.5,0,0,0,0,0,0]
["PGKN_2_PDRP40",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0.17,0.15,0,0.21,0.28000000000000003,0,0,0,0,0,0]
["PGKN_2_PDRP48",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.5,1.5,1.5,1.5,1.5,1.5,0,0,0,0,0,0]
["PGNB_2_PDRP19",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.12,0,0,0.71,0.43,0,0,0,0,0,0]
["PGNB_2_PDRP20",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.25,0.13,0,0.24,0.35,0,0,0,0,0,0]
["PGNB_2_PDRP43",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.61,0.75,0.75,0.75,0.75,0.7,0,0,0,0,0,0]
["PGNC_1_PDRP01",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.12,0.14000000000000001,0.26,0.39,0.54,0,0,0,0,0,0]
["PGNC_1_PDRP19",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.24,0,0,0,0,0,0,0,0,0,0,0]
["PGNC_1_PDRP26",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.28000000000000003,0.12,0,0.11,0.14000000000000001,0.17,0,0,0,0,0,0]
["PGNP_2_PDRP08",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,2.1,2.1,2.1,2.1,2.1,2.1,0,0,0,0,0,0]
["PGNP_2_PDRP10",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.4,0.16,0.13,0.17,0.15,0,0,0,0,0,0]
["PGNP_2_PDRP30",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.16,0.28999999999999998,0.13,0,0.16,0.28999999999999998,0,0,0,0,0,0]
["PGNP_2_PDRP34",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.15,0,0.11,0,0.62,0.99,0,0,0,0,0,0]
["PGNP_2_PDRP41",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0.13,0,0.14000000000000001,0.62,0,0,0,0,0,0]
["PGNP_2_PDRP46",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.32,0.32,0.99,0,0.9,0.55000000000000004,0,0,0,0,0,0]
["PGNP_2_PDRP49",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.49,0,0,0,0.54,0.51,0,0,0,0,0,0]
["PGNP_2_PDRP53",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.33,1.33,1.33,1.33,1.6,1.5,0,0,0,0,0,0]
["PGP2_2_PDRP08",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.35,0.16,0.17,0.19,0.15,0,0,0,0,0,0]
["PGP2_2_PDRP38",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.37,0.37,0.99,0,0.14000000000000001,0.99,0,0,0,0,0,0]
["PGP2_2_PDRP62",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.36,0.13,0,0.36,0.25,0,0,0,0,0,0]
["PGP2_2_PDRP67",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.19,0.15,0,0,0,0,0,0,0,0,0,0]
["PGP2_2_PDRP68",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.14000000000000001,0,0,0,0,0,0,0,0,0]
["PGSB_1_PDRP104",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.53,0.73,0.99,0,0,0,0,0,0,0,0,0]
["PGSB_1_PDRP11",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.44,0.16,0.15,0.2,0.21,0,0,0,0,0,0]
["PGSB_1_PDRP56",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.14000000000000001,0.16,0.31,0.45,0.63,0,0,0,0,0,0]
["PGSB_1_PDRP57",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.1,0.1,0.11,0.16,0.22,0,0,0,0,0,0]
["PGSB_1_PDRP58",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0.17,0.18,0.36,0.52,0.72,0,0,0,0,0,0]
["PGSB_1_PDRP67",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.41,0.44,0.22,0,0,0,0,0,0,0,0,0]
["PGSB_1_PDRP70",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0.64,0,0.18,0,0,0,0,0,0]
["PGSB_1_PDRP73",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.28000000000000003,0.2,0,0.48,0.52,0,0,0,0,0,0]
["PGSB_1_PDRP76",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0,0,0,0,0.99,0,0,0,0,0,0]
["PGSB_1_PDRP77",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.13,0.17,0,0.64,0.14000000000000001,0,0,0,0,0,0]
["PGSB_1_PDRP83",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.35,0.15,0.32,0,0.61,0.99,0,0,0,0,0,0]
["PGSB_1_PDRP87",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.18,0.21,0.21,0.21,0.21,0.2,0,0,0,0,0,0]
["PGSB_1_PDRP97",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.16,0.16,0,0.16,0.15,0,0,0,0,0,0]
["PGSF_2_PDRP38",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.16,0.14000000000000001,0,0,0,0,0,0,0,0,0,0]
["PGSF_2_PDRP51",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.31,0.56999999999999995,0.99,0,0,0,0,0,0,0,0,0]
["PGSF_2_PDRP56",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.47,0.14000000000000001,0.99,0,0.62,0.14000000000000001,0,0,0,0,0,0]
["PGSF_2_PDRP57",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.28000000000000003,0.12,0,0.99,0.26,0,0,0,0,0,0]
["PGSF_2_PDRP58",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.23,0.27,0.27,1.07,1.07,1,0,0,0,0,0,0]
["PGSI_1_PDRP09",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.13,0.16,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGSI_1_PDRP10",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.13,0.16,0.13,0.17,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP11",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.13,0.16,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGSI_1_PDRP12",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.12,0.16,0.13,0.17,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP29",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.5,1.5,1.5,1.5,1.5,1.5,0,0,0,0,0,0]
["PGSI_1_PDRP37",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.11,0,0,0,0,0,0,0,0,0,0]
["PGSI_1_PDRP44",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0,0,0.44,0,0.11,0,0,0,0,0,0]
["PGSI_1_PDRP49",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0.19,0,0,0.1,0.23,0,0,0,0,0,0]
["PGSI_1_PDRP51",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.61,0.75,1.28,1.28,1.28,1.2,0,0,0,0,0,0]
["PGST_2_PDRP08",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0.15,0,0,0,0,0,0]
["PGST_2_PDRP09",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.12,0.16,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGST_2_PDRP10",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0.15,0,0,0,0,0,0]
["PGST_2_PDRP11",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.12,0.16,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGST_2_PDRP14",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.1,0.16,0.13,0.17,0.15,0,0,0,0,0,0]
["PGST_2_PDRP22",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.56999999999999995,0.75,0.75,0,0,0,0,0,0,0,0,0]
["PGST_2_PDRP32",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.12,0.1,0,0.12,0.16,0,0,0,0,0,0]
["PGST_2_PDRP34",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.77,0.37,0.99,0,0.99,0,0,0,0,0,0,0]
["PGST_2_PDRP35",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0,0,0.4,0,0,0,0,0,0]
["PGST_2_PDRP37",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.26,0,0,0,0,0,0,0,0,0,0,0]
["PGZP_2_PDRP22",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.5,1.5,1.5,1.5,1.5,1.5,0,0,0,0,0,0]
["PGZP_2_PDRP25",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.27,0.27,0,0,0,0.99,0,0,0,0,0,0]
["PGZP_2_PDRP28",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.18,0.99,0,0.2,0.13,0,0,0,0,0,0]
["PGZP_2_PDRP35",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.26,0,0,1.03,0,2.4,0,0,0,0,0,0]
["PGZP_2_PDRP36",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.61,0,0.61,0.99,0,0,0,0,0,0]
["PGZP_2_PDRP45",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,2.2799999999999998,2.67,2.13,2.13,2.13,2,0,0,0,0,0,0]
["SCEC_1_PDRP05",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.22,0.22,0.24,0.46,0.68,0.94,0,0,0,0,0,0]
["SCEC_1_PDRP06",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.14000000000000001,0.16,0.31,0.45,0.63,0,0,0,0,0,0]
["SCEC_1_PDRP07",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.52,1.52,1.52,1.52,1.52,1.52,0,0,0,0,0,0]
["SCEC_1_PDRP09",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.4,0.1,0.1,0,1.1499999999999999,1.2,0,0,0,0,0,0]
["SCEC_1_PDRP102",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.4,0.1,0.1,0.18,1.1000000000000001,1.1000000000000001,0,0,0,0,0,0]
["SCEC_1_PDRP108",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.33,0,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP109",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.68,0,0,0,2.2400000000000002,3.55,0,0,0,0,0,0]
["SCEC_1_PDRP110",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,4.95,3.67,0,0,9.99,0,0,0,0,0,0]
["SCEC_1_PDRP111",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0.99,0,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP113",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.62,0.79,0.99,0,0.99,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP114",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.44,0,0,0,0.63,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP115",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.63,0.99,0.99,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP117",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0,0,0,0.5,0,0,0,0,0,0,0]
["SCEC_1_PDRP118",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.21,0.99,0.71,0,0.78,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP122",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0,0.4,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP126",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.84,0.99,0.79,0,0.89,0,0,0,0,0,0,0]
["SCEC_1_PDRP127",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.44,0.99,0.99,0,0,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP128",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0.99,0,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP129",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.56999999999999995,0,0,0.99,0.99,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP130",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.52,0,0,0,0,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP132",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.8,0.99,0.5,0,0.99,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP135",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.39,0.99,0.99,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP136",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.63,0,0,0,0,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP139",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.65,0.99,0.99,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP140",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.64,0,0,0.53,0.91,0.78,0,0,0,0,0,0]
["SCEC_1_PDRP141",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0,0,0.11,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP142",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.59,0.99,0.99,0,0.99,0,0,0,0,0,0,0]
["SCEC_1_PDRP143",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.63,0,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP144",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.28000000000000003,0,0,0,0.17,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP146",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.64,0,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP147",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.56000000000000005,0,0,0,0,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP148",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.55000000000000004,0,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP150",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.64,0,0,0,0.3,0,0,0,0,0,0,0]
["SCEC_1_PDRP151",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.67,0,0,0.99,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP152",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.35,0.99,0.17,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP153",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.64,0,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP156",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.45,0.99,0.99,0,0.99,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP157",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.39,0.99,0.99,0.99,0,0.1,0,0,0,0,0,0]
["SCEC_1_PDRP158",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP159",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.36,0,0,0,0.99,0,0,0,0,0,0,0]
["SCEC_1_PDRP160",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,3.65,4.6500000000000004,6.65,4.55,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP175",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.11,0.32,0.32,0.3,0,0,0,0,0,0]
["SCEC_1_PDRP176",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.68,1.68,1.68,1.89,1.89,1.8,0,0,0,0,0,0]
["SCEC_1_PDRP185",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.11,0.42,0.42,0.4,0,0,0,0,0,0]
["SCEN_6_PDRP01",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0.14000000000000001,0.16,0.31,0.45,0.63,0,0,0,0,0,0]
["SCEN_6_PDRP02",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.8,1.8,1.8,1.8,1.8,1.8,0,0,0,0,0,0]
["SCEN_6_PDRP07",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.22,0.22,0.24,0.46,0.68,0.94,0,0,0,0,0,0]
["SCEN_6_PDRP58",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.15,0.99,0,0,0,0.42,0,0,0,0,0,0]
["SCEN_6_PDRP59",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,1.04,1.74,0,0,0,0,0,0,0,0,0]
["SCEN_6_PDRP65",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.18,0,0,0,0,0,0,0,0,0,0,0]
["SCEN_6_PDRP66",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0,0.99,0,0.99,0.99,0,0,0,0,0,0]
["SCEN_6_PDRP79",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.53,0.53,0.53,1.68,1.68,1.6,0,0,0,0,0,0]
["SCEN_6_PDRP80",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0,0,0,0.99,0.99,0,0,0,0,0,0]
["SCEN_6_PDRP81",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.37,0.99,0.99,0,0.11,0.99,0,0,0,0,0,0]
["SCEN_6_PDRP87",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.37,0.99,0.99,0.61,0,0,0,0,0,0,0,0]
["SCEW_2_PDRP103",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.48,0.48,0.48,0.78,0.78,0.57999999999999996,0,0,0,0,0,0]
["SCEW_2_PDRP104",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.4,0.2,0.2,0,1.2,1.2,0,0,0,0,0,0]
["SCEW_2_PDRP106",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0,0,0.31,0,0,0,0,0,0,0,0]
["SCEW_2_PDRP107",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.99,0,0,0,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP108",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.28000000000000003,0.99,0.99,0.99,0.99,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP109",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.28999999999999998,0,0,0,0.61,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP110",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.38,0.99,0,0,0,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP111",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.46,0,0,0,0,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP116",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.53,0.99,0.99,0.9,0.56000000000000005,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP118",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.61,0.99,0.41,0.31,0.99,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP120",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.28000000000000003,0.99,0.56999999999999995,0.6,0,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP121",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.74,0.99,0.99,0.99,0.33,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP123",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.16,0,0,0,0,0,0,0,0,0,0,0]
["SCEW_2_PDRP124",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.16,0,0,0,0,0.86,0,0,0,0,0,0]
["SCEW_2_PDRP125",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.39,0.99,0.34,0,0.11,0.1,0,0,0,0,0,0]
["SCEW_2_PDRP133",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.23,0.99,0.99,0.99,0.99,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP168",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.42,0.42,0.42,1.1599999999999999,1.1599999999999999,1.1000000000000001,0,0,0,0,0,0]
["SCEW_2_PDRP172",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0,0,0,0.73,0,0,0,0,0,0,0]
["SCEW_2_PDRP177",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.84,0.84,0.84,2.1,2.1,2,0,0,0,0,0,0]
["SCEW_2_PDRP180",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.11,0.63,0.63,0.6,0,0,0,0,0,0]
["SCEW_2_PDRP19",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.93,0.93,1.02,1,1.51,2.02,0,0,0,0,0,0]
["SCEW_2_PDRP20",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.51,0.51,0.56000000000000005,1.08,0.8,1.19,0,0,0,0,0,0]
["SCHD_1_PDRP12",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.5,1.5,1.5,1.5,1.5,1.5,0,0,0,0,0,0]
["SCHD_1_PDRP41",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.31,0.99,0.99,0.28999999999999998,0,0.99,0,0,0,0,0,0]
["SCHD_1_PDRP42",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0,0,0,0,0,0,0,0,0,0,0]
["SCHD_1_PDRP44",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.99,0.13,0,0.16,0.6,0,0,0,0,0,0]
["SCHD_1_PDRP48",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.43,0,0,0,0,0,0,0,0,0,0,0]
["SCHD_1_PDRP64",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.61,0.99,0.99,0.99,0.99,0.99,0,0,0,0,0,0]
["SCLD_1_PDRP10",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.5,1.5,1.5,1.5,1.5,1.5,0,0,0,0,0,0]
["SCNW_6_PDRP07",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.36,0.36,0.4,0.77,1.1299999999999999,1.56,0,0,0,0,0,0]
["SCNW_6_PDRP41",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.14000000000000001,0,0,0,0.53,0.93,0,0,0,0,0,0]
["SCNW_6_PDRP43",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.18,0.99,0.99,0.45,0,0.15,0,0,0,0,0,0]
["SCNW_6_PDRP44",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.27,0.99,0.15,0,0.14000000000000001,0.99,0,0,0,0,0,0]
["SCNW_6_PDRP45",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,2.13,0,0,0.12,0,0,0,0,0,0,0]
["SCNW_6_PDRP47",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0,0.41,0,0,0,0,0,0,0,0,0]
["SCNW_6_PDRP48",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.31,0.99,0,0,0.11,0.49,0,0,0,0,0,0]
["SCNW_6_PDRP49",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.19,0.99,0.99,0.99,0.99,0.99,0,0,0,0,0,0]
["SCNW_6_PDRP50",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.99,0.99,0.99,0,0.99,0,0,0,0,0,0]
["SCNW_6_PDRP59",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.21,0.21,0.21,0.95,0.53,0.5,0,0,0,0,0,0]
["SCNW_6_PDRP68",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.11,0.11,0.21,0.21,0.2,0,0,0,0,0,0]
["SCNW_6_PDRP69",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,1.05,1.05,1.05,0.84,1.26,1.2,0,0,0,0,0,0]
["SDG1_1_PDRP04",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.62,0.62,0.68,1.31,1.93,2.66,0,0,0,0,0,0]
["SDG1_1_PDRP05",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.25,0.25,0.27,0.52,0.77,1.06,0,0,0,0,0,0]
["SDG1_1_PDRP06",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.3,0.3,0.3,0.15,1.1000000000000001,1.1000000000000001,0,0,0,0,0,0]
["SDG1_1_PDRP07",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.5,0.5,0.5,0,0,0,0,0,0,0,0,0]
["SDG1_1_PDRP100",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.56000000000000005,0.99,0.99,0.99,0.79,0.27,0,0,0,0,0,0]
["SDG1_1_PDRP101",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.61,0.99,0.99,0.99,0,0.26,0,0,0,0,0,0]
["SDG1_1_PDRP102",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.32,0.78,0.48,0.47,0.59,0.46,0,0,0,0,0,0]
["SDG1_1_PDRP103",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.13,0.99,0.99,0.99,0.12,0.32,0,0,0,0,0,0]
["SDG1_1_PDRP104",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.19,0,0,0.31,0.17,0,0,0,0,0,0,0]
["SDG1_1_PDRP105",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.34,0.99,0.99,0.99,0.28999999999999998,0,0,0,0,0,0,0]
["SDG1_1_PDRP111",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.26,0.99,0.99,0.5,0.7,0,0,0,0,0,0,0]
["SDG1_1_PDRP113",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.16,0.17,0.19,0,0,0,0,0,0,0,0,0]
["SDG1_1_PDRP117",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.27,0,0,0,0,0.13,0,0,0,0,0,0]
["SDG1_1_PDRP118",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.1,0.24,0.15,0.99,0.12,0,0,0,0,0,0,0]
["SDG1_1_PDRP119",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0,0,0.36,0.39,0.13,0,0,0,0,0,0]
["SDG1_1_PDRP15",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.28000000000000003,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP25",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.28000000000000003,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP26",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP27",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.28000000000000003,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP28",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP32",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP33",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP34",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.14000000000000001,0.1,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP37",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.15,0.1,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP38",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.1,0.14000000000000001,0.17,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP39",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.15,0.15,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP40",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP41",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.15,0.15,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP43",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.15,0.15,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP44",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP45",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.15,0.15,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP46",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP47",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.12,0.14000000000000001,0.14000000000000001,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP48",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP49",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP51",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.16,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP60",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.3,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP62",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.28999999999999998,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP64",null,"OhmConnect",null,null,"OhmConnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.11,0.14000000000000001,0.14000000000000001,0.17,0.28999999999999998,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP85",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.56999999999999995,0.86,3.57,4.47,0,0,0,0,0,0,0,0]
["SDG1_1_PDRP86",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,3.21,3.66,3.59,4.4400000000000004,5.67,5.95,0,0,0,0,0,0]
["SDG1_1_PDRP88",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.17,0,0,0.99,0,0,0,0,0,0,0,0]
["SDG1_1_PDRP91",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,0.87,0.93,0.99,0.99,0.12,0.99,0,0,0,0,0,0]
["SDG1_1_PDRP96",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,{"$error":"#N/A"},0,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["SDG1_1_PDRP97",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,{"$error":"#N/A"},0.99,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["SCEC_1_PDRP187",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,9.94,9.98,9.5,9.98,6.52,6.62,0,0,0,0,0,0]
["SCEC_1_PDRP188",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,9.94,9.98,9.5,9.98,6.52,6.62,0,0,0,0,0,0]
["SCEC_1_PDRP189",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,9.94,9.98,9.5,9.98,6.52,6.62,0,0,0,0,0,0]
["SCEC_1_PDRP192",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,5.26,5.26,5.26,6.58,5.58,5.58,0,0,0,0,0,0]
["SCEN_6_PDRP103",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,7.05,7.04,6.7,7.04,4.62,1.68,0,0,0,0,0,0]
["SCEW_2_PDRP182",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,8.01,7.99,7.6,7.99,5.15,2.52,0,0,0,0,0,0]
["SCHD_1_PDRP53",null,"Voltus",null,null,"Voltus Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.11,0.11,0.32,0.32,0.3,0,0,0,0,0,0]
["SCHD_1_PDRP58",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,3.78,3.78,3.6,3.78,2.42,3.15,0,0,0,0,0,0]
["SCLD_1_PDRP07",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.84,0.8,0.84,0.53,0.11,0,0,0,0,0,0]
["SCNW_6_PDRP66",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,3.01,2.94,2.8,2.94,1.89,0.21,0,0,0,0,0,0]
["PGCC_1_PDRP16",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.13,0,0.12,0,0,0,0,0,0,0,0]
["PGCC_1_PDRP18",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.11,0.6,0,0.68,0.99,0,0,0,0,0,0]
["PGCC_1_PDRP19",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.37,0,0.37,0.64,0.91,0,0,0,0,0,0]
["PGEB_2_PDRP105",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.89,0,0.62,0,0,0,0,0,0,0]
["PGF1_2_PDRP69",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.11,0.15,0,0.61,0.99,0,0,0,0,0,0]
["PGF1_2_PDRP71",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.26,0,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP86",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.27,0,0,0.5,0,0,0,0,0,0]
["PGKN_2_PDRP41",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.37,0.38,0,0,0.42,0,0,0,0,0,0]
["PGNB_2_PDRP30",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.1,0,0.89,0,0,0,0,0,0,0]
["PGNP_2_PDRP40",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.21,0.12,0,0.28999999999999998,0.39,0,0,0,0,0,0]
["PGNP_2_PDRP47",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.15,0,0,0,0.11,0,0,0,0,0,0]
["PGP2_2_PDRP63",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.13,0,0,0.24,0,0,0,0,0,0]
["PGSB_1_PDRP69",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.23,0,0,0.12,0,0,0,0,0,0]
["PGSI_1_PDRP31",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.13,0.14000000000000001,0,0.51,0.2,0,0,0,0,0,0]
["PGSI_1_PDRP35",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.15,0,0.14000000000000001,0.18,0,0,0,0,0,0]
["PGSI_1_PDRP42",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.19,0.12,0,0.22,0.41,0,0,0,0,0,0]
["PGSI_1_PDRP45",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.15,0,0,0.1,0,0,0,0,0,0]
["PGST_2_PDRP31",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.12,0.43,0,0.91,0.48,0,0,0,0,0,0]
["PGST_2_PDRP36",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.2,0.18,0,0.1,0,0,0,0,0,0,0]
["PGZP_2_PDRP24",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.13,0,0.23,0.2,0,0,0,0,0,0]
["PGZP_2_PDRP31",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.11,0.38,0,0.1,0.57999999999999996,0,0,0,0,0,0]
["PGZP_2_PDRP32",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.43,0.52,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP116",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0.73,0,0.67,0,0,0,0,0,0,0]
["SCEC_1_PDRP154",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0,0,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP181",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.63,0,0.2,0.86,0,0,0,0,0,0]
["SCEN_6_PDRP84",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0.99,0,0,0,0,0,0,0,0,0]
["SCEW_2_PDRP112",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0,0.8,0.68,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP117",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0.64,0.99,0.68,0,0,0,0,0,0,0]
["SCEW_2_PDRP122",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,4.18,0,0,3.3,2.85,0,0,0,0,0,0]
["SCEW_2_PDRP130",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0.99,0,0.11,0.11,0,0,0,0,0,0]
["SCEW_2_PDRP131",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,0.99,0.13,0,0.11,0.99,0,0,0,0,0,0]
["SCNW_6_PDRP46",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.11,0.47,0,0.13,0,0,0,0,0,0]
["SDG1_1_PDRP114",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.99,0.99,0.64,0.75,0,0,0,0,0,0]
["SDG1_1_PDRP121",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.21,0.21,0.99,0.17,0,0,0,0,0,0]
["SDG1_1_PDRP99",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,{"$error":"#N/A"},0.99,0.31,0.1,0,0.2,0,0,0,0,0,0]
["PGP2_2_PDRP69",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,0.12,0,0,0,0,0,0,0,0,0]
["PGCC_1_PDRP41",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,1.07,2.13,1.07,0,0,0,0,0,0]
["PGEB_2_PDRP25",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.2,0.2,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP26",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.18,0.17,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP27",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.18,0.2,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP28",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP60",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.23,0,0,0,0,0,0,0,0]
["PGEB_2_PDRP79",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.77,0,0,0,0,0,0,0,0]
["PGEB_2_PDRP93",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,2.13,2.67,2.67,0,0,0,0,0,0]
["PGEB_2_PDRP96",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP116",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.21,0.53,0.53,0,0,0,0,0,0]
["PGF1_2_PDRP28",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP30",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP36",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP37",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP38",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP63",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.43,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP87",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0,0,0,0,0,0,0,0]
["PGF1_2_PDRP93",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.19,0.37,0,0,0,0,0,0,0]
["PGFG_1_PDRP36",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.46,0.36,0.88,0,0,0,0,0,0]
["PGHB_6_PDRP05",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.14000000000000001,0.2,0,0,0,0,0,0,0]
["PGKN_2_PDRP08",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGKN_2_PDRP13",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGKN_2_PDRP14",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGKN_2_PDRP15",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.14000000000000001,0.2,0.2,0,0,0,0,0,0]
["PGKN_2_PDRP25",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.65,0.73,0.55000000000000004,0,0,0,0,0,0]
["PGKN_2_PDRP34",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.23,0,0,0,0,0,0,0,0]
["PGNB_2_PDRP02",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.18,0.17,0.15,0,0,0,0,0,0]
["PGNB_2_PDRP15",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.14000000000000001,0.23,0.2,0,0,0,0,0,0]
["PGNB_2_PDRP27",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.32,0.79,0,0,0,0,0,0,0]
["PGNC_2_PDRP13",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.75,1.07,1.07,0,0,0,0,0,0]
["PGNP_2_PDRP39",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,1.06,1.6,1.6,0,0,0,0,0,0]
["PGNP_2_PDRP44",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.38,0,0,0,0,0,0,0,0]
["PGNP_2_PDRP48",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.16,0,0,0,0,0,0,0,0]
["PGP2_2_PDRP07",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.16,0.3,0.2,0,0,0,0,0,0]
["PGP2_2_PDRP42",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.31,0.66,0.54,0,0,0,0,0,0]
["PGP2_2_PDRP60",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0.89,0.99,0,0,0,0,0,0]
["PGSB_1_PDRP04",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.17,0.17,0.22,0,0,0,0,0,0]
["PGSB_1_PDRP101",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,2.13,2.67,2.67,0,0,0,0,0,0]
["PGSB_1_PDRP68",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0,0.69,0,0,0,0,0,0]
["PGSB_1_PDRP74",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.37,0,0,0,0,0,0,0,0]
["PGSF_2_PDRP33",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.55000000000000004,0.95,0,0,0,0,0,0,0]
["PGSF_2_PDRP36",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.59,0,0,0,0,0,0,0,0]
["PGSF_2_PDRP46",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.2,0,0.12,0,0,0,0,0,0]
["PGSF_2_PDRP49",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.32,0.53,0.53,0,0,0,0,0,0]
["PGSF_2_PDRP52",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.15,0,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP16",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP33",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.48,0.12,0,0,0,0,0,0,0]
["PGSI_1_PDRP48",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.21,0.83,0.89,0,0,0,0,0,0]
["PGSI_1_PDRP59",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.32,0.53,0.53,0,0,0,0,0,0]
["PGST_2_PDRP39",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.36,0,1.19,0,0,0,0,0,0]
["PGZP_2_PDRP07",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.14000000000000001,0.2,0.1,0,0,0,0,0,0]
["PGZP_2_PDRP08",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.13,0.17,0.1,0,0,0,0,0,0]
["SCEC_1_PDRP106",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.53,0.48,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP120",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.65,0.89,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP125",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,1.28,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP131",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.95,0,0,0,0,0,0,0,0]
["SCEC_1_PDRP133",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.94,0.45,0,0,0,0,0,0,0]
["SCEC_1_PDRP191",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,9.93,7.67,7.67,0,0,0,0,0,0]
["SCEN_6_PDRP101",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0,0,0,0,0,0,0,0]
["SCEN_6_PDRP104",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,3.28,2.84,2.84,0,0,0,0,0,0]
["SCEN_6_PDRP105",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.21,0.2,0.99,0,0,0,0,0,0]
["SCEN_6_PDRP106",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.52,0,0,0,0,0,0,0,0]
["SCEN_6_PDRP60",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0,0,0,0,0,0,0,0]
["SCEN_6_PDRP64",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.11,0,1.1100000000000001,0,0,0,0,0,0]
["SCEN_6_PDRP88",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.33,0,0,0,0,0,0,0,0]
["SCEN_6_PDRP98",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.23,0.57999999999999996,0,0,0,0,0,0,0]
["SCEW_2_PDRP119",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.99,0.99,0,0,0,0,0,0,0]
["SCEW_2_PDRP183",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,3.78,3.25,3.25,0,0,0,0,0,0]
["SCEW_2_PDRP185",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,1.54,1.39,1.39,0,0,0,0,0,0]
["SCEW_2_PDRP47",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.98,1.4,2,0,0,0,0,0,0]
["SCHD_1_PDRP59",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,1.1000000000000001,1.03,1.03,0,0,0,0,0,0]
["SCNW_6_PDRP42",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.23,0,0,0,0,0,0,0,0]
["SCNW_6_PDRP51",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.1,0.62,0,0,0,0,0,0,0]
["SCNW_6_PDRP67",null,"Enersponse",null,null,"Enersponse Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,5.31,4.5199999999999996,4.5199999999999996,0,0,0,0,0,0]
["SDG1_1_PDRP120",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.27,0,0,0,0,0,0,0,0]
["SDG1_1_PDRP61",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.15,0.27,0.1,0,0,0,0,0,0]
["SDG1_1_PDRP63",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.15,0.27,0.35,0,0,0,0,0,0]
["SDG1_1_PDRP65",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.15,0.27,0.35,0,0,0,0,0,0]
["SDG1_1_PDRP66",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.17,0.28999999999999998,0.26,0,0,0,0,0,0]
["SDG1_1_PDRP67",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.15,0.27,0.35,0,0,0,0,0,0]
["SDG1_1_PDRP68",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.17,0.28999999999999998,0.38,0,0,0,0,0,0]
["SDG1_1_PDRP69",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.15,0.27,0.35,0,0,0,0,0,0]
["SDG1_1_PDRP70",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.17,0.28999999999999998,0.38,0,0,0,0,0,0]
["SDG1_1_PDRP98",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,0.12,0.15,0.15,0,0,0,0,0,0]
["PGCC_1_PDRP13",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGCC_1_PDRP21",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.53,0,0,0,0,0,0,0]
["PGEB_2_PDRP100",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.99,0,0,0,0,0,0]
["PGEB_2_PDRP101",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.99,0,0,0,0,0,0]
["PGEB_2_PDRP29",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP30",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP31",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.1,0,0,0,0,0,0]
["PGEB_2_PDRP34",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP35",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGEB_2_PDRP36",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP40",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP42",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP44",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP46",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP48",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGEB_2_PDRP62",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,1.04,0.85,0,0,0,0,0,0]
["PGEB_2_PDRP64",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.61,0,0,0,0,0,0]
["PGEB_2_PDRP65",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.53,0,0,0,0,0,0,0]
["PGEB_2_PDRP66",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.89,0,0,0,0,0,0,0]
["PGEB_2_PDRP74",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.66,0.99,0,0,0,0,0,0]
["PGEB_2_PDRP80",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.72,0.9,0,0,0,0,0,0]
["PGEB_2_PDRP98",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.33,0,0,0,0,0,0,0]
["PGF1_2_PDRP39",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP40",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP41",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP42",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP43",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP44",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP45",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP46",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGF1_2_PDRP47",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.3,0,0,0,0,0,0]
["PGF1_2_PDRP48",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP50",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP52",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGF1_2_PDRP61",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.9,0.85,0,0,0,0,0,0]
["PGF1_2_PDRP76",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.1499999999999999,0,0,0,0,0,0]
["PGF1_2_PDRP82",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.11,0.48,0,0,0,0,0,0]
["PGF1_2_PDRP85",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.68,0,0,0,0,0,0,0]
["PGF1_2_PDRP88",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.91,0,0,0,0,0,0,0]
["PGF1_2_PDRP94",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.48,0.11,0,0,0,0,0,0]
["PGFG_1_PDRP05",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.2,0,0,0,0,0,0]
["PGFG_1_PDRP14",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGFG_1_PDRP19",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.13,0,0,0,0,0,0]
["PGFG_1_PDRP23",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.24,0.28000000000000003,0,0,0,0,0,0]
["PGFG_1_PDRP25",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.11,0.46,0,0,0,0,0,0]
["PGFG_1_PDRP32",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.11,0,0,0,0,0,0,0]
["PGHB_6_PDRP10",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.76,0,0,0,0,0,0,0]
["PGKN_2_PDRP06",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGKN_2_PDRP09",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.2,0,0,0,0,0,0]
["PGKN_2_PDRP12",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.9,0,0,0,0,0,0]
["PGKN_2_PDRP16",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGKN_2_PDRP18",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGKN_2_PDRP33",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.3,0,0,0,0,0,0]
["PGKN_2_PDRP36",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.66,0.73,0,0,0,0,0,0]
["PGKN_2_PDRP38",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.5,0.46,0,0,0,0,0,0]
["PGKN_2_PDRP44",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.32,0,0,0,0,0,0]
["PGNB_2_PDRP12",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.6,0,0,0,0,0,0]
["PGNB_2_PDRP25",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.52,0,0,0,0,0,0]
["PGNB_2_PDRP35",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.35,0.33,0,0,0,0,0,0]
["PGNC_1_PDRP04",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGNC_1_PDRP09",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.69,0,0,0,0,0,0,0]
["PGNP_2_PDRP09",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGNP_2_PDRP11",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.21,0,0,0,0,0,0]
["PGNP_2_PDRP16",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.17,0,0,0,0,0,0]
["PGNP_2_PDRP18",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.18,0,0,0,0,0,0]
["PGNP_2_PDRP20",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.18,0,0,0,0,0,0]
["PGNP_2_PDRP21",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.22,0.8,0,0,0,0,0,0]
["PGNP_2_PDRP31",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.61,0.95,0,0,0,0,0,0]
["PGNP_2_PDRP43",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.55000000000000004,0,0,0,0,0,0]
["PGNP_2_PDRP50",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.26,0.7,0,0,0,0,0,0]
["PGP2_2_PDRP17",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.23,0.8,0,0,0,0,0,0]
["PGP2_2_PDRP35",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.34,0.35,0,0,0,0,0,0]
["PGP2_2_PDRP55",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.14000000000000001,0,0,0,0,0,0,0]
["PGP2_2_PDRP58",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.56999999999999995,1.4,0,0,0,0,0,0]
["PGSB_1_PDRP17",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGSB_1_PDRP30",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.22,0,0,0,0,0,0]
["PGSB_1_PDRP32",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.22,0,0,0,0,0,0]
["PGSB_1_PDRP60",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,2.16,0,0,0,0,0,0,0]
["PGSB_1_PDRP66",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.69,0.59,0,0,0,0,0,0]
["PGSB_1_PDRP78",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.38,0,0,0,0,0,0,0]
["PGSB_1_PDRP91",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.9,0,0,0,0,0,0,0]
["PGSB_1_PDRP92",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.83,0,0,0,0,0,0,0]
["PGSF_2_PDRP04",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGSF_2_PDRP08",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.1,0.2,0,0,0,0,0,0]
["PGSF_2_PDRP34",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.19,0.17,0,0,0,0,0,0]
["PGSF_2_PDRP37",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,2.17,0,0,0,0,0,0,0]
["PGSF_2_PDRP53",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.13,0.12,0,0,0,0,0,0]
["PGSI_1_PDRP15",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.2,0,0,0,0,0,0]
["PGSI_1_PDRP17",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.2,0.3,0,0,0,0,0,0]
["PGSI_1_PDRP20",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.17,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP22",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP24",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.15,0,0,0,0,0,0]
["PGSI_1_PDRP26",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.2,0,0,0,0,0,0]
["PGSI_1_PDRP28",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.8,0,0,0,0,0,0]
["PGSI_1_PDRP40",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.1,0,0,0,0,0,0,0]
["PGSI_1_PDRP43",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.11,0.47,0,0,0,0,0,0]
["PGST_2_PDRP15",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.1,0.8,0,0,0,0,0,0]
["PGST_2_PDRP38",null,"CPower",null,null,"CPower Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.28999999999999998,0.24,0,0,0,0,0,0]
["PGST_2_PDRP40",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.07,0,0,0,0,0,0]
["PGZP_2_PDRP27",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.19,0,0,0,0,0,0]
["PGZP_2_PDRP29",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.14000000000000001,0,0,0,0,0,0]
["PGZP_2_PDRP33",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.48,0.62,0,0,0,0,0,0]
["PGZP_2_PDRP34",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.56000000000000005,2.61,0,0,0,0,0,0]
["PGZP_2_PDRP37",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.66,0,0,0,0,0,0,0]
["PGZP_2_PDRP40",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.12,0,0,0,0,0,0]
["PGZP_2_PDRP41",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.99,0,0,0,0,0,0,0]
["PGZP_2_PDRP43",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.89,0,0,0,0,0,0,0]
["PGZP_2_PDRP50",null,"Voltus",null,null,"Voltus Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.75,0.75,0,0,0,0,0,0]
["SCEC_1_PDRP08",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.5,0,0,0,0,0,0]
["SCEC_1_PDRP107",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.16,0,0,0,0,0,0,0]
["SCEC_1_PDRP119",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.7,0,0,0,0,0,0,0]
["SCEC_1_PDRP121",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,2.5499999999999998,2.71,0,0,0,0,0,0]
["SCEC_1_PDRP137",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.49,0,0,0,0,0,0,0]
["SCEC_1_PDRP145",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.99,0,0,0,0,0,0]
["SCEC_1_PDRP161",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.94,2.11,0,0,0,0,0,0]
["SCEC_1_PDRP163",null,"CPower",null,null,"CPower Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,3.44,3.89,0,0,0,0,0,0]
["SCEN_6_PDRP03",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.4,1,0,0,0,0,0,0]
["SCEN_6_PDRP61",null,"CPower",null,null,"CPower Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,1.02,1.0900000000000001,0,0,0,0,0,0]
["SCEN_6_PDRP62",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.1,1.39,0,0,0,0,0,0]
["SCEN_6_PDRP89",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.99,0,0,0,0,0,0]
["SCEN_6_PDRP91",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.13,0.12,0,0,0,0,0,0]
["SCEN_6_PDRP94",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.84,0,0,0,0,0,0,0]
["SCEN_6_PDRP95",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.36,0,0,0,0,0,0,0]
["SCEN_6_PDRP97",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.1,0,0,0,0,0,0,0]
["SCEW_2_PDRP105",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.5,0,0,0,0,0,0]
["SCEW_2_PDRP173",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.12,0.99,0,0,0,0,0,0]
["SCEW_2_PDRP174",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.87,0,0,0,0,0,0,0]
["SCEW_2_PDRP37",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.78,1,0,0,0,0,0,0]
["SCHD_1_PDRP43",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,2.21,0,0,0,0,0,0,0]
["SCHD_1_PDRP61",null,"CPower",null,null,"CPower Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.32,0.3,0,0,0,0,0,0]
["SCHD_1_PDRP63",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.1,0.99,0,0,0,0,0,0]
["SCNW_6_PDRP40",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,0.8,0.11,0,0,0,0,0,0]
["SDG1_1_PDRP84",null,"Leapfrog",null,null,"Leapfrog Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,0.73,0,0,0,0,0,0]
["PGF1_2_PDRP59",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.2,0,0,0,0,0,0]
["PGNB_2_PDRP17",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.2,0,0,0,0,0,0]
["PGP2_2_PDRP23",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.2,0,0,0,0,0,0]
["PGSB_1_PDRP10",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.2,0,0,0,0,0,0]
["PGSB_1_PDRP55",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.3,0,0,0,0,0,0]
["PGSI_1_PDRP23",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.3,0,0,0,0,0,0]
["PGST_2_PDRP13",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"PGE","North",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1.3,0,0,0,0,0,0]
["SCEC_1_PDRP100",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1,0,0,0,0,0,0]
["SCEN_6_PDRP06",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1,0,0,0,0,0,0]
["SCHD_1_PDRP04",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1,0,0,0,0,0,0]
["SCNW_6_PDRP09",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SCE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,1,0,0,0,0,0,0]
["SDG1_1_PDRP30",null,"Ohmconnect",null,null,"Ohmconnect Demand Response",null,"SDGE","South",null,null,null,null,null,null,null,null,null,null,null,null,null,17,22,6,null,null,null,null,null,2.2999999999999998,0,0,0,0,0,0]

{"sheet":"Resource Default Profiles","index":23,"n_rows":7825,"n_cols":5,"rows_kept":7825,"cut":false,"hidden":false,"merged":[]}
["Profile Category","Region","Month","Hour Ending","Shape Factor"]
["Battery Storage","Any",0,1,0]
["Battery Storage","Any",0,2,0]
["Battery Storage","Any",0,3,0]
["Battery Storage","Any",0,4,0]
["Battery Storage","Any",0,5,0]
["Battery Storage","Any",0,6,0]
["Battery Storage","Any",0,7,0]
["Battery Storage","Any",0,8,0]
["Battery Storage","Any",0,9,0]
["Battery Storage","Any",0,10,0]
["Battery Storage","Any",0,11,0]
["Battery Storage","Any",0,12,0]
["Battery Storage","Any",0,13,0]
["Battery Storage","Any",0,14,0]
["Battery Storage","Any",0,15,0]
["Battery Storage","Any",0,16,0]
["Battery Storage","Any",0,17,0]
["Battery Storage","Any",0,18,1]
["Battery Storage","Any",0,19,1]
["Battery Storage","Any",0,20,1]
["Battery Storage","Any",0,21,1]
["Battery Storage","Any",0,22,0]
["Battery Storage","Any",0,23,0]
["Battery Storage","Any",0,24,0]
["CAM Peaker","Any",0,1,0]
["CAM Peaker","Any",0,2,0]
["CAM Peaker","Any",0,3,0]
["CAM Peaker","Any",0,4,0]
["CAM Peaker","Any",0,5,0]
["CAM Peaker","Any",0,6,0]
["CAM Peaker","Any",0,7,0]
["CAM Peaker","Any",0,8,0]
["CAM Peaker","Any",0,9,0]
["CAM Peaker","Any",0,10,0]
["CAM Peaker","Any",0,11,0]
["CAM Peaker","Any",0,12,0]
["CAM Peaker","Any",0,13,0]
["CAM Peaker","Any",0,14,1]
["CAM Peaker","Any",0,15,1]
["CAM Peaker","Any",0,16,1]
["CAM Peaker","Any",0,17,1]
["CAM Peaker","Any",0,18,1]
["CAM Peaker","Any",0,19,1]
["CAM Peaker","Any",0,20,1]
["CAM Peaker","Any",0,21,1]
["CAM Peaker","Any",0,22,1]
["CAM Peaker","Any",0,23,0]
["CAM Peaker","Any",0,24,0]
["Solar Fixed","Norcal",1,1,0]
["Solar Fixed","Norcal",1,2,0]
["Solar Fixed","Norcal",1,3,0]
["Solar Fixed","Norcal",1,4,0]
["Solar Fixed","Norcal",1,5,0]
["Solar Fixed","Norcal",1,6,0]
["Solar Fixed","Norcal",1,7,0]
["Solar Fixed","Norcal",1,8,3.0811252358278699E-2]
["Solar Fixed","Norcal",1,9,0.21601762927749216]
["Solar Fixed","Norcal",1,10,0.42276820809229515]
["Solar Fixed","Norcal",1,11,0.53250751625276904]
["Solar Fixed","Norcal",1,12,0.55816391267415721]
["Solar Fixed","Norcal",1,13,0.5821767807004361]
["Solar Fixed","Norcal",1,14,0.51225111079488728]
["Solar Fixed","Norcal",1,15,0.4813586396061571]
["Solar Fixed","Norcal",1,16,0.32832726694938413]
["Solar Fixed","Norcal",1,17,7.7039619160484518E-2]
["Solar Fixed","Norcal",1,18,6.7363043724811571E-5]
["Solar Fixed","Norcal",1,19,0]
["Solar Fixed","Norcal",1,20,0]
["Solar Fixed","Norcal",1,21,0]
["Solar Fixed","Norcal",1,22,0]
["Solar Fixed","Norcal",1,23,0]
["Solar Fixed","Norcal",1,24,0]
["Solar Fixed","Norcal",2,1,0]
["Solar Fixed","Norcal",2,2,0]
["Solar Fixed","Norcal",2,3,0]
["Solar Fixed","Norcal",2,4,0]
["Solar Fixed","Norcal",2,5,0]
["Solar Fixed","Norcal",2,6,0]
["Solar Fixed","Norcal",2,7,1.5723733690831905E-4]
["Solar Fixed","Norcal",2,8,0.11469951262160773]
["Solar Fixed","Norcal",2,9,0.44612688926265448]
["Solar Fixed","Norcal",2,10,0.61458490533071874]
["Solar Fixed","Norcal",2,11,0.67405832957359335]
["Solar Fixed","Norcal",2,12,0.69018890249832321]
["Solar Fixed","Norcal",2,13,0.70771479999890841]
["Solar Fixed","Norcal",2,14,0.66692192431245345]
["Solar Fixed","Norcal",2,15,0.62085206399923898]
["Solar Fixed","Norcal",2,16,0.50419212096835175]
["Solar Fixed","Norcal",2,17,0.25542986577396176]
["Solar Fixed","Norcal",2,18,1.835483413139433E-2]
["Solar Fixed","Norcal",2,19,0]
["Solar Fixed","Norcal",2,20,0]
["Solar Fixed","Norcal",2,21,0]
["Solar Fixed","Norcal",2,22,0]
["Solar Fixed","Norcal",2,23,0]
["Solar Fixed","Norcal",2,24,0]
["Solar Fixed","Norcal",3,1,0]
["Solar Fixed","Norcal",3,2,0]
["Solar Fixed","Norcal",3,3,0]
["Solar Fixed","Norcal",3,4,0]
["Solar Fixed","Norcal",3,5,0]
["Solar Fixed","Norcal",3,6,0]
["Solar Fixed","Norcal",3,7,2.1833360841994974E-6]
["Solar Fixed","Norcal",3,8,6.3492485695747281E-2]
["Solar Fixed","Norcal",3,9,0.34349502999563492]
["Solar Fixed","Norcal",3,10,0.55988870654156087]
["Solar Fixed","Norcal",3,11,0.67076688955013231]
["Solar Fixed","Norcal",3,12,0.68618010819972342]
["Solar Fixed","Norcal",3,13,0.68083381704180657]
["Solar Fixed","Norcal",3,14,0.65669014159824934]
["Solar Fixed","Norcal",3,15,0.61483911672886038]
["Solar Fixed","Norcal",3,16,0.54791889483019363]
["Solar Fixed","Norcal",3,17,0.4224913917954557]
["Solar Fixed","Norcal",3,18,0.14951538232794262]
["Solar Fixed","Norcal",3,19,3.2226579610052854E-2]
["Solar Fixed","Norcal",3,20,1.0582898477207567E-4]
["Solar Fixed","Norcal",3,21,0]
["Solar Fixed","Norcal",3,22,0]
["Solar Fixed","Norcal",3,23,0]
["Solar Fixed","Norcal",3,24,0]
["Solar Fixed","Norcal",4,1,0]
["Solar Fixed","Norcal",4,2,0]
["Solar Fixed","Norcal",4,3,0]
["Solar Fixed","Norcal",4,4,0]
["Solar Fixed","Norcal",4,5,0]
["Solar Fixed","Norcal",4,6,0]
["Solar Fixed","Norcal",4,7,5.8841469504664649E-3]
["Solar Fixed","Norcal",4,8,0.17802473672154437]
["Solar Fixed","Norcal",4,9,0.50179875649496397]
["Solar Fixed","Norcal",4,10,0.679026952075792]
["Solar Fixed","Norcal",4,11,0.75774727109858231]
["Solar Fixed","Norcal",4,12,0.78726692215394944]
["Solar Fixed","Norcal",4,13,0.81295085150668334]
["Solar Fixed","Norcal",4,14,0.79896112178051271]
["Solar Fixed","Norcal",4,15,0.79561949322270697]
["Solar Fixed","Norcal",4,16,0.76007081989705405]
["Solar Fixed","Norcal",4,17,0.67265902486871509]
["Solar Fixed","Norcal",4,18,0.51254440541846547]
["Solar Fixed","Norcal",4,19,0.19715287078456184]
["Solar Fixed","Norcal",4,20,8.4003584591367496E-3]
["Solar Fixed","Norcal",4,21,0]
["Solar Fixed","Norcal",4,22,0]
["Solar Fixed","Norcal",4,23,0]
["Solar Fixed","Norcal",4,24,0]
["Solar Fixed","Norcal",5,1,0]
["Solar Fixed","Norcal",5,2,0]
["Solar Fixed","Norcal",5,3,0]
["Solar Fixed","Norcal",5,4,0]
["Solar Fixed","Norcal",5,5,0]
["Solar Fixed","Norcal",5,6,6.5661669454536469E-6]
["Solar Fixed","Norcal",5,7,5.6620352777019829E-2]
["Solar Fixed","Norcal",5,8,0.32690125934403713]
["Solar Fixed","Norcal",5,9,0.57261559648081983]
["Solar Fixed","Norcal",5,10,0.72094920181182376]
["Solar Fixed","Norcal",5,11,0.79374637078818322]
["Solar Fixed","Norcal",5,12,0.82466363511340668]
["Solar Fixed","Norcal",5,13,0.82263533773905806]
["Solar Fixed","Norcal",5,14,0.82245449309355501]
["Solar Fixed","Norcal",5,15,0.82213529066387436]
["Solar Fixed","Norcal",5,16,0.7911566135012571]
["Solar Fixed","Norcal",5,17,0.7052308228185169]
["Solar Fixed","Norcal",5,18,0.57145466113352805]
["Solar Fixed","Norcal",5,19,0.29968547891128855]
["Solar Fixed","Norcal",5,20,4.0274942203467293E-2]
["Solar Fixed","Norcal",5,21,9.2408267115957713E-6]
["Solar Fixed","Norcal",5,22,0]
["Solar Fixed","Norcal",5,23,0]
["Solar Fixed","Norcal",5,24,0]
["Solar Fixed","Norcal",6,1,0]
["Solar Fixed","Norcal",6,2,0]
["Solar Fixed","Norcal",6,3,0]
["Solar Fixed","Norcal",6,4,0]
["Solar Fixed","Norcal",6,5,0]
["Solar Fixed","Norcal",6,6,3.1848768015055833E-4]
["Solar Fixed","Norcal",6,7,8.6538647523322687E-2]
["Solar Fixed","Norcal",6,8,0.36470705056404168]
["Solar Fixed","Norcal",6,9,0.59718843668112986]
["Solar Fixed","Norcal",6,10,0.73415695824514349]
["Solar Fixed","Norcal",6,11,0.81520025982196709]
["Solar Fixed","Norcal",6,12,0.85575385743722521]
["Solar Fixed","Norcal",6,13,0.86935859560208095]
["Solar Fixed","Norcal",6,14,0.87616162143645571]
["Solar Fixed","Norcal",6,15,0.85766885105084811]
["Solar Fixed","Norcal",6,16,0.82406718548688251]
["Solar Fixed","Norcal",6,17,0.73664995391139199]
["Solar Fixed","Norcal",6,18,0.59864446688176776]
["Solar Fixed","Norcal",6,19,0.36433142704775739]
["Solar Fixed","Norcal",6,20,9.0433444017613621E-2]
["Solar Fixed","Norcal",6,21,9.7748924722226588E-4]
["Solar Fixed","Norcal",6,22,0]
["Solar Fixed","Norcal",6,23,0]
["Solar Fixed","Norcal",6,24,0]
["Solar Fixed","Norcal",7,1,0]
["Solar Fixed","Norcal",7,2,0]
["Solar Fixed","Norcal",7,3,0]
["Solar Fixed","Norcal",7,4,0]
["Solar Fixed","Norcal",7,5,0]
["Solar Fixed","Norcal",7,6,5.0275075688457023E-8]
["Solar Fixed","Norcal",7,7,4.2922303696431685E-2]
["Solar Fixed","Norcal",7,8,0.30954885872115234]
["Solar Fixed","Norcal",7,9,0.58677863429594113]
["Solar Fixed","Norcal",7,10,0.74945576284853077]
["Solar Fixed","Norcal",7,11,0.83573340956694131]
["Solar Fixed","Norcal",7,12,0.87969267426018671]
["Solar Fixed","Norcal",7,13,0.89455531477542349]
["Solar Fixed","Norcal",7,14,0.88662536922241353]
["Solar Fixed","Norcal",7,15,0.86734065362650348]
["Solar Fixed","Norcal",7,16,0.82452348934773712]
["Solar Fixed","Norcal",7,17,0.74375490680747791]
["Solar Fixed","Norcal",7,18,0.60357140299180423]
["Solar Fixed","Norcal",7,19,0.36279085397413813]
["Solar Fixed","Norcal",7,20,7.9270415119937807E-2]
["Solar Fixed","Norcal",7,21,4.3715722628872238E-4]
["Solar Fixed","Norcal",7,22,0]
["Solar Fixed","Norcal",7,23,0]
["Solar Fixed","Norcal",7,24,0]
["Solar Fixed","Norcal",8,1,0]
["Solar Fixed","Norcal",8,2,0]
["Solar Fixed","Norcal",8,3,0]
["Solar Fixed","Norcal",8,4,0]
["Solar Fixed","Norcal",8,5,0]
["Solar Fixed","Norcal",8,6,0]
["Solar Fixed","Norcal",8,7,8.3045332129821747E-3]
["Solar Fixed","Norcal",8,8,0.19228797485941701]
["Solar Fixed","Norcal",8,9,0.50939567414198805]
["Solar Fixed","Norcal",8,10,0.7025236323156151]
["Solar Fixed","Norcal",8,11,0.80739951960194345]
["Solar Fixed","Norcal",8,12,0.85329624441198326]
["Solar Fixed","Norcal",8,13,0.86247299409861711]
["Solar Fixed","Norcal",8,14,0.86172509325770286]
["Solar Fixed","Norcal",8,15,0.84540756492468294]
["Solar Fixed","Norcal",8,16,0.80299525095918833]
["Solar Fixed","Norcal",8,17,0.70566569327958339]
["Solar Fixed","Norcal",8,18,0.51915933877610665]
["Solar Fixed","Norcal",8,19,0.21056478711233356]
["Solar Fixed","Norcal",8,20,1.4081729522182559E-2]
["Solar Fixed","Norcal",8,21,0]
["Solar Fixed","Norcal",8,22,0]
["Solar Fixed","Norcal",8,23,0]
["Solar Fixed","Norcal",8,24,0]
["Solar Fixed","Norcal",9,1,0]
["Solar Fixed","Norcal",9,2,0]
["Solar Fixed","Norcal",9,3,0]
["Solar Fixed","Norcal",9,4,0]
["Solar Fixed","Norcal",9,5,0]
["Solar Fixed","Norcal",9,6,0]
["Solar Fixed","Norcal",9,7,2.5124097348946283E-4]
["Solar Fixed","Norcal",9,8,0.10760772096265996]
["Solar Fixed","Norcal",9,9,0.4281571400919979]
["Solar Fixed","Norcal",9,10,0.64693102095721788]
["Solar Fixed","Norcal",9,11,0.75633723434054934]
["Solar Fixed","Norcal",9,12,0.79728859992410184]
["Solar Fixed","Norcal",9,13,0.81398293053577131]
["Solar Fixed","Norcal",9,14,0.80479691578499324]
["Solar Fixed","Norcal",9,15,0.78840288530328051]
["Solar Fixed","Norcal",9,16,0.74556225401427811]
["Solar Fixed","Norcal",9,17,0.61790594978606217]
["Solar Fixed","Norcal",9,18,0.34784531561506404]
["Solar Fixed","Norcal",9,19,5.3212037551135079E-2]
["Solar Fixed","Norcal",9,20,7.0609305731229742E-6]
["Solar Fixed","Norcal",9,21,0]
["Solar Fixed","Norcal",9,22,0]
["Solar Fixed","Norcal",9,23,0]
["Solar Fixed","Norcal",9,24,0]
["Solar Fixed","Norcal",10,1,0]
["Solar Fixed","Norcal",10,2,0]
["Solar Fixed","Norcal",10,3,0]
["Solar Fixed","Norcal",10,4,0]
["Solar Fixed","Norcal",10,5,0]
["Solar Fixed","Norcal",10,6,0]
["Solar Fixed","Norcal",10,7,0]
["Solar Fixed","Norcal",10,8,3.4252364814186205E-2]
["Solar Fixed","Norcal",10,9,0.30671189748697453]
["Solar Fixed","Norcal",10,10,0.55919045826286162]
["Solar Fixed","Norcal",10,11,0.66519645640229874]
["Solar Fixed","Norcal",10,12,0.698905535994234]
["Solar Fixed","Norcal",10,13,0.70895306327603247]
["Solar Fixed","Norcal",10,14,0.70314488013059784]
["Solar Fixed","Norcal",10,15,0.68305027003349406]
["Solar Fixed","Norcal",10,16,0.61715645391314944]
["Solar Fixed","Norcal",10,17,0.44826368478282025]
["Solar Fixed","Norcal",10,18,0.13661241977124278]
["Solar Fixed","Norcal",10,19,1.1679573601306589E-3]
["Solar Fixed","Norcal",10,20,0]
["Solar Fixed","Norcal",10,21,0]
["Solar Fixed","Norcal",10,22,0]
["Solar Fixed","Norcal",10,23,0]
["Solar Fixed","Norcal",10,24,0]
["Solar Fixed","Norcal",11,1,0]
["Solar Fixed","Norcal",11,2,0]
["Solar Fixed","Norcal",11,3,0]
["Solar Fixed","Norcal",11,4,0]
["Solar Fixed","Norcal",11,5,0]
["Solar Fixed","Norcal",11,6,0]
["Solar Fixed","Norcal",11,7,1.0785822467466683E-3]
["Solar Fixed","Norcal",11,8,0.12164039321982506]
["Solar Fixed","Norcal",11,9,0.41234220642100461]
["Solar Fixed","Norcal",11,10,0.57876883404181534]
["Solar Fixed","Norcal",11,11,0.64506272960549338]
["Solar Fixed","Norcal",11,12,0.65753283340795021]
["Solar Fixed","Norcal",11,13,0.65389958533824466]
["Solar Fixed","Norcal",11,14,0.61672221157945273]
["Solar Fixed","Norcal",11,15,0.54060164281831435]
["Solar Fixed","Norcal",11,16,0.30916686895233969]
["Solar Fixed","Norcal",11,17,4.0996593735647416E-2]
["Solar Fixed","Norcal",11,18,0]
["Solar Fixed","Norcal",11,19,0]
["Solar Fixed","Norcal",11,20,0]
["Solar Fixed","Norcal",11,21,0]
["Solar Fixed","Norcal",11,22,0]
["Solar Fixed","Norcal",11,23,0]
["Solar Fixed","Norcal",11,24,0]
["Solar Fixed","Norcal",12,1,0]
["Solar Fixed","Norcal",12,2,0]
["Solar Fixed","Norcal",12,3,0]
["Solar Fixed","Norcal",12,4,0]
["Solar Fixed","Norcal",12,5,0]
["Solar Fixed","Norcal",12,6,0]
["Solar Fixed","Norcal",12,7,0]
["Solar Fixed","Norcal",12,8,3.9001020449775131E-2]
["Solar Fixed","Norcal",12,9,0.22524216315912646]
["Solar Fixed","Norcal",12,10,0.39243849776742823]
["Solar Fixed","Norcal",12,11,0.48398786786552234]
["Solar Fixed","Norcal",12,12,0.51703266505482492]
["Solar Fixed","Norcal",12,13,0.49430932454586296]
["Solar Fixed","Norcal",12,14,0.44669957657323717]
["Solar Fixed","Norcal",12,15,0.41082364135559168]
["Solar Fixed","Norcal",12,16,0.2117814298922838]
["Solar Fixed","Norcal",12,17,2.5899053797320853E-2]
["Solar Fixed","Norcal",12,18,0]
["Solar Fixed","Norcal",12,19,0]
["Solar Fixed","Norcal",12,20,0]
["Solar Fixed","Norcal",12,21,0]
["Solar Fixed","Norcal",12,22,0]
["Solar Fixed","Norcal",12,23,0]
["Solar Fixed","Norcal",12,24,0]
["Solar Fixed","Socal",1,1,2.707946006594789E-7]
["Solar Fixed","Socal",1,2,-3.3727843647755268E-7]
["Solar Fixed","Socal",1,3,-6.867231468279616E-7]
["Solar Fixed","Socal",1,4,-8.6996526244345332E-7]
["Solar Fixed","Socal",1,5,-9.6676897534183392E-7]
["Solar Fixed","Socal",1,6,-3.4017940267944353E-7]
["Solar Fixed","Socal",1,7,1.6158851086070657E-3]
["Solar Fixed","Socal",1,8,0.13239431143853209]
["Solar Fixed","Socal",1,9,0.44426584163058674]
["Solar Fixed","Socal",1,10,0.60269970790249372]
["Solar Fixed","Socal",1,11,0.65125790898450409]
["Solar Fixed","Socal",1,12,0.67255623969310108]
["Solar Fixed","Socal",1,13,0.65513248302711713]
["Solar Fixed","Socal",1,14,0.63083386997624225]
["Solar Fixed","Socal",1,15,0.52682733758472877]
["Solar Fixed","Socal",1,16,0.30743699245027595]
["Solar Fixed","Socal",1,17,4.4636019221846485E-2]
["Solar Fixed","Socal",1,18,1.7638307037168781E-5]
["Solar Fixed","Socal",1,19,4.5157168684939214E-6]
["Solar Fixed","Socal",1,20,4.6610851063876981E-6]
["Solar Fixed","Socal",1,21,4.5142529488281493E-6]
["Solar Fixed","Socal",1,22,3.618459117740765E-6]
["Solar Fixed","Socal",1,23,2.3549139747019381E-6]
["Solar Fixed","Socal",1,24,1.1694066721416669E-6]
["Solar Fixed","Socal",2,1,1.0570793293270668E-7]
["Solar Fixed","Socal",2,2,-5.2262696679916687E-7]
["Solar Fixed","Socal",2,3,-1.1022478087967213E-6]
["Solar Fixed","Socal",2,4,-1.1635241683028481E-6]
["Solar Fixed","Socal",2,5,-1.2255818936927811E-6]
["Solar Fixed","Socal",2,6,-3.2706996759057733E-7]
["Solar Fixed","Socal",2,7,1.1027803921520149E-2]
["Solar Fixed","Socal",2,8,0.24644100513214073]
["Solar Fixed","Socal",2,9,0.58457397198050853]
["Solar Fixed","Socal",2,10,0.69634791414784514]
["Solar Fixed","Socal",2,11,0.74504213341281633]
["Solar Fixed","Socal",2,12,0.74774865678225855]
["Solar Fixed","Socal",2,13,0.73442523535992865]
["Solar Fixed","Socal",2,14,0.70720381708334634]
["Solar Fixed","Socal",2,15,0.65065942806269872]
["Solar Fixed","Socal",2,16,0.49964450231632629]
["Solar Fixed","Socal",2,17,0.19370346554409237]
["Solar Fixed","Socal",2,18,4.7742526407390951E-3]
["Solar Fixed","Socal",2,19,4.5249173932132265E-6]
["Solar Fixed","Socal",2,20,4.5022968714150506E-6]
["Solar Fixed","Socal",2,21,4.5425680994225923E-6]
["Solar Fixed","Socal",2,22,3.7459793455633973E-6]
["Solar Fixed","Socal",2,23,2.466694433409161E-6]
["Solar Fixed","Socal",2,24,1.2526190766986711E-6]
["Solar Fixed","Socal",3,1,-1.8252406174143219E-7]
["Solar Fixed","Socal",3,2,-8.6218300717028598E-7]
["Solar Fixed","Socal",3,3,-1.288571302040876E-6]
["Solar Fixed","Socal",3,4,-1.4171873500736019E-6]
["Solar Fixed","Socal",3,5,-1.5286839595642953E-6]
["Solar Fixed","Socal",3,6,-8.8833796299515814E-7]
["Solar Fixed","Socal",3,7,2.1551253888738692E-3]
["Solar Fixed","Socal",3,8,0.1413696122178747]
["Solar Fixed","Socal",3,9,0.49319850120582281]
["Solar Fixed","Socal",3,10,0.68367168393756106]
["Solar Fixed","Socal",3,11,0.75046426774802444]
["Solar Fixed","Socal",3,12,0.76316913851930701]
["Solar Fixed","Socal",3,13,0.75375243932018898]
["Solar Fixed","Socal",3,14,0.73565611408781784]
["Solar Fixed","Socal",3,15,0.69185159473775271]
["Solar Fixed","Socal",3,16,0.61173778108082288]
["Solar Fixed","Socal",3,17,0.38592413536200598]
["Solar Fixed","Socal",3,18,0.1794178446368285]
["Solar Fixed","Socal",3,19,2.7039915356120086E-2]
["Solar Fixed","Socal",3,20,7.538903438066309E-6]
["Solar Fixed","Socal",3,21,4.0859275553775491E-6]
["Solar Fixed","Socal",3,22,3.5361532299434869E-6]
["Solar Fixed","Socal",3,23,2.1871721092193205E-6]
["Solar Fixed","Socal",3,24,9.603654972894871E-7]
["Solar Fixed","Socal",4,1,-1.1929611584770108E-7]
["Solar Fixed","Socal",4,2,-6.4239222007039111E-7]
["Solar Fixed","Socal",4,3,-1.0537846735645889E-6]
["Solar Fixed","Socal",4,4,-1.3891801648730828E-6]
["Solar Fixed","Socal",4,5,-1.4842109815754564E-6]
["Solar Fixed","Socal",4,6,-3.9950735096238574E-7]
["Solar Fixed","Socal",4,7,2.7400704164537718E-2]
["Solar Fixed","Socal",4,8,0.27629637045885802]
["Solar Fixed","Socal",4,9,0.59488575047028669]
["Solar Fixed","Socal",4,10,0.74681541839783272]
["Solar Fixed","Socal",4,11,0.81492618011017237]
["Solar Fixed","Socal",4,12,0.84859985371160707]
["Solar Fixed","Socal",4,13,0.84987028776239015]
["Solar Fixed","Socal",4,14,0.832545397478475]
["Solar Fixed","Socal",4,15,0.81110967810632384]
["Solar Fixed","Socal",4,16,0.74396149729417438]
["Solar Fixed","Socal",4,17,0.63295072390474438]
["Solar Fixed","Socal",4,18,0.43418182342358935]
["Solar Fixed","Socal",4,19,0.10837401457993323]
["Solar Fixed","Socal",4,20,1.4275611624247348E-3]
["Solar Fixed","Socal",4,21,6.6949653229225659E-6]
["Solar Fixed","Socal",4,22,3.8536144247149945E-6]
["Solar Fixed","Socal",4,23,2.4830966384252345E-6]
["Solar Fixed","Socal",4,24,1.0789070981656649E-6]
["Solar Fixed","Socal",5,1,2.6960250372015843E-7]
["Solar Fixed","Socal",5,2,-5.1414480031041065E-7]
["Solar Fixed","Socal",5,3,-9.8076681854957754E-7]
["Solar Fixed","Socal",5,4,-1.2513857463135398E-6]
["Solar Fixed","Socal",5,5,-1.4412871516860848E-6]
["Solar Fixed","Socal",5,6,1.4373884673775088E-3]
["Solar Fixed","Socal",5,7,0.1143702104520835]
["Solar Fixed","Socal",5,8,0.42015119080535468]
["Solar Fixed","Socal",5,9,0.6373694952388238]
["Solar Fixed","Socal",5,10,0.75751622187376]
["Solar Fixed","Socal",5,11,0.84195614368208704]
["Solar Fixed","Socal",5,12,0.87533188312741861]
["Solar Fixed","Socal",5,13,0.88007102238333279]
["Solar Fixed","Socal",5,14,0.87042714492307549]
["Solar Fixed","Socal",5,15,0.85276765565355117]
["Solar Fixed","Socal",5,16,0.79428059462094081]
["Solar Fixed","Socal",5,17,0.69451888017035923]
["Solar Fixed","Socal",5,18,0.50417164215513821]
["Solar Fixed","Socal",5,19,0.18936502634634789]
["Solar Fixed","Socal",5,20,1.2363480882888899E-2]
["Solar Fixed","Socal",5,21,1.151636432656676E-5]
["Solar Fixed","Socal",5,22,4.2909532572797973E-6]
["Solar Fixed","Socal",5,23,2.9310557579420342E-6]
["Solar Fixed","Socal",5,24,1.3511306062159925E-6]
["Solar Fixed","Socal",6,1,2.2481829546404261E-6]
["Solar Fixed","Socal",6,2,1.1384840352193138E-6]
["Solar Fixed","Socal",6,3,1.2137482051524995E-7]
["Solar Fixed","Socal",6,4,-5.4237498361829168E-7]
["Solar Fixed","Socal",6,5,-9.3321121008457171E-7]
["Solar Fixed","Socal",6,6,3.7050244269847526E-3]
["Solar Fixed","Socal",6,7,0.14057897809304987]
["Solar Fixed","Socal",6,8,0.42882059200299039]
["Solar Fixed","Socal",6,9,0.65103510981746038]
["Solar Fixed","Socal",6,10,0.77771676793328337]
["Solar Fixed","Socal",6,11,0.86075952689414392]
["Solar Fixed","Socal",6,12,0.89975850361178356]
["Solar Fixed","Socal",6,13,0.90678956837591917]
["Solar Fixed","Socal",6,14,0.90566958059391689]
["Solar Fixed","Socal",6,15,0.87463224414955953]
["Solar Fixed","Socal",6,16,0.80974641994295982]
["Solar Fixed","Socal",6,17,0.70976175510124417]
["Solar Fixed","Socal",6,18,0.54246980223663255]
["Solar Fixed","Socal",6,19,0.25880259001661932]
["Solar Fixed","Socal",6,20,3.2679684170460348E-2]
["Solar Fixed","Socal",6,21,4.7217696294517851E-5]
["Solar Fixed","Socal",6,22,8.2604518542519982E-6]
["Solar Fixed","Socal",6,23,6.3892615316746807E-6]
["Solar Fixed","Socal",6,24,4.3133456843293713E-6]
["Solar Fixed","Socal",7,1,5.5020223254336754E-6]
["Solar Fixed","Socal",7,2,3.9524367149644E-6]
["Solar Fixed","Socal",7,3,2.513266919499019E-6]
["Solar Fixed","Socal",7,4,1.4765945027125247E-6]
["Solar Fixed","Socal",7,5,7.9615416652685541E-7]
["Solar Fixed","Socal",7,6,1.6410887323183766E-4]
["Solar Fixed","Socal",7,7,6.7432782643183101E-2]
["Solar Fixed","Socal",7,8,0.29483410130614329]
["Solar Fixed","Socal",7,9,0.54446077515883873]
["Solar Fixed","Socal",7,10,0.7005381071415101]
["Solar Fixed","Socal",7,11,0.80446771982502374]
["Solar Fixed","Socal",7,12,0.85735064761288893]
["Solar Fixed","Socal",7,13,0.87457080616373262]
["Solar Fixed","Socal",7,14,0.86751997607034181]
["Solar Fixed","Socal",7,15,0.82849723942237019]
["Solar Fixed","Socal",7,16,0.77503514217185854]
["Solar Fixed","Socal",7,17,0.67094394446322747]
["Solar Fixed","Socal",7,18,0.50463889495019776]
["Solar Fixed","Socal",7,19,0.22951687661330081]
["Solar Fixed","Socal",7,20,2.6173165499402365E-2]
["Solar Fixed","Socal",7,21,3.2181956519599985E-5]
["Solar Fixed","Socal",7,22,1.4855490137762763E-5]
["Solar Fixed","Socal",7,23,1.1437069908357072E-5]
["Solar Fixed","Socal",7,24,7.652925515161189E-6]
["Solar Fixed","Socal",8,1,6.9042927323063562E-6]
["Solar Fixed","Socal",8,2,4.9854676771183054E-6]
["Solar Fixed","Socal",8,3,3.636857703060492E-6]
["Solar Fixed","Socal",8,4,2.6227115652320301E-6]
["Solar Fixed","Socal",8,5,1.5370910728927203E-6]
["Solar Fixed","Socal",8,6,2.9560707277074849E-6]
["Solar Fixed","Socal",8,7,2.996164261111587E-2]
["Solar Fixed","Socal",8,8,0.265335148838029]
["Solar Fixed","Socal",8,9,0.56627683665800665]
["Solar Fixed","Socal",8,10,0.72816075312954276]
["Solar Fixed","Socal",8,11,0.82757047669852735]
["Solar Fixed","Socal",8,12,0.87890160090548419]
["Solar Fixed","Socal",8,13,0.89546416915952776]
["Solar Fixed","Socal",8,14,0.88090874176492706]
["Solar Fixed","Socal",8,15,0.84409143589406643]
["Solar Fixed","Socal",8,16,0.76828549356144671]
["Solar Fixed","Socal",8,17,0.65015425624328405]
["Solar Fixed","Socal",8,18,0.43373546028051752]
["Solar Fixed","Socal",8,19,0.12390606931610887]
["Solar Fixed","Socal",8,20,3.3590947205156176E-3]
["Solar Fixed","Socal",8,21,2.8719394882328023E-5]
["Solar Fixed","Socal",8,22,1.8020141705869651E-5]
["Solar Fixed","Socal",8,23,1.2334573983476779E-5]
["Solar Fixed","Socal",8,24,9.1481279730331709E-6]
["Solar Fixed","Socal",9,1,3.9213685180480706E-6]
["Solar Fixed","Socal",9,2,2.1525160316975176E-6]
["Solar Fixed","Socal",9,3,1.3101925319791238E-6]
["Solar Fixed","Socal",9,4,6.7290260564135553E-7]
["Solar Fixed","Socal",9,5,1.1233730345622463E-7]
["Solar Fixed","Socal",9,6,8.7397867212599188E-8]
["Solar Fixed","Socal",9,7,8.299498428439564E-3]
["Solar Fixed","Socal",9,8,0.20394073266328211]
["Solar Fixed","Socal",9,9,0.52891509761854683]
["Solar Fixed","Socal",9,10,0.71266805165412483]
["Solar Fixed","Socal",9,11,0.81252809860794839]
["Solar Fixed","Socal",9,12,0.85756876216289657]
["Solar Fixed","Socal",9,13,0.86789000759786772]
["Solar Fixed","Socal",9,14,0.86008214699728125]
["Solar Fixed","Socal",9,15,0.82012679998675053]
["Solar Fixed","Socal",9,16,0.72212604176400064]
["Solar Fixed","Socal",9,17,0.58148704072356761]
["Solar Fixed","Socal",9,18,0.25736805042524163]
["Solar Fixed","Socal",9,19,2.2987719226754126E-2]
["Solar Fixed","Socal",9,20,9.5070221882472705E-5]
["Solar Fixed","Socal",9,21,1.3990864642350627E-5]
["Solar Fixed","Socal",9,22,1.0677724539430046E-5]
["Solar Fixed","Socal",9,23,8.3435506069648067E-6]
["Solar Fixed","Socal",9,24,5.6819304675159933E-6]
["Solar Fixed","Socal",10,1,1.0262586590200684E-6]
["Solar Fixed","Socal",10,2,1.9644941719965103E-7]
["Solar Fixed","Socal",10,3,-4.3679711187941258E-7]
["Solar Fixed","Socal",10,4,-7.2037315802921581E-7]
["Solar Fixed","Socal",10,5,-9.607557941145247E-7]
["Solar Fixed","Socal",10,6,-4.8582322431713267E-7]
["Solar Fixed","Socal",10,7,9.3566814666746069E-4]
["Solar Fixed","Socal",10,8,0.10870290824897606]
["Solar Fixed","Socal",10,9,0.45849398050230655]
["Solar Fixed","Socal",10,10,0.65606781307751949]
["Solar Fixed","Socal",10,11,0.74658027232767277]
["Solar Fixed","Socal",10,12,0.79349729063508267]
["Solar Fixed","Socal",10,13,0.8045439022086136]
["Solar Fixed","Socal",10,14,0.79287051108521434]
["Solar Fixed","Socal",10,15,0.75398008283602502]
["Solar Fixed","Socal",10,16,0.67097338910474891]
["Solar Fixed","Socal",10,17,0.4245554324939434]
["Solar Fixed","Socal",10,18,8.5169808859421603E-2]
["Solar Fixed","Socal",10,19,3.8855923559136534E-4]
["Solar Fixed","Socal",10,20,8.2330959994694269E-6]
["Solar Fixed","Socal",10,21,6.3424003553840271E-6]
["Solar Fixed","Socal",10,22,5.7941078286261108E-6]
["Solar Fixed","Socal",10,23,4.0855820405451271E-6]
["Solar Fixed","Socal",10,24,2.1955768507808169E-6]
["Solar Fixed","Socal",11,1,-5.8526389894473243E-8]
["Solar Fixed","Socal",11,2,-6.3305428994239966E-7]
["Solar Fixed","Socal",11,3,-1.1351623842023863E-6]
["Solar Fixed","Socal",11,4,-1.3264963213465873E-6]
["Solar Fixed","Socal",11,5,-1.2689952846240631E-6]
["Solar Fixed","Socal",11,6,6.5385625098243661E-6]
["Solar Fixed","Socal",11,7,2.4688113390975104E-2]
["Solar Fixed","Socal",11,8,0.26989563720833115]
["Solar Fixed","Socal",11,9,0.53992419286077609]
["Solar Fixed","Socal",11,10,0.67143636918080796]
["Solar Fixed","Socal",11,11,0.71670275922611426]
["Solar Fixed","Socal",11,12,0.73363676881361817]
["Solar Fixed","Socal",11,13,0.71092034071200561]
["Solar Fixed","Socal",11,14,0.6731220026024447]
["Solar Fixed","Socal",11,15,0.55413351386574272]
["Solar Fixed","Socal",11,16,0.25305152546056398]
["Solar Fixed","Socal",11,17,1.7049542539256356E-2]
["Solar Fixed","Socal",11,18,4.8960871565052103E-6]
["Solar Fixed","Socal",11,19,4.0670169908190497E-6]
["Solar Fixed","Socal",11,20,4.1720029404334294E-6]
["Solar Fixed","Socal",11,21,3.9669875626460336E-6]
["Solar Fixed","Socal",11,22,3.2237135252959546E-6]
["Solar Fixed","Socal",11,23,2.0587463936481821E-6]
["Solar Fixed","Socal",11,24,7.8113444397067025E-7]
["Solar Fixed","Socal",12,1,1.0825510034365778E-6]
["Solar Fixed","Socal",12,2,1.9128276506103262E-7]
["Solar Fixed","Socal",12,3,-2.8650174674948896E-7]
["Solar Fixed","Socal",12,4,-5.918247906811115E-7]
["Solar Fixed","Socal",12,5,-2.8550722108195536E-7]
["Solar Fixed","Socal",12,6,2.0994014180698647E-9]
["Solar Fixed","Socal",12,7,3.0231705452576241E-3]
["Solar Fixed","Socal",12,8,0.14243413391126397]
["Solar Fixed","Socal",12,9,0.39981302231033866]
["Solar Fixed","Socal",12,10,0.5352294568585223]
["Solar Fixed","Socal",12,11,0.58985433604685245]
["Solar Fixed","Socal",12,12,0.62100296509897057]
["Solar Fixed","Socal",12,13,0.60207552816649856]
["Solar Fixed","Socal",12,14,0.55296624180320975]
["Solar Fixed","Socal",12,15,0.45082019122228967]
["Solar Fixed","Socal",12,16,0.20174450572893618]
["Solar Fixed","Socal",12,17,1.2426294475731922E-2]
["Solar Fixed","Socal",12,18,5.4903138612164999E-6]
["Solar Fixed","Socal",12,19,5.6868090445963236E-6]
["Solar Fixed","Socal",12,20,6.0155590539510055E-6]
["Solar Fixed","Socal",12,21,5.8452984138728724E-6]
["Solar Fixed","Socal",12,22,5.1284222996238097E-6]
["Solar Fixed","Socal",12,23,3.6667662448883569E-6]
["Solar Fixed","Socal",12,24,2.3466849663224737E-6]
["Solar Tracking","Norcal",1,1,0]
["Solar Tracking","Norcal",1,2,0]
["Solar Tracking","Norcal",1,3,0]
["Solar Tracking","Norcal",1,4,0]
["Solar Tracking","Norcal",1,5,0]
["Solar Tracking","Norcal",1,6,0]
["Solar Tracking","Norcal",1,7,1.2522007095849141E-7]
["Solar Tracking","Norcal",1,8,2.3455069838785383E-2]
["Solar Tracking","Norcal",1,9,0.18903362532739215]
["Solar Tracking","Norcal",1,10,0.33482128706295677]
["Solar Tracking","Norcal",1,11,0.40825872759330073]
["Solar Tracking","Norcal",1,12,0.44136617645580334]
["Solar Tracking","Norcal",1,13,0.4558951581963368]
["Solar Tracking","Norcal",1,14,0.42530005005121668]
["Solar Tracking","Norcal",1,15,0.39690081033310953]
["Solar Tracking","Norcal",1,16,0.27235911900106757]
["Solar Tracking","Norcal",1,17,6.0319737143228074E-2]
["Solar Tracking","Norcal",1,18,3.7203345572991036E-5]
["Solar Tracking","Norcal",1,19,0]
["Solar Tracking","Norcal",1,20,0]
["Solar Tracking","Norcal",1,21,0]
["Solar Tracking","Norcal",1,22,0]
["Solar Tracking","Norcal",1,23,0]
["Solar Tracking","Norcal",1,24,0]
["Solar Tracking","Norcal",2,1,0]
["Solar Tracking","Norcal",2,2,0]
["Solar Tracking","Norcal",2,3,0]
["Solar Tracking","Norcal",2,4,0]
["Solar Tracking","Norcal",2,5,0]
["Solar Tracking","Norcal",2,6,0]
["Solar Tracking","Norcal",2,7,2.3114090632639866E-4]
["Solar Tracking","Norcal",2,8,0.12680628750847758]
["Solar Tracking","Norcal",2,9,0.51660498748965555]
["Solar Tracking","Norcal",2,10,0.66258766881361708]
["Solar Tracking","Norcal",2,11,0.66022790630406125]
["Solar Tracking","Norcal",2,12,0.63020759828534822]
["Solar Tracking","Norcal",2,13,0.62228767830817655]
["Solar Tracking","Norcal",2,14,0.62077445438159062]
["Solar Tracking","Norcal",2,15,0.63438549136869649]
["Solar Tracking","Norcal",2,16,0.55079259725749818]
["Solar Tracking","Norcal",2,17,0.2876163419094383]
["Solar Tracking","Norcal",2,18,1.5326627797084876E-2]
["Solar Tracking","Norcal",2,19,0]
["Solar Tracking","Norcal",2,20,0]
["Solar Tracking","Norcal",2,21,0]
["Solar Tracking","Norcal",2,22,0]
["Solar Tracking","Norcal",2,23,0]
["Solar Tracking","Norcal",2,24,0]
["Solar Tracking","Norcal",3,1,0]
["Solar Tracking","Norcal",3,2,0]
["Solar Tracking","Norcal",3,3,0]
["Solar Tracking","Norcal",3,4,0]
["Solar Tracking","Norcal",3,5,0]
["Solar Tracking","Norcal",3,6,0]
["Solar Tracking","Norcal",3,7,1.1336247432309892E-5]
["Solar Tracking","Norcal",3,8,7.7946530608562187E-2]
["Solar Tracking","Norcal",3,9,0.43984975182837538]
["Solar Tracking","Norcal",3,10,0.66021671949960159]
["Solar Tracking","Norcal",3,11,0.6960495891277646]
["Solar Tracking","Norcal",3,12,0.6706380099155117]
["Solar Tracking","Norcal",3,13,0.67615936786465958]
["Solar Tracking","Norcal",3,14,0.64744087338105905]
["Solar Tracking","Norcal",3,15,0.61558897731329743]
["Solar Tracking","Norcal",3,16,0.57942916863237182]
["Solar Tracking","Norcal",3,17,0.48519473636283061]
["Solar Tracking","Norcal",3,18,0.14700228689888911]
["Solar Tracking","Norcal",3,19,3.0450205789856261E-2]
["Solar Tracking","Norcal",3,20,4.1475832183462411E-5]
["Solar Tracking","Norcal",3,21,0]
["Solar Tracking","Norcal",3,22,0]
["Solar Tracking","Norcal",3,23,0]
["Solar Tracking","Norcal",3,24,0]
["Solar Tracking","Norcal",4,1,0]
["Solar Tracking","Norcal",4,2,0]
["Solar Tracking","Norcal",4,3,0]
["Solar Tracking","Norcal",4,4,0]
["Solar Tracking","Norcal",4,5,0]
["Solar Tracking","Norcal",4,6,0]
["Solar Tracking","Norcal",4,7,7.8392191125671133E-3]
["Solar Tracking","Norcal",4,8,0.25713519816718905]
["Solar Tracking","Norcal",4,9,0.61409673717612789]
["Solar Tracking","Norcal",4,10,0.7224500981641524]
["Solar Tracking","Norcal",4,11,0.71826120772625546]
["Solar Tracking","Norcal",4,12,0.70754115315329724]
["Solar Tracking","Norcal",4,13,0.731194394222762]
["Solar Tracking","Norcal",4,14,0.72708618813259673]
["Solar Tracking","Norcal",4,15,0.71326457866302395]
["Solar Tracking","Norcal",4,16,0.72278176475952405]
["Solar Tracking","Norcal",4,17,0.68053952170156085]
["Solar Tracking","Norcal",4,18,0.60473939107135677]
["Solar Tracking","Norcal",4,19,0.26002128595505669]
["Solar Tracking","Norcal",4,20,1.0357168603078861E-2]
["Solar Tracking","Norcal",4,21,0]
["Solar Tracking","Norcal",4,22,0]
["Solar Tracking","Norcal",4,23,0]
["Solar Tracking","Norcal",4,24,0]
["Solar Tracking","Norcal",5,1,0]
["Solar Tracking","Norcal",5,2,0]
["Solar Tracking","Norcal",5,3,0]
["Solar Tracking","Norcal",5,4,0]
["Solar Tracking","Norcal",5,5,0]
["Solar Tracking","Norcal",5,6,4.9571809427060944E-5]
["Solar Tracking","Norcal",5,7,9.340210552533075E-2]
["Solar Tracking","Norcal",5,8,0.4988397897366022]
["Solar Tracking","Norcal",5,9,0.70185924471333283]
["Solar Tracking","Norcal",5,10,0.75086640794709392]
["Solar Tracking","Norcal",5,11,0.76343916732694961]
["Solar Tracking","Norcal",5,12,0.7574118774435481]
["Solar Tracking","Norcal",5,13,0.7734027954627859]
["Solar Tracking","Norcal",5,14,0.77469994284200339]
["Solar Tracking","Norcal",5,15,0.77648795191666342]
["Solar Tracking","Norcal",5,16,0.78692055375346803]
["Solar Tracking","Norcal",5,17,0.76483439374754525]
["Solar Tracking","Norcal",5,18,0.71747612721357434]
["Solar Tracking","Norcal",5,19,0.43706796427814676]
["Solar Tracking","Norcal",5,20,5.8020543604933923E-2]
["Solar Tracking","Norcal",5,21,3.9278125266856535E-6]
["Solar Tracking","Norcal",5,22,0]
["Solar Tracking","Norcal",5,23,0]
["Solar Tracking","Norcal",5,24,0]
["Solar Tracking","Norcal",6,1,0]
["Solar Tracking","Norcal",6,2,0]
["Solar Tracking","Norcal",6,3,0]
["Solar Tracking","Norcal",6,4,0]
["Solar Tracking","Norcal",6,5,0]
["Solar Tracking","Norcal",6,6,5.564148037087072E-4]
["Solar Tracking","Norcal",6,7,0.15531841417443534]
["Solar Tracking","Norcal",6,8,0.56416455178585123]
["Solar Tracking","Norcal",6,9,0.76085030965461986]
["Solar Tracking","Norcal",6,10,0.82711354747138954]
["Solar Tracking","Norcal",6,11,0.83822065796885747]
["Solar Tracking","Norcal",6,12,0.84544114866510922]
["Solar Tracking","Norcal",6,13,0.85086370567907665]
["Solar Tracking","Norcal",6,14,0.84596954512092526]
["Solar Tracking","Norcal",6,15,0.84008161760937594]
["Solar Tracking","Norcal",6,16,0.84258022189677995]
["Solar Tracking","Norcal",6,17,0.81050479688236898]
["Solar Tracking","Norcal",6,18,0.75930390647069668]
["Solar Tracking","Norcal",6,19,0.547791762910254]
["Solar Tracking","Norcal",6,20,0.14828497145636382]
["Solar Tracking","Norcal",6,21,1.2890369230925754E-3]
["Solar Tracking","Norcal",6,22,0]
["Solar Tracking","Norcal",6,23,0]
["Solar Tracking","Norcal",6,24,0]
["Solar Tracking","Norcal",7,1,0]
["Solar Tracking","Norcal",7,2,0]
["Solar Tracking","Norcal",7,3,0]
["Solar Tracking","Norcal",7,4,0]
["Solar Tracking","Norcal",7,5,0]
["Solar Tracking","Norcal",7,6,5.8446859471452442E-6]
["Solar Tracking","Norcal",7,7,6.9784390860860385E-2]
["Solar Tracking","Norcal",7,8,0.46219696539701755]
["Solar Tracking","Norcal",7,9,0.7633345348529319]
["Solar Tracking","Norcal",7,10,0.84291586648637407]
["Solar Tracking","Norcal",7,11,0.85568882911313116]
["Solar Tracking","Norcal",7,12,0.85813159958356822]
["Solar Tracking","Norcal",7,13,0.85175911612433108]
["Solar Tracking","Norcal",7,14,0.85160414373745164]
["Solar Tracking","Norcal",7,15,0.8381339064999016]
["Solar Tracking","Norcal",7,16,0.83745209564726197]
["Solar Tracking","Norcal",7,17,0.80723595080963739]
["Solar Tracking","Norcal",7,18,0.74663482369585077]
["Solar Tracking","Norcal",7,19,0.51791166499739594]
["Solar Tracking","Norcal",7,20,0.11955889728877482]
["Solar Tracking","Norcal",7,21,6.2820592466334769E-4]
["Solar Tracking","Norcal",7,22,0]
["Solar Tracking","Norcal",7,23,0]
["Solar Tracking","Norcal",7,24,0]
["Solar Tracking","Norcal",8,1,0]
["Solar Tracking","Norcal",8,2,0]
["Solar Tracking","Norcal",8,3,0]
["Solar Tracking","Norcal",8,4,0]
["Solar Tracking","Norcal",8,5,0]
["Solar Tracking","Norcal",8,6,0]
["Solar Tracking","Norcal",8,7,1.0254789792153241E-2]
["Solar Tracking","Norcal",8,8,0.27315643801856943]
["Solar Tracking","Norcal",8,9,0.63782162417345178]
["Solar Tracking","Norcal",8,10,0.77674208433403191]
["Solar Tracking","Norcal",8,11,0.80764757393083153]
["Solar Tracking","Norcal",8,12,0.81785634425250164]
["Solar Tracking","Norcal",8,13,0.81679772715411147]
["Solar Tracking","Norcal",8,14,0.80923254512169274]
["Solar Tracking","Norcal",8,15,0.80797866861065271]
["Solar Tracking","Norcal",8,16,0.80504696875741732]
["Solar Tracking","Norcal",8,17,0.76990275472665182]
["Solar Tracking","Norcal",8,18,0.62699690513838369]
["Solar Tracking","Norcal",8,19,0.2756793840569603]
["Solar Tracking","Norcal",8,20,1.6082575578981684E-2]
["Solar Tracking","Norcal",8,21,0]
["Solar Tracking","Norcal",8,22,0]
["Solar Tracking","Norcal",8,23,0]
["Solar Tracking","Norcal",8,24,0]
["Solar Tracking","Norcal",9,1,0]
["Solar Tracking","Norcal",9,2,0]
["Solar Tracking","Norcal",9,3,0]
["Solar Tracking","Norcal",9,4,0]
["Solar Tracking","Norcal",9,5,0]
["Solar Tracking","Norcal",9,6,0]
["Solar Tracking","Norcal",9,7,3.7545451381835933E-4]
["Solar Tracking","Norcal",9,8,0.13212352911159464]
["Solar Tracking","Norcal",9,9,0.50930981374403517]
["Solar Tracking","Norcal",9,10,0.6810148686976919]
["Solar Tracking","Norcal",9,11,0.72145005389886607]
["Solar Tracking","Norcal",9,12,0.7299777417513138]
["Solar Tracking","Norcal",9,13,0.72143034947128781]
["Solar Tracking","Norcal",9,14,0.71685803315710839]
["Solar Tracking","Norcal",9,15,0.71894360869595153]
["Solar Tracking","Norcal",9,16,0.72923341262065089]
["Solar Tracking","Norcal",9,17,0.65642605592456882]
["Solar Tracking","Norcal",9,18,0.40700246242502308]
["Solar Tracking","Norcal",9,19,5.2193834164426328E-2]
["Solar Tracking","Norcal",9,20,4.4623253458578917E-7]
["Solar Tracking","Norcal",9,21,0]
["Solar Tracking","Norcal",9,22,0]
["Solar Tracking","Norcal",9,23,0]
["Solar Tracking","Norcal",9,24,0]
["Solar Tracking","Norcal",10,1,0]
["Solar Tracking","Norcal",10,2,0]
["Solar Tracking","Norcal",10,3,0]
["Solar Tracking","Norcal",10,4,0]
["Solar Tracking","Norcal",10,5,0]
["Solar Tracking","Norcal",10,6,0]
["Solar Tracking","Norcal",10,7,7.1953953573263415E-10]
["Solar Tracking","Norcal",10,8,3.445686161771102E-2]
["Solar Tracking","Norcal",10,9,0.32563077406328916]
["Solar Tracking","Norcal",10,10,0.56916940676236771]
["Solar Tracking","Norcal",10,11,0.62770746235590558]
["Solar Tracking","Norcal",10,12,0.61925436539063183]
["Solar Tracking","Norcal",10,13,0.59646885377511638]
["Solar Tracking","Norcal",10,14,0.60353913878882526]
["Solar Tracking","Norcal",10,15,0.62193834941767545]
["Solar Tracking","Norcal",10,16,0.60713253838152925]
["Solar Tracking","Norcal",10,17,0.47586541355106915]
["Solar Tracking","Norcal",10,18,0.13442869043680344]
["Solar Tracking","Norcal",10,19,8.9633489550705559E-4]
["Solar Tracking","Norcal",10,20,0]
["Solar Tracking","Norcal",10,21,0]
["Solar Tracking","Norcal",10,22,0]
["Solar Tracking","Norcal",10,23,0]
["Solar Tracking","Norcal",10,24,0]
["Solar Tracking","Norcal",11,1,0]
["Solar Tracking","Norcal",11,2,0]
["Solar Tracking","Norcal",11,3,0]
["Solar Tracking","Norcal",11,4,0]
["Solar Tracking","Norcal",11,5,0]
["Solar Tracking","Norcal",11,6,0]
["Solar Tracking","Norcal",11,7,1.0385647397455208E-3]
["Solar Tracking","Norcal",11,8,0.10728273671909874]
["Solar Tracking","Norcal",11,9,0.3723336971787703]
["Solar Tracking","Norcal",11,10,0.50808341998301065]
["Solar Tracking","Norcal",11,11,0.52766166229610623]
["Solar Tracking","Norcal",11,12,0.50525481572986441]
["Solar Tracking","Norcal",11,13,0.51974512533832729]
["Solar Tracking","Norcal",11,14,0.53204123911846302]
["Solar Tracking","Norcal",11,15,0.50254262673646322]
["Solar Tracking","Norcal",11,16,0.30672173019239146]
["Solar Tracking","Norcal",11,17,3.6646466558980288E-2]
["Solar Tracking","Norcal",11,18,0]
["Solar Tracking","Norcal",11,19,0]
["Solar Tracking","Norcal",11,20,0]
["Solar Tracking","Norcal",11,21,0]
["Solar Tracking","Norcal",11,22,0]
["Solar Tracking","Norcal",11,23,0]
["Solar Tracking","Norcal",11,24,0]
["Solar Tracking","Norcal",12,1,0]
["Solar Tracking","Norcal",12,2,0]
["Solar Tracking","Norcal",12,3,0]
["Solar Tracking","Norcal",12,4,0]
["Solar Tracking","Norcal",12,5,0]
["Solar Tracking","Norcal",12,6,0]
["Solar Tracking","Norcal",12,7,3.71084872549192E-6]
["Solar Tracking","Norcal",12,8,2.5203708953400933E-2]
["Solar Tracking","Norcal",12,9,0.1872977789667018]
["Solar Tracking","Norcal",12,10,0.3065823357791948]
["Solar Tracking","Norcal",12,11,0.36721590590742531]
["Solar Tracking","Norcal",12,12,0.40201611266272763]
["Solar Tracking","Norcal",12,13,0.39610547882997982]
["Solar Tracking","Norcal",12,14,0.38157314384345881]
["Solar Tracking","Norcal",12,15,0.32081518919493923]
["Solar Tracking","Norcal",12,16,0.17093877941218455]
["Solar Tracking","Norcal",12,17,2.0065053547852214E-2]
["Solar Tracking","Norcal",12,18,0]
["Solar Tracking","Norcal",12,19,0]
["Solar Tracking","Norcal",12,20,0]
["Solar Tracking","Norcal",12,21,0]
["Solar Tracking","Norcal",12,22,0]
["Solar Tracking","Norcal",12,23,0]
["Solar Tracking","Norcal",12,24,0]
["Solar Tracking","Socal",1,1,0]
["Solar Tracking","Socal",1,2,0]
["Solar Tracking","Socal",1,3,0]
["Solar Tracking","Socal",1,4,0]
["Solar Tracking","Socal",1,5,0]
["Solar Tracking","Socal",1,6,0]
["Solar Tracking","Socal",1,7,4.9799666277957136E-4]
["Solar Tracking","Socal",1,8,0.1197753049047672]
["Solar Tracking","Socal",1,9,0.469181402376249]
["Solar Tracking","Socal",1,10,0.61089556617336682]
["Solar Tracking","Socal",1,11,0.60480492514890904]
["Solar Tracking","Socal",1,12,0.5940939433444431]
["Solar Tracking","Socal",1,13,0.58766310624063989]
["Solar Tracking","Socal",1,14,0.58909493302807558]
["Solar Tracking","Socal",1,15,0.53358211070082173]
["Solar Tracking","Socal",1,16,0.3850430246845456]
["Solar Tracking","Socal",1,17,6.4962864173754672E-2]
["Solar Tracking","Socal",1,18,2.3165802725897424E-5]
["Solar Tracking","Socal",1,19,0]
["Solar Tracking","Socal",1,20,0]
["Solar Tracking","Socal",1,21,0]
["Solar Tracking","Socal",1,22,0]
["Solar Tracking","Socal",1,23,0]
["Solar Tracking","Socal",1,24,0]
["Solar Tracking","Socal",2,1,0]
["Solar Tracking","Socal",2,2,0]
["Solar Tracking","Socal",2,3,0]
["Solar Tracking","Socal",2,4,0]
["Solar Tracking","Socal",2,5,0]
["Solar Tracking","Socal",2,6,0]
["Solar Tracking","Socal",2,7,6.8857666015631584E-3]
["Solar Tracking","Socal",2,8,0.26155421098912135]
["Solar Tracking","Socal",2,9,0.63644242181633848]
["Solar Tracking","Socal",2,10,0.70326178408663642]
["Solar Tracking","Socal",2,11,0.68788352359387617]
["Solar Tracking","Socal",2,12,0.6818550156122607]
["Solar Tracking","Socal",2,13,0.67807272716887412]
["Solar Tracking","Socal",2,14,0.65389191054488605]
["Solar Tracking","Socal",2,15,0.63791734794331101]
["Solar Tracking","Socal",2,16,0.57984576266590093]
["Solar Tracking","Socal",2,17,0.24632516431707285]
["Solar Tracking","Socal",2,18,9.8686767155693935E-3]
["Solar Tracking","Socal",2,19,0]
["Solar Tracking","Socal",2,20,0]
["Solar Tracking","Socal",2,21,0]
["Solar Tracking","Socal",2,22,0]
["Solar Tracking","Socal",2,23,0]
["Solar Tracking","Socal",2,24,0]
["Solar Tracking","Socal",3,1,0]
["Solar Tracking","Socal",3,2,0]
["Solar Tracking","Socal",3,3,0]
["Solar Tracking","Socal",3,4,0]
["Solar Tracking","Socal",3,5,0]
["Solar Tracking","Socal",3,6,0]
["Solar Tracking","Socal",3,7,1.4858384619493292E-3]
["Solar Tracking","Socal",3,8,0.17106539567547008]
["Solar Tracking","Socal",3,9,0.5944178724876904]
["Solar Tracking","Socal",3,10,0.72966129859813356]
["Solar Tracking","Socal",3,11,0.7322731215902224]
["Solar Tracking","Socal",3,12,0.71737549353158003]
["Solar Tracking","Socal",3,13,0.70992778349343355]
["Solar Tracking","Socal",3,14,0.70665946844392946]
["Solar Tracking","Socal",3,15,0.67120528061146079]
["Solar Tracking","Socal",3,16,0.61888245549259158]
["Solar Tracking","Socal",3,17,0.46181180469631344]
["Solar Tracking","Socal",3,18,0.17371887063270774]
["Solar Tracking","Socal",3,19,2.8055378481300006E-2]
["Solar Tracking","Socal",3,20,5.9208354563399097E-7]
["Solar Tracking","Socal",3,21,0]
["Solar Tracking","Socal",3,22,0]
["Solar Tracking","Socal",3,23,0]
["Solar Tracking","Socal",3,24,0]
["Solar Tracking","Socal",4,1,0]
["Solar Tracking","Socal",4,2,0]
["Solar Tracking","Socal",4,3,0]
["Solar Tracking","Socal",4,4,0]
["Solar Tracking","Socal",4,5,0]
["Solar Tracking","Socal",4,6,0]
["Solar Tracking","Socal",4,7,3.0629470412307708E-2]
["Solar Tracking","Socal",4,8,0.36534038386428724]
["Solar Tracking","Socal",4,9,0.7157528342712054]
["Solar Tracking","Socal",4,10,0.765626817970537]
["Solar Tracking","Socal",4,11,0.79729919999919985]
["Solar Tracking","Socal",4,12,0.79500217908806414]
["Solar Tracking","Socal",4,13,0.8000660726623271]
["Solar Tracking","Socal",4,14,0.79158654576564669]
["Solar Tracking","Socal",4,15,0.78239093923363179]
["Solar Tracking","Socal",4,16,0.75399857764602474]
["Solar Tracking","Socal",4,17,0.71098859029408623]
["Solar Tracking","Socal",4,18,0.57637541656325608]
["Solar Tracking","Socal",4,19,0.18225391371972116]
["Solar Tracking","Socal",4,20,2.9474305581036666E-3]
["Solar Tracking","Socal",4,21,0]
["Solar Tracking","Socal",4,22,0]
["Solar Tracking","Socal",4,23,0]
["Solar Tracking","Socal",4,24,0]
["Solar Tracking","Socal",5,1,0]
["Solar Tracking","Socal",5,2,0]
["Solar Tracking","Socal",5,3,0]
["Solar Tracking","Socal",5,4,0]
["Solar Tracking","Socal",5,5,0]
["Solar Tracking","Socal",5,6,5.7868927302587769E-4]
["Solar Tracking","Socal",5,7,0.14828639633735008]
["Solar Tracking","Socal",5,8,0.54762166611784857]
["Solar Tracking","Socal",5,9,0.75220831947935629]
["Solar Tracking","Socal",5,10,0.814644019019238]
["Solar Tracking","Socal",5,11,0.84131514647009864]
["Solar Tracking","Socal",5,12,0.84846443570560215]
["Solar Tracking","Socal",5,13,0.851276249893818]
["Solar Tracking","Socal",5,14,0.84764236389037706]
["Solar Tracking","Socal",5,15,0.83328959068284136]
["Solar Tracking","Socal",5,16,0.81315439357005381]
["Solar Tracking","Socal",5,17,0.77539488738127615]
["Solar Tracking","Socal",5,18,0.68007457313535613]
["Solar Tracking","Socal",5,19,0.32830873316158565]
["Solar Tracking","Socal",5,20,2.602292800778289E-2]
["Solar Tracking","Socal",5,21,0]
["Solar Tracking","Socal",5,22,0]
["Solar Tracking","Socal",5,23,0]
["Solar Tracking","Socal",5,24,0]
["Solar Tracking","Socal",6,1,0]
["Solar Tracking","Socal",6,2,0]
["Solar Tracking","Socal",6,3,0]
["Solar Tracking","Socal",6,4,0]
["Solar Tracking","Socal",6,5,0]
["Solar Tracking","Socal",6,6,2.3942296035279992E-3]
["Solar Tracking","Socal",6,7,0.18213625061811606]
["Solar Tracking","Socal",6,8,0.5564026011366513]
["Solar Tracking","Socal",6,9,0.74302409648464562]
["Solar Tracking","Socal",6,10,0.80737908352955412]
["Solar Tracking","Socal",6,11,0.84444198633429124]
["Solar Tracking","Socal",6,12,0.8605901180417701]
["Solar Tracking","Socal",6,13,0.85500241974147861]
["Solar Tracking","Socal",6,14,0.85517267430955113]
["Solar Tracking","Socal",6,15,0.84188888867299549]
["Solar Tracking","Socal",6,16,0.81949968048400124]
["Solar Tracking","Socal",6,17,0.78545587336850387]
["Solar Tracking","Socal",6,18,0.70947198137463152]
["Solar Tracking","Socal",6,19,0.42443047428957364]
["Solar Tracking","Socal",6,20,6.8897941329551265E-2]
["Solar Tracking","Socal",6,21,3.3729074635822969E-5]
["Solar Tracking","Socal",6,22,0]
["Solar Tracking","Socal",6,23,0]
["Solar Tracking","Socal",6,24,0]
["Solar Tracking","Socal",7,1,0]
["Solar Tracking","Socal",7,2,0]
["Solar Tracking","Socal",7,3,0]
["Solar Tracking","Socal",7,4,0]
["Solar Tracking","Socal",7,5,0]
["Solar Tracking","Socal",7,6,4.8193361246208658E-5]
["Solar Tracking","Socal",7,7,8.0775588175740223E-2]
["Solar Tracking","Socal",7,8,0.42764768362941752]
["Solar Tracking","Socal",7,9,0.6854719515523412]
["Solar Tracking","Socal",7,10,0.78817156910670072]
["Solar Tracking","Socal",7,11,0.83020108976232942]
["Solar Tracking","Socal",7,12,0.84646234679511134]
["Solar Tracking","Socal",7,13,0.83866049072799143]
["Solar Tracking","Socal",7,14,0.82888864419393471]
["Solar Tracking","Socal",7,15,0.82170224502240019]
["Solar Tracking","Socal",7,16,0.80187723171870851]
["Solar Tracking","Socal",7,17,0.76084704728380881]
["Solar Tracking","Socal",7,18,0.65797433982239295]
["Solar Tracking","Socal",7,19,0.37729877379339621]
["Solar Tracking","Socal",7,20,5.6431579684739684E-2]
["Solar Tracking","Socal",7,21,1.3632573314456335E-5]
["Solar Tracking","Socal",7,22,0]
["Solar Tracking","Socal",7,23,0]
["Solar Tracking","Socal",7,24,0]
["Solar Tracking","Socal",8,1,0]
["Solar Tracking","Socal",8,2,0]
["Solar Tracking","Socal",8,3,0]
["Solar Tracking","Socal",8,4,0]
["Solar Tracking","Socal",8,5,0]
["Solar Tracking","Socal",8,6,0]
["Solar Tracking","Socal",8,7,3.0964674246504599E-2]
["Solar Tracking","Socal",8,8,0.34253487573328056]
["Solar Tracking","Socal",8,9,0.67290563299250372]
["Solar Tracking","Socal",8,10,0.78832921877789386]
["Solar Tracking","Socal",8,11,0.83054286478814821]
["Solar Tracking","Socal",8,12,0.85150978446533387]
["Solar Tracking","Socal",8,13,0.85453156224706006]
["Solar Tracking","Socal",8,14,0.83535488873686703]
["Solar Tracking","Socal",8,15,0.79423541593579972]
["Solar Tracking","Socal",8,16,0.77582898018026591]
["Solar Tracking","Socal",8,17,0.71304482365743049]
["Solar Tracking","Socal",8,18,0.56792504353449635]
["Solar Tracking","Socal",8,19,0.20301135153267935]
["Solar Tracking","Socal",8,20,5.5692522330099865E-3]
["Solar Tracking","Socal",8,21,0]
["Solar Tracking","Socal",8,22,0]
["Solar Tracking","Socal",8,23,0]
["Solar Tracking","Socal",8,24,0]
["Solar Tracking","Socal",9,1,0]
["Solar Tracking","Socal",9,2,0]
["Solar Tracking","Socal",9,3,0]
["Solar Tracking","Socal",9,4,0]
["Solar Tracking","Socal",9,5,0]
["Solar Tracking","Socal",9,6,0]
["Solar Tracking","Socal",9,7,4.9352760752721762E-3]
["Solar Tracking","Socal",9,8,0.22844117996153598]
["Solar Tracking","Socal",9,9,0.58478742052973132]
["Solar Tracking","Socal",9,10,0.7203840198342526]
["Solar Tracking","Socal",9,11,0.77179718115018625]
["Solar Tracking","Socal",9,12,0.78594590435169742]
["Solar Tracking","Socal",9,13,0.79900953868556912]
["Solar Tracking","Socal",9,14,0.78428374151124491]
["Solar Tracking","Socal",9,15,0.76207255718458278]
["Solar Tracking","Socal",9,16,0.71276307075824652]
["Solar Tracking","Socal",9,17,0.6460841881144983]
["Solar Tracking","Socal",9,18,0.34295964924614014]
["Solar Tracking","Socal",9,19,3.0451362505652384E-2]
["Solar Tracking","Socal",9,20,1.1527754822319176E-7]
["Solar Tracking","Socal",9,21,0]
["Solar Tracking","Socal",9,22,0]
["Solar Tracking","Socal",9,23,0]
["Solar Tracking","Socal",9,24,0]
["Solar Tracking","Socal",10,1,0]
["Solar Tracking","Socal",10,2,0]
["Solar Tracking","Socal",10,3,0]
["Solar Tracking","Socal",10,4,0]
["Solar Tracking","Socal",10,5,0]
["Solar Tracking","Socal",10,6,0]
["Solar Tracking","Socal",10,7,4.0102544932998095E-5]
["Solar Tracking","Socal",10,8,9.9952289070932537E-2]
["Solar Tracking","Socal",10,9,0.493380324512178]
["Solar Tracking","Socal",10,10,0.65943493254901431]
["Solar Tracking","Socal",10,11,0.6937335493040695]
["Solar Tracking","Socal",10,12,0.70368374233444364]
["Solar Tracking","Socal",10,13,0.70202328621344823]
["Solar Tracking","Socal",10,14,0.69517299337862537]
["Solar Tracking","Socal",10,15,0.70564582212204852]
["Solar Tracking","Socal",10,16,0.65998751429639702]
["Solar Tracking","Socal",10,17,0.49767592473749434]
["Solar Tracking","Socal",10,18,0.10839985201101611]
["Solar Tracking","Socal",10,19,6.7424431312892869E-5]
["Solar Tracking","Socal",10,20,0]
["Solar Tracking","Socal",10,21,0]
["Solar Tracking","Socal",10,22,0]
["Solar Tracking","Socal",10,23,0]
["Solar Tracking","Socal",10,24,0]
["Solar Tracking","Socal",11,1,0]
["Solar Tracking","Socal",11,2,0]
["Solar Tracking","Socal",11,3,0]
["Solar Tracking","Socal",11,4,0]
["Solar Tracking","Socal",11,5,0]
["Solar Tracking","Socal",11,6,0]
["Solar Tracking","Socal",11,7,1.5715034957496002E-2]
["Solar Tracking","Socal",11,8,0.27960601426531217]
["Solar Tracking","Socal",11,9,0.58447722814050174]
["Solar Tracking","Socal",11,10,0.65643112553897309]
["Solar Tracking","Socal",11,11,0.64373764988918269]
["Solar Tracking","Socal",11,12,0.62556638632101791]
["Solar Tracking","Socal",11,13,0.63572840764111982]
["Solar Tracking","Socal",11,14,0.63204551669855991]
["Solar Tracking","Socal",11,15,0.5813933000281909]
["Solar Tracking","Socal",11,16,0.34148355909006639]
["Solar Tracking","Socal",11,17,3.1696910004051254E-2]
["Solar Tracking","Socal",11,18,5.4153972085151131E-9]
["Solar Tracking","Socal",11,19,0]
["Solar Tracking","Socal",11,20,0]
["Solar Tracking","Socal",11,21,0]
["Solar Tracking","Socal",11,22,0]
["Solar Tracking","Socal",11,23,0]
["Solar Tracking","Socal",11,24,0]
["Solar Tracking","Socal",12,1,0]
["Solar Tracking","Socal",12,2,0]
["Solar Tracking","Socal",12,3,0]
["Solar Tracking","Socal",12,4,0]
["Solar Tracking","Socal",12,5,0]
["Solar Tracking","Socal",12,6,0]
["Solar Tracking","Socal",12,7,1.0778431142612721E-3]
["Solar Tracking","Socal",12,8,0.13226251185580623]
["Solar Tracking","Socal",12,9,0.41668762229554335]
["Solar Tracking","Socal",12,10,0.52225839785429462]
["Solar Tracking","Socal",12,11,0.51478632716460571]
["Solar Tracking","Socal",12,12,0.49521226861058021]
["Solar Tracking","Socal",12,13,0.51547038916214671]
["Solar Tracking","Socal",12,14,0.50734433779199006]
["Solar Tracking","Socal",12,15,0.46742800852205807]
["Solar Tracking","Socal",12,16,0.25539708441100578]
["Solar Tracking","Socal",12,17,2.1011080565261984E-2]
["Solar Tracking","Socal",12,18,0]
["Solar Tracking","Socal",12,19,0]
["Solar Tracking","Socal",12,20,0]
["Solar Tracking","Socal",12,21,0]
["Solar Tracking","Socal",12,22,0]
["Solar Tracking","Socal",12,23,0]
["Solar Tracking","Socal",12,24,0]
["Solar Thermal","Socal",1,1,0]
["Solar Thermal","Socal",1,2,0]
["Solar Thermal","Socal",1,3,0]
["Solar Thermal","Socal",1,4,0]
["Solar Thermal","Socal",1,5,0]
["Solar Thermal","Socal",1,6,0]
["Solar Thermal","Socal",1,7,0]
["Solar Thermal","Socal",1,8,0]
["Solar Thermal","Socal",1,9,2.1761642006775623E-2]
["Solar Thermal","Socal",1,10,0.16724232490212498]
["Solar Thermal","Socal",1,11,0.23282823612690434]
["Solar Thermal","Socal",1,12,0.2891422663939256]
["Solar Thermal","Socal",1,13,0.2659617858728946]
["Solar Thermal","Socal",1,14,0.22704141133241668]
["Solar Thermal","Socal",1,15,0.23703996505048849]
["Solar Thermal","Socal",1,16,0.19114567835708821]
["Solar Thermal","Socal",1,17,5.6771572595012983E-2]
["Solar Thermal","Socal",1,18,0]
["Solar Thermal","Socal",1,19,0]
["Solar Thermal","Socal",1,20,0]
["Solar Thermal","Socal",1,21,0]
["Solar Thermal","Socal",1,22,0]
["Solar Thermal","Socal",1,23,0]
["Solar Thermal","Socal",1,24,0]
["Solar Thermal","Socal",2,1,0]
["Solar Thermal","Socal",2,2,0]
["Solar Thermal","Socal",2,3,0]
["Solar Thermal","Socal",2,4,0]
["Solar Thermal","Socal",2,5,0]
["Solar Thermal","Socal",2,6,0]
["Solar Thermal","Socal",2,7,0]
["Solar Thermal","Socal",2,8,1.0777580892846199E-3]
["Solar Thermal","Socal",2,9,0.13866905039594901]
["Solar Thermal","Socal",2,10,0.35390514955200608]
["Solar Thermal","Socal",2,11,0.38670246512452289]
["Solar Thermal","Socal",2,12,0.36377217654151089]
["Solar Thermal","Socal",2,13,0.32968441296416978]
["Solar Thermal","Socal",2,14,0.32779249323612536]
["Solar Thermal","Socal",2,15,0.34974010655400284]
["Solar Thermal","Socal",2,16,0.33440860053352267]
["Solar Thermal","Socal",2,17,0.18741691279877523]
["Solar Thermal","Socal",2,18,4.0754286100240456E-2]
["Solar Thermal","Socal",2,19,0]
["Solar Thermal","Socal",2,20,0]
["Solar Thermal","Socal",2,21,0]
["Solar Thermal","Socal",2,22,0]
["Solar Thermal","Socal",2,23,0]
["Solar Thermal","Socal",2,24,0]
["Solar Thermal","Socal",3,1,0]
["Solar Thermal","Socal",3,2,0]
["Solar Thermal","Socal",3,3,0]
["Solar Thermal","Socal",3,4,0]
["Solar Thermal","Socal",3,5,0]
["Solar Thermal","Socal",3,6,0]
["Solar Thermal","Socal",3,7,0]
["Solar Thermal","Socal",3,8,0]
["Solar Thermal","Socal",3,9,0.14567525323374156]
["Solar Thermal","Socal",3,10,0.4411615682754999]
["Solar Thermal","Socal",3,11,0.49793060421415752]
["Solar Thermal","Socal",3,12,0.49052165259175473]
["Solar Thermal","Socal",3,13,0.49802868952636936]
["Solar Thermal","Socal",3,14,0.53819093694705356]
["Solar Thermal","Socal",3,15,0.52277375957234684]
["Solar Thermal","Socal",3,16,0.49056159440520553]
["Solar Thermal","Socal",3,17,0.40336421406460721]
["Solar Thermal","Socal",3,18,0.16505995697187106]
["Solar Thermal","Socal",3,19,7.3699629306679974E-3]
["Solar Thermal","Socal",3,20,0]
["Solar Thermal","Socal",3,21,0]
["Solar Thermal","Socal",3,22,0]
["Solar Thermal","Socal",3,23,0]
["Solar Thermal","Socal",3,24,0]
["Solar Thermal","Socal",4,1,0]
["Solar Thermal","Socal",4,2,0]
["Solar Thermal","Socal",4,3,0]
["Solar Thermal","Socal",4,4,0]
["Solar Thermal","Socal",4,5,0]
["Solar Thermal","Socal",4,6,0]
["Solar Thermal","Socal",4,7,0]
["Solar Thermal","Socal",4,8,3.077301786882675E-2]
["Solar Thermal","Socal",4,9,0.38819327494055383]
["Solar Thermal","Socal",4,10,0.6150861225493337]
["Solar Thermal","Socal",4,11,0.6916754768811062]
["Solar Thermal","Socal",4,12,0.6945384818216932]
["Solar Thermal","Socal",4,13,0.69935373695056979]
["Solar Thermal","Socal",4,14,0.68118032758754221]
["Solar Thermal","Socal",4,15,0.62731806682860836]
["Solar Thermal","Socal",4,16,0.56365530209668246]
["Solar Thermal","Socal",4,17,0.51718778534736631]
["Solar Thermal","Socal",4,18,0.44846253866835689]
["Solar Thermal","Socal",4,19,0.20354881765669788]
["Solar Thermal","Socal",4,20,2.2588013072170104E-2]
["Solar Thermal","Socal",4,21,0]
["Solar Thermal","Socal",4,22,0]
["Solar Thermal","Socal",4,23,0]
["Solar Thermal","Socal",4,24,0]
["Solar Thermal","Socal",5,1,0]
["Solar Thermal","Socal",5,2,0]
["Solar Thermal","Socal",5,3,0]
["Solar Thermal","Socal",5,4,0]
["Solar Thermal","Socal",5,5,0]
["Solar Thermal","Socal",5,6,0]
["Solar Thermal","Socal",5,7,1.0913538553151532E-2]
["Solar Thermal","Socal",5,8,0.2500364532720899]
["Solar Thermal","Socal",5,9,0.67169716455798834]
["Solar Thermal","Socal",5,10,0.81622142094588146]
["Solar Thermal","Socal",5,11,0.8390352883455463]
["Solar Thermal","Socal",5,12,0.83765421911007942]
["Solar Thermal","Socal",5,13,0.82410274547224249]
["Solar Thermal","Socal",5,14,0.80736816399460987]
["Solar Thermal","Socal",5,15,0.78726065593221772]
["Solar Thermal","Socal",5,16,0.72745515852103571]
["Solar Thermal","Socal",5,17,0.65765082069273784]
["Solar Thermal","Socal",5,18,0.55497737058395402]
["Solar Thermal","Socal",5,19,0.36270736263205117]
["Solar Thermal","Socal",5,20,8.0975033002241834E-2]
["Solar Thermal","Socal",5,21,0]
["Solar Thermal","Socal",5,22,0]
["Solar Thermal","Socal",5,23,0]
["Solar Thermal","Socal",5,24,0]
["Solar Thermal","Socal",6,1,0]
["Solar Thermal","Socal",6,2,0]
["Solar Thermal","Socal",6,3,0]
["Solar Thermal","Socal",6,4,0]
["Solar Thermal","Socal",6,5,0]
["Solar Thermal","Socal",6,6,0]
["Solar Thermal","Socal",6,7,2.8102046221995566E-2]
["Solar Thermal","Socal",6,8,0.31925972439361677]
["Solar Thermal","Socal",6,9,0.68826122292748804]
["Solar Thermal","Socal",6,10,0.77602099815552872]
["Solar Thermal","Socal",6,11,0.79972680015970887]
["Solar Thermal","Socal",6,12,0.79056314634035851]
["Solar Thermal","Socal",6,13,0.78549468222626861]
["Solar Thermal","Socal",6,14,0.76979090741921419]
["Solar Thermal","Socal",6,15,0.73141123791502116]
["Solar Thermal","Socal",6,16,0.69900231249315214]
["Solar Thermal","Socal",6,17,0.66780687901631552]
["Solar Thermal","Socal",6,18,0.59161332936995792]
["Solar Thermal","Socal",6,19,0.41235806071966741]
["Solar Thermal","Socal",6,20,0.14421874596574083]
["Solar Thermal","Socal",6,21,2.6280268665102241E-3]
["Solar Thermal","Socal",6,22,0]
["Solar Thermal","Socal",6,23,0]
["Solar Thermal","Socal",6,24,0]
["Solar Thermal","Socal",7,1,0]
["Solar Thermal","Socal",7,2,0]
["Solar Thermal","Socal",7,3,0]
["Solar Thermal","Socal",7,4,0]
["Solar Thermal","Socal",7,5,0]
["Solar Thermal","Socal",7,6,0]
["Solar Thermal","Socal",7,7,0]
["Solar Thermal","Socal",7,8,5.5601976811140971E-2]
["Solar Thermal","Socal",7,9,0.3099601940771578]
["Solar Thermal","Socal",7,10,0.50188705094840169]
["Solar Thermal","Socal",7,11,0.56992597095410269]
["Solar Thermal","Socal",7,12,0.58882540435408737]
["Solar Thermal","Socal",7,13,0.59868673666775274]
["Solar Thermal","Socal",7,14,0.57095694981256284]
["Solar Thermal","Socal",7,15,0.55623973521994752]
["Solar Thermal","Socal",7,16,0.52218122328508909]
["Solar Thermal","Socal",7,17,0.50356258906402807]
["Solar Thermal","Socal",7,18,0.41047252235743392]
["Solar Thermal","Socal",7,19,0.30204131858116251]
["Solar Thermal","Socal",7,20,9.628837661577723E-2]
["Solar Thermal","Socal",7,21,0]
["Solar Thermal","Socal",7,22,0]
["Solar Thermal","Socal",7,23,0]
["Solar Thermal","Socal",7,24,0]
["Solar Thermal","Socal",8,1,0]
["Solar Thermal","Socal",8,2,0]
["Solar Thermal","Socal",8,3,0]
["Solar Thermal","Socal",8,4,0]
["Solar Thermal","Socal",8,5,0]
["Solar Thermal","Socal",8,6,0]
["Solar Thermal","Socal",8,7,0]
["Solar Thermal","Socal",8,8,2.8332995151608212E-2]
["Solar Thermal","Socal",8,9,0.35026522003260546]
["Solar Thermal","Socal",8,10,0.5842601467636227]
["Solar Thermal","Socal",8,11,0.69912733562988083]
["Solar Thermal","Socal",8,12,0.72640491708869392]
["Solar Thermal","Socal",8,13,0.71708407462620982]
["Solar Thermal","Socal",8,14,0.61655085456157621]
["Solar Thermal","Socal",8,15,0.58324422266129738]
["Solar Thermal","Socal",8,16,0.54813192784408538]
["Solar Thermal","Socal",8,17,0.51699563837494145]
["Solar Thermal","Socal",8,18,0.4339834086239705]
["Solar Thermal","Socal",8,19,0.2622560887536467]
["Solar Thermal","Socal",8,20,4.1377695996105128E-2]
["Solar Thermal","Socal",8,21,0]
["Solar Thermal","Socal",8,22,0]
["Solar Thermal","Socal",8,23,0]
["Solar Thermal","Socal",8,24,0]
["Solar Thermal","Socal",9,1,0]
["Solar Thermal","Socal",9,2,0]
["Solar Thermal","Socal",9,3,0]
["Solar Thermal","Socal",9,4,0]
["Solar Thermal","Socal",9,5,0]
["Solar Thermal","Socal",9,6,0]
["Solar Thermal","Socal",9,7,0]
["Solar Thermal","Socal",9,8,8.3863832845579109E-3]
["Solar Thermal","Socal",9,9,0.28366571519036149]
["Solar Thermal","Socal",9,10,0.58090934142864803]
["Solar Thermal","Socal",9,11,0.68880824480678216]
["Solar Thermal","Socal",9,12,0.69360312111494871]
["Solar Thermal","Socal",9,13,0.68447021031650335]
["Solar Thermal","Socal",9,14,0.65349360956116487]
["Solar Thermal","Socal",9,15,0.61067327811694627]
["Solar Thermal","Socal",9,16,0.58051406672308115]
["Solar Thermal","Socal",9,17,0.54081982967667663]
["Solar Thermal","Socal",9,18,0.40143822005192814]
["Solar Thermal","Socal",9,19,9.7772380768851988E-2]
["Solar Thermal","Socal",9,20,3.5236179815891703E-4]
["Solar Thermal","Socal",9,21,0]
["Solar Thermal","Socal",9,22,0]
["Solar Thermal","Socal",9,23,0]
["Solar Thermal","Socal",9,24,0]
["Solar Thermal","Socal",10,1,0]
["Solar Thermal","Socal",10,2,0]
["Solar Thermal","Socal",10,3,0]
["Solar Thermal","Socal",10,4,0]
["Solar Thermal","Socal",10,5,0]
["Solar Thermal","Socal",10,6,0]
["Solar Thermal","Socal",10,7,0]
["Solar Thermal","Socal",10,8,0]
["Solar Thermal","Socal",10,9,0.14153682452507399]
["Solar Thermal","Socal",10,10,0.53712177393051763]
["Solar Thermal","Socal",10,11,0.66959324487895566]
["Solar Thermal","Socal",10,12,0.6620574816713074]
["Solar Thermal","Socal",10,13,0.65635041080422607]
["Solar Thermal","Socal",10,14,0.64261585170939572]
["Solar Thermal","Socal",10,15,0.65372406506931557]
["Solar Thermal","Socal",10,16,0.62145335898811327]
["Solar Thermal","Socal",10,17,0.50085357664901387]
["Solar Thermal","Socal",10,18,0.21488376409395757]
["Solar Thermal","Socal",10,19,1.5533074423687687E-2]
["Solar Thermal","Socal",10,20,0]
["Solar Thermal","Socal",10,21,0]
["Solar Thermal","Socal",10,22,0]
["Solar Thermal","Socal",10,23,0]
["Solar Thermal","Socal",10,24,0]
["Solar Thermal","Socal",11,1,0]
["Solar Thermal","Socal",11,2,0]
["Solar Thermal","Socal",11,3,0]
["Solar Thermal","Socal",11,4,0]
["Solar Thermal","Socal",11,5,0]
["Solar Thermal","Socal",11,6,0]
["Solar Thermal","Socal",11,7,0]
["Solar Thermal","Socal",11,8,3.6379907207498585E-3]
["Solar Thermal","Socal",11,9,0.18767371109688469]
["Solar Thermal","Socal",11,10,0.47339090511059401]
["Solar Thermal","Socal",11,11,0.53310026994294124]
["Solar Thermal","Socal",11,12,0.52242715119338223]
["Solar Thermal","Socal",11,13,0.50907590615133935]
["Solar Thermal","Socal",11,14,0.50509628374301163]
["Solar Thermal","Socal",11,15,0.46619705663031025]
["Solar Thermal","Socal",11,16,0.31968129153010211]
["Solar Thermal","Socal",11,17,8.3858170468933901E-2]
["Solar Thermal","Socal",11,18,0]
["Solar Thermal","Socal",11,19,0]
["Solar Thermal","Socal",11,20,0]
["Solar Thermal","Socal",11,21,0]
["Solar Thermal","Socal",11,22,0]
["Solar Thermal","Socal",11,23,0]
["Solar Thermal","Socal",11,24,0]
["Solar Thermal","Socal",12,1,0]
["Solar Thermal","Socal",12,2,0]
["Solar Thermal","Socal",12,3,0]
["Solar Thermal","Socal",12,4,0]
["Solar Thermal","Socal",12,5,0]
["Solar Thermal","Socal",12,6,0]
["Solar Thermal","Socal",12,7,0]
["Solar Thermal","Socal",12,8,0]
["Solar Thermal","Socal",12,9,1.2953617175472557E-2]
["Solar Thermal","Socal",12,10,0.10806109039667944]
["Solar Thermal","Socal",12,11,0.17033276729003552]
["Solar Thermal","Socal",12,12,0.18070196497735536]
["Solar Thermal","Socal",12,13,0.1788950777032825]
["Solar Thermal","Socal",12,14,0.18525601345659423]
["Solar Thermal","Socal",12,15,0.18296869041150879]
["Solar Thermal","Socal",12,16,0.13120392818020726]
["Solar Thermal","Socal",12,17,2.9846529902928295E-2]
["Solar Thermal","Socal",12,18,0]
["Solar Thermal","Socal",12,19,0]
["Solar Thermal","Socal",12,20,0]
["Solar Thermal","Socal",12,21,0]
["Solar Thermal","Socal",12,22,0]
["Solar Thermal","Socal",12,23,0]
["Solar Thermal","Socal",12,24,0]
["Wind","Norcal",1,1,5.3085056827508047E-2]
["Wind","Norcal",1,2,5.0638264924133806E-2]
["Wind","Norcal",1,3,4.3876133369858093E-2]
["Wind","Norcal",1,4,4.1397869260019586E-2]
["Wind","Norcal",1,5,4.5511641518202715E-2]
["Wind","Norcal",1,6,4.6890100346191559E-2]
["Wind","Norcal",1,7,4.6313780017991822E-2]
["Wind","Norcal",1,8,4.8841924152803709E-2]
["Wind","Norcal",1,9,4.4704276099371339E-2]
["Wind","Norcal",1,10,3.8276324020288986E-2]
["Wind","Norcal",1,11,4.0005032286970402E-2]
["Wind","Norcal",1,12,4.2397797276122119E-2]
["Wind","Norcal",1,13,3.6477647081987849E-2]
["Wind","Norcal",1,14,3.3496273035701747E-2]
["Wind","Norcal",1,15,2.9986886431384356E-2]
["Wind","Norcal",1,16,2.6133240094131035E-2]
["Wind","Norcal",1,17,2.7127625200472731E-2]
["Wind","Norcal",1,18,3.5703707235980438E-2]
["Wind","Norcal",1,19,4.2380322726084246E-2]
["Wind","Norcal",1,20,4.6584928707288704E-2]
["Wind","Norcal",1,21,4.3306334879574457E-2]
["Wind","Norcal",1,22,4.6222436250110251E-2]
["Wind","Norcal",1,23,5.0484870258676998E-2]
["Wind","Norcal",1,24,5.0801869439478925E-2]
["Wind","Norcal",2,1,0.12078285391787964]
["Wind","Norcal",2,2,0.12802352178903587]
["Wind","Norcal",2,3,0.12090950074166183]
["Wind","Norcal",2,4,0.10205858427187471]
["Wind","Norcal",2,5,9.3501723912593565E-2]
["Wind","Norcal",2,6,9.5406471594732131E-2]
["Wind","Norcal",2,7,9.5423224232634107E-2]
["Wind","Norcal",2,8,0.10171034737850719]
["Wind","Norcal",2,9,8.1451613842600454E-2]
["Wind","Norcal",2,10,7.6552214003399607E-2]
["Wind","Norcal",2,11,8.0939814332090659E-2]
["Wind","Norcal",2,12,7.224873125390513E-2]
["Wind","Norcal",2,13,6.7395704236953347E-2]
["Wind","Norcal",2,14,6.5373109191371473E-2]
["Wind","Norcal",2,15,6.0287185654583138E-2]
["Wind","Norcal",2,16,6.2923570756411876E-2]
["Wind","Norcal",2,17,6.0339517593574303E-2]
["Wind","Norcal",2,18,6.8975462586074912E-2]
["Wind","Norcal",2,19,7.3287335436227216E-2]
["Wind","Norcal",2,20,7.6339479499387547E-2]
["Wind","Norcal",2,21,8.4367130406493809E-2]
["Wind","Norcal",2,22,0.10548742596098734]
["Wind","Norcal",2,23,0.11296188965731123]
["Wind","Norcal",2,24,0.12270264058358046]
["Wind","Norcal",3,1,0.13902621559706832]
["Wind","Norcal",3,2,0.13180120408257207]
["Wind","Norcal",3,3,0.1190938049174526]
["Wind","Norcal",3,4,0.11244361175327675]
["Wind","Norcal",3,5,0.10020706330125168]
["Wind","Norcal",3,6,7.9014560790776053E-2]
["Wind","Norcal",3,7,7.6058435718060216E-2]
["Wind","Norcal",3,8,7.0394934273860191E-2]
["Wind","Norcal",3,9,6.9954642193430019E-2]
["Wind","Norcal",3,10,5.8129860896841155E-2]
["Wind","Norcal",3,11,4.9074700065340045E-2]
["Wind","Norcal",3,12,4.9711935435430468E-2]
["Wind","Norcal",3,13,4.8469476859845546E-2]
["Wind","Norcal",3,14,5.2154933373963687E-2]
["Wind","Norcal",3,15,5.3802873119345881E-2]
["Wind","Norcal",3,16,5.4361443400644173E-2]
["Wind","Norcal",3,17,6.3067662564612034E-2]
["Wind","Norcal",3,18,7.1316843565313093E-2]
["Wind","Norcal",3,19,9.8598682007620078E-2]
["Wind","Norcal",3,20,0.13321708563589188]
["Wind","Norcal",3,21,0.15995238046718788]
["Wind","Norcal",3,22,0.15210416202870344]
["Wind","Norcal",3,23,0.14993042980000873]
["Wind","Norcal",3,24,0.14014879246558648]
["Wind","Norcal",4,1,0.37722584999089109]
["Wind","Norcal",4,2,0.34358749657063403]
["Wind","Norcal",4,3,0.33828940011380543]
["Wind","Norcal",4,4,0.28029323487147134]
["Wind","Norcal",4,5,0.24832308211852494]
["Wind","Norcal",4,6,0.2176876946988342]
["Wind","Norcal",4,7,0.20207018267712579]
["Wind","Norcal",4,8,0.15944222055601501]
["Wind","Norcal",4,9,0.11586422800252381]
["Wind","Norcal",4,10,0.12226544983185822]
["Wind","Norcal",4,11,0.10801241695809255]
["Wind","Norcal",4,12,8.5695543195671089E-2]
["Wind","Norcal",4,13,8.7927858379940882E-2]
["Wind","Norcal",4,14,0.10157537643432236]
["Wind","Norcal",4,15,0.1196451389829387]
["Wind","Norcal",4,16,0.15914049441214409]
["Wind","Norcal",4,17,0.21313163744072083]
["Wind","Norcal",4,18,0.27236890736135205]
["Wind","Norcal",4,19,0.29075435036041658]
["Wind","Norcal",4,20,0.30563963191179355]
["Wind","Norcal",4,21,0.34203076183815634]
["Wind","Norcal",4,22,0.34876648604306365]
["Wind","Norcal",4,23,0.37159625901562265]
["Wind","Norcal",4,24,0.3867603946400191]
["Wind","Norcal",5,1,0.48661802973794549]
["Wind","Norcal",5,2,0.46140034327478868]
["Wind","Norcal",5,3,0.45887742973004836]
["Wind","Norcal",5,4,0.45129308371361837]
["Wind","Norcal",5,5,0.38580323908109593]
["Wind","Norcal",5,6,0.3308597563586087]
["Wind","Norcal",5,7,0.30381127849836959]
["Wind","Norcal",5,8,0.25097625202004636]
["Wind","Norcal",5,9,0.25350413580900072]
["Wind","Norcal",5,10,0.2212558725556516]
["Wind","Norcal",5,11,0.17990318989401027]
["Wind","Norcal",5,12,0.14213534377441395]
["Wind","Norcal",5,13,0.1603398219652305]
["Wind","Norcal",5,14,0.18643839553238653]
["Wind","Norcal",5,15,0.20984490488689245]
["Wind","Norcal",5,16,0.2812535069519333]
["Wind","Norcal",5,17,0.37567159918379345]
["Wind","Norcal",5,18,0.43562775452951841]
["Wind","Norcal",5,19,0.48080625522717479]
["Wind","Norcal",5,20,0.46691880822354609]
["Wind","Norcal",5,21,0.47999381772455502]
["Wind","Norcal",5,22,0.50375563435432802]
["Wind","Norcal",5,23,0.48271364271738204]
["Wind","Norcal",5,24,0.46185293182347847]
["Wind","Norcal",6,1,0.37016565113937744]
["Wind","Norcal",6,2,0.39560081964690241]
["Wind","Norcal",6,3,0.35208282717184525]
["Wind","Norcal",6,4,0.32376257701684458]
["Wind","Norcal",6,5,0.29130397892915788]
["Wind","Norcal",6,6,0.26560167082401087]
["Wind","Norcal",6,7,0.22475118597443114]
["Wind","Norcal",6,8,0.1572219948899336]
["Wind","Norcal",6,9,0.12527318031836718]
["Wind","Norcal",6,10,8.7537733675994253E-2]
["Wind","Norcal",6,11,7.5085138754824976E-2]
["Wind","Norcal",6,12,5.3356264483429693E-2]
["Wind","Norcal",6,13,4.3173400272373111E-2]
["Wind","Norcal",6,14,5.7294037426860178E-2]
["Wind","Norcal",6,15,6.3437079398693863E-2]
["Wind","Norcal",6,16,9.6578682773827182E-2]
["Wind","Norcal",6,17,0.16417693710002637]
["Wind","Norcal",6,18,0.24620022761099392]
["Wind","Norcal",6,19,0.30719815732768729]
["Wind","Norcal",6,20,0.32074070963625295]
["Wind","Norcal",6,21,0.35104426825222035]
["Wind","Norcal",6,22,0.35660895580982743]
["Wind","Norcal",6,23,0.35785209602786011]
["Wind","Norcal",6,24,0.37216847701249378]
["Wind","Norcal",7,1,0.59658667623191719]
["Wind","Norcal",7,2,0.58190143102309122]
["Wind","Norcal",7,3,0.53891619697157234]
["Wind","Norcal",7,4,0.48093265899542498]
["Wind","Norcal",7,5,0.4538724925842712]
["Wind","Norcal",7,6,0.42489248316938028]
["Wind","Norcal",7,7,0.36210834492869021]
["Wind","Norcal",7,8,0.30190083570417009]
["Wind","Norcal",7,9,0.21479541814020731]
["Wind","Norcal",7,10,0.17432849202800113]
["Wind","Norcal",7,11,0.11089347993934073]
["Wind","Norcal",7,12,7.9077866011073111E-2]
["Wind","Norcal",7,13,7.1723093781475761E-2]
["Wind","Norcal",7,14,0.11037687149006356]
["Wind","Norcal",7,15,0.13048003649944387]
["Wind","Norcal",7,16,0.19069156576015206]
["Wind","Norcal",7,17,0.31224433957041142]
["Wind","Norcal",7,18,0.39383250123361124]
["Wind","Norcal",7,19,0.41677073365753259]
["Wind","Norcal",7,20,0.43604908498729783]
["Wind","Norcal",7,21,0.49982088086051923]
["Wind","Norcal",7,22,0.51794104822907028]
["Wind","Norcal",7,23,0.56866207453090489]
["Wind","Norcal",7,24,0.5982739314219121]
["Wind","Norcal",8,1,0.48750051838438291]
["Wind","Norcal",8,2,0.46609300430758988]
["Wind","Norcal",8,3,0.43802468616404366]
["Wind","Norcal",8,4,0.38838768171505939]
["Wind","Norcal",8,5,0.33653773260832853]
["Wind","Norcal",8,6,0.29048631390397511]
["Wind","Norcal",8,7,0.25136780263847314]
["Wind","Norcal",8,8,0.21419001532743978]
["Wind","Norcal",8,9,0.13670672903052622]
["Wind","Norcal",8,10,0.1016782263977236]
["Wind","Norcal",8,11,7.4398834757295501E-2]
["Wind","Norcal",8,12,4.9625555800467673E-2]
["Wind","Norcal",8,13,3.0854417519360192E-2]
["Wind","Norcal",8,14,4.3311841775743883E-2]
["Wind","Norcal",8,15,5.356199593963825E-2]
["Wind","Norcal",8,16,8.293055415630976E-2]
["Wind","Norcal",8,17,0.13649806848394722]
["Wind","Norcal",8,18,0.21509692232088826]
["Wind","Norcal",8,19,0.29101416424002696]
["Wind","Norcal",8,20,0.37850910897214018]
["Wind","Norcal",8,21,0.46129599718827158]
["Wind","Norcal",8,22,0.48670071328774639]
["Wind","Norcal",8,23,0.49321401619701699]
["Wind","Norcal",8,24,0.50234185230266615]
["Wind","Norcal",9,1,0.18399125017240101]
["Wind","Norcal",9,2,0.18103027786921155]
["Wind","Norcal",9,3,0.17062581642965285]
["Wind","Norcal",9,4,0.1590536412152975]
["Wind","Norcal",9,5,0.12223313032689544]
["Wind","Norcal",9,6,9.8365742936700404E-2]
["Wind","Norcal",9,7,9.4843651075090865E-2]
["Wind","Norcal",9,8,7.4153806870675257E-2]
["Wind","Norcal",9,9,5.5234031468289743E-2]
["Wind","Norcal",9,10,3.361383507650878E-2]
["Wind","Norcal",9,11,2.6026139115855679E-2]
["Wind","Norcal",9,12,1.2966139224753334E-2]
["Wind","Norcal",9,13,8.9131119521424045E-3]
["Wind","Norcal",9,14,1.3725884086331552E-2]
["Wind","Norcal",9,15,2.1118541812983237E-2]
["Wind","Norcal",9,16,2.9385828765863778E-2]
["Wind","Norcal",9,17,5.1097029746948436E-2]
["Wind","Norcal",9,18,6.6064161398895926E-2]
["Wind","Norcal",9,19,7.4180053213361088E-2]
["Wind","Norcal",9,20,0.11214709995073896]
["Wind","Norcal",9,21,0.14839879394349681]
["Wind","Norcal",9,22,0.16488339120944964]
["Wind","Norcal",9,23,0.17150528962488526]
["Wind","Norcal",9,24,0.1747275794453983]
["Wind","Norcal",10,1,7.6618976832837124E-2]
["Wind","Norcal",10,2,7.0444264500533815E-2]
["Wind","Norcal",10,3,5.1805669667071792E-2]
["Wind","Norcal",10,4,4.1716704217394207E-2]
["Wind","Norcal",10,5,3.4274916215456613E-2]
["Wind","Norcal",10,6,2.8531198090799199E-2]
["Wind","Norcal",10,7,3.2745277409927387E-2]
["Wind","Norcal",10,8,2.7337795272232693E-2]
["Wind","Norcal",10,9,2.5093835632288453E-2]
["Wind","Norcal",10,10,1.6955622996352546E-2]
["Wind","Norcal",10,11,1.0330791874263168E-2]
["Wind","Norcal",10,12,8.2884188314906806E-3]
["Wind","Norcal",10,13,6.5801865849471914E-3]
["Wind","Norcal",10,14,6.9429689742474265E-3]
["Wind","Norcal",10,15,9.3192805646047927E-3]
["Wind","Norcal",10,16,9.9044503016968294E-3]
["Wind","Norcal",10,17,8.8048374635772437E-3]
["Wind","Norcal",10,18,9.938834136868524E-3]
["Wind","Norcal",10,19,1.7972492103281605E-2]
["Wind","Norcal",10,20,2.4395160814257029E-2]
["Wind","Norcal",10,21,3.5462962591471338E-2]
["Wind","Norcal",10,22,4.2833201776685668E-2]
["Wind","Norcal",10,23,5.5153672329706901E-2]
["Wind","Norcal",10,24,6.3096976918871978E-2]
["Wind","Norcal",11,1,5.7683016329250054E-2]
["Wind","Norcal",11,2,5.0759781303477441E-2]
["Wind","Norcal",11,3,4.6106859631283047E-2]
["Wind","Norcal",11,4,5.4727010739121403E-2]
["Wind","Norcal",11,5,5.0210707802524901E-2]
["Wind","Norcal",11,6,4.9895744854068252E-2]
["Wind","Norcal",11,7,4.7293883849067908E-2]
["Wind","Norcal",11,8,5.1898441961387085E-2]
["Wind","Norcal",11,9,4.297435439954371E-2]
["Wind","Norcal",11,10,3.3407280822018895E-2]
["Wind","Norcal",11,11,2.9661949218577004E-2]
["Wind","Norcal",11,12,2.621381762770271E-2]
["Wind","Norcal",11,13,2.6347228716471504E-2]
["Wind","Norcal",11,14,2.3570755232518802E-2]
["Wind","Norcal",11,15,2.5623099668723372E-2]
["Wind","Norcal",11,16,2.8791859566236911E-2]
["Wind","Norcal",11,17,2.6936859495974037E-2]
["Wind","Norcal",11,18,2.8298918487035918E-2]
["Wind","Norcal",11,19,3.4189357078444241E-2]
["Wind","Norcal",11,20,3.5380312921822248E-2]
["Wind","Norcal",11,21,4.7230252635220418E-2]
["Wind","Norcal",11,22,5.131670908762466E-2]
["Wind","Norcal",11,23,5.8831316241689059E-2]
["Wind","Norcal",11,24,5.8485902504259113E-2]
["Wind","Norcal",12,1,5.4650141353725583E-2]
["Wind","Norcal",12,2,5.454876236861847E-2]
["Wind","Norcal",12,3,5.2535693799390305E-2]
["Wind","Norcal",12,4,4.6632382863547213E-2]
["Wind","Norcal",12,5,5.0768371398258148E-2]
["Wind","Norcal",12,6,5.2292230767035257E-2]
["Wind","Norcal",12,7,4.5613508479625163E-2]
["Wind","Norcal",12,8,5.1955149761481904E-2]
["Wind","Norcal",12,9,4.8811394253826641E-2]
["Wind","Norcal",12,10,3.9990825165361447E-2]
["Wind","Norcal",12,11,3.7885316119125073E-2]
["Wind","Norcal",12,12,3.2054886845114219E-2]
["Wind","Norcal",12,13,3.2672247420338481E-2]
["Wind","Norcal",12,14,3.1719400428269102E-2]
["Wind","Norcal",12,15,3.4025773395026403E-2]
["Wind","Norcal",12,16,3.6044748521811713E-2]
["Wind","Norcal",12,17,3.3370847256997342E-2]
["Wind","Norcal",12,18,3.4194216166276034E-2]
["Wind","Norcal",12,19,4.2829850101829652E-2]
["Wind","Norcal",12,20,5.1490980823976518E-2]
["Wind","Norcal",12,21,5.913770004887052E-2]
["Wind","Norcal",12,22,5.6704206232255305E-2]
["Wind","Norcal",12,23,5.2207294795709652E-2]
["Wind","Norcal",12,24,5.9984837234016861E-2]
["Wind","Socal",1,1,5.2487762542652375E-2]
["Wind","Socal",1,2,5.5575713772126625E-2]
["Wind","Socal",1,3,5.2387007606211906E-2]
["Wind","Socal",1,4,4.9930590498812898E-2]
["Wind","Socal",1,5,5.580982931544342E-2]
["Wind","Socal",1,6,5.4268187554475003E-2]
["Wind","Socal",1,7,5.5668501557034865E-2]
["Wind","Socal",1,8,5.1071634238275751E-2]
["Wind","Socal",1,9,4.4369783629185928E-2]
["Wind","Socal",1,10,5.0336711046517157E-2]
["Wind","Socal",1,11,4.4765312646398984E-2]
["Wind","Socal",1,12,4.9034403173318003E-2]
["Wind","Socal",1,13,5.5065938895259715E-2]
["Wind","Socal",1,14,5.0245067680896122E-2]
["Wind","Socal",1,15,5.5379627474687512E-2]
["Wind","Socal",1,16,5.5245014612695487E-2]
["Wind","Socal",1,17,4.7235141743032942E-2]
["Wind","Socal",1,18,4.5566944565532577E-2]
["Wind","Socal",1,19,5.4514475231448527E-2]
["Wind","Socal",1,20,5.1492876177743681E-2]
["Wind","Socal",1,21,5.0810060332053417E-2]
["Wind","Socal",1,22,5.577387010469631E-2]
["Wind","Socal",1,23,4.8119341887916736E-2]
["Wind","Socal",1,24,5.0790753027897775E-2]
["Wind","Socal",2,1,9.6938362398822947E-2]
["Wind","Socal",2,2,9.2433573402241759E-2]
["Wind","Socal",2,3,0.10602569057875122]
["Wind","Socal",2,4,0.10334176734665435]
["Wind","Socal",2,5,8.7276147435430482E-2]
["Wind","Socal",2,6,9.2511920838720701E-2]
["Wind","Socal",2,7,9.1084593506595146E-2]
["Wind","Socal",2,8,7.4695034378745209E-2]
["Wind","Socal",2,9,7.8071096573629706E-2]
["Wind","Socal",2,10,8.6236872791036812E-2]
["Wind","Socal",2,11,0.10737802164417369]
["Wind","Socal",2,12,0.11123142900474133]
["Wind","Socal",2,13,0.10029108567797869]
["Wind","Socal",2,14,9.2817054736948304E-2]
["Wind","Socal",2,15,0.11848180985154705]
["Wind","Socal",2,16,0.12142780199153083]
["Wind","Socal",2,17,0.1190874926667055]
["Wind","Socal",2,18,0.12447397061280789]
["Wind","Socal",2,19,0.11763144103080346]
["Wind","Socal",2,20,0.12794493848585733]
["Wind","Socal",2,21,0.14685127280612056]
["Wind","Socal",2,22,0.12686652352677272]
["Wind","Socal",2,23,0.11162470941975924]
["Wind","Socal",2,24,0.10981431482890908]
["Wind","Socal",3,1,0.107969977278686]
["Wind","Socal",3,2,0.10139115216273006]
["Wind","Socal",3,3,8.8906380454966336E-2]
["Wind","Socal",3,4,8.8125093834731411E-2]
["Wind","Socal",3,5,8.9902674113158457E-2]
["Wind","Socal",3,6,8.9600147358140272E-2]
["Wind","Socal",3,7,8.9817193770357809E-2]
["Wind","Socal",3,8,7.3878836090796055E-2]
["Wind","Socal",3,9,5.7086777403893361E-2]
["Wind","Socal",3,10,5.6920033230822481E-2]
["Wind","Socal",3,11,5.7915880821479804E-2]
["Wind","Socal",3,12,6.5527894219842009E-2]
["Wind","Socal",3,13,7.9459733542895247E-2]
["Wind","Socal",3,14,8.5775539111573568E-2]
["Wind","Socal",3,15,9.6905400541770825E-2]
["Wind","Socal",3,16,9.4539772922532447E-2]
["Wind","Socal",3,17,0.12664372388608497]
["Wind","Socal",3,18,0.13479931392385025]
["Wind","Socal",3,19,0.12708007673961408]
["Wind","Socal",3,20,0.13664346576423692]
["Wind","Socal",3,21,0.13246543307765718]
["Wind","Socal",3,22,0.13584010390448589]
["Wind","Socal",3,23,0.11202369427900963]
["Wind","Socal",3,24,0.10613571651063532]
["Wind","Socal",4,1,0.3693233113643799]
["Wind","Socal",4,2,0.38303707828539574]
["Wind","Socal",4,3,0.34989239211793638]
["Wind","Socal",4,4,0.31998802306619417]
["Wind","Socal",4,5,0.2992502094897751]
["Wind","Socal",4,6,0.26749308016920986]
["Wind","Socal",4,7,0.22066021166794841]
["Wind","Socal",4,8,0.18204675200492595]
["Wind","Socal",4,9,0.13288775826442639]
["Wind","Socal",4,10,0.11837969235162379]
["Wind","Socal",4,11,0.11749927265955983]
["Wind","Socal",4,12,0.11714225133290358]
["Wind","Socal",4,13,0.11402165673261705]
["Wind","Socal",4,14,0.13305563624549946]
["Wind","Socal",4,15,0.19953310590713225]
["Wind","Socal",4,16,0.27569365841824406]
["Wind","Socal",4,17,0.32767376957158534]
["Wind","Socal",4,18,0.36794657450926582]
["Wind","Socal",4,19,0.39483904268449149]
["Wind","Socal",4,20,0.40348192605230165]
["Wind","Socal",4,21,0.40352957771982773]
["Wind","Socal",4,22,0.40709311403337001]
["Wind","Socal",4,23,0.38805796015194943]
["Wind","Socal",4,24,0.38790404218190727]
["Wind","Socal",5,1,0.43191954726082393]
["Wind","Socal",5,2,0.40938462716502627]
["Wind","Socal",5,3,0.39132819089562298]
["Wind","Socal",5,4,0.39111516817193365]
["Wind","Socal",5,5,0.34447729088548168]
["Wind","Socal",5,6,0.27685482869121647]
["Wind","Socal",5,7,0.21212670312526388]
["Wind","Socal",5,8,0.15953928583723606]
["Wind","Socal",5,9,0.1182561934129273]
["Wind","Socal",5,10,8.821273733207198E-2]
["Wind","Socal",5,11,6.6313804693113737E-2]
["Wind","Socal",5,12,6.3868510840885434E-2]
["Wind","Socal",5,13,5.4758639783372746E-2]
["Wind","Socal",5,14,7.5902283028611933E-2]
["Wind","Socal",5,15,0.12626255013496721]
["Wind","Socal",5,16,0.2039125716092397]
["Wind","Socal",5,17,0.31801649224410206]
["Wind","Socal",5,18,0.38070052977620988]
["Wind","Socal",5,19,0.43004600023908762]
["Wind","Socal",5,20,0.41465048841805835]
["Wind","Socal",5,21,0.41896978609536317]
["Wind","Socal",5,22,0.44250046757652034]
["Wind","Socal",5,23,0.43607753311696679]
["Wind","Socal",5,24,0.44557153864429094]
["Wind","Socal",6,1,0.44436716288538802]
["Wind","Socal",6,2,0.43374974457826559]
["Wind","Socal",6,3,0.40342756028754495]
["Wind","Socal",6,4,0.36835907680605284]
["Wind","Socal",6,5,0.33625190399459115]
["Wind","Socal",6,6,0.27143974970364082]
["Wind","Socal",6,7,0.21231328120849921]
["Wind","Socal",6,8,0.15595079016119165]
["Wind","Socal",6,9,9.5805731690762772E-2]
["Wind","Socal",6,10,6.9391583665745105E-2]
["Wind","Socal",6,11,4.9763294936317037E-2]
["Wind","Socal",6,12,5.7965261137581194E-2]
["Wind","Socal",6,13,6.2721192680943894E-2]
["Wind","Socal",6,14,7.371656028963787E-2]
["Wind","Socal",6,15,0.12111264727268096]
["Wind","Socal",6,16,0.19359520883506709]
["Wind","Socal",6,17,0.27940628219276609]
["Wind","Socal",6,18,0.33004473818394908]
["Wind","Socal",6,19,0.37913553380540038]
["Wind","Socal",6,20,0.42504317345850923]
["Wind","Socal",6,21,0.46417663685828359]
["Wind","Socal",6,22,0.46263563632685295]
["Wind","Socal",6,23,0.45715381827572682]
["Wind","Socal",6,24,0.46056413050144895]
["Wind","Socal",7,1,0.41839567580172504]
["Wind","Socal",7,2,0.39310248205397053]
["Wind","Socal",7,3,0.37070730825813464]
["Wind","Socal",7,4,0.3265131200621183]
["Wind","Socal",7,5,0.27057230286635214]
["Wind","Socal",7,6,0.23260129473585553]
["Wind","Socal",7,7,0.1728883774350784]
["Wind","Socal",7,8,0.11172120206769608]
["Wind","Socal",7,9,5.690897621941686E-2]
["Wind","Socal",7,10,3.7979929065659189E-2]
["Wind","Socal",7,11,3.2483364972758465E-2]
["Wind","Socal",7,12,3.8361943138088536E-2]
["Wind","Socal",7,13,5.1066238197175429E-2]
["Wind","Socal",7,14,7.4847646727616332E-2]
["Wind","Socal",7,15,0.1223179608367148]
["Wind","Socal",7,16,0.18239909550378824]
["Wind","Socal",7,17,0.26216377542448477]
["Wind","Socal",7,18,0.33322416623812362]
["Wind","Socal",7,19,0.38514171465066727]
["Wind","Socal",7,20,0.42040121350468274]
["Wind","Socal",7,21,0.4550393553095487]
["Wind","Socal",7,22,0.46619640608699109]
["Wind","Socal",7,23,0.45153302471159296]
["Wind","Socal",7,24,0.43537216495179187]
["Wind","Socal",8,1,0.3745530066582835]
["Wind","Socal",8,2,0.36318224096364243]
["Wind","Socal",8,3,0.33327857505811265]
["Wind","Socal",8,4,0.28490523253791206]
["Wind","Socal",8,5,0.22954919430788195]
["Wind","Socal",8,6,0.20012848696761176]
["Wind","Socal",8,7,0.14721765022086294]
["Wind","Socal",8,8,0.10615699938042658]
["Wind","Socal",8,9,6.5159073781236213E-2]
["Wind","Socal",8,10,4.4621352606554872E-2]
["Wind","Socal",8,11,3.4951188855407329E-2]
["Wind","Socal",8,12,3.8831545319138711E-2]
["Wind","Socal",8,13,5.2560264103768774E-2]
["Wind","Socal",8,14,7.4029791093811331E-2]
["Wind","Socal",8,15,0.11373240301076316]
["Wind","Socal",8,16,0.16589549939615217]
["Wind","Socal",8,17,0.22758902939163936]
["Wind","Socal",8,18,0.29180572387452508]
["Wind","Socal",8,19,0.32876578704044451]
["Wind","Socal",8,20,0.39863355691193342]
["Wind","Socal",8,21,0.42270369488470527]
["Wind","Socal",8,22,0.42129439482368547]
["Wind","Socal",8,23,0.40755369839465005]
["Wind","Socal",8,24,0.38869284902510481]
["Wind","Socal",9,1,0.18895678526413723]
["Wind","Socal",9,2,0.17416779003230606]
["Wind","Socal",9,3,0.15781095016883628]
["Wind","Socal",9,4,0.12287917455744535]
["Wind","Socal",9,5,0.10113754014810196]
["Wind","Socal",9,6,7.3183817138248619E-2]
["Wind","Socal",9,7,5.8720926992473742E-2]
["Wind","Socal",9,8,4.0562935999579948E-2]
["Wind","Socal",9,9,3.3806928584782694E-2]
["Wind","Socal",9,10,3.3950127709779176E-2]
["Wind","Socal",9,11,3.8939233186384058E-2]
["Wind","Socal",9,12,5.1813758707722216E-2]
["Wind","Socal",9,13,6.0166227508895671E-2]
["Wind","Socal",9,14,7.146700871084459E-2]
["Wind","Socal",9,15,8.8735981351032375E-2]
["Wind","Socal",9,16,0.10957506912162265]
["Wind","Socal",9,17,0.12392460657665855]
["Wind","Socal",9,18,0.16345276833565359]
["Wind","Socal",9,19,0.2000684663298935]
["Wind","Socal",9,20,0.24013456602561975]
["Wind","Socal",9,21,0.24032228929384261]
["Wind","Socal",9,22,0.2399566305238878]
["Wind","Socal",9,23,0.22550666218208917]
["Wind","Socal",9,24,0.20614500848309714]
["Wind","Socal",10,1,9.8489242058259568E-2]
["Wind","Socal",10,2,9.1295958482916537E-2]
["Wind","Socal",10,3,9.257166689026923E-2]
["Wind","Socal",10,4,9.1115366453072347E-2]
["Wind","Socal",10,5,8.3495144702011692E-2]
["Wind","Socal",10,6,6.8662708511435119E-2]
["Wind","Socal",10,7,5.5401864779414771E-2]
["Wind","Socal",10,8,4.5878522968233408E-2]
["Wind","Socal",10,9,3.0639906949509636E-2]
["Wind","Socal",10,10,2.750001414737329E-2]
["Wind","Socal",10,11,2.9416292568417497E-2]
["Wind","Socal",10,12,3.6723155254387428E-2]
["Wind","Socal",10,13,4.3326857515442352E-2]
["Wind","Socal",10,14,4.3422077699096201E-2]
["Wind","Socal",10,15,4.4097526899328172E-2]
["Wind","Socal",10,16,5.0906004644850213E-2]
["Wind","Socal",10,17,6.4941578289782684E-2]
["Wind","Socal",10,18,7.7583236127162891E-2]
["Wind","Socal",10,19,9.3606026335565931E-2]
["Wind","Socal",10,20,0.10779735970822349]
["Wind","Socal",10,21,0.11902746153557175]
["Wind","Socal",10,22,0.12110455152300199]
["Wind","Socal",10,23,0.1119471795457077]
["Wind","Socal",10,24,9.6321280904786685E-2]
["Wind","Socal",11,1,4.4099813464274988E-2]
["Wind","Socal",11,2,3.905020090465873E-2]
["Wind","Socal",11,3,3.9961115305993014E-2]
["Wind","Socal",11,4,4.0593072655849542E-2]
["Wind","Socal",11,5,4.1179589118954384E-2]
["Wind","Socal",11,6,4.1779866676975648E-2]
["Wind","Socal",11,7,3.987334098592505E-2]
["Wind","Socal",11,8,3.5881972770371605E-2]
["Wind","Socal",11,9,3.2663665847655732E-2]
["Wind","Socal",11,10,3.5661366782801331E-2]
["Wind","Socal",11,11,3.884454694272986E-2]
["Wind","Socal",11,12,4.4242380785565041E-2]
["Wind","Socal",11,13,4.1999244409544799E-2]
["Wind","Socal",11,14,4.4428017814745306E-2]
["Wind","Socal",11,15,4.4798052270579904E-2]
["Wind","Socal",11,16,3.7489391263161108E-2]
["Wind","Socal",11,17,3.4032023616345539E-2]
["Wind","Socal",11,18,4.3268112006108042E-2]
["Wind","Socal",11,19,5.4433511042200081E-2]
["Wind","Socal",11,20,5.8670987650421495E-2]
["Wind","Socal",11,21,6.2501757622385939E-2]
["Wind","Socal",11,22,4.6395409394018532E-2]
["Wind","Socal",11,23,4.9144859207755215E-2]
["Wind","Socal",11,24,4.7347078681793872E-2]
["Wind","Socal",12,1,3.7252252748731188E-2]
["Wind","Socal",12,2,3.6189257974471527E-2]
["Wind","Socal",12,3,3.5493521055217143E-2]
["Wind","Socal",12,4,4.0741267217231161E-2]
["Wind","Socal",12,5,3.9878978900861423E-2]
["Wind","Socal",12,6,4.0533245134050259E-2]
["Wind","Socal",12,7,4.0176386208066905E-2]
["Wind","Socal",12,8,3.7442486948737343E-2]
["Wind","Socal",12,9,3.5067539125661233E-2]
["Wind","Socal",12,10,3.4956974539695748E-2]
["Wind","Socal",12,11,3.4732473946177587E-2]
["Wind","Socal",12,12,3.792839917515016E-2]
["Wind","Socal",12,13,3.7669720228406887E-2]
["Wind","Socal",12,14,3.4831258574471675E-2]
["Wind","Socal",12,15,3.3180744245735333E-2]
["Wind","Socal",12,16,3.481054967706055E-2]
["Wind","Socal",12,17,3.8526562440130863E-2]
["Wind","Socal",12,18,4.0611089500615392E-2]
["Wind","Socal",12,19,4.5915883680076618E-2]
["Wind","Socal",12,20,4.3003737414902682E-2]
["Wind","Socal",12,21,4.8698900882382011E-2]
["Wind","Socal",12,22,4.3794439692735346E-2]
["Wind","Socal",12,23,4.1352931067331664E-2]
["Wind","Socal",12,24,4.1011605184658212E-2]
["Wind","AZ",1,1,0.24061230445237292]
["Wind","AZ",1,2,0.21000095970251725]
["Wind","AZ",1,3,0.19061241706882512]
["Wind","AZ",1,4,0.21061232480476172]
["Wind","AZ",1,5,0.23000098977152564]
["Wind","AZ",1,6,0.25000101482903264]
["Wind","AZ",1,7,0.25061237962489386]
["Wind","AZ",1,8,0.27061239702281953]
["Wind","AZ",1,9,0.27061239702281953]
["Wind","AZ",1,10,0.22061239702281957]
["Wind","AZ",1,11,0.23000098977152564]
["Wind","AZ",1,12,0.2200010398865396]
["Wind","AZ",1,13,0.17183511276717986]
["Wind","AZ",1,14,0.17061239091163447]
["Wind","AZ",1,15,0.19061241706882512]
["Wind","AZ",1,16,0.17000103362216287]
["Wind","AZ",1,17,0.1206123700176437]
["Wind","AZ",1,18,0.21061232480476172]
["Wind","AZ",1,19,0.20061236695381121]
["Wind","AZ",1,20,0.14122375297738879]
["Wind","AZ",1,21,0.1400010348750382]
["Wind","AZ",1,22,0.10061234564949903]
["Wind","AZ",1,23,0.18000098601289957]
["Wind","AZ",1,24,0.2200010398865396]
["Wind","AZ",2,1,0.20000100981753124]
["Wind","AZ",2,2,0.16000099728877773]
["Wind","AZ",2,3,0.16452900030360029]
["Wind","AZ",2,4,0.19000105993254515]
["Wind","AZ",2,5,0.16226500829850851]
["Wind","AZ",2,6,0.17000103362216287]
["Wind","AZ",2,7,0.15452901108235076]
["Wind","AZ",2,8,0.16226500829850851]
["Wind","AZ",2,9,0.15000099728877775]
["Wind","AZ",2,10,8.6793005356653172E-2]
["Wind","AZ",2,11,9.000100981753123E-2]
["Wind","AZ",2,12,7.0000984760024254E-2]
["Wind","AZ",2,13,8.0000997288777728E-2]
["Wind","AZ",2,14,0.10226499009672846]
["Wind","AZ",2,15,9.2265006928346938E-2]
["Wind","AZ",2,16,9.000100981753123E-2]
["Wind","AZ",2,17,9.2265006928346938E-2]
["Wind","AZ",2,18,0.14226502914934064]
["Wind","AZ",2,19,0.21226498064004448]
["Wind","AZ",2,20,0.20679301363063676]
["Wind","AZ",2,21,0.16226500829850851]
["Wind","AZ",2,22,0.17000103362216287]
["Wind","AZ",2,23,0.15452901108235076]
["Wind","AZ",2,24,0.20000100981753124]
["Wind","AZ",3,1,0.18061235073216497]
["Wind","AZ",3,2,0.12000100981753123]
["Wind","AZ",3,3,0.12183508965191052]
["Wind","AZ",3,4,0.12000100981753123]
["Wind","AZ",3,5,0.18061235073216497]
["Wind","AZ",3,6,0.18000098601289957]
["Wind","AZ",3,7,0.19061241706882512]
["Wind","AZ",3,8,0.18000098601289957]
["Wind","AZ",3,9,0.12000100981753123]
["Wind","AZ",3,10,0.11061235707856878]
["Wind","AZ",3,11,0.15061235748889021]
["Wind","AZ",3,12,0.20000100981753124]
["Wind","AZ",3,13,0.19061241706882512]
["Wind","AZ",3,14,0.21000095970251725]
["Wind","AZ",3,15,0.22122375415909956]
["Wind","AZ",3,16,0.24061230445237292]
["Wind","AZ",3,17,0.20122373205605568]
["Wind","AZ",3,18,0.2200010398865396]
["Wind","AZ",3,19,0.20061236695381121]
["Wind","AZ",3,20,0.21061232480476172]
["Wind","AZ",3,21,0.21122368194104169]
["Wind","AZ",3,22,0.18000098601289957]
["Wind","AZ",3,23,0.20000100981753124]
["Wind","AZ",3,24,0.20000100981753124]
["Wind","AZ",4,1,0.20303149758799388]
["Wind","AZ",4,2,0.15000099728877775]
["Wind","AZ",4,3,0.10303149113501489]
["Wind","AZ",4,4,9.000100981753123E-2]
["Wind","AZ",4,5,8.6061999407600162E-2]
["Wind","AZ",4,6,8.3031504043452622E-2]
["Wind","AZ",4,7,0.10000098476002425]
["Wind","AZ",4,8,6.0001007311780541E-2]
["Wind","AZ",4,9,4.0001007311780537E-2]
["Wind","AZ",4,10,3.3031502410893046E-2]
["Wind","AZ",4,11,4.3031506852454771E-2]
["Wind","AZ",4,12,5.0000996035902391E-2]
["Wind","AZ",4,13,5.0000996035902391E-2]
["Wind","AZ",4,14,9.303150518167877E-2]
["Wind","AZ",4,15,8.0000997288777728E-2]
["Wind","AZ",4,16,0.16303151125745327]
["Wind","AZ",4,17,0.20000100981753124]
["Wind","AZ",4,18,0.2200010398865396]
["Wind","AZ",4,19,0.26303157777201613]
["Wind","AZ",4,20,0.29303146919224132]
["Wind","AZ",4,21,0.2200010398865396]
["Wind","AZ",4,22,0.2200010398865396]
["Wind","AZ",4,23,0.20000100981753124]
["Wind","AZ",4,24,0.20000100981753124]
["Wind","AZ",5,1,0.21000095970251725]
["Wind","AZ",5,2,0.1400010348750382]
["Wind","AZ",5,3,9.000100981753123E-2]
["Wind","AZ",5,4,7.0612345726094844E-2]
["Wind","AZ",5,5,7.0612345726094844E-2]
["Wind","AZ",5,6,9.000100981753123E-2]
["Wind","AZ",5,7,5.0000996035902391E-2]
["Wind","AZ",5,8,2.0000995910614862E-2]
["Wind","AZ",5,9,2.0612356118386917E-2]
["Wind","AZ",5,10,3.0000996035902398E-2]
["Wind","AZ",5,11,3.0612356925377181E-2]
["Wind","AZ",5,12,4.0001007311780537E-2]
["Wind","AZ",5,13,5.0000996035902391E-2]
["Wind","AZ",5,14,7.0000984760024254E-2]
["Wind","AZ",5,15,9.000100981753123E-2]
["Wind","AZ",5,16,0.1206123700176437]
["Wind","AZ",5,17,0.17000103362216287]
["Wind","AZ",5,18,0.19000105993254515]
["Wind","AZ",5,19,0.2200010398865396]
["Wind","AZ",5,20,0.31061232950987988]
["Wind","AZ",5,21,0.37061227939486591]
["Wind","AZ",5,22,0.37000091459900469]
["Wind","AZ",5,23,0.300612383728108]
["Wind","AZ",5,24,0.2306123469078056]
["Wind","AZ",6,1,0.20547626669526528]
["Wind","AZ",6,2,0.13000100981753124]
["Wind","AZ",6,3,6.0001007311780541E-2]
["Wind","AZ",6,4,4.5476285455045715E-2]
["Wind","AZ",6,5,3.0000996035902398E-2]
["Wind","AZ",6,6,3.0000996035902398E-2]
["Wind","AZ",6,7,1.0000999669240907E-2]
["Wind","AZ",6,8,1.0000999669240907E-2]
["Wind","AZ",6,9,1.0000999669240907E-2]
["Wind","AZ",6,10,1.0000999669240907E-2]
["Wind","AZ",6,11,1.0000999669240907E-2]
["Wind","AZ",6,12,1.0000999669240907E-2]
["Wind","AZ",6,13,2.0000995910614862E-2]
["Wind","AZ",6,14,3.0000996035902398E-2]
["Wind","AZ",6,15,4.0001007311780537E-2]
["Wind","AZ",6,16,6.0001007311780541E-2]
["Wind","AZ",6,17,6.0001007311780541E-2]
["Wind","AZ",6,18,0.10547627525101717]
["Wind","AZ",6,19,0.16547630149946818]
["Wind","AZ",6,20,0.26642685406072231]
["Wind","AZ",6,21,0.36000096471401871]
["Wind","AZ",6,22,0.27547629676427365]
["Wind","AZ",6,23,0.23095155364200773]
["Wind","AZ",6,24,0.22547629676427366]
["Wind","AZ",7,1,0.13776119708616433]
["Wind","AZ",7,2,7.7761162306134377E-2]
["Wind","AZ",7,3,4.0001007311780537E-2]
["Wind","AZ",7,4,4.0001007311780537E-2]
["Wind","AZ",7,5,2.0000995910614862E-2]
["Wind","AZ",7,6,2.0000995910614862E-2]
["Wind","AZ",7,7,1.0000999669240907E-2]
["Wind","AZ",7,8,9.9999999999999995E-7]
["Wind","AZ",7,9,9.9999999999999995E-7]
["Wind","AZ",7,10,9.9999999999999995E-7]
["Wind","AZ",7,11,1.0000999669240907E-2]
["Wind","AZ",7,12,1.0000999669240907E-2]
["Wind","AZ",7,13,2.0000995910614862E-2]
["Wind","AZ",7,14,2.0000995910614862E-2]
["Wind","AZ",7,15,3.0000996035902398E-2]
["Wind","AZ",7,16,4.0001007311780537E-2]
["Wind","AZ",7,17,6.0001007311780541E-2]
["Wind","AZ",7,18,0.10000098476002425]
["Wind","AZ",7,19,0.16000099728877773]
["Wind","AZ",7,20,0.31000096471401867]
["Wind","AZ",7,21,0.31776119087274368]
["Wind","AZ",7,22,0.30000102735778617]
["Wind","AZ",7,23,0.22776116882003489]
["Wind","AZ",7,24,0.19776118886604047]
["Wind","AZ",8,1,9.000100981753123E-2]
["Wind","AZ",8,2,6.0001007311780541E-2]
["Wind","AZ",8,3,4.0001007311780537E-2]
["Wind","AZ",8,4,2.7761163831427259E-2]
["Wind","AZ",8,5,3.0000996035902398E-2]
["Wind","AZ",8,6,2.0000995910614862E-2]
["Wind","AZ",8,7,1.0000999669240907E-2]
["Wind","AZ",8,8,7.7611675669125614E-3]
["Wind","AZ",8,9,9.9999999999999995E-7]
["Wind","AZ",8,10,9.9999999999999995E-7]
["Wind","AZ",8,11,1.0000999669240907E-2]
["Wind","AZ",8,12,2.0000995910614862E-2]
["Wind","AZ",8,13,2.0000995910614862E-2]
["Wind","AZ",8,14,2.0000995910614862E-2]
["Wind","AZ",8,15,3.0000996035902398E-2]
["Wind","AZ",8,16,4.0001007311780537E-2]
["Wind","AZ",8,17,5.0000996035902391E-2]
["Wind","AZ",8,18,6.0001007311780541E-2]
["Wind","AZ",8,19,9.000100981753123E-2]
["Wind","AZ",8,20,0.16000099728877773]
["Wind","AZ",8,21,0.16000099728877773]
["Wind","AZ",8,22,0.10000098476002425]
["Wind","AZ",8,23,0.11000099603590238]
["Wind","AZ",8,24,0.11000099603590238]
["Wind","AZ",9,1,9.5476280414962783E-2]
["Wind","AZ",9,2,6.547627928118184E-2]
["Wind","AZ",9,3,2.5476280296342402E-2]
["Wind","AZ",9,4,4.0951564670160499E-2]
["Wind","AZ",9,5,3.0000996035902398E-2]
["Wind","AZ",9,6,3.0000996035902398E-2]
["Wind","AZ",9,7,3.0000996035902398E-2]
["Wind","AZ",9,8,3.0000996035902398E-2]
["Wind","AZ",9,9,2.0000995910614862E-2]
["Wind","AZ",9,10,1.0000999669240907E-2]
["Wind","AZ",9,11,1.0000999669240907E-2]
["Wind","AZ",9,12,1.5476281928415336E-2]
["Wind","AZ",9,13,2.0000995910614862E-2]
["Wind","AZ",9,14,2.0000995910614862E-2]
["Wind","AZ",9,15,2.0000995910614862E-2]
["Wind","AZ",9,16,4.0001007311780537E-2]
["Wind","AZ",9,17,5.5476286526895326E-2]
["Wind","AZ",9,18,8.0951567113979855E-2]
["Wind","AZ",9,19,0.11642685143110891]
["Wind","AZ",9,20,0.1254762941346603]
["Wind","AZ",9,21,0.11000099603590238]
["Wind","AZ",9,22,5.0000996035902391E-2]
["Wind","AZ",9,23,6.0001007311780541E-2]
["Wind","AZ",9,24,9.000100981753123E-2]
["Wind","AZ",10,1,0.10000098476002425]
["Wind","AZ",10,2,7.0000984760024254E-2]
["Wind","AZ",10,3,4.0001007311780537E-2]
["Wind","AZ",10,4,5.0000996035902391E-2]
["Wind","AZ",10,5,5.0000996035902391E-2]
["Wind","AZ",10,6,5.0000996035902391E-2]
["Wind","AZ",10,7,7.0000984760024254E-2]
["Wind","AZ",10,8,5.0000996035902391E-2]
["Wind","AZ",10,9,5.0000996035902391E-2]
["Wind","AZ",10,10,3.0000996035902398E-2]
["Wind","AZ",10,11,3.0000996035902398E-2]
["Wind","AZ",10,12,2.7761163831427259E-2]
["Wind","AZ",10,13,2.0000995910614862E-2]
["Wind","AZ",10,14,2.0000995910614862E-2]
["Wind","AZ",10,15,2.0000995910614862E-2]
["Wind","AZ",10,16,2.0000995910614862E-2]
["Wind","AZ",10,17,3.0000996035902398E-2]
["Wind","AZ",10,18,7.0000984760024254E-2]
["Wind","AZ",10,19,6.7761157634826361E-2]
["Wind","AZ",10,20,7.0000984760024254E-2]
["Wind","AZ",10,21,7.0000984760024254E-2]
["Wind","AZ",10,22,5.0000996035902391E-2]
["Wind","AZ",10,23,7.7761162306134377E-2]
["Wind","AZ",10,24,0.11000099603590238]
["Wind","AZ",11,1,0.21000095970251725]
["Wind","AZ",11,2,0.16000099728877773]
["Wind","AZ",11,3,0.17000103362216287]
["Wind","AZ",11,4,0.17000103362216287]
["Wind","AZ",11,5,0.15303150024661019]
["Wind","AZ",11,6,0.18000098601289957]
["Wind","AZ",11,7,0.18000098601289957]
["Wind","AZ",11,8,0.18303151137210247]
["Wind","AZ",11,9,0.18303151137210247]
["Wind","AZ",11,10,0.12606202332688102]
["Wind","AZ",11,11,8.3031504043452622E-2]
["Wind","AZ",11,12,9.000100981753123E-2]
["Wind","AZ",11,13,8.3031504043452622E-2]
["Wind","AZ",11,14,8.90925057825908E-2]
["Wind","AZ",11,15,0.11000099603590238]
["Wind","AZ",11,16,9.000100981753123E-2]
["Wind","AZ",11,17,9.303150518167877E-2]
["Wind","AZ",11,18,0.10303149113501489]
["Wind","AZ",11,19,0.10000098476002425]
["Wind","AZ",11,20,0.10000098476002425]
["Wind","AZ",11,21,0.11000099603590238]
["Wind","AZ",11,22,0.11909251667961129]
["Wind","AZ",11,23,0.16000099728877773]
["Wind","AZ",11,24,0.2200010398865396]
["Wind","AZ",12,1,0.31122368664615985]
["Wind","AZ",12,2,0.300612383728108]
["Wind","AZ",12,3,0.32244647609124077]
["Wind","AZ",12,4,0.29061230521833104]
["Wind","AZ",12,5,0.26061244713783349]
["Wind","AZ",12,6,0.27000103988653956]
["Wind","AZ",12,7,0.26061244713783349]
["Wind","AZ",12,8,0.26000109000155353]
["Wind","AZ",12,9,0.25061237962489386]
["Wind","AZ",12,10,0.26000109000155353]
["Wind","AZ",12,11,0.26000109000155353]
["Wind","AZ",12,12,0.2200010398865396]
["Wind","AZ",12,13,0.17061239091163447]
["Wind","AZ",12,14,0.1400010348750382]
["Wind","AZ",12,15,0.15000099728877775]
["Wind","AZ",12,16,0.13244645207330155]
["Wind","AZ",12,17,0.17000103362216287]
["Wind","AZ",12,18,0.19000105993254515]
["Wind","AZ",12,19,0.15061235748889021]
["Wind","AZ",12,20,0.16000099728877773]
["Wind","AZ",12,21,0.17183511276717986]
["Wind","AZ",12,22,0.16061235971016877]
["Wind","AZ",12,23,0.2200010398865396]
["Wind","AZ",12,24,0.26000109000155353]
["Wind","NM",1,1,0.49072063457089343]
["Wind","NM",1,2,0.49122899611995441]
["Wind","NM",1,3,0.44420666749305071]
["Wind","NM",1,4,0.46374479517405581]
["Wind","NM",1,5,0.49139124121060346]
["Wind","NM",1,6,0.47483766099202529]
["Wind","NM",1,7,0.45364357733180621]
["Wind","NM",1,8,0.46240990211319621]
["Wind","NM",1,9,0.40718845868589848]
["Wind","NM",1,10,0.38994485774793802]
["Wind","NM",1,11,0.41522531673460394]
["Wind","NM",1,12,0.35860383141762453]
["Wind","NM",1,13,0.36938195250611006]
["Wind","NM",1,14,0.37603827690049607]
["Wind","NM",1,15,0.40249668182331488]
["Wind","NM",1,16,0.38264825698811467]
["Wind","NM",1,17,0.42466222483362515]
["Wind","NM",1,18,0.4555982559834994]
["Wind","NM",1,19,0.48128372239155542]
["Wind","NM",1,20,0.49072063457089343]
["Wind","NM",1,21,0.51903143639397908]
["Wind","NM",1,22,0.50336947392451237]
["Wind","NM",1,23,0.53790521994948559]
["Wind","NM",1,24,0.50015755083054858]
["Wind","NM",2,1,0.40578840047494891]
["Wind","NM",2,2,0.35860383141762453]
["Wind","NM",2,3,0.36092927476271797]
["Wind","NM",2,4,0.35381781308363536]
["Wind","NM",2,5,0.34272935040984126]
["Wind","NM",2,6,0.35860383141762453]
["Wind","NM",2,7,0.36590227699319861]
["Wind","NM",2,8,0.31374470263054854]
["Wind","NM",2,9,0.3043077720021401]
["Wind","NM",2,10,0.3043077720021401]
["Wind","NM",2,11,0.34916692739892036]
["Wind","NM",2,12,0.35820164480690375]
["Wind","NM",2,13,0.3208561704593213]
["Wind","NM",2,14,0.35381781308363536]
["Wind","NM",2,15,0.39851888909463351]
["Wind","NM",2,16,0.39545440267267268]
["Wind","NM",2,17,0.3798031155010913]
["Wind","NM",2,18,0.3798031155010913]
["Wind","NM",2,19,0.41522531673460394]
["Wind","NM",2,20,0.40100236877767814]
["Wind","NM",2,21,0.42477481268198936]
["Wind","NM",2,22,0.43642462742777505]
["Wind","NM",2,23,0.41522531673460394]
["Wind","NM",2,24,0.42466222483362515]
["Wind","NM",3,1,0.41589592279440257]
["Wind","NM",3,2,0.40780022358359164]
["Wind","NM",3,3,0.40785906474569705]
["Wind","NM",3,4,0.39635147605465987]
["Wind","NM",3,5,0.35860383141762453]
["Wind","NM",3,6,0.3776191655118577]
["Wind","NM",3,7,0.36804073951664573]
["Wind","NM",3,8,0.28512033700087053]
["Wind","NM",3,9,0.21772067726132957]
["Wind","NM",3,10,0.22547606091604527]
["Wind","NM",3,11,0.23592392004210891]
["Wind","NM",3,12,0.22017526517457831]
["Wind","NM",3,13,0.2268172751978523]
["Wind","NM",3,14,0.25479775256141901]
["Wind","NM",3,15,0.2831085176616519]
["Wind","NM",3,16,0.29254541760003916]
["Wind","NM",3,17,0.27367158100041211]
["Wind","NM",3,18,0.31208986462973753]
["Wind","NM",3,19,0.33973000297863132]
["Wind","NM",3,20,0.37747767617788547]
["Wind","NM",3,21,0.40578840047494891]
["Wind","NM",3,22,0.38691456795563878]
["Wind","NM",3,23,0.40578840047494891]
["Wind","NM",3,24,0.41522531673460394]
["Wind","NM",4,1,0.40578840047494891]
["Wind","NM",4,2,0.41511984943500074]
["Wind","NM",4,3,0.38688554356123506]
["Wind","NM",4,4,0.35846816144601201]
["Wind","NM",4,5,0.38227748443905041]
["Wind","NM",4,6,0.40561537962041538]
["Wind","NM",4,7,0.33973000297863132]
["Wind","NM",4,8,0.29254541760003916]
["Wind","NM",4,9,0.29245890732239332]
["Wind","NM",4,10,0.29245890732239332]
["Wind","NM",4,11,0.29254541760003916]
["Wind","NM",4,12,0.33095905807836618]
["Wind","NM",4,13,0.36804073951664573]
["Wind","NM",4,14,0.38230881470287265]
["Wind","NM",4,15,0.4008542794447581]
["Wind","NM",4,16,0.41513880630733718]
["Wind","NM",4,17,0.44207688825485342]
["Wind","NM",4,18,0.42457571448116882]
["Wind","NM",4,19,0.39635147605465987]
["Wind","NM",4,20,0.40578840047494891]
["Wind","NM",4,21,0.41522531673460394]
["Wind","NM",4,22,0.4649523626740214]
["Wind","NM",4,23,0.43068240632914562]
["Wind","NM",4,24,0.43401268322386594]
["Wind","NM",5,1,0.37747767617788547]
["Wind","NM",5,2,0.35860383141762453]
["Wind","NM",5,3,0.33029307447802536]
["Wind","NM",5,4,0.30198232161874333]
["Wind","NM",5,5,0.28118246184493451]
["Wind","NM",5,6,0.26423466474075696]
["Wind","NM",5,7,0.18873932650288278]
["Wind","NM",5,8,0.17839146325481933]
["Wind","NM",5,9,0.17930240249062546]
["Wind","NM",5,10,0.19817623052158689]
["Wind","NM",5,11,0.22715758767999628]
["Wind","NM",5,12,0.25479775256141901]
["Wind","NM",5,13,0.2831085176616519]
["Wind","NM",5,14,0.33029307447802536]
["Wind","NM",5,15,0.36804073951664573]
["Wind","NM",5,16,0.3781482810778613]
["Wind","NM",5,17,0.38691456795563878]
["Wind","NM",5,18,0.40594557748260235]
["Wind","NM",5,19,0.37747767617788547]
["Wind","NM",5,20,0.38758517401543741]
["Wind","NM",5,21,0.36871134760613422]
["Wind","NM",5,22,0.38397345605268834]
["Wind","NM",5,23,0.38758517401543741]
["Wind","NM",5,24,0.37999785901799127]
["Wind","NM",6,1,0.34789228371347547]
["Wind","NM",6,2,0.2831085176616519]
["Wind","NM",6,3,0.27189981713446409]
["Wind","NM",6,4,0.27189981713446409]
["Wind","NM",6,5,0.23415215157972835]
["Wind","NM",6,6,0.21350654193749072]
["Wind","NM",6,7,0.12241390864274257]
["Wind","NM",6,8,0.11324399234532538]
["Wind","NM",6,9,9.4370159826015293E-2]
["Wind","NM",6,10,7.5496324858514999E-2]
["Wind","NM",6,11,8.3161485206409716E-2]
["Wind","NM",6,12,0.11102985304520771]
["Wind","NM",6,13,0.14921988807127232]
["Wind","NM",6,14,0.19766263378442675]
["Wind","NM",6,15,0.24536082406081308]
["Wind","NM",6,16,0.26423466474075696]
["Wind","NM",6,17,0.28191573132291498]
["Wind","NM",6,18,0.29254541760003916]
["Wind","NM",6,19,0.30198232161874333]
["Wind","NM",6,20,0.31731263966313689]
["Wind","NM",6,21,0.3208561704593213]
["Wind","NM",6,22,0.33029307447802536]
["Wind","NM",6,23,0.33795823681446702]
["Wind","NM",6,24,0.35796795658202524]
["Wind","NM",7,1,0.2076131508615589]
["Wind","NM",7,2,0.1334573283002348]
["Wind","NM",7,3,0.11324399234532538]
["Wind","NM",7,4,9.7152323900935214E-2]
["Wind","NM",7,5,6.896236435604064E-2]
["Wind","NM",7,6,5.6622495195426774E-2]
["Wind","NM",7,7,2.5847832437934731E-2]
["Wind","NM",7,8,1.8874831788933365E-2]
["Wind","NM",7,9,1.8874831788933365E-2]
["Wind","NM",7,10,2.5037687219017241E-2]
["Wind","NM",7,11,1.8874831788933365E-2]
["Wind","NM",7,12,2.8311748048588416E-2]
["Wind","NM",7,13,7.5496324858514999E-2]
["Wind","NM",7,14,9.4370159826015293E-2]
["Wind","NM",7,15,0.13320872650965818]
["Wind","NM",7,16,0.169865498879953]
["Wind","NM",7,17,0.2076131508615589]
["Wind","NM",7,18,0.20727189875794005]
["Wind","NM",7,19,0.23168595969723804]
["Wind","NM",7,20,0.23168595969723804]
["Wind","NM",7,21,0.24112288020751482]
["Wind","NM",7,22,0.21281212001864486]
["Wind","NM",7,23,0.19817623052158689]
["Wind","NM",7,24,0.22648697930055206]
["Wind","NM",8,1,0.20337519967867282]
["Wind","NM",8,2,0.15099164963134334]
["Wind","NM",8,3,0.10900604317807594]
["Wind","NM",8,4,9.4370159826015293E-2]
["Wind","NM",8,5,5.6622495195426774E-2]
["Wind","NM",8,6,6.2914542439855531E-2]
["Wind","NM",8,7,2.8311748048588416E-2]
["Wind","NM",8,8,1.8874831788933365E-2]
["Wind","NM",8,9,1.8874831788933365E-2]
["Wind","NM",8,10,1.8874831788933365E-2]
["Wind","NM",8,11,1.8874831788933365E-2]
["Wind","NM",8,12,4.7185580975930209E-2]
["Wind","NM",8,13,6.6059413495240318E-2]
["Wind","NM",8,14,9.4370159826015293E-2]
["Wind","NM",8,15,0.12268090448386031]
["Wind","NM",8,16,0.14155474565344237]
["Wind","NM",8,17,0.1750644588205669]
["Wind","NM",8,18,0.19817623052158689]
["Wind","NM",8,19,0.19817623052158689]
["Wind","NM",8,20,0.19817623052158689]
["Wind","NM",8,21,0.17216643907596521]
["Wind","NM",8,22,0.16562754549819059]
["Wind","NM",8,23,0.18873932650288278]
["Wind","NM",8,24,0.19817623052158689]
["Wind","NM",9,1,0.19640446895385513]
["Wind","NM",9,2,0.15865680832211565]
["Wind","NM",9,3,0.14149393455954226]
["Wind","NM",9,4,0.15099164963134334]
["Wind","NM",9,5,0.14069042435321208]
["Wind","NM",9,6,0.16042857364360064]
["Wind","NM",9,7,0.12695944131958761]
["Wind","NM",9,8,7.5496324858514999E-2]
["Wind","NM",9,9,4.9414819841018545E-2]
["Wind","NM",9,10,4.5325580786677894E-2]
["Wind","NM",9,11,4.7185580975930209E-2]
["Wind","NM",9,12,4.7185580975930209E-2]
["Wind","NM",9,13,7.2656885256055556E-2]
["Wind","NM",9,14,6.508674101067248E-2]
["Wind","NM",9,15,0.10380707649370202]
["Wind","NM",9,16,0.11743656689100009]
["Wind","NM",9,17,0.17753064099950092]
["Wind","NM",9,18,0.2076131508615589]
["Wind","NM",9,19,0.22648697930055206]
["Wind","NM",9,20,0.25479775256141901]
["Wind","NM",9,21,0.19817623052158689]
["Wind","NM",9,22,0.19070629142782403]
["Wind","NM",9,23,0.17885045533564861]
["Wind","NM",9,24,0.21705007120153097]
["Wind","NM",10,1,0.30198232161874333]
["Wind","NM",10,2,0.24536082406081308]
["Wind","NM",10,3,0.22982372653344815]
["Wind","NM",10,4,0.21705007120153097]
["Wind","NM",10,5,0.19902693663939303]
["Wind","NM",10,6,0.18873932650288278]
["Wind","NM",10,7,0.14012799144477786]
["Wind","NM",10,8,8.5297519338248973E-2]
["Wind","NM",10,9,8.4989192574204439E-2]
["Wind","NM",10,10,8.4933250910930763E-2]
["Wind","NM",10,11,9.0132213773840675E-2]
["Wind","NM",10,12,0.10380707649370202]
["Wind","NM",10,13,0.10380707649370202]
["Wind","NM",10,14,0.11299940946407505]
["Wind","NM",10,15,0.12268090448386031]
["Wind","NM",10,16,0.169865498879953]
["Wind","NM",10,17,0.18873932650288278]
["Wind","NM",10,18,0.21299538905947449]
["Wind","NM",10,19,0.23592392004210891]
["Wind","NM",10,20,0.26216971573094799]
["Wind","NM",10,21,0.27463260979868886]
["Wind","NM",10,22,0.26943363164992296]
["Wind","NM",10,23,0.23568178715771082]
["Wind","NM",10,24,0.26943363164992296]
["Wind","NM",11,1,0.3793639801928928]
["Wind","NM",11,2,0.40939344839103875]
["Wind","NM",11,3,0.36804073951664573]
["Wind","NM",11,4,0.35235075545357231]
["Wind","NM",11,5,0.38510447710973761]
["Wind","NM",11,6,0.38682805775280338]
["Wind","NM",11,7,0.39617845549936814]
["Wind","NM",11,8,0.33973000297863132]
["Wind","NM",11,9,0.25468517768807297]
["Wind","NM",11,10,0.21700890562452188]
["Wind","NM",11,11,0.25471124202193657]
["Wind","NM",11,12,0.245274313745762]
["Wind","NM",11,13,0.27349856018328383]
["Wind","NM",11,14,0.2831085176616519]
["Wind","NM",11,15,0.2831085176616519]
["Wind","NM",11,16,0.29236210165618798]
["Wind","NM",11,17,0.33961042093221583]
["Wind","NM",11,18,0.37747767617788547]
["Wind","NM",11,19,0.40578840047494891]
["Wind","NM",11,20,0.42466222483362515]
["Wind","NM",11,21,0.40578840047494891]
["Wind","NM",11,22,0.43072079393080176]
["Wind","NM",11,23,0.40570188997287171]
["Wind","NM",11,24,0.41522531673460394]
["Wind","NM",12,1,0.49072063457089343]
["Wind","NM",12,2,0.51903143639397908]
["Wind","NM",12,3,0.45559825624853928]
["Wind","NM",12,4,0.43409919413740061]
["Wind","NM",12,5,0.45364357733180621]
["Wind","NM",12,6,0.48128372239155542]
["Wind","NM",12,7,0.50959451605400707]
["Wind","NM",12,8,0.49072063457089343]
["Wind","NM",12,9,0.42734465226233226]
["Wind","NM",12,10,0.42533283524275922]
["Wind","NM",12,11,0.4529729695322734]
["Wind","NM",12,12,0.44353606143325208]
["Wind","NM",12,13,0.43409919413740061]
["Wind","NM",12,14,0.46240990211319621]
["Wind","NM",12,15,0.47184681021221736]
["Wind","NM",12,16,0.48128372239155542]
["Wind","NM",12,17,0.50149876787939263]
["Wind","NM",12,18,0.52846834857331726]
["Wind","NM",12,19,0.52846834857331726]
["Wind","NM",12,20,0.50268285651125655]
["Wind","NM",12,21,0.51903143639397908]
["Wind","NM",12,22,0.55677905246879567]
["Wind","NM",12,23,0.52257685445512125]
["Wind","NM",12,24,0.49072063457089343]
["Wind","WA/OR",1,1,0.24061230445237292]
["Wind","WA/OR",1,2,0.21000095970251725]
["Wind","WA/OR",1,3,0.19061241706882512]
["Wind","WA/OR",1,4,0.21061232480476172]
["Wind","WA/OR",1,5,0.23000098977152564]
["Wind","WA/OR",1,6,0.25000101482903264]
["Wind","WA/OR",1,7,0.25061237962489386]
["Wind","WA/OR",1,8,0.27061239702281953]
["Wind","WA/OR",1,9,0.27061239702281953]
["Wind","WA/OR",1,10,0.22061239702281957]
["Wind","WA/OR",1,11,0.23000098977152564]
["Wind","WA/OR",1,12,0.2200010398865396]
["Wind","WA/OR",1,13,0.17183511276717986]
["Wind","WA/OR",1,14,0.17061239091163447]
["Wind","WA/OR",1,15,0.19061241706882512]
["Wind","WA/OR",1,16,0.17000103362216287]
["Wind","WA/OR",1,17,0.1206123700176437]
["Wind","WA/OR",1,18,0.21061232480476172]
["Wind","WA/OR",1,19,0.20061236695381121]
["Wind","WA/OR",1,20,0.14122375297738879]
["Wind","WA/OR",1,21,0.1400010348750382]
["Wind","WA/OR",1,22,0.10061234564949903]
["Wind","WA/OR",1,23,0.18000098601289957]
["Wind","WA/OR",1,24,0.2200010398865396]
["Wind","WA/OR",2,1,0.20000100981753124]
["Wind","WA/OR",2,2,0.16000099728877773]
["Wind","WA/OR",2,3,0.16452900030360029]
["Wind","WA/OR",2,4,0.19000105993254515]
["Wind","WA/OR",2,5,0.16226500829850851]
["Wind","WA/OR",2,6,0.17000103362216287]
["Wind","WA/OR",2,7,0.15452901108235076]
["Wind","WA/OR",2,8,0.16226500829850851]
["Wind","WA/OR",2,9,0.15000099728877775]
["Wind","WA/OR",2,10,8.6793005356653172E-2]
["Wind","WA/OR",2,11,9.000100981753123E-2]
["Wind","WA/OR",2,12,7.0000984760024254E-2]
["Wind","WA/OR",2,13,8.0000997288777728E-2]
["Wind","WA/OR",2,14,0.10226499009672846]
["Wind","WA/OR",2,15,9.2265006928346938E-2]
["Wind","WA/OR",2,16,9.000100981753123E-2]
["Wind","WA/OR",2,17,9.2265006928346938E-2]
["Wind","WA/OR",2,18,0.14226502914934064]
["Wind","WA/OR",2,19,0.21226498064004448]
["Wind","WA/OR",2,20,0.20679301363063676]
["Wind","WA/OR",2,21,0.16226500829850851]
["Wind","WA/OR",2,22,0.17000103362216287]
["Wind","WA/OR",2,23,0.15452901108235076]
["Wind","WA/OR",2,24,0.20000100981753124]
["Wind","WA/OR",3,1,0.18061235073216497]
["Wind","WA/OR",3,2,0.12000100981753123]
["Wind","WA/OR",3,3,0.12183508965191052]
["Wind","WA/OR",3,4,0.12000100981753123]
["Wind","WA/OR",3,5,0.18061235073216497]
["Wind","WA/OR",3,6,0.18000098601289957]
["Wind","WA/OR",3,7,0.19061241706882512]
["Wind","WA/OR",3,8,0.18000098601289957]
["Wind","WA/OR",3,9,0.12000100981753123]
["Wind","WA/OR",3,10,0.11061235707856878]
["Wind","WA/OR",3,11,0.15061235748889021]
["Wind","WA/OR",3,12,0.20000100981753124]
["Wind","WA/OR",3,13,0.19061241706882512]
["Wind","WA/OR",3,14,0.21000095970251725]
["Wind","WA/OR",3,15,0.22122375415909956]
["Wind","WA/OR",3,16,0.24061230445237292]
["Wind","WA/OR",3,17,0.20122373205605568]
["Wind","WA/OR",3,18,0.2200010398865396]
["Wind","WA/OR",3,19,0.20061236695381121]
["Wind","WA/OR",3,20,0.21061232480476172]
["Wind","WA/OR",3,21,0.21122368194104169]
["Wind","WA/OR",3,22,0.18000098601289957]
["Wind","WA/OR",3,23,0.20000100981753124]
["Wind","WA/OR",3,24,0.20000100981753124]
["Wind","WA/OR",4,1,0.20303149758799388]
["Wind","WA/OR",4,2,0.15000099728877775]
["Wind","WA/OR",4,3,0.10303149113501489]
["Wind","WA/OR",4,4,9.000100981753123E-2]
["Wind","WA/OR",4,5,8.6061999407600162E-2]
["Wind","WA/OR",4,6,8.3031504043452622E-2]
["Wind","WA/OR",4,7,0.10000098476002425]
["Wind","WA/OR",4,8,6.0001007311780541E-2]
["Wind","WA/OR",4,9,4.0001007311780537E-2]
["Wind","WA/OR",4,10,3.3031502410893046E-2]
["Wind","WA/OR",4,11,4.3031506852454771E-2]
["Wind","WA/OR",4,12,5.0000996035902391E-2]
["Wind","WA/OR",4,13,5.0000996035902391E-2]
["Wind","WA/OR",4,14,9.303150518167877E-2]
["Wind","WA/OR",4,15,8.0000997288777728E-2]
["Wind","WA/OR",4,16,0.16303151125745327]
["Wind","WA/OR",4,17,0.20000100981753124]
["Wind","WA/OR",4,18,0.2200010398865396]
["Wind","WA/OR",4,19,0.26303157777201613]
["Wind","WA/OR",4,20,0.29303146919224132]
["Wind","WA/OR",4,21,0.2200010398865396]
["Wind","WA/OR",4,22,0.2200010398865396]
["Wind","WA/OR",4,23,0.20000100981753124]
["Wind","WA/OR",4,24,0.20000100981753124]
["Wind","WA/OR",5,1,0.21000095970251725]
["Wind","WA/OR",5,2,0.1400010348750382]
["Wind","WA/OR",5,3,9.000100981753123E-2]
["Wind","WA/OR",5,4,7.0612345726094844E-2]
["Wind","WA/OR",5,5,7.0612345726094844E-2]
["Wind","WA/OR",5,6,9.000100981753123E-2]
["Wind","WA/OR",5,7,5.0000996035902391E-2]
["Wind","WA/OR",5,8,2.0000995910614862E-2]
["Wind","WA/OR",5,9,2.0612356118386917E-2]
["Wind","WA/OR",5,10,3.0000996035902398E-2]
["Wind","WA/OR",5,11,3.0612356925377181E-2]
["Wind","WA/OR",5,12,4.0001007311780537E-2]
["Wind","WA/OR",5,13,5.0000996035902391E-2]
["Wind","WA/OR",5,14,7.0000984760024254E-2]
["Wind","WA/OR",5,15,9.000100981753123E-2]
["Wind","WA/OR",5,16,0.1206123700176437]
["Wind","WA/OR",5,17,0.17000103362216287]
["Wind","WA/OR",5,18,0.19000105993254515]
["Wind","WA/OR",5,19,0.2200010398865396]
["Wind","WA/OR",5,20,0.31061232950987988]
["Wind","WA/OR",5,21,0.37061227939486591]
["Wind","WA/OR",5,22,0.37000091459900469]
["Wind","WA/OR",5,23,0.300612383728108]
["Wind","WA/OR",5,24,0.2306123469078056]
["Wind","WA/OR",6,1,0.20547626669526528]
["Wind","WA/OR",6,2,0.13000100981753124]
["Wind","WA/OR",6,3,6.0001007311780541E-2]
["Wind","WA/OR",6,4,4.5476285455045715E-2]
["Wind","WA/OR",6,5,3.0000996035902398E-2]
["Wind","WA/OR",6,6,3.0000996035902398E-2]
["Wind","WA/OR",6,7,1.0000999669240907E-2]
["Wind","WA/OR",6,8,1.0000999669240907E-2]
["Wind","WA/OR",6,9,1.0000999669240907E-2]
["Wind","WA/OR",6,10,1.0000999669240907E-2]
["Wind","WA/OR",6,11,1.0000999669240907E-2]
["Wind","WA/OR",6,12,1.0000999669240907E-2]
["Wind","WA/OR",6,13,2.0000995910614862E-2]
["Wind","WA/OR",6,14,3.0000996035902398E-2]
["Wind","WA/OR",6,15,4.0001007311780537E-2]
["Wind","WA/OR",6,16,6.0001007311780541E-2]
["Wind","WA/OR",6,17,6.0001007311780541E-2]
["Wind","WA/OR",6,18,0.10547627525101717]
["Wind","WA/OR",6,19,0.16547630149946818]
["Wind","WA/OR",6,20,0.26642685406072231]
["Wind","WA/OR",6,21,0.36000096471401871]
["Wind","WA/OR",6,22,0.27547629676427365]
["Wind","WA/OR",6,23,0.23095155364200773]
["Wind","WA/OR",6,24,0.22547629676427366]
["Wind","WA/OR",7,1,0.13776119708616433]
["Wind","WA/OR",7,2,7.7761162306134377E-2]
["Wind","WA/OR",7,3,4.0001007311780537E-2]
["Wind","WA/OR",7,4,4.0001007311780537E-2]
["Wind","WA/OR",7,5,2.0000995910614862E-2]
["Wind","WA/OR",7,6,2.0000995910614862E-2]
["Wind","WA/OR",7,7,1.0000999669240907E-2]
["Wind","WA/OR",7,8,9.9999999999999995E-7]
["Wind","WA/OR",7,9,9.9999999999999995E-7]
["Wind","WA/OR",7,10,9.9999999999999995E-7]
["Wind","WA/OR",7,11,1.0000999669240907E-2]
["Wind","WA/OR",7,12,1.0000999669240907E-2]
["Wind","WA/OR",7,13,2.0000995910614862E-2]
["Wind","WA/OR",7,14,2.0000995910614862E-2]
["Wind","WA/OR",7,15,3.0000996035902398E-2]
["Wind","WA/OR",7,16,4.0001007311780537E-2]
["Wind","WA/OR",7,17,6.0001007311780541E-2]
["Wind","WA/OR",7,18,0.10000098476002425]
["Wind","WA/OR",7,19,0.16000099728877773]
["Wind","WA/OR",7,20,0.31000096471401867]
["Wind","WA/OR",7,21,0.31776119087274368]
["Wind","WA/OR",7,22,0.30000102735778617]
["Wind","WA/OR",7,23,0.22776116882003489]
["Wind","WA/OR",7,24,0.19776118886604047]
["Wind","WA/OR",8,1,9.000100981753123E-2]
["Wind","WA/OR",8,2,6.0001007311780541E-2]
["Wind","WA/OR",8,3,4.0001007311780537E-2]
["Wind","WA/OR",8,4,2.7761163831427259E-2]
["Wind","WA/OR",8,5,3.0000996035902398E-2]
["Wind","WA/OR",8,6,2.0000995910614862E-2]
["Wind","WA/OR",8,7,1.0000999669240907E-2]
["Wind","WA/OR",8,8,7.7611675669125614E-3]
["Wind","WA/OR",8,9,9.9999999999999995E-7]
["Wind","WA/OR",8,10,9.9999999999999995E-7]
["Wind","WA/OR",8,11,1.0000999669240907E-2]
["Wind","WA/OR",8,12,2.0000995910614862E-2]
["Wind","WA/OR",8,13,2.0000995910614862E-2]
["Wind","WA/OR",8,14,2.0000995910614862E-2]
["Wind","WA/OR",8,15,3.0000996035902398E-2]
["Wind","WA/OR",8,16,4.0001007311780537E-2]
["Wind","WA/OR",8,17,5.0000996035902391E-2]
["Wind","WA/OR",8,18,6.0001007311780541E-2]
["Wind","WA/OR",8,19,9.000100981753123E-2]
["Wind","WA/OR",8,20,0.16000099728877773]
["Wind","WA/OR",8,21,0.16000099728877773]
["Wind","WA/OR",8,22,0.10000098476002425]
["Wind","WA/OR",8,23,0.11000099603590238]
["Wind","WA/OR",8,24,0.11000099603590238]
["Wind","WA/OR",9,1,9.5476280414962783E-2]
["Wind","WA/OR",9,2,6.547627928118184E-2]
["Wind","WA/OR",9,3,2.5476280296342402E-2]
["Wind","WA/OR",9,4,4.0951564670160499E-2]
["Wind","WA/OR",9,5,3.0000996035902398E-2]
["Wind","WA/OR",9,6,3.0000996035902398E-2]
["Wind","WA/OR",9,7,3.0000996035902398E-2]
["Wind","WA/OR",9,8,3.0000996035902398E-2]
["Wind","WA/OR",9,9,2.0000995910614862E-2]
["Wind","WA/OR",9,10,1.0000999669240907E-2]
["Wind","WA/OR",9,11,1.0000999669240907E-2]
["Wind","WA/OR",9,12,1.5476281928415336E-2]
["Wind","WA/OR",9,13,2.0000995910614862E-2]
["Wind","WA/OR",9,14,2.0000995910614862E-2]
["Wind","WA/OR",9,15,2.0000995910614862E-2]
["Wind","WA/OR",9,16,4.0001007311780537E-2]
["Wind","WA/OR",9,17,5.5476286526895326E-2]
["Wind","WA/OR",9,18,8.0951567113979855E-2]
["Wind","WA/OR",9,19,0.11642685143110891]
["Wind","WA/OR",9,20,0.1254762941346603]
["Wind","WA/OR",9,21,0.11000099603590238]
["Wind","WA/OR",9,22,5.0000996035902391E-2]
["Wind","WA/OR",9,23,6.0001007311780541E-2]
["Wind","WA/OR",9,24,9.000100981753123E-2]
["Wind","WA/OR",10,1,0.10000098476002425]
["Wind","WA/OR",10,2,7.0000984760024254E-2]
["Wind","WA/OR",10,3,4.0001007311780537E-2]
["Wind","WA/OR",10,4,5.0000996035902391E-2]
["Wind","WA/OR",10,5,5.0000996035902391E-2]
["Wind","WA/OR",10,6,5.0000996035902391E-2]
["Wind","WA/OR",10,7,7.0000984760024254E-2]
["Wind","WA/OR",10,8,5.0000996035902391E-2]
["Wind","WA/OR",10,9,5.0000996035902391E-2]
["Wind","WA/OR",10,10,3.0000996035902398E-2]
["Wind","WA/OR",10,11,3.0000996035902398E-2]
["Wind","WA/OR",10,12,2.7761163831427259E-2]
["Wind","WA/OR",10,13,2.0000995910614862E-2]
["Wind","WA/OR",10,14,2.0000995910614862E-2]
["Wind","WA/OR",10,15,2.0000995910614862E-2]
["Wind","WA/OR",10,16,2.0000995910614862E-2]
["Wind","WA/OR",10,17,3.0000996035902398E-2]
["Wind","WA/OR",10,18,7.0000984760024254E-2]
["Wind","WA/OR",10,19,6.7761157634826361E-2]
["Wind","WA/OR",10,20,7.0000984760024254E-2]
["Wind","WA/OR",10,21,7.0000984760024254E-2]
["Wind","WA/OR",10,22,5.0000996035902391E-2]
["Wind","WA/OR",10,23,7.7761162306134377E-2]
["Wind","WA/OR",10,24,0.11000099603590238]
["Wind","WA/OR",11,1,0.21000095970251725]
["Wind","WA/OR",11,2,0.16000099728877773]
["Wind","WA/OR",11,3,0.17000103362216287]
["Wind","WA/OR",11,4,0.17000103362216287]
["Wind","WA/OR",11,5,0.15303150024661019]
["Wind","WA/OR",11,6,0.18000098601289957]
["Wind","WA/OR",11,7,0.18000098601289957]
["Wind","WA/OR",11,8,0.18303151137210247]
["Wind","WA/OR",11,9,0.18303151137210247]
["Wind","WA/OR",11,10,0.12606202332688102]
["Wind","WA/OR",11,11,8.3031504043452622E-2]
["Wind","WA/OR",11,12,9.000100981753123E-2]
["Wind","WA/OR",11,13,8.3031504043452622E-2]
["Wind","WA/OR",11,14,8.90925057825908E-2]
["Wind","WA/OR",11,15,0.11000099603590238]
["Wind","WA/OR",11,16,9.000100981753123E-2]
["Wind","WA/OR",11,17,9.303150518167877E-2]
["Wind","WA/OR",11,18,0.10303149113501489]
["Wind","WA/OR",11,19,0.10000098476002425]
["Wind","WA/OR",11,20,0.10000098476002425]
["Wind","WA/OR",11,21,0.11000099603590238]
["Wind","WA/OR",11,22,0.11909251667961129]
["Wind","WA/OR",11,23,0.16000099728877773]
["Wind","WA/OR",11,24,0.2200010398865396]
["Wind","WA/OR",12,1,0.31122368664615985]
["Wind","WA/OR",12,2,0.300612383728108]
["Wind","WA/OR",12,3,0.32244647609124077]
["Wind","WA/OR",12,4,0.29061230521833104]
["Wind","WA/OR",12,5,0.26061244713783349]
["Wind","WA/OR",12,6,0.27000103988653956]
["Wind","WA/OR",12,7,0.26061244713783349]
["Wind","WA/OR",12,8,0.26000109000155353]
["Wind","WA/OR",12,9,0.25061237962489386]
["Wind","WA/OR",12,10,0.26000109000155353]
["Wind","WA/OR",12,11,0.26000109000155353]
["Wind","WA/OR",12,12,0.2200010398865396]
["Wind","WA/OR",12,13,0.17061239091163447]
["Wind","WA/OR",12,14,0.1400010348750382]
["Wind","WA/OR",12,15,0.15000099728877775]
["Wind","WA/OR",12,16,0.13244645207330155]
["Wind","WA/OR",12,17,0.17000103362216287]
["Wind","WA/OR",12,18,0.19000105993254515]
["Wind","WA/OR",12,19,0.15061235748889021]
["Wind","WA/OR",12,20,0.16000099728877773]
["Wind","WA/OR",12,21,0.17183511276717986]
["Wind","WA/OR",12,22,0.16061235971016877]
["Wind","WA/OR",12,23,0.2200010398865396]
["Wind","WA/OR",12,24,0.26000109000155353]
["OhmConnect","PGE",1,1,0]
["OhmConnect","PGE",1,2,0]
["OhmConnect","PGE",1,3,0]
["OhmConnect","PGE",1,4,0]
["OhmConnect","PGE",1,5,0]
["OhmConnect","PGE",1,6,0]
["OhmConnect","PGE",1,7,0]
["OhmConnect","PGE",1,8,0]
["OhmConnect","PGE",1,9,0]
["OhmConnect","PGE",1,10,0]
["OhmConnect","PGE",1,11,0]
["OhmConnect","PGE",1,12,0]
["OhmConnect","PGE",1,13,0]
["OhmConnect","PGE",1,14,0]
["OhmConnect","PGE",1,15,0]
["OhmConnect","PGE",1,16,0]
["OhmConnect","PGE",1,17,1.1441647597253992]
["OhmConnect","PGE",1,18,1.0983981693363878]
["OhmConnect","PGE",1,19,1.0297482837528613]
["OhmConnect","PGE",1,20,0.98398169336384045]
["OhmConnect","PGE",1,21,0.74370709382151046]
["OhmConnect","PGE",1,22,0]
["OhmConnect","PGE",1,23,0]
["OhmConnect","PGE",1,24,0]
["OhmConnect","PGE",2,1,0]
["OhmConnect","PGE",2,2,0]
["OhmConnect","PGE",2,3,0]
["OhmConnect","PGE",2,4,0]
["OhmConnect","PGE",2,5,0]
["OhmConnect","PGE",2,6,0]
["OhmConnect","PGE",2,7,0]
["OhmConnect","PGE",2,8,0]
["OhmConnect","PGE",2,9,0]
["OhmConnect","PGE",2,10,0]
["OhmConnect","PGE",2,11,0]
["OhmConnect","PGE",2,12,0]
["OhmConnect","PGE",2,13,0]
["OhmConnect","PGE",2,14,0]
["OhmConnect","PGE",2,15,0]
["OhmConnect","PGE",2,16,0]
["OhmConnect","PGE",2,17,1.1441647597253992]
["OhmConnect","PGE",2,18,1.0983981693363878]
["OhmConnect","PGE",2,19,1.0297482837528613]
["OhmConnect","PGE",2,20,0.98398169336384045]
["OhmConnect","PGE",2,21,0.74370709382151046]
["OhmConnect","PGE",2,22,0]
["OhmConnect","PGE",2,23,0]
["OhmConnect","PGE",2,24,0]
["OhmConnect","PGE",3,1,0]
["OhmConnect","PGE",3,2,0]
["OhmConnect","PGE",3,3,0]
["OhmConnect","PGE",3,4,0]
["OhmConnect","PGE",3,5,0]
["OhmConnect","PGE",3,6,0]
["OhmConnect","PGE",3,7,0]
["OhmConnect","PGE",3,8,0]
["OhmConnect","PGE",3,9,0]
["OhmConnect","PGE",3,10,0]
["OhmConnect","PGE",3,11,0]
["OhmConnect","PGE",3,12,0]
["OhmConnect","PGE",3,13,0]
["OhmConnect","PGE",3,14,0]
["OhmConnect","PGE",3,15,0]
["OhmConnect","PGE",3,16,0]
["OhmConnect","PGE",3,17,0]
["OhmConnect","PGE",3,18,1.1441647597254057]
["OhmConnect","PGE",3,19,1.0983981693363847]
["OhmConnect","PGE",3,20,1.0297482837528598]
["OhmConnect","PGE",3,21,0.98398169336384422]
["OhmConnect","PGE",3,22,0.74370709382151057]
["OhmConnect","PGE",3,23,0]
["OhmConnect","PGE",3,24,0]
["OhmConnect","PGE",4,1,0]
["OhmConnect","PGE",4,2,0]
["OhmConnect","PGE",4,3,0]
["OhmConnect","PGE",4,4,0]
["OhmConnect","PGE",4,5,0]
["OhmConnect","PGE",4,6,0]
["OhmConnect","PGE",4,7,0]
["OhmConnect","PGE",4,8,0]
["OhmConnect","PGE",4,9,0]
["OhmConnect","PGE",4,10,0]
["OhmConnect","PGE",4,11,0]
["OhmConnect","PGE",4,12,0]
["OhmConnect","PGE",4,13,0]
["OhmConnect","PGE",4,14,0]
["OhmConnect","PGE",4,15,0]
["OhmConnect","PGE",4,16,0]
["OhmConnect","PGE",4,17,0]
["OhmConnect","PGE",4,18,1.1441647597254057]
["OhmConnect","PGE",4,19,1.0983981693363847]
["OhmConnect","PGE",4,20,1.0297482837528598]
["OhmConnect","PGE",4,21,0.98398169336384422]
["OhmConnect","PGE",4,22,0.74370709382151057]
["OhmConnect","PGE",4,23,0]
["OhmConnect","PGE",4,24,0]
["OhmConnect","PGE",5,1,0]
["OhmConnect","PGE",5,2,0]
["OhmConnect","PGE",5,3,0]
["OhmConnect","PGE",5,4,0]
["OhmConnect","PGE",5,5,0]
["OhmConnect","PGE",5,6,0]
["OhmConnect","PGE",5,7,0]
["OhmConnect","PGE",5,8,0]
["OhmConnect","PGE",5,9,0]
["OhmConnect","PGE",5,10,0]
["OhmConnect","PGE",5,11,0]
["OhmConnect","PGE",5,12,0]
["OhmConnect","PGE",5,13,0]
["OhmConnect","PGE",5,14,0]
["OhmConnect","PGE",5,15,0]
["OhmConnect","PGE",5,16,0]
["OhmConnect","PGE",5,17,0]
["OhmConnect","PGE",5,18,1.1441647597254057]
["OhmConnect","PGE",5,19,1.0983981693363847]
["OhmConnect","PGE",5,20,1.0297482837528598]
["OhmConnect","PGE",5,21,0.98398169336384422]
["OhmConnect","PGE",5,22,0.74370709382151057]
["OhmConnect","PGE",5,23,0]
["OhmConnect","PGE",5,24,0]
["OhmConnect","PGE",6,1,0]
["OhmConnect","PGE",6,2,0]
["OhmConnect","PGE",6,3,0]
["OhmConnect","PGE",6,4,0]
["OhmConnect","PGE",6,5,0]
["OhmConnect","PGE",6,6,0]
["OhmConnect","PGE",6,7,0]
["OhmConnect","PGE",6,8,0]
["OhmConnect","PGE",6,9,0]
["OhmConnect","PGE",6,10,0]
["OhmConnect","PGE",6,11,0]
["OhmConnect","PGE",6,12,0]
["OhmConnect","PGE",6,13,0]
["OhmConnect","PGE",6,14,0]
["OhmConnect","PGE",6,15,0]
["OhmConnect","PGE",6,16,0]
["OhmConnect","PGE",6,17,1.1441647597253992]
["OhmConnect","PGE",6,18,1.0983981693363878]
["OhmConnect","PGE",6,19,1.0297482837528613]
["OhmConnect","PGE",6,20,0.98398169336384045]
["OhmConnect","PGE",6,21,0.74370709382151046]
["OhmConnect","PGE",6,22,0]
["OhmConnect","PGE",6,23,0]
["OhmConnect","PGE",6,24,0]
["OhmConnect","PGE",7,1,0]
["OhmConnect","PGE",7,2,0]
["OhmConnect","PGE",7,3,0]
["OhmConnect","PGE",7,4,0]
["OhmConnect","PGE",7,5,0]
["OhmConnect","PGE",7,6,0]
["OhmConnect","PGE",7,7,0]
["OhmConnect","PGE",7,8,0]
["OhmConnect","PGE",7,9,0]
["OhmConnect","PGE",7,10,0]
["OhmConnect","PGE",7,11,0]
["OhmConnect","PGE",7,12,0]
["OhmConnect","PGE",7,13,0]
["OhmConnect","PGE",7,14,0]
["OhmConnect","PGE",7,15,0]
["OhmConnect","PGE",7,16,0]
["OhmConnect","PGE",7,17,1.1441647597253992]
["OhmConnect","PGE",7,18,1.0983981693363878]
["OhmConnect","PGE",7,19,1.0297482837528613]
["OhmConnect","PGE",7,20,0.98398169336384045]
["OhmConnect","PGE",7,21,0.74370709382151046]
["OhmConnect","PGE",7,22,0]
["OhmConnect","PGE",7,23,0]
["OhmConnect","PGE",7,24,0]
["OhmConnect","PGE",8,1,0]
["OhmConnect","PGE",8,2,0]
["OhmConnect","PGE",8,3,0]
["OhmConnect","PGE",8,4,0]
["OhmConnect","PGE",8,5,0]
["OhmConnect","PGE",8,6,0]
["OhmConnect","PGE",8,7,0]
["OhmConnect","PGE",8,8,0]
["OhmConnect","PGE",8,9,0]
["OhmConnect","PGE",8,10,0]
["OhmConnect","PGE",8,11,0]
["OhmConnect","PGE",8,12,0]
["OhmConnect","PGE",8,13,0]
["OhmConnect","PGE",8,14,0]
["OhmConnect","PGE",8,15,0]
["OhmConnect","PGE",8,16,0]
["OhmConnect","PGE",8,17,1.1441647597253992]
["OhmConnect","PGE",8,18,1.0983981693363878]
["OhmConnect","PGE",8,19,1.0297482837528613]
["OhmConnect","PGE",8,20,0.98398169336384045]
["OhmConnect","PGE",8,21,0.74370709382151046]
["OhmConnect","PGE",8,22,0]
["OhmConnect","PGE",8,23,0]
["OhmConnect","PGE",8,24,0]
["OhmConnect","PGE",9,1,0]
["OhmConnect","PGE",9,2,0]
["OhmConnect","PGE",9,3,0]
["OhmConnect","PGE",9,4,0]
["OhmConnect","PGE",9,5,0]
["OhmConnect","PGE",9,6,0]
["OhmConnect","PGE",9,7,0]
["OhmConnect","PGE",9,8,0]
["OhmConnect","PGE",9,9,0]
["OhmConnect","PGE",9,10,0]
["OhmConnect","PGE",9,11,0]
["OhmConnect","PGE",9,12,0]
["OhmConnect","PGE",9,13,0]
["OhmConnect","PGE",9,14,0]
["OhmConnect","PGE",9,15,0]
["OhmConnect","PGE",9,16,0]
["OhmConnect","PGE",9,17,1.1441647597253992]
["OhmConnect","PGE",9,18,1.0983981693363878]
["OhmConnect","PGE",9,19,1.0297482837528613]
["OhmConnect","PGE",9,20,0.98398169336384045]
["OhmConnect","PGE",9,21,0.74370709382151046]
["OhmConnect","PGE",9,22,0]
["OhmConnect","PGE",9,23,0]
["OhmConnect","PGE",9,24,0]
["OhmConnect","PGE",10,1,0]
["OhmConnect","PGE",10,2,0]
["OhmConnect","PGE",10,3,0]
["OhmConnect","PGE",10,4,0]
["OhmConnect","PGE",10,5,0]
["OhmConnect","PGE",10,6,0]
["OhmConnect","PGE",10,7,0]
["OhmConnect","PGE",10,8,0]
["OhmConnect","PGE",10,9,0]
["OhmConnect","PGE",10,10,0]
["OhmConnect","PGE",10,11,0]
["OhmConnect","PGE",10,12,0]
["OhmConnect","PGE",10,13,0]
["OhmConnect","PGE",10,14,0]
["OhmConnect","PGE",10,15,0]
["OhmConnect","PGE",10,16,0]
["OhmConnect","PGE",10,17,1.1441647597253992]
["OhmConnect","PGE",10,18,1.0983981693363878]
["OhmConnect","PGE",10,19,1.0297482837528613]
["OhmConnect","PGE",10,20,0.98398169336384045]
["OhmConnect","PGE",10,21,0.74370709382151046]
["OhmConnect","PGE",10,22,0]
["OhmConnect","PGE",10,23,0]
["OhmConnect","PGE",10,24,0]
["OhmConnect","PGE",11,1,0]
["OhmConnect","PGE",11,2,0]
["OhmConnect","PGE",11,3,0]
["OhmConnect","PGE",11,4,0]
["OhmConnect","PGE",11,5,0]
["OhmConnect","PGE",11,6,0]
["OhmConnect","PGE",11,7,0]
["OhmConnect","PGE",11,8,0]
["OhmConnect","PGE",11,9,0]
["OhmConnect","PGE",11,10,0]
["OhmConnect","PGE",11,11,0]
["OhmConnect","PGE",11,12,0]
["OhmConnect","PGE",11,13,0]
["OhmConnect","PGE",11,14,0]
["OhmConnect","PGE",11,15,0]
["OhmConnect","PGE",11,16,0]
["OhmConnect","PGE",11,17,1.1441647597253992]
["OhmConnect","PGE",11,18,1.0983981693363878]
["OhmConnect","PGE",11,19,1.0297482837528613]
["OhmConnect","PGE",11,20,0.98398169336384045]
["OhmConnect","PGE",11,21,0.74370709382151046]
["OhmConnect","PGE",11,22,0]
["OhmConnect","PGE",11,23,0]
["OhmConnect","PGE",11,24,0]
["OhmConnect","PGE",12,1,0]
["OhmConnect","PGE",12,2,0]
["OhmConnect","PGE",12,3,0]
["OhmConnect","PGE",12,4,0]
["OhmConnect","PGE",12,5,0]
["OhmConnect","PGE",12,6,0]
["OhmConnect","PGE",12,7,0]
["OhmConnect","PGE",12,8,0]
["OhmConnect","PGE",12,9,0]
["OhmConnect","PGE",12,10,0]
["OhmConnect","PGE",12,11,0]
["OhmConnect","PGE",12,12,0]
["OhmConnect","PGE",12,13,0]
["OhmConnect","PGE",12,14,0]
["OhmConnect","PGE",12,15,0]
["OhmConnect","PGE",12,16,0]
["OhmConnect","PGE",12,17,1.1441647597253992]
["OhmConnect","PGE",12,18,1.0983981693363878]
["OhmConnect","PGE",12,19,1.0297482837528613]
["OhmConnect","PGE",12,20,0.98398169336384045]
["OhmConnect","PGE",12,21,0.74370709382151046]
["OhmConnect","PGE",12,22,0]
["OhmConnect","PGE",12,23,0]
["OhmConnect","PGE",12,24,0]
["OhmConnect","SCE",1,1,0]
["OhmConnect","SCE",1,2,0]
["OhmConnect","SCE",1,3,0]
["OhmConnect","SCE",1,4,0]
["OhmConnect","SCE",1,5,0]
["OhmConnect","SCE",1,6,0]
["OhmConnect","SCE",1,7,0]
["OhmConnect","SCE",1,8,0]
["OhmConnect","SCE",1,9,0]
["OhmConnect","SCE",1,10,0]
["OhmConnect","SCE",1,11,0]
["OhmConnect","SCE",1,12,0]
["OhmConnect","SCE",1,13,0]
["OhmConnect","SCE",1,14,0]
["OhmConnect","SCE",1,15,0]
["OhmConnect","SCE",1,16,0]
["OhmConnect","SCE",1,17,1.1441647597253992]
["OhmConnect","SCE",1,18,1.0983981693363878]
["OhmConnect","SCE",1,19,1.0297482837528613]
["OhmConnect","SCE",1,20,0.98398169336384045]
["OhmConnect","SCE",1,21,0.74370709382151046]
["OhmConnect","SCE",1,22,0]
["OhmConnect","SCE",1,23,0]
["OhmConnect","SCE",1,24,0]
["OhmConnect","SCE",2,1,0]
["OhmConnect","SCE",2,2,0]
["OhmConnect","SCE",2,3,0]
["OhmConnect","SCE",2,4,0]
["OhmConnect","SCE",2,5,0]
["OhmConnect","SCE",2,6,0]
["OhmConnect","SCE",2,7,0]
["OhmConnect","SCE",2,8,0]
["OhmConnect","SCE",2,9,0]
["OhmConnect","SCE",2,10,0]
["OhmConnect","SCE",2,11,0]
["OhmConnect","SCE",2,12,0]
["OhmConnect","SCE",2,13,0]
["OhmConnect","SCE",2,14,0]
["OhmConnect","SCE",2,15,0]
["OhmConnect","SCE",2,16,0]
["OhmConnect","SCE",2,17,1.1441647597253992]
["OhmConnect","SCE",2,18,1.0983981693363878]
["OhmConnect","SCE",2,19,1.0297482837528613]
["OhmConnect","SCE",2,20,0.98398169336384045]
["OhmConnect","SCE",2,21,0.74370709382151046]
["OhmConnect","SCE",2,22,0]
["OhmConnect","SCE",2,23,0]
["OhmConnect","SCE",2,24,0]
["OhmConnect","SCE",3,1,0]
["OhmConnect","SCE",3,2,0]
["OhmConnect","SCE",3,3,0]
["OhmConnect","SCE",3,4,0]
["OhmConnect","SCE",3,5,0]
["OhmConnect","SCE",3,6,0]
["OhmConnect","SCE",3,7,0]
["OhmConnect","SCE",3,8,0]
["OhmConnect","SCE",3,9,0]
["OhmConnect","SCE",3,10,0]
["OhmConnect","SCE",3,11,0]
["OhmConnect","SCE",3,12,0]
["OhmConnect","SCE",3,13,0]
["OhmConnect","SCE",3,14,0]
["OhmConnect","SCE",3,15,0]
["OhmConnect","SCE",3,16,0]
["OhmConnect","SCE",3,17,0]
["OhmConnect","SCE",3,18,1.1441647597254057]
["OhmConnect","SCE",3,19,1.0983981693363847]
["OhmConnect","SCE",3,20,1.0297482837528598]
["OhmConnect","SCE",3,21,0.98398169336384422]
["OhmConnect","SCE",3,22,0.74370709382151057]
["OhmConnect","SCE",3,23,0]
["OhmConnect","SCE",3,24,0]
["OhmConnect","SCE",4,1,0]
["OhmConnect","SCE",4,2,0]
["OhmConnect","SCE",4,3,0]
["OhmConnect","SCE",4,4,0]
["OhmConnect","SCE",4,5,0]
["OhmConnect","SCE",4,6,0]
["OhmConnect","SCE",4,7,0]
["OhmConnect","SCE",4,8,0]
["OhmConnect","SCE",4,9,0]
["OhmConnect","SCE",4,10,0]
["OhmConnect","SCE",4,11,0]
["OhmConnect","SCE",4,12,0]
["OhmConnect","SCE",4,13,0]
["OhmConnect","SCE",4,14,0]
["OhmConnect","SCE",4,15,0]
["OhmConnect","SCE",4,16,0]
["OhmConnect","SCE",4,17,0]
["OhmConnect","SCE",4,18,1.1441647597254057]
["OhmConnect","SCE",4,19,1.0983981693363847]
["OhmConnect","SCE",4,20,1.0297482837528598]
["OhmConnect","SCE",4,21,0.98398169336384422]
["OhmConnect","SCE",4,22,0.74370709382151057]
["OhmConnect","SCE",4,23,0]
["OhmConnect","SCE",4,24,0]
["OhmConnect","SCE",5,1,0]
["OhmConnect","SCE",5,2,0]
["OhmConnect","SCE",5,3,0]
["OhmConnect","SCE",5,4,0]
["OhmConnect","SCE",5,5,0]
["OhmConnect","SCE",5,6,0]
["OhmConnect","SCE",5,7,0]
["OhmConnect","SCE",5,8,0]
["OhmConnect","SCE",5,9,0]
["OhmConnect","SCE",5,10,0]
["OhmConnect","SCE",5,11,0]
["OhmConnect","SCE",5,12,0]
["OhmConnect","SCE",5,13,0]
["OhmConnect","SCE",5,14,0]
["OhmConnect","SCE",5,15,0]
["OhmConnect","SCE",5,16,0]
["OhmConnect","SCE",5,17,0]
["OhmConnect","SCE",5,18,1.1441647597254057]
["OhmConnect","SCE",5,19,1.0983981693363847]
["OhmConnect","SCE",5,20,1.0297482837528598]
["OhmConnect","SCE",5,21,0.98398169336384422]
["OhmConnect","SCE",5,22,0.74370709382151057]
["OhmConnect","SCE",5,23,0]
["OhmConnect","SCE",5,24,0]
["OhmConnect","SCE",6,1,0]
["OhmConnect","SCE",6,2,0]
["OhmConnect","SCE",6,3,0]
["OhmConnect","SCE",6,4,0]
["OhmConnect","SCE",6,5,0]
["OhmConnect","SCE",6,6,0]
["OhmConnect","SCE",6,7,0]
["OhmConnect","SCE",6,8,0]
["OhmConnect","SCE",6,9,0]
["OhmConnect","SCE",6,10,0]
["OhmConnect","SCE",6,11,0]
["OhmConnect","SCE",6,12,0]
["OhmConnect","SCE",6,13,0]
["OhmConnect","SCE",6,14,0]
["OhmConnect","SCE",6,15,0]
["OhmConnect","SCE",6,16,0]
["OhmConnect","SCE",6,17,1.1441647597253992]
["OhmConnect","SCE",6,18,1.0983981693363878]
["OhmConnect","SCE",6,19,1.0297482837528613]
["OhmConnect","SCE",6,20,0.98398169336384045]
["OhmConnect","SCE",6,21,0.74370709382151046]
["OhmConnect","SCE",6,22,0]
["OhmConnect","SCE",6,23,0]
["OhmConnect","SCE",6,24,0]
["OhmConnect","SCE",7,1,0]
["OhmConnect","SCE",7,2,0]
["OhmConnect","SCE",7,3,0]
["OhmConnect","SCE",7,4,0]
["OhmConnect","SCE",7,5,0]
["OhmConnect","SCE",7,6,0]
["OhmConnect","SCE",7,7,0]
["OhmConnect","SCE",7,8,0]
["OhmConnect","SCE",7,9,0]
["OhmConnect","SCE",7,10,0]
["OhmConnect","SCE",7,11,0]
["OhmConnect","SCE",7,12,0]
["OhmConnect","SCE",7,13,0]
["OhmConnect","SCE",7,14,0]
["OhmConnect","SCE",7,15,0]
["OhmConnect","SCE",7,16,0]
["OhmConnect","SCE",7,17,1.1441647597253992]
["OhmConnect","SCE",7,18,1.0983981693363878]
["OhmConnect","SCE",7,19,1.0297482837528613]
["OhmConnect","SCE",7,20,0.98398169336384045]
["OhmConnect","SCE",7,21,0.74370709382151046]
["OhmConnect","SCE",7,22,0]
["OhmConnect","SCE",7,23,0]
["OhmConnect","SCE",7,24,0]
["OhmConnect","SCE",8,1,0]
["OhmConnect","SCE",8,2,0]
["OhmConnect","SCE",8,3,0]
["OhmConnect","SCE",8,4,0]
["OhmConnect","SCE",8,5,0]
["OhmConnect","SCE",8,6,0]
["OhmConnect","SCE",8,7,0]
["OhmConnect","SCE",8,8,0]
["OhmConnect","SCE",8,9,0]
["OhmConnect","SCE",8,10,0]
["OhmConnect","SCE",8,11,0]
["OhmConnect","SCE",8,12,0]
["OhmConnect","SCE",8,13,0]
["OhmConnect","SCE",8,14,0]
["OhmConnect","SCE",8,15,0]
["OhmConnect","SCE",8,16,0]
["OhmConnect","SCE",8,17,1.1441647597253992]
["OhmConnect","SCE",8,18,1.0983981693363878]
["OhmConnect","SCE",8,19,1.0297482837528613]
["OhmConnect","SCE",8,20,0.98398169336384045]
["OhmConnect","SCE",8,21,0.74370709382151046]
["OhmConnect","SCE",8,22,0]
["OhmConnect","SCE",8,23,0]
["OhmConnect","SCE",8,24,0]
["OhmConnect","SCE",9,1,0]
["OhmConnect","SCE",9,2,0]
["OhmConnect","SCE",9,3,0]
["OhmConnect","SCE",9,4,0]
["OhmConnect","SCE",9,5,0]
["OhmConnect","SCE",9,6,0]
["OhmConnect","SCE",9,7,0]
["OhmConnect","SCE",9,8,0]
["OhmConnect","SCE",9,9,0]
["OhmConnect","SCE",9,10,0]
["OhmConnect","SCE",9,11,0]
["OhmConnect","SCE",9,12,0]
["OhmConnect","SCE",9,13,0]
["OhmConnect","SCE",9,14,0]
["OhmConnect","SCE",9,15,0]
["OhmConnect","SCE",9,16,0]
["OhmConnect","SCE",9,17,1.1441647597253992]
["OhmConnect","SCE",9,18,1.0983981693363878]
["OhmConnect","SCE",9,19,1.0297482837528613]
["OhmConnect","SCE",9,20,0.98398169336384045]
["OhmConnect","SCE",9,21,0.74370709382151046]
["OhmConnect","SCE",9,22,0]
["OhmConnect","SCE",9,23,0]
["OhmConnect","SCE",9,24,0]
["OhmConnect","SCE",10,1,0]
["OhmConnect","SCE",10,2,0]
["OhmConnect","SCE",10,3,0]
["OhmConnect","SCE",10,4,0]
["OhmConnect","SCE",10,5,0]
["OhmConnect","SCE",10,6,0]
["OhmConnect","SCE",10,7,0]
["OhmConnect","SCE",10,8,0]
["OhmConnect","SCE",10,9,0]
["OhmConnect","SCE",10,10,0]
["OhmConnect","SCE",10,11,0]
["OhmConnect","SCE",10,12,0]
["OhmConnect","SCE",10,13,0]
["OhmConnect","SCE",10,14,0]
["OhmConnect","SCE",10,15,0]
["OhmConnect","SCE",10,16,0]
["OhmConnect","SCE",10,17,1.1441647597253992]
["OhmConnect","SCE",10,18,1.0983981693363878]
["OhmConnect","SCE",10,19,1.0297482837528613]
["OhmConnect","SCE",10,20,0.98398169336384045]
["OhmConnect","SCE",10,21,0.74370709382151046]
["OhmConnect","SCE",10,22,0]
["OhmConnect","SCE",10,23,0]
["OhmConnect","SCE",10,24,0]
["OhmConnect","SCE",11,1,0]
["OhmConnect","SCE",11,2,0]
["OhmConnect","SCE",11,3,0]
["OhmConnect","SCE",11,4,0]
["OhmConnect","SCE",11,5,0]
["OhmConnect","SCE",11,6,0]
["OhmConnect","SCE",11,7,0]
["OhmConnect","SCE",11,8,0]
["OhmConnect","SCE",11,9,0]
["OhmConnect","SCE",11,10,0]
["OhmConnect","SCE",11,11,0]
["OhmConnect","SCE",11,12,0]
["OhmConnect","SCE",11,13,0]
["OhmConnect","SCE",11,14,0]
["OhmConnect","SCE",11,15,0]
["OhmConnect","SCE",11,16,0]
["OhmConnect","SCE",11,17,1.1441647597253992]
["OhmConnect","SCE",11,18,1.0983981693363878]
["OhmConnect","SCE",11,19,1.0297482837528613]
["OhmConnect","SCE",11,20,0.98398169336384045]
["OhmConnect","SCE",11,21,0.74370709382151046]
["OhmConnect","SCE",11,22,0]
["OhmConnect","SCE",11,23,0]
["OhmConnect","SCE",11,24,0]
["OhmConnect","SCE",12,1,0]
["OhmConnect","SCE",12,2,0]
["OhmConnect","SCE",12,3,0]
["OhmConnect","SCE",12,4,0]
["OhmConnect","SCE",12,5,0]
["OhmConnect","SCE",12,6,0]
["OhmConnect","SCE",12,7,0]
["OhmConnect","SCE",12,8,0]
["OhmConnect","SCE",12,9,0]
["OhmConnect","SCE",12,10,0]
["OhmConnect","SCE",12,11,0]
["OhmConnect","SCE",12,12,0]
["OhmConnect","SCE",12,13,0]
["OhmConnect","SCE",12,14,0]
["OhmConnect","SCE",12,15,0]
["OhmConnect","SCE",12,16,0]
["OhmConnect","SCE",12,17,1.1441647597253992]
["OhmConnect","SCE",12,18,1.0983981693363878]
["OhmConnect","SCE",12,19,1.0297482837528613]
["OhmConnect","SCE",12,20,0.98398169336384045]
["OhmConnect","SCE",12,21,0.74370709382151046]
["OhmConnect","SCE",12,22,0]
["OhmConnect","SCE",12,23,0]
["OhmConnect","SCE",12,24,0]
["OhmConnect","SDGE",1,1,0]
["OhmConnect","SDGE",1,2,0]
["OhmConnect","SDGE",1,3,0]
["OhmConnect","SDGE",1,4,0]
["OhmConnect","SDGE",1,5,0]
["OhmConnect","SDGE",1,6,0]
["OhmConnect","SDGE",1,7,0]
["OhmConnect","SDGE",1,8,0]
["OhmConnect","SDGE",1,9,0]
["OhmConnect","SDGE",1,10,0]
["OhmConnect","SDGE",1,11,0]
["OhmConnect","SDGE",1,12,0]
["OhmConnect","SDGE",1,13,0]
["OhmConnect","SDGE",1,14,0]
["OhmConnect","SDGE",1,15,0]
["OhmConnect","SDGE",1,16,0]
["OhmConnect","SDGE",1,17,1.1441647597253992]
["OhmConnect","SDGE",1,18,1.0983981693363878]
["OhmConnect","SDGE",1,19,1.0297482837528613]
["OhmConnect","SDGE",1,20,0.98398169336384045]
["OhmConnect","SDGE",1,21,0.74370709382151046]
["OhmConnect","SDGE",1,22,0]
["OhmConnect","SDGE",1,23,0]
["OhmConnect","SDGE",1,24,0]
["OhmConnect","SDGE",2,1,0]
["OhmConnect","SDGE",2,2,0]
["OhmConnect","SDGE",2,3,0]
["OhmConnect","SDGE",2,4,0]
["OhmConnect","SDGE",2,5,0]
["OhmConnect","SDGE",2,6,0]
["OhmConnect","SDGE",2,7,0]
["OhmConnect","SDGE",2,8,0]
["OhmConnect","SDGE",2,9,0]
["OhmConnect","SDGE",2,10,0]
["OhmConnect","SDGE",2,11,0]
["OhmConnect","SDGE",2,12,0]
["OhmConnect","SDGE",2,13,0]
["OhmConnect","SDGE",2,14,0]
["OhmConnect","SDGE",2,15,0]
["OhmConnect","SDGE",2,16,0]
["OhmConnect","SDGE",2,17,1.1441647597253992]
["OhmConnect","SDGE",2,18,1.0983981693363878]
["OhmConnect","SDGE",2,19,1.0297482837528613]
["OhmConnect","SDGE",2,20,0.98398169336384045]
["OhmConnect","SDGE",2,21,0.74370709382151046]
["OhmConnect","SDGE",2,22,0]
["OhmConnect","SDGE",2,23,0]
["OhmConnect","SDGE",2,24,0]
["OhmConnect","SDGE",3,1,0]
["OhmConnect","SDGE",3,2,0]
["OhmConnect","SDGE",3,3,0]
["OhmConnect","SDGE",3,4,0]
["OhmConnect","SDGE",3,5,0]
["OhmConnect","SDGE",3,6,0]
["OhmConnect","SDGE",3,7,0]
["OhmConnect","SDGE",3,8,0]
["OhmConnect","SDGE",3,9,0]
["OhmConnect","SDGE",3,10,0]
["OhmConnect","SDGE",3,11,0]
["OhmConnect","SDGE",3,12,0]
["OhmConnect","SDGE",3,13,0]
["OhmConnect","SDGE",3,14,0]
["OhmConnect","SDGE",3,15,0]
["OhmConnect","SDGE",3,16,0]
["OhmConnect","SDGE",3,17,0]
["OhmConnect","SDGE",3,18,1.1441647597254057]
["OhmConnect","SDGE",3,19,1.0983981693363847]
["OhmConnect","SDGE",3,20,1.0297482837528598]
["OhmConnect","SDGE",3,21,0.98398169336384422]
["OhmConnect","SDGE",3,22,0.74370709382151057]
["OhmConnect","SDGE",3,23,0]
["OhmConnect","SDGE",3,24,0]
["OhmConnect","SDGE",4,1,0]
["OhmConnect","SDGE",4,2,0]
["OhmConnect","SDGE",4,3,0]
["OhmConnect","SDGE",4,4,0]
["OhmConnect","SDGE",4,5,0]
["OhmConnect","SDGE",4,6,0]
["OhmConnect","SDGE",4,7,0]
["OhmConnect","SDGE",4,8,0]
["OhmConnect","SDGE",4,9,0]
["OhmConnect","SDGE",4,10,0]
["OhmConnect","SDGE",4,11,0]
["OhmConnect","SDGE",4,12,0]
["OhmConnect","SDGE",4,13,0]
["OhmConnect","SDGE",4,14,0]
["OhmConnect","SDGE",4,15,0]
["OhmConnect","SDGE",4,16,0]
["OhmConnect","SDGE",4,17,0]
["OhmConnect","SDGE",4,18,1.1441647597254057]
["OhmConnect","SDGE",4,19,1.0983981693363847]
["OhmConnect","SDGE",4,20,1.0297482837528598]
["OhmConnect","SDGE",4,21,0.98398169336384422]
["OhmConnect","SDGE",4,22,0.74370709382151057]
["OhmConnect","SDGE",4,23,0]
["OhmConnect","SDGE",4,24,0]
["OhmConnect","SDGE",5,1,0]
["OhmConnect","SDGE",5,2,0]
["OhmConnect","SDGE",5,3,0]
["OhmConnect","SDGE",5,4,0]
["OhmConnect","SDGE",5,5,0]
["OhmConnect","SDGE",5,6,0]
["OhmConnect","SDGE",5,7,0]
["OhmConnect","SDGE",5,8,0]
["OhmConnect","SDGE",5,9,0]
["OhmConnect","SDGE",5,10,0]
["OhmConnect","SDGE",5,11,0]
["OhmConnect","SDGE",5,12,0]
["OhmConnect","SDGE",5,13,0]
["OhmConnect","SDGE",5,14,0]
["OhmConnect","SDGE",5,15,0]
["OhmConnect","SDGE",5,16,0]
["OhmConnect","SDGE",5,17,0]
["OhmConnect","SDGE",5,18,1.1441647597254057]
["OhmConnect","SDGE",5,19,1.0983981693363847]
["OhmConnect","SDGE",5,20,1.0297482837528598]
["OhmConnect","SDGE",5,21,0.98398169336384422]
["OhmConnect","SDGE",5,22,0.74370709382151057]
["OhmConnect","SDGE",5,23,0]
["OhmConnect","SDGE",5,24,0]
["OhmConnect","SDGE",6,1,0]
["OhmConnect","SDGE",6,2,0]
["OhmConnect","SDGE",6,3,0]
["OhmConnect","SDGE",6,4,0]
["OhmConnect","SDGE",6,5,0]
["OhmConnect","SDGE",6,6,0]
["OhmConnect","SDGE",6,7,0]
["OhmConnect","SDGE",6,8,0]
["OhmConnect","SDGE",6,9,0]
["OhmConnect","SDGE",6,10,0]
["OhmConnect","SDGE",6,11,0]
["OhmConnect","SDGE",6,12,0]
["OhmConnect","SDGE",6,13,0]
["OhmConnect","SDGE",6,14,0]
["OhmConnect","SDGE",6,15,0]
["OhmConnect","SDGE",6,16,0]
["OhmConnect","SDGE",6,17,1.1441647597253992]
["OhmConnect","SDGE",6,18,1.0983981693363878]
["OhmConnect","SDGE",6,19,1.0297482837528613]
["OhmConnect","SDGE",6,20,0.98398169336384045]
["OhmConnect","SDGE",6,21,0.74370709382151046]
["OhmConnect","SDGE",6,22,0]
["OhmConnect","SDGE",6,23,0]
["OhmConnect","SDGE",6,24,0]
["OhmConnect","SDGE",7,1,0]
["OhmConnect","SDGE",7,2,0]
["OhmConnect","SDGE",7,3,0]
["OhmConnect","SDGE",7,4,0]
["OhmConnect","SDGE",7,5,0]
["OhmConnect","SDGE",7,6,0]
["OhmConnect","SDGE",7,7,0]
["OhmConnect","SDGE",7,8,0]
["OhmConnect","SDGE",7,9,0]
["OhmConnect","SDGE",7,10,0]
["OhmConnect","SDGE",7,11,0]
["OhmConnect","SDGE",7,12,0]
["OhmConnect","SDGE",7,13,0]
["OhmConnect","SDGE",7,14,0]
["OhmConnect","SDGE",7,15,0]
["OhmConnect","SDGE",7,16,0]
["OhmConnect","SDGE",7,17,1.1441647597253992]
["OhmConnect","SDGE",7,18,1.0983981693363878]
["OhmConnect","SDGE",7,19,1.0297482837528613]
["OhmConnect","SDGE",7,20,0.98398169336384045]
["OhmConnect","SDGE",7,21,0.74370709382151046]
["OhmConnect","SDGE",7,22,0]
["OhmConnect","SDGE",7,23,0]
["OhmConnect","SDGE",7,24,0]
["OhmConnect","SDGE",8,1,0]
["OhmConnect","SDGE",8,2,0]
["OhmConnect","SDGE",8,3,0]
["OhmConnect","SDGE",8,4,0]
["OhmConnect","SDGE",8,5,0]
["OhmConnect","SDGE",8,6,0]
["OhmConnect","SDGE",8,7,0]
["OhmConnect","SDGE",8,8,0]
["OhmConnect","SDGE",8,9,0]
["OhmConnect","SDGE",8,10,0]
["OhmConnect","SDGE",8,11,0]
["OhmConnect","SDGE",8,12,0]
["OhmConnect","SDGE",8,13,0]
["OhmConnect","SDGE",8,14,0]
["OhmConnect","SDGE",8,15,0]
["OhmConnect","SDGE",8,16,0]
["OhmConnect","SDGE",8,17,1.1441647597253992]
["OhmConnect","SDGE",8,18,1.0983981693363878]
["OhmConnect","SDGE",8,19,1.0297482837528613]
["OhmConnect","SDGE",8,20,0.98398169336384045]
["OhmConnect","SDGE",8,21,0.74370709382151046]
["OhmConnect","SDGE",8,22,0]
["OhmConnect","SDGE",8,23,0]
["OhmConnect","SDGE",8,24,0]
["OhmConnect","SDGE",9,1,0]
["OhmConnect","SDGE",9,2,0]
["OhmConnect","SDGE",9,3,0]
["OhmConnect","SDGE",9,4,0]
["OhmConnect","SDGE",9,5,0]
["OhmConnect","SDGE",9,6,0]
["OhmConnect","SDGE",9,7,0]
["OhmConnect","SDGE",9,8,0]
["OhmConnect","SDGE",9,9,0]
["OhmConnect","SDGE",9,10,0]
["OhmConnect","SDGE",9,11,0]
["OhmConnect","SDGE",9,12,0]
["OhmConnect","SDGE",9,13,0]
["OhmConnect","SDGE",9,14,0]
["OhmConnect","SDGE",9,15,0]
["OhmConnect","SDGE",9,16,0]
["OhmConnect","SDGE",9,17,1.1441647597253992]
["OhmConnect","SDGE",9,18,1.0983981693363878]
["OhmConnect","SDGE",9,19,1.0297482837528613]
["OhmConnect","SDGE",9,20,0.98398169336384045]
["OhmConnect","SDGE",9,21,0.74370709382151046]
["OhmConnect","SDGE",9,22,0]
["OhmConnect","SDGE",9,23,0]
["OhmConnect","SDGE",9,24,0]
["OhmConnect","SDGE",10,1,0]
["OhmConnect","SDGE",10,2,0]
["OhmConnect","SDGE",10,3,0]
["OhmConnect","SDGE",10,4,0]
["OhmConnect","SDGE",10,5,0]
["OhmConnect","SDGE",10,6,0]
["OhmConnect","SDGE",10,7,0]
["OhmConnect","SDGE",10,8,0]
["OhmConnect","SDGE",10,9,0]
["OhmConnect","SDGE",10,10,0]
["OhmConnect","SDGE",10,11,0]
["OhmConnect","SDGE",10,12,0]
["OhmConnect","SDGE",10,13,0]
["OhmConnect","SDGE",10,14,0]
["OhmConnect","SDGE",10,15,0]
["OhmConnect","SDGE",10,16,0]
["OhmConnect","SDGE",10,17,1.1441647597253992]
["OhmConnect","SDGE",10,18,1.0983981693363878]
["OhmConnect","SDGE",10,19,1.0297482837528613]
["OhmConnect","SDGE",10,20,0.98398169336384045]
["OhmConnect","SDGE",10,21,0.74370709382151046]
["OhmConnect","SDGE",10,22,0]
["OhmConnect","SDGE",10,23,0]
["OhmConnect","SDGE",10,24,0]
["OhmConnect","SDGE",11,1,0]
["OhmConnect","SDGE",11,2,0]
["OhmConnect","SDGE",11,3,0]
["OhmConnect","SDGE",11,4,0]
["OhmConnect","SDGE",11,5,0]
["OhmConnect","SDGE",11,6,0]
["OhmConnect","SDGE",11,7,0]
["OhmConnect","SDGE",11,8,0]
["OhmConnect","SDGE",11,9,0]
["OhmConnect","SDGE",11,10,0]
["OhmConnect","SDGE",11,11,0]
["OhmConnect","SDGE",11,12,0]
["OhmConnect","SDGE",11,13,0]
["OhmConnect","SDGE",11,14,0]
["OhmConnect","SDGE",11,15,0]
["OhmConnect","SDGE",11,16,0]
["OhmConnect","SDGE",11,17,1.1441647597253992]
["OhmConnect","SDGE",11,18,1.0983981693363878]
["OhmConnect","SDGE",11,19,1.0297482837528613]
["OhmConnect","SDGE",11,20,0.98398169336384045]
["OhmConnect","SDGE",11,21,0.74370709382151046]
["OhmConnect","SDGE",11,22,0]
["OhmConnect","SDGE",11,23,0]
["OhmConnect","SDGE",11,24,0]
["OhmConnect","SDGE",12,1,0]
["OhmConnect","SDGE",12,2,0]
["OhmConnect","SDGE",12,3,0]
["OhmConnect","SDGE",12,4,0]
["OhmConnect","SDGE",12,5,0]
["OhmConnect","SDGE",12,6,0]
["OhmConnect","SDGE",12,7,0]
["OhmConnect","SDGE",12,8,0]
["OhmConnect","SDGE",12,9,0]
["OhmConnect","SDGE",12,10,0]
["OhmConnect","SDGE",12,11,0]
["OhmConnect","SDGE",12,12,0]
["OhmConnect","SDGE",12,13,0]
["OhmConnect","SDGE",12,14,0]
["OhmConnect","SDGE",12,15,0]
["OhmConnect","SDGE",12,16,0]
["OhmConnect","SDGE",12,17,1.1441647597253992]
["OhmConnect","SDGE",12,18,1.0983981693363878]
["OhmConnect","SDGE",12,19,1.0297482837528613]
["OhmConnect","SDGE",12,20,0.98398169336384045]
["OhmConnect","SDGE",12,21,0.74370709382151046]
["OhmConnect","SDGE",12,22,0]
["OhmConnect","SDGE",12,23,0]
["OhmConnect","SDGE",12,24,0]
["NexusRenewables","PGE",1,1,0]
["NexusRenewables","PGE",1,2,0]
["NexusRenewables","PGE",1,3,0]
["NexusRenewables","PGE",1,4,0]
["NexusRenewables","PGE",1,5,0]
["NexusRenewables","PGE",1,6,0]
["NexusRenewables","PGE",1,7,0]
["NexusRenewables","PGE",1,8,0]
["NexusRenewables","PGE",1,9,0]
["NexusRenewables","PGE",1,10,0]
["NexusRenewables","PGE",1,11,0]
["NexusRenewables","PGE",1,12,0]
["NexusRenewables","PGE",1,13,0]
["NexusRenewables","PGE",1,14,0]
["NexusRenewables","PGE",1,15,0]
["NexusRenewables","PGE",1,16,0]
["NexusRenewables","PGE",1,17,0]
["NexusRenewables","PGE",1,18,0]
["NexusRenewables","PGE",1,19,0]
["NexusRenewables","PGE",1,20,0]
["NexusRenewables","PGE",1,21,0]
["NexusRenewables","PGE",1,22,0]
["NexusRenewables","PGE",1,23,0]
["NexusRenewables","PGE",1,24,0]
["NexusRenewables","PGE",2,1,0]
["NexusRenewables","PGE",2,2,0]
["NexusRenewables","PGE",2,3,0]
["NexusRenewables","PGE",2,4,0]
["NexusRenewables","PGE",2,5,0]
["NexusRenewables","PGE",2,6,0]
["NexusRenewables","PGE",2,7,0]
["NexusRenewables","PGE",2,8,0]
["NexusRenewables","PGE",2,9,0]
["NexusRenewables","PGE",2,10,0]
["NexusRenewables","PGE",2,11,0]
["NexusRenewables","PGE",2,12,0]
["NexusRenewables","PGE",2,13,0]
["NexusRenewables","PGE",2,14,0]
["NexusRenewables","PGE",2,15,0]
["NexusRenewables","PGE",2,16,0]
["NexusRenewables","PGE",2,17,0]
["NexusRenewables","PGE",2,18,0]
["NexusRenewables","PGE",2,19,0]
["NexusRenewables","PGE",2,20,0]
["NexusRenewables","PGE",2,21,0]
["NexusRenewables","PGE",2,22,0]
["NexusRenewables","PGE",2,23,0]
["NexusRenewables","PGE",2,24,0]
["NexusRenewables","PGE",3,1,0]
["NexusRenewables","PGE",3,2,0]
["NexusRenewables","PGE",3,3,0]
["NexusRenewables","PGE",3,4,0]
["NexusRenewables","PGE",3,5,0]
["NexusRenewables","PGE",3,6,0]
["NexusRenewables","PGE",3,7,0]
["NexusRenewables","PGE",3,8,0]
["NexusRenewables","PGE",3,9,0]
["NexusRenewables","PGE",3,10,0]
["NexusRenewables","PGE",3,11,0]
["NexusRenewables","PGE",3,12,0]
["NexusRenewables","PGE",3,13,0]
["NexusRenewables","PGE",3,14,0]
["NexusRenewables","PGE",3,15,0]
["NexusRenewables","PGE",3,16,0]
["NexusRenewables","PGE",3,17,0]
["NexusRenewables","PGE",3,18,1]
["NexusRenewables","PGE",3,19,1]
["NexusRenewables","PGE",3,20,1]
["NexusRenewables","PGE",3,21,1]
["NexusRenewables","PGE",3,22,1]
["NexusRenewables","PGE",3,23,0]
["NexusRenewables","PGE",3,24,0]
["NexusRenewables","PGE",4,1,0]
["NexusRenewables","PGE",4,2,0]
["NexusRenewables","PGE",4,3,0]
["NexusRenewables","PGE",4,4,0]
["NexusRenewables","PGE",4,5,0]
["NexusRenewables","PGE",4,6,0]
["NexusRenewables","PGE",4,7,0]
["NexusRenewables","PGE",4,8,0]
["NexusRenewables","PGE",4,9,0]
["NexusRenewables","PGE",4,10,0]
["NexusRenewables","PGE",4,11,0]
["NexusRenewables","PGE",4,12,0]
["NexusRenewables","PGE",4,13,0]
["NexusRenewables","PGE",4,14,0]
["NexusRenewables","PGE",4,15,0]
["NexusRenewables","PGE",4,16,0]
["NexusRenewables","PGE",4,17,0]
["NexusRenewables","PGE",4,18,1]
["NexusRenewables","PGE",4,19,1]
["NexusRenewables","PGE",4,20,1]
["NexusRenewables","PGE",4,21,1]
["NexusRenewables","PGE",4,22,1]
["NexusRenewables","PGE",4,23,0]
["NexusRenewables","PGE",4,24,0]
["NexusRenewables","PGE",5,1,0]
["NexusRenewables","PGE",5,2,0]
["NexusRenewables","PGE",5,3,0]
["NexusRenewables","PGE",5,4,0]
["NexusRenewables","PGE",5,5,0]
["NexusRenewables","PGE",5,6,0]
["NexusRenewables","PGE",5,7,0]
["NexusRenewables","PGE",5,8,0]
["NexusRenewables","PGE",5,9,0]
["NexusRenewables","PGE",5,10,0]
["NexusRenewables","PGE",5,11,0]
["NexusRenewables","PGE",5,12,0]
["NexusRenewables","PGE",5,13,0]
["NexusRenewables","PGE",5,14,0]
["NexusRenewables","PGE",5,15,0]
["NexusRenewables","PGE",5,16,0]
["NexusRenewables","PGE",5,17,0]
["NexusRenewables","PGE",5,18,1]
["NexusRenewables","PGE",5,19,1]
["NexusRenewables","PGE",5,20,1]
["NexusRenewables","PGE",5,21,1]
["NexusRenewables","PGE",5,22,1]
["NexusRenewables","PGE",5,23,0]
["NexusRenewables","PGE",5,24,0]
["NexusRenewables","PGE",6,1,0]
["NexusRenewables","PGE",6,2,0]
["NexusRenewables","PGE",6,3,0]
["NexusRenewables","PGE",6,4,0]
["NexusRenewables","PGE",6,5,0]
["NexusRenewables","PGE",6,6,0]
["NexusRenewables","PGE",6,7,0]
["NexusRenewables","PGE",6,8,0]
["NexusRenewables","PGE",6,9,0]
["NexusRenewables","PGE",6,10,0]
["NexusRenewables","PGE",6,11,0]
["NexusRenewables","PGE",6,12,0]
["NexusRenewables","PGE",6,13,0]
["NexusRenewables","PGE",6,14,0]
["NexusRenewables","PGE",6,15,0]
["NexusRenewables","PGE",6,16,0]
["NexusRenewables","PGE",6,17,1]
["NexusRenewables","PGE",6,18,1]
["NexusRenewables","PGE",6,19,1]
["NexusRenewables","PGE",6,20,1]
["NexusRenewables","PGE",6,21,1]
["NexusRenewables","PGE",6,22,0]
["NexusRenewables","PGE",6,23,0]
["NexusRenewables","PGE",6,24,0]
["NexusRenewables","PGE",7,1,0]
["NexusRenewables","PGE",7,2,0]
["NexusRenewables","PGE",7,3,0]
["NexusRenewables","PGE",7,4,0]
["NexusRenewables","PGE",7,5,0]
["NexusRenewables","PGE",7,6,0]
["NexusRenewables","PGE",7,7,0]
["NexusRenewables","PGE",7,8,0]
["NexusRenewables","PGE",7,9,0]
["NexusRenewables","PGE",7,10,0]
["NexusRenewables","PGE",7,11,0]
["NexusRenewables","PGE",7,12,0]
["NexusRenewables","PGE",7,13,0]
["NexusRenewables","PGE",7,14,0]
["NexusRenewables","PGE",7,15,0]
["NexusRenewables","PGE",7,16,0]
["NexusRenewables","PGE",7,17,1]
["NexusRenewables","PGE",7,18,1]
["NexusRenewables","PGE",7,19,1]
["NexusRenewables","PGE",7,20,1]
["NexusRenewables","PGE",7,21,1]
["NexusRenewables","PGE",7,22,0]
["NexusRenewables","PGE",7,23,0]
["NexusRenewables","PGE",7,24,0]
["NexusRenewables","PGE",8,1,0]
["NexusRenewables","PGE",8,2,0]
["NexusRenewables","PGE",8,3,0]
["NexusRenewables","PGE",8,4,0]
["NexusRenewables","PGE",8,5,0]
["NexusRenewables","PGE",8,6,0]
["NexusRenewables","PGE",8,7,0]
["NexusRenewables","PGE",8,8,0]
["NexusRenewables","PGE",8,9,0]
["NexusRenewables","PGE",8,10,0]
["NexusRenewables","PGE",8,11,0]
["NexusRenewables","PGE",8,12,0]
["NexusRenewables","PGE",8,13,0]
["NexusRenewables","PGE",8,14,0]
["NexusRenewables","PGE",8,15,0]
["NexusRenewables","PGE",8,16,0]
["NexusRenewables","PGE",8,17,1]
["NexusRenewables","PGE",8,18,1]
["NexusRenewables","PGE",8,19,1]
["NexusRenewables","PGE",8,20,1]
["NexusRenewables","PGE",8,21,1]
["NexusRenewables","PGE",8,22,0]
["NexusRenewables","PGE",8,23,0]
["NexusRenewables","PGE",8,24,0]
["NexusRenewables","PGE",9,1,0]
["NexusRenewables","PGE",9,2,0]
["NexusRenewables","PGE",9,3,0]
["NexusRenewables","PGE",9,4,0]
["NexusRenewables","PGE",9,5,0]
["NexusRenewables","PGE",9,6,0]
["NexusRenewables","PGE",9,7,0]
["NexusRenewables","PGE",9,8,0]
["NexusRenewables","PGE",9,9,0]
["NexusRenewables","PGE",9,10,0]
["NexusRenewables","PGE",9,11,0]
["NexusRenewables","PGE",9,12,0]
["NexusRenewables","PGE",9,13,0]
["NexusRenewables","PGE",9,14,0]
["NexusRenewables","PGE",9,15,0]
["NexusRenewables","PGE",9,16,0]
["NexusRenewables","PGE",9,17,1]
["NexusRenewables","PGE",9,18,1]
["NexusRenewables","PGE",9,19,1]
["NexusRenewables","PGE",9,20,1]
["NexusRenewables","PGE",9,21,1]
["NexusRenewables","PGE",9,22,0]
["NexusRenewables","PGE",9,23,0]
["NexusRenewables","PGE",9,24,0]
["NexusRenewables","PGE",10,1,0]
["NexusRenewables","PGE",10,2,0]
["NexusRenewables","PGE",10,3,0]
["NexusRenewables","PGE",10,4,0]
["NexusRenewables","PGE",10,5,0]
["NexusRenewables","PGE",10,6,0]
["NexusRenewables","PGE",10,7,0]
["NexusRenewables","PGE",10,8,0]
["NexusRenewables","PGE",10,9,0]
["NexusRenewables","PGE",10,10,0]
["NexusRenewables","PGE",10,11,0]
["NexusRenewables","PGE",10,12,0]
["NexusRenewables","PGE",10,13,0]
["NexusRenewables","PGE",10,14,0]
["NexusRenewables","PGE",10,15,0]
["NexusRenewables","PGE",10,16,0]
["NexusRenewables","PGE",10,17,1]
["NexusRenewables","PGE",10,18,1]
["NexusRenewables","PGE",10,19,1]
["NexusRenewables","PGE",10,20,1]
["NexusRenewables","PGE",10,21,1]
["NexusRenewables","PGE",10,22,0]
["NexusRenewables","PGE",10,23,0]
["NexusRenewables","PGE",10,24,0]
["NexusRenewables","PGE",11,1,0]
["NexusRenewables","PGE",11,2,0]
["NexusRenewables","PGE",11,3,0]
["NexusRenewables","PGE",11,4,0]
["NexusRenewables","PGE",11,5,0]
["NexusRenewables","PGE",11,6,0]
["NexusRenewables","PGE",11,7,0]
["NexusRenewables","PGE",11,8,0]
["NexusRenewables","PGE",11,9,0]
["NexusRenewables","PGE",11,10,0]
["NexusRenewables","PGE",11,11,0]
["NexusRenewables","PGE",11,12,0]
["NexusRenewables","PGE",11,13,0]
["NexusRenewables","PGE",11,14,0]
["NexusRenewables","PGE",11,15,0]
["NexusRenewables","PGE",11,16,0]
["NexusRenewables","PGE",11,17,1]
["NexusRenewables","PGE",11,18,1]
["NexusRenewables","PGE",11,19,1]
["NexusRenewables","PGE",11,20,1]
["NexusRenewables","PGE",11,21,1]
["NexusRenewables","PGE",11,22,0]
["NexusRenewables","PGE",11,23,0]
["NexusRenewables","PGE",11,24,0]
["NexusRenewables","PGE",12,1,0]
["NexusRenewables","PGE",12,2,0]
["NexusRenewables","PGE",12,3,0]
["NexusRenewables","PGE",12,4,0]
["NexusRenewables","PGE",12,5,0]
["NexusRenewables","PGE",12,6,0]
["NexusRenewables","PGE",12,7,0]
["NexusRenewables","PGE",12,8,0]
["NexusRenewables","PGE",12,9,0]
["NexusRenewables","PGE",12,10,0]
["NexusRenewables","PGE",12,11,0]
["NexusRenewables","PGE",12,12,0]
["NexusRenewables","PGE",12,13,0]
["NexusRenewables","PGE",12,14,0]
["NexusRenewables","PGE",12,15,0]
["NexusRenewables","PGE",12,16,0]
["NexusRenewables","PGE",12,17,1]
["NexusRenewables","PGE",12,18,1]
["NexusRenewables","PGE",12,19,1]
["NexusRenewables","PGE",12,20,1]
["NexusRenewables","PGE",12,21,1]
["NexusRenewables","PGE",12,22,0]
["NexusRenewables","PGE",12,23,0]
["NexusRenewables","PGE",12,24,0]
["Enersponse","PGE",1,1,0]
["Enersponse","PGE",1,2,0]
["Enersponse","PGE",1,3,0]
["Enersponse","PGE",1,4,0]
["Enersponse","PGE",1,5,0]
["Enersponse","PGE",1,6,0]
["Enersponse","PGE",1,7,0]
["Enersponse","PGE",1,8,0]
["Enersponse","PGE",1,9,0]
["Enersponse","PGE",1,10,0]
["Enersponse","PGE",1,11,0]
["Enersponse","PGE",1,12,0]
["Enersponse","PGE",1,13,0]
["Enersponse","PGE",1,14,0]
["Enersponse","PGE",1,15,0]
["Enersponse","PGE",1,16,0]
["Enersponse","PGE",1,17,0]
["Enersponse","PGE",1,18,0]
["Enersponse","PGE",1,19,0]
["Enersponse","PGE",1,20,0]
["Enersponse","PGE",1,21,0]
["Enersponse","PGE",1,22,0]
["Enersponse","PGE",1,23,0]
["Enersponse","PGE",1,24,0]
["Enersponse","PGE",2,1,0]
["Enersponse","PGE",2,2,0]
["Enersponse","PGE",2,3,0]
["Enersponse","PGE",2,4,0]
["Enersponse","PGE",2,5,0]
["Enersponse","PGE",2,6,0]
["Enersponse","PGE",2,7,0]
["Enersponse","PGE",2,8,0]
["Enersponse","PGE",2,9,0]
["Enersponse","PGE",2,10,0]
["Enersponse","PGE",2,11,0]
["Enersponse","PGE",2,12,0]
["Enersponse","PGE",2,13,0]
["Enersponse","PGE",2,14,0]
["Enersponse","PGE",2,15,0]
["Enersponse","PGE",2,16,0]
["Enersponse","PGE",2,17,0]
["Enersponse","PGE",2,18,0]
["Enersponse","PGE",2,19,0]
["Enersponse","PGE",2,20,0]
["Enersponse","PGE",2,21,0]
["Enersponse","PGE",2,22,0]
["Enersponse","PGE",2,23,0]
["Enersponse","PGE",2,24,0]
["Enersponse","PGE",3,1,0]
["Enersponse","PGE",3,2,0]
["Enersponse","PGE",3,3,0]
["Enersponse","PGE",3,4,0]
["Enersponse","PGE",3,5,0]
["Enersponse","PGE",3,6,0]
["Enersponse","PGE",3,7,0]
["Enersponse","PGE",3,8,0]
["Enersponse","PGE",3,9,0]
["Enersponse","PGE",3,10,0]
["Enersponse","PGE",3,11,0]
["Enersponse","PGE",3,12,0]
["Enersponse","PGE",3,13,0]
["Enersponse","PGE",3,14,0]
["Enersponse","PGE",3,15,0]
["Enersponse","PGE",3,16,0]
["Enersponse","PGE",3,17,0]
["Enersponse","PGE",3,18,0]
["Enersponse","PGE",3,19,0]
["Enersponse","PGE",3,20,0]
["Enersponse","PGE",3,21,0]
["Enersponse","PGE",3,22,0]
["Enersponse","PGE",3,23,0]
["Enersponse","PGE",3,24,0]
["Enersponse","PGE",4,1,0]
["Enersponse","PGE",4,2,0]
["Enersponse","PGE",4,3,0]
["Enersponse","PGE",4,4,0]
["Enersponse","PGE",4,5,0]
["Enersponse","PGE",4,6,0]
["Enersponse","PGE",4,7,0]
["Enersponse","PGE",4,8,0]
["Enersponse","PGE",4,9,0]
["Enersponse","PGE",4,10,0]
["Enersponse","PGE",4,11,0]
["Enersponse","PGE",4,12,0]
["Enersponse","PGE",4,13,0]
["Enersponse","PGE",4,14,0]
["Enersponse","PGE",4,15,0]
["Enersponse","PGE",4,16,0]
["Enersponse","PGE",4,17,0]
["Enersponse","PGE",4,18,1]
["Enersponse","PGE",4,19,1]
["Enersponse","PGE",4,20,1]
["Enersponse","PGE",4,21,1]
["Enersponse","PGE",4,22,1]
["Enersponse","PGE",4,23,0]
["Enersponse","PGE",4,24,0]
["Enersponse","PGE",5,1,0]
["Enersponse","PGE",5,2,0]
["Enersponse","PGE",5,3,0]
["Enersponse","PGE",5,4,0]
["Enersponse","PGE",5,5,0]
["Enersponse","PGE",5,6,0]
["Enersponse","PGE",5,7,0]
["Enersponse","PGE",5,8,0]
["Enersponse","PGE",5,9,0]
["Enersponse","PGE",5,10,0]
["Enersponse","PGE",5,11,0]
["Enersponse","PGE",5,12,0]
["Enersponse","PGE",5,13,0]
["Enersponse","PGE",5,14,0]
["Enersponse","PGE",5,15,0]
["Enersponse","PGE",5,16,0]
["Enersponse","PGE",5,17,0]
["Enersponse","PGE",5,18,1]
["Enersponse","PGE",5,19,1]
["Enersponse","PGE",5,20,1]
["Enersponse","PGE",5,21,1]
["Enersponse","PGE",5,22,1]
["Enersponse","PGE",5,23,0]
["Enersponse","PGE",5,24,0]
["Enersponse","PGE",6,1,0]
["Enersponse","PGE",6,2,0]
["Enersponse","PGE",6,3,0]
["Enersponse","PGE",6,4,0]
["Enersponse","PGE",6,5,0]
["Enersponse","PGE",6,6,0]
["Enersponse","PGE",6,7,0]
["Enersponse","PGE",6,8,0]
["Enersponse","PGE",6,9,0]
["Enersponse","PGE",6,10,0]
["Enersponse","PGE",6,11,0]
["Enersponse","PGE",6,12,0]
["Enersponse","PGE",6,13,0]
["Enersponse","PGE",6,14,0]
["Enersponse","PGE",6,15,0]
["Enersponse","PGE",6,16,0]
["Enersponse","PGE",6,17,1]
["Enersponse","PGE",6,18,1]
["Enersponse","PGE",6,19,1]
["Enersponse","PGE",6,20,1]
["Enersponse","PGE",6,21,1]
["Enersponse","PGE",6,22,0]
["Enersponse","PGE",6,23,0]
["Enersponse","PGE",6,24,0]
["Enersponse","PGE",7,1,0]
["Enersponse","PGE",7,2,0]
["Enersponse","PGE",7,3,0]
["Enersponse","PGE",7,4,0]
["Enersponse","PGE",7,5,0]
["Enersponse","PGE",7,6,0]
["Enersponse","PGE",7,7,0]
["Enersponse","PGE",7,8,0]
["Enersponse","PGE",7,9,0]
["Enersponse","PGE",7,10,0]
["Enersponse","PGE",7,11,0]
["Enersponse","PGE",7,12,0]
["Enersponse","PGE",7,13,0]
["Enersponse","PGE",7,14,0]
["Enersponse","PGE",7,15,0]
["Enersponse","PGE",7,16,0]
["Enersponse","PGE",7,17,1]
["Enersponse","PGE",7,18,1]
["Enersponse","PGE",7,19,1]
["Enersponse","PGE",7,20,1]
["Enersponse","PGE",7,21,1]
["Enersponse","PGE",7,22,0]
["Enersponse","PGE",7,23,0]
["Enersponse","PGE",7,24,0]
["Enersponse","PGE",8,1,0]
["Enersponse","PGE",8,2,0]
["Enersponse","PGE",8,3,0]
["Enersponse","PGE",8,4,0]
["Enersponse","PGE",8,5,0]
["Enersponse","PGE",8,6,0]
["Enersponse","PGE",8,7,0]
["Enersponse","PGE",8,8,0]
["Enersponse","PGE",8,9,0]
["Enersponse","PGE",8,10,0]
["Enersponse","PGE",8,11,0]
["Enersponse","PGE",8,12,0]
["Enersponse","PGE",8,13,0]
["Enersponse","PGE",8,14,0]
["Enersponse","PGE",8,15,0]
["Enersponse","PGE",8,16,0]
["Enersponse","PGE",8,17,1]
["Enersponse","PGE",8,18,1]
["Enersponse","PGE",8,19,1]
["Enersponse","PGE",8,20,1]
["Enersponse","PGE",8,21,1]
["Enersponse","PGE",8,22,0]
["Enersponse","PGE",8,23,0]
["Enersponse","PGE",8,24,0]
["Enersponse","PGE",9,1,0]
["Enersponse","PGE",9,2,0]
["Enersponse","PGE",9,3,0]
["Enersponse","PGE",9,4,0]
["Enersponse","PGE",9,5,0]
["Enersponse","PGE",9,6,0]
["Enersponse","PGE",9,7,0]
["Enersponse","PGE",9,8,0]
["Enersponse","PGE",9,9,0]
["Enersponse","PGE",9,10,0]
["Enersponse","PGE",9,11,0]
["Enersponse","PGE",9,12,0]
["Enersponse","PGE",9,13,0]
["Enersponse","PGE",9,14,0]
["Enersponse","PGE",9,15,0]
["Enersponse","PGE",9,16,0]
["Enersponse","PGE",9,17,1]
["Enersponse","PGE",9,18,1]
["Enersponse","PGE",9,19,1]
["Enersponse","PGE",9,20,1]
["Enersponse","PGE",9,21,1]
["Enersponse","PGE",9,22,0]
["Enersponse","PGE",9,23,0]
["Enersponse","PGE",9,24,0]
["Enersponse","PGE",10,1,0]
["Enersponse","PGE",10,2,0]
["Enersponse","PGE",10,3,0]
["Enersponse","PGE",10,4,0]
["Enersponse","PGE",10,5,0]
["Enersponse","PGE",10,6,0]
["Enersponse","PGE",10,7,0]
["Enersponse","PGE",10,8,0]
["Enersponse","PGE",10,9,0]
["Enersponse","PGE",10,10,0]
["Enersponse","PGE",10,11,0]
["Enersponse","PGE",10,12,0]
["Enersponse","PGE",10,13,0]
["Enersponse","PGE",10,14,0]
["Enersponse","PGE",10,15,0]
["Enersponse","PGE",10,16,0]
["Enersponse","PGE",10,17,1]
["Enersponse","PGE",10,18,1]
["Enersponse","PGE",10,19,1]
["Enersponse","PGE",10,20,1]
["Enersponse","PGE",10,21,1]
["Enersponse","PGE",10,22,0]
["Enersponse","PGE",10,23,0]
["Enersponse","PGE",10,24,0]
["Enersponse","PGE",11,1,0]
["Enersponse","PGE",11,2,0]
["Enersponse","PGE",11,3,0]
["Enersponse","PGE",11,4,0]
["Enersponse","PGE",11,5,0]
["Enersponse","PGE",11,6,0]
["Enersponse","PGE",11,7,0]
["Enersponse","PGE",11,8,0]
["Enersponse","PGE",11,9,0]
["Enersponse","PGE",11,10,0]
["Enersponse","PGE",11,11,0]
["Enersponse","PGE",11,12,0]
["Enersponse","PGE",11,13,0]
["Enersponse","PGE",11,14,0]
["Enersponse","PGE",11,15,0]
["Enersponse","PGE",11,16,0]
["Enersponse","PGE",11,17,1]
["Enersponse","PGE",11,18,1]
["Enersponse","PGE",11,19,1]
["Enersponse","PGE",11,20,1]
["Enersponse","PGE",11,21,1]
["Enersponse","PGE",11,22,0]
["Enersponse","PGE",11,23,0]
["Enersponse","PGE",11,24,0]
["Enersponse","PGE",12,1,0]
["Enersponse","PGE",12,2,0]
["Enersponse","PGE",12,3,0]
["Enersponse","PGE",12,4,0]
["Enersponse","PGE",12,5,0]
["Enersponse","PGE",12,6,0]
["Enersponse","PGE",12,7,0]
["Enersponse","PGE",12,8,0]
["Enersponse","PGE",12,9,0]
["Enersponse","PGE",12,10,0]
["Enersponse","PGE",12,11,0]
["Enersponse","PGE",12,12,0]
["Enersponse","PGE",12,13,0]
["Enersponse","PGE",12,14,0]
["Enersponse","PGE",12,15,0]
["Enersponse","PGE",12,16,0]
["Enersponse","PGE",12,17,1]
["Enersponse","PGE",12,18,1]
["Enersponse","PGE",12,19,1]
["Enersponse","PGE",12,20,1]
["Enersponse","PGE",12,21,1]
["Enersponse","PGE",12,22,0]
["Enersponse","PGE",12,23,0]
["Enersponse","PGE",12,24,0]
["Enersponse","SCE",1,1,0]
["Enersponse","SCE",1,2,0]
["Enersponse","SCE",1,3,0]
["Enersponse","SCE",1,4,0]
["Enersponse","SCE",1,5,0]
["Enersponse","SCE",1,6,0]
["Enersponse","SCE",1,7,0]
["Enersponse","SCE",1,8,0]
["Enersponse","SCE",1,9,0]
["Enersponse","SCE",1,10,0]
["Enersponse","SCE",1,11,0]
["Enersponse","SCE",1,12,0]
["Enersponse","SCE",1,13,0]
["Enersponse","SCE",1,14,0]
["Enersponse","SCE",1,15,0]
["Enersponse","SCE",1,16,0]
["Enersponse","SCE",1,17,1]
["Enersponse","SCE",1,18,1]
["Enersponse","SCE",1,19,1]
["Enersponse","SCE",1,20,1]
["Enersponse","SCE",1,21,1]
["Enersponse","SCE",1,22,0]
["Enersponse","SCE",1,23,0]
["Enersponse","SCE",1,24,0]
["Enersponse","SCE",2,1,0]
["Enersponse","SCE",2,2,0]
["Enersponse","SCE",2,3,0]
["Enersponse","SCE",2,4,0]
["Enersponse","SCE",2,5,0]
["Enersponse","SCE",2,6,0]
["Enersponse","SCE",2,7,0]
["Enersponse","SCE",2,8,0]
["Enersponse","SCE",2,9,0]
["Enersponse","SCE",2,10,0]
["Enersponse","SCE",2,11,0]
["Enersponse","SCE",2,12,0]
["Enersponse","SCE",2,13,0]
["Enersponse","SCE",2,14,0]
["Enersponse","SCE",2,15,0]
["Enersponse","SCE",2,16,0]
["Enersponse","SCE",2,17,1]
["Enersponse","SCE",2,18,1]
["Enersponse","SCE",2,19,1]
["Enersponse","SCE",2,20,1]
["Enersponse","SCE",2,21,1]
["Enersponse","SCE",2,22,0]
["Enersponse","SCE",2,23,0]
["Enersponse","SCE",2,24,0]
["Enersponse","SCE",3,1,0]
["Enersponse","SCE",3,2,0]
["Enersponse","SCE",3,3,0]
["Enersponse","SCE",3,4,0]
["Enersponse","SCE",3,5,0]
["Enersponse","SCE",3,6,0]
["Enersponse","SCE",3,7,0]
["Enersponse","SCE",3,8,0]
["Enersponse","SCE",3,9,0]
["Enersponse","SCE",3,10,0]
["Enersponse","SCE",3,11,0]
["Enersponse","SCE",3,12,0]
["Enersponse","SCE",3,13,0]
["Enersponse","SCE",3,14,0]
["Enersponse","SCE",3,15,0]
["Enersponse","SCE",3,16,0]
["Enersponse","SCE",3,17,0]
["Enersponse","SCE",3,18,1]
["Enersponse","SCE",3,19,1]
["Enersponse","SCE",3,20,1]
["Enersponse","SCE",3,21,1]
["Enersponse","SCE",3,22,1]
["Enersponse","SCE",3,23,0]
["Enersponse","SCE",3,24,0]
["Enersponse","SCE",4,1,0]
["Enersponse","SCE",4,2,0]
["Enersponse","SCE",4,3,0]
["Enersponse","SCE",4,4,0]
["Enersponse","SCE",4,5,0]
["Enersponse","SCE",4,6,0]
["Enersponse","SCE",4,7,0]
["Enersponse","SCE",4,8,0]
["Enersponse","SCE",4,9,0]
["Enersponse","SCE",4,10,0]
["Enersponse","SCE",4,11,0]
["Enersponse","SCE",4,12,0]
["Enersponse","SCE",4,13,0]
["Enersponse","SCE",4,14,0]
["Enersponse","SCE",4,15,0]
["Enersponse","SCE",4,16,0]
["Enersponse","SCE",4,17,0]
["Enersponse","SCE",4,18,1]
["Enersponse","SCE",4,19,1]
["Enersponse","SCE",4,20,1]
["Enersponse","SCE",4,21,1]
["Enersponse","SCE",4,22,1]
["Enersponse","SCE",4,23,0]
["Enersponse","SCE",4,24,0]
["Enersponse","SCE",5,1,0]
["Enersponse","SCE",5,2,0]
["Enersponse","SCE",5,3,0]
["Enersponse","SCE",5,4,0]
["Enersponse","SCE",5,5,0]
["Enersponse","SCE",5,6,0]
["Enersponse","SCE",5,7,0]
["Enersponse","SCE",5,8,0]
["Enersponse","SCE",5,9,0]
["Enersponse","SCE",5,10,0]
["Enersponse","SCE",5,11,0]
["Enersponse","SCE",5,12,0]
["Enersponse","SCE",5,13,0]
["Enersponse","SCE",5,14,0]
["Enersponse","SCE",5,15,0]
["Enersponse","SCE",5,16,0]
["Enersponse","SCE",5,17,0]
["Enersponse","SCE",5,18,1]
["Enersponse","SCE",5,19,1]
["Enersponse","SCE",5,20,1]
["Enersponse","SCE",5,21,1]
["Enersponse","SCE",5,22,1]
["Enersponse","SCE",5,23,0]
["Enersponse","SCE",5,24,0]
["Enersponse","SCE",6,1,0]
["Enersponse","SCE",6,2,0]
["Enersponse","SCE",6,3,0]
["Enersponse","SCE",6,4,0]
["Enersponse","SCE",6,5,0]
["Enersponse","SCE",6,6,0]
["Enersponse","SCE",6,7,0]
["Enersponse","SCE",6,8,0]
["Enersponse","SCE",6,9,0]
["Enersponse","SCE",6,10,0]
["Enersponse","SCE",6,11,0]
["Enersponse","SCE",6,12,0]
["Enersponse","SCE",6,13,0]
["Enersponse","SCE",6,14,0]
["Enersponse","SCE",6,15,0]
["Enersponse","SCE",6,16,0]
["Enersponse","SCE",6,17,1]
["Enersponse","SCE",6,18,1]
["Enersponse","SCE",6,19,1]
["Enersponse","SCE",6,20,1]
["Enersponse","SCE",6,21,1]
["Enersponse","SCE",6,22,0]
["Enersponse","SCE",6,23,0]
["Enersponse","SCE",6,24,0]
["Enersponse","SCE",7,1,0]
["Enersponse","SCE",7,2,0]
["Enersponse","SCE",7,3,0]
["Enersponse","SCE",7,4,0]
["Enersponse","SCE",7,5,0]
["Enersponse","SCE",7,6,0]
["Enersponse","SCE",7,7,0]
["Enersponse","SCE",7,8,0]
["Enersponse","SCE",7,9,0]
["Enersponse","SCE",7,10,0]
["Enersponse","SCE",7,11,0]
["Enersponse","SCE",7,12,0]
["Enersponse","SCE",7,13,0]
["Enersponse","SCE",7,14,0]
["Enersponse","SCE",7,15,0]
["Enersponse","SCE",7,16,0]
["Enersponse","SCE",7,17,1]
["Enersponse","SCE",7,18,1]
["Enersponse","SCE",7,19,1]
["Enersponse","SCE",7,20,1]
["Enersponse","SCE",7,21,1]
["Enersponse","SCE",7,22,0]
["Enersponse","SCE",7,23,0]
["Enersponse","SCE",7,24,0]
["Enersponse","SCE",8,1,0]
["Enersponse","SCE",8,2,0]
["Enersponse","SCE",8,3,0]
["Enersponse","SCE",8,4,0]
["Enersponse","SCE",8,5,0]
["Enersponse","SCE",8,6,0]
["Enersponse","SCE",8,7,0]
["Enersponse","SCE",8,8,0]
["Enersponse","SCE",8,9,0]
["Enersponse","SCE",8,10,0]
["Enersponse","SCE",8,11,0]
["Enersponse","SCE",8,12,0]
["Enersponse","SCE",8,13,0]
["Enersponse","SCE",8,14,0]
["Enersponse","SCE",8,15,0]
["Enersponse","SCE",8,16,0]
["Enersponse","SCE",8,17,1]
["Enersponse","SCE",8,18,1]
["Enersponse","SCE",8,19,1]
["Enersponse","SCE",8,20,1]
["Enersponse","SCE",8,21,1]
["Enersponse","SCE",8,22,0]
["Enersponse","SCE",8,23,0]
["Enersponse","SCE",8,24,0]
["Enersponse","SCE",9,1,0]
["Enersponse","SCE",9,2,0]
["Enersponse","SCE",9,3,0]
["Enersponse","SCE",9,4,0]
["Enersponse","SCE",9,5,0]
["Enersponse","SCE",9,6,0]
["Enersponse","SCE",9,7,0]
["Enersponse","SCE",9,8,0]
["Enersponse","SCE",9,9,0]
["Enersponse","SCE",9,10,0]
["Enersponse","SCE",9,11,0]
["Enersponse","SCE",9,12,0]
["Enersponse","SCE",9,13,0]
["Enersponse","SCE",9,14,0]
["Enersponse","SCE",9,15,0]
["Enersponse","SCE",9,16,0]
["Enersponse","SCE",9,17,1]
["Enersponse","SCE",9,18,1]
["Enersponse","SCE",9,19,1]
["Enersponse","SCE",9,20,1]
["Enersponse","SCE",9,21,1]
["Enersponse","SCE",9,22,0]
["Enersponse","SCE",9,23,0]
["Enersponse","SCE",9,24,0]
["Enersponse","SCE",10,1,0]
["Enersponse","SCE",10,2,0]
["Enersponse","SCE",10,3,0]
["Enersponse","SCE",10,4,0]
["Enersponse","SCE",10,5,0]
["Enersponse","SCE",10,6,0]
["Enersponse","SCE",10,7,0]
["Enersponse","SCE",10,8,0]
["Enersponse","SCE",10,9,0]
["Enersponse","SCE",10,10,0]
["Enersponse","SCE",10,11,0]
["Enersponse","SCE",10,12,0]
["Enersponse","SCE",10,13,0]
["Enersponse","SCE",10,14,0]
["Enersponse","SCE",10,15,0]
["Enersponse","SCE",10,16,0]
["Enersponse","SCE",10,17,1]
["Enersponse","SCE",10,18,1]
["Enersponse","SCE",10,19,1]
["Enersponse","SCE",10,20,1]
["Enersponse","SCE",10,21,1]
["Enersponse","SCE",10,22,0]
["Enersponse","SCE",10,23,0]
["Enersponse","SCE",10,24,0]
["Enersponse","SCE",11,1,0]
["Enersponse","SCE",11,2,0]
["Enersponse","SCE",11,3,0]
["Enersponse","SCE",11,4,0]
["Enersponse","SCE",11,5,0]
["Enersponse","SCE",11,6,0]
["Enersponse","SCE",11,7,0]
["Enersponse","SCE",11,8,0]
["Enersponse","SCE",11,9,0]
["Enersponse","SCE",11,10,0]
["Enersponse","SCE",11,11,0]
["Enersponse","SCE",11,12,0]
["Enersponse","SCE",11,13,0]
["Enersponse","SCE",11,14,0]
["Enersponse","SCE",11,15,0]
["Enersponse","SCE",11,16,0]
["Enersponse","SCE",11,17,1]
["Enersponse","SCE",11,18,1]
["Enersponse","SCE",11,19,1]
["Enersponse","SCE",11,20,1]
["Enersponse","SCE",11,21,1]
["Enersponse","SCE",11,22,0]
["Enersponse","SCE",11,23,0]
["Enersponse","SCE",11,24,0]
["Enersponse","SCE",12,1,0]
["Enersponse","SCE",12,2,0]
["Enersponse","SCE",12,3,0]
["Enersponse","SCE",12,4,0]
["Enersponse","SCE",12,5,0]
["Enersponse","SCE",12,6,0]
["Enersponse","SCE",12,7,0]
["Enersponse","SCE",12,8,0]
["Enersponse","SCE",12,9,0]
["Enersponse","SCE",12,10,0]
["Enersponse","SCE",12,11,0]
["Enersponse","SCE",12,12,0]
["Enersponse","SCE",12,13,0]
["Enersponse","SCE",12,14,0]
["Enersponse","SCE",12,15,0]
["Enersponse","SCE",12,16,0]
["Enersponse","SCE",12,17,1]
["Enersponse","SCE",12,18,1]
["Enersponse","SCE",12,19,1]
["Enersponse","SCE",12,20,1]
["Enersponse","SCE",12,21,1]
["Enersponse","SCE",12,22,0]
["Enersponse","SCE",12,23,0]
["Enersponse","SCE",12,24,0]
["Enersponse","SDGE",1,1,0]
["Enersponse","SDGE",1,2,0]
["Enersponse","SDGE",1,3,0]
["Enersponse","SDGE",1,4,0]
["Enersponse","SDGE",1,5,0]
["Enersponse","SDGE",1,6,0]
["Enersponse","SDGE",1,7,0]
["Enersponse","SDGE",1,8,0]
["Enersponse","SDGE",1,9,0]
["Enersponse","SDGE",1,10,0]
["Enersponse","SDGE",1,11,0]
["Enersponse","SDGE",1,12,0]
["Enersponse","SDGE",1,13,0]
["Enersponse","SDGE",1,14,0]
["Enersponse","SDGE",1,15,0]
["Enersponse","SDGE",1,16,0]
["Enersponse","SDGE",1,17,0]
["Enersponse","SDGE",1,18,0]
["Enersponse","SDGE",1,19,0]
["Enersponse","SDGE",1,20,0]
["Enersponse","SDGE",1,21,0]
["Enersponse","SDGE",1,22,0]
["Enersponse","SDGE",1,23,0]
["Enersponse","SDGE",1,24,0]
["Enersponse","SDGE",2,1,0]
["Enersponse","SDGE",2,2,0]
["Enersponse","SDGE",2,3,0]
["Enersponse","SDGE",2,4,0]
["Enersponse","SDGE",2,5,0]
["Enersponse","SDGE",2,6,0]
["Enersponse","SDGE",2,7,0]
["Enersponse","SDGE",2,8,0]
["Enersponse","SDGE",2,9,0]
["Enersponse","SDGE",2,10,0]
["Enersponse","SDGE",2,11,0]
["Enersponse","SDGE",2,12,0]
["Enersponse","SDGE",2,13,0]
["Enersponse","SDGE",2,14,0]
["Enersponse","SDGE",2,15,0]
["Enersponse","SDGE",2,16,0]
["Enersponse","SDGE",2,17,0]
["Enersponse","SDGE",2,18,0]
["Enersponse","SDGE",2,19,0]
["Enersponse","SDGE",2,20,0]
["Enersponse","SDGE",2,21,0]
["Enersponse","SDGE",2,22,0]
["Enersponse","SDGE",2,23,0]
["Enersponse","SDGE",2,24,0]
["Enersponse","SDGE",3,1,0]
["Enersponse","SDGE",3,2,0]
["Enersponse","SDGE",3,3,0]
["Enersponse","SDGE",3,4,0]
["Enersponse","SDGE",3,5,0]
["Enersponse","SDGE",3,6,0]
["Enersponse","SDGE",3,7,0]
["Enersponse","SDGE",3,8,0]
["Enersponse","SDGE",3,9,0]
["Enersponse","SDGE",3,10,0]
["Enersponse","SDGE",3,11,0]
["Enersponse","SDGE",3,12,0]
["Enersponse","SDGE",3,13,0]
["Enersponse","SDGE",3,14,0]
["Enersponse","SDGE",3,15,0]
["Enersponse","SDGE",3,16,0]
["Enersponse","SDGE",3,17,0]
["Enersponse","SDGE",3,18,0]
["Enersponse","SDGE",3,19,0]
["Enersponse","SDGE",3,20,0]
["Enersponse","SDGE",3,21,0]
["Enersponse","SDGE",3,22,0]
["Enersponse","SDGE",3,23,0]
["Enersponse","SDGE",3,24,0]
["Enersponse","SDGE",4,1,0]
["Enersponse","SDGE",4,2,0]
["Enersponse","SDGE",4,3,0]
["Enersponse","SDGE",4,4,0]
["Enersponse","SDGE",4,5,0]
["Enersponse","SDGE",4,6,0]
["Enersponse","SDGE",4,7,0]
["Enersponse","SDGE",4,8,0]
["Enersponse","SDGE",4,9,0]
["Enersponse","SDGE",4,10,0]
["Enersponse","SDGE",4,11,0]
["Enersponse","SDGE",4,12,0]
["Enersponse","SDGE",4,13,0]
["Enersponse","SDGE",4,14,0]
["Enersponse","SDGE",4,15,0]
["Enersponse","SDGE",4,16,0]
["Enersponse","SDGE",4,17,0]
["Enersponse","SDGE",4,18,1]
["Enersponse","SDGE",4,19,1]
["Enersponse","SDGE",4,20,1]
["Enersponse","SDGE",4,21,1]
["Enersponse","SDGE",4,22,1]
["Enersponse","SDGE",4,23,0]
["Enersponse","SDGE",4,24,0]
["Enersponse","SDGE",5,1,0]
["Enersponse","SDGE",5,2,0]
["Enersponse","SDGE",5,3,0]
["Enersponse","SDGE",5,4,0]
["Enersponse","SDGE",5,5,0]
["Enersponse","SDGE",5,6,0]
["Enersponse","SDGE",5,7,0]
["Enersponse","SDGE",5,8,0]
["Enersponse","SDGE",5,9,0]
["Enersponse","SDGE",5,10,0]
["Enersponse","SDGE",5,11,0]
["Enersponse","SDGE",5,12,0]
["Enersponse","SDGE",5,13,0]
["Enersponse","SDGE",5,14,0]
["Enersponse","SDGE",5,15,0]
["Enersponse","SDGE",5,16,0]
["Enersponse","SDGE",5,17,0]
["Enersponse","SDGE",5,18,1]
["Enersponse","SDGE",5,19,1]
["Enersponse","SDGE",5,20,1]
["Enersponse","SDGE",5,21,1]
["Enersponse","SDGE",5,22,1]
["Enersponse","SDGE",5,23,0]
["Enersponse","SDGE",5,24,0]
["Enersponse","SDGE",6,1,0]
["Enersponse","SDGE",6,2,0]
["Enersponse","SDGE",6,3,0]
["Enersponse","SDGE",6,4,0]
["Enersponse","SDGE",6,5,0]
["Enersponse","SDGE",6,6,0]
["Enersponse","SDGE",6,7,0]
["Enersponse","SDGE",6,8,0]
["Enersponse","SDGE",6,9,0]
["Enersponse","SDGE",6,10,0]
["Enersponse","SDGE",6,11,0]
["Enersponse","SDGE",6,12,0]
["Enersponse","SDGE",6,13,0]
["Enersponse","SDGE",6,14,0]
["Enersponse","SDGE",6,15,0]
["Enersponse","SDGE",6,16,0]
["Enersponse","SDGE",6,17,1]
["Enersponse","SDGE",6,18,1]
["Enersponse","SDGE",6,19,1]
["Enersponse","SDGE",6,20,1]
["Enersponse","SDGE",6,21,1]
["Enersponse","SDGE",6,22,0]
["Enersponse","SDGE",6,23,0]
["Enersponse","SDGE",6,24,0]
["Enersponse","SDGE",7,1,0]
["Enersponse","SDGE",7,2,0]
["Enersponse","SDGE",7,3,0]
["Enersponse","SDGE",7,4,0]
["Enersponse","SDGE",7,5,0]
["Enersponse","SDGE",7,6,0]
["Enersponse","SDGE",7,7,0]
["Enersponse","SDGE",7,8,0]
["Enersponse","SDGE",7,9,0]
["Enersponse","SDGE",7,10,0]
["Enersponse","SDGE",7,11,0]
["Enersponse","SDGE",7,12,0]
["Enersponse","SDGE",7,13,0]
["Enersponse","SDGE",7,14,0]
["Enersponse","SDGE",7,15,0]
["Enersponse","SDGE",7,16,0]
["Enersponse","SDGE",7,17,1]
["Enersponse","SDGE",7,18,1]
["Enersponse","SDGE",7,19,1]
["Enersponse","SDGE",7,20,1]
["Enersponse","SDGE",7,21,1]
["Enersponse","SDGE",7,22,0]
["Enersponse","SDGE",7,23,0]
["Enersponse","SDGE",7,24,0]
["Enersponse","SDGE",8,1,0]
["Enersponse","SDGE",8,2,0]
["Enersponse","SDGE",8,3,0]
["Enersponse","SDGE",8,4,0]
["Enersponse","SDGE",8,5,0]
["Enersponse","SDGE",8,6,0]
["Enersponse","SDGE",8,7,0]
["Enersponse","SDGE",8,8,0]
["Enersponse","SDGE",8,9,0]
["Enersponse","SDGE",8,10,0]
["Enersponse","SDGE",8,11,0]
["Enersponse","SDGE",8,12,0]
["Enersponse","SDGE",8,13,0]
["Enersponse","SDGE",8,14,0]
["Enersponse","SDGE",8,15,0]
["Enersponse","SDGE",8,16,0]
["Enersponse","SDGE",8,17,1]
["Enersponse","SDGE",8,18,1]
["Enersponse","SDGE",8,19,1]
["Enersponse","SDGE",8,20,1]
["Enersponse","SDGE",8,21,1]
["Enersponse","SDGE",8,22,0]
["Enersponse","SDGE",8,23,0]
["Enersponse","SDGE",8,24,0]
["Enersponse","SDGE",9,1,0]
["Enersponse","SDGE",9,2,0]
["Enersponse","SDGE",9,3,0]
["Enersponse","SDGE",9,4,0]
["Enersponse","SDGE",9,5,0]
["Enersponse","SDGE",9,6,0]
["Enersponse","SDGE",9,7,0]
["Enersponse","SDGE",9,8,0]
["Enersponse","SDGE",9,9,0]
["Enersponse","SDGE",9,10,0]
["Enersponse","SDGE",9,11,0]
["Enersponse","SDGE",9,12,0]
["Enersponse","SDGE",9,13,0]
["Enersponse","SDGE",9,14,0]
["Enersponse","SDGE",9,15,0]
["Enersponse","SDGE",9,16,0]
["Enersponse","SDGE",9,17,1]
["Enersponse","SDGE",9,18,1]
["Enersponse","SDGE",9,19,1]
["Enersponse","SDGE",9,20,1]
["Enersponse","SDGE",9,21,1]
["Enersponse","SDGE",9,22,0]
["Enersponse","SDGE",9,23,0]
["Enersponse","SDGE",9,24,0]
["Enersponse","SDGE",10,1,0]
["Enersponse","SDGE",10,2,0]
["Enersponse","SDGE",10,3,0]
["Enersponse","SDGE",10,4,0]
["Enersponse","SDGE",10,5,0]
["Enersponse","SDGE",10,6,0]
["Enersponse","SDGE",10,7,0]
["Enersponse","SDGE",10,8,0]
["Enersponse","SDGE",10,9,0]
["Enersponse","SDGE",10,10,0]
["Enersponse","SDGE",10,11,0]
["Enersponse","SDGE",10,12,0]
["Enersponse","SDGE",10,13,0]
["Enersponse","SDGE",10,14,0]
["Enersponse","SDGE",10,15,0]
["Enersponse","SDGE",10,16,0]
["Enersponse","SDGE",10,17,1]
["Enersponse","SDGE",10,18,1]
["Enersponse","SDGE",10,19,1]
["Enersponse","SDGE",10,20,1]
["Enersponse","SDGE",10,21,1]
["Enersponse","SDGE",10,22,0]
["Enersponse","SDGE",10,23,0]
["Enersponse","SDGE",10,24,0]
["Enersponse","SDGE",11,1,0]
["Enersponse","SDGE",11,2,0]
["Enersponse","SDGE",11,3,0]
["Enersponse","SDGE",11,4,0]
["Enersponse","SDGE",11,5,0]
["Enersponse","SDGE",11,6,0]
["Enersponse","SDGE",11,7,0]
["Enersponse","SDGE",11,8,0]
["Enersponse","SDGE",11,9,0]
["Enersponse","SDGE",11,10,0]
["Enersponse","SDGE",11,11,0]
["Enersponse","SDGE",11,12,0]
["Enersponse","SDGE",11,13,0]
["Enersponse","SDGE",11,14,0]
["Enersponse","SDGE",11,15,0]
["Enersponse","SDGE",11,16,0]
["Enersponse","SDGE",11,17,1]
["Enersponse","SDGE",11,18,1]
["Enersponse","SDGE",11,19,1]
["Enersponse","SDGE",11,20,1]
["Enersponse","SDGE",11,21,1]
["Enersponse","SDGE",11,22,0]
["Enersponse","SDGE",11,23,0]
["Enersponse","SDGE",11,24,0]
["Enersponse","SDGE",12,1,0]
["Enersponse","SDGE",12,2,0]
["Enersponse","SDGE",12,3,0]
["Enersponse","SDGE",12,4,0]
["Enersponse","SDGE",12,5,0]
["Enersponse","SDGE",12,6,0]
["Enersponse","SDGE",12,7,0]
["Enersponse","SDGE",12,8,0]
["Enersponse","SDGE",12,9,0]
["Enersponse","SDGE",12,10,0]
["Enersponse","SDGE",12,11,0]
["Enersponse","SDGE",12,12,0]
["Enersponse","SDGE",12,13,0]
["Enersponse","SDGE",12,14,0]
["Enersponse","SDGE",12,15,0]
["Enersponse","SDGE",12,16,0]
["Enersponse","SDGE",12,17,1]
["Enersponse","SDGE",12,18,1]
["Enersponse","SDGE",12,19,1]
["Enersponse","SDGE",12,20,1]
["Enersponse","SDGE",12,21,1]
["Enersponse","SDGE",12,22,0]
["Enersponse","SDGE",12,23,0]
["Enersponse","SDGE",12,24,0]
["Leapfrog","PGE",1,1,0]
["Leapfrog","PGE",1,2,0]
["Leapfrog","PGE",1,3,0]
["Leapfrog","PGE",1,4,0]
["Leapfrog","PGE",1,5,0]
["Leapfrog","PGE",1,6,0]
["Leapfrog","PGE",1,7,0]
["Leapfrog","PGE",1,8,0]
["Leapfrog","PGE",1,9,0]
["Leapfrog","PGE",1,10,0]
["Leapfrog","PGE",1,11,0]
["Leapfrog","PGE",1,12,0]
["Leapfrog","PGE",1,13,0]
["Leapfrog","PGE",1,14,0]
["Leapfrog","PGE",1,15,0]
["Leapfrog","PGE",1,16,0]
["Leapfrog","PGE",1,17,1.2532808427920283]
["Leapfrog","PGE",1,18,1.3057742812335773]
["Leapfrog","PGE",1,19,0.76771653720767752]
["Leapfrog","PGE",1,20,0.83333333525961706]
["Leapfrog","PGE",1,21,0.83989501506481601]
["Leapfrog","PGE",1,22,0]
["Leapfrog","PGE",1,23,0]
["Leapfrog","PGE",1,24,0]
["Leapfrog","PGE",2,1,0]
["Leapfrog","PGE",2,2,0]
["Leapfrog","PGE",2,3,0]
["Leapfrog","PGE",2,4,0]
["Leapfrog","PGE",2,5,0]
["Leapfrog","PGE",2,6,0]
["Leapfrog","PGE",2,7,0]
["Leapfrog","PGE",2,8,0]
["Leapfrog","PGE",2,9,0]
["Leapfrog","PGE",2,10,0]
["Leapfrog","PGE",2,11,0]
["Leapfrog","PGE",2,12,0]
["Leapfrog","PGE",2,13,0]
["Leapfrog","PGE",2,14,0]
["Leapfrog","PGE",2,15,0]
["Leapfrog","PGE",2,16,0]
["Leapfrog","PGE",2,17,1.2652418281340696]
["Leapfrog","PGE",2,18,1.3076993721604222]
["Leapfrog","PGE",2,19,0.76547237938887591]
["Leapfrog","PGE",2,20,0.82809761536055171]
["Leapfrog","PGE",2,21,0.8334888186256334]
["Leapfrog","PGE",2,22,0]
["Leapfrog","PGE",2,23,0]
["Leapfrog","PGE",2,24,0]
["Leapfrog","PGE",3,1,0]
["Leapfrog","PGE",3,2,0]
["Leapfrog","PGE",3,3,0]
["Leapfrog","PGE",3,4,0]
["Leapfrog","PGE",3,5,0]
["Leapfrog","PGE",3,6,0]
["Leapfrog","PGE",3,7,0]
["Leapfrog","PGE",3,8,0]
["Leapfrog","PGE",3,9,0]
["Leapfrog","PGE",3,10,0]
["Leapfrog","PGE",3,11,0]
["Leapfrog","PGE",3,12,0]
["Leapfrog","PGE",3,13,0]
["Leapfrog","PGE",3,14,0]
["Leapfrog","PGE",3,15,0]
["Leapfrog","PGE",3,16,0]
["Leapfrog","PGE",3,17,0]
["Leapfrog","PGE",3,18,1.2277611338933354]
["Leapfrog","PGE",3,19,1.2958524488185494]
["Leapfrog","PGE",3,20,0.77795689422000447]
["Leapfrog","PGE",3,21,0.8454751194441027]
["Leapfrog","PGE",3,22,0.85295441004495087]
["Leapfrog","PGE",3,23,0]
["Leapfrog","PGE",3,24,0]
["Leapfrog","PGE",4,1,0]
["Leapfrog","PGE",4,2,0]
["Leapfrog","PGE",4,3,0]
["Leapfrog","PGE",4,4,0]
["Leapfrog","PGE",4,5,0]
["Leapfrog","PGE",4,6,0]
["Leapfrog","PGE",4,7,0]
["Leapfrog","PGE",4,8,0]
["Leapfrog","PGE",4,9,0]
["Leapfrog","PGE",4,10,0]
["Leapfrog","PGE",4,11,0]
["Leapfrog","PGE",4,12,0]
["Leapfrog","PGE",4,13,0]
["Leapfrog","PGE",4,14,0]
["Leapfrog","PGE",4,15,0]
["Leapfrog","PGE",4,16,0]
["Leapfrog","PGE",4,17,0]
["Leapfrog","PGE",4,18,0.91710373543059742]
["Leapfrog","PGE",4,19,0.95736444510100538]
["Leapfrog","PGE",4,20,1.0884039328562971]
["Leapfrog","PGE",4,21,1.0388294924858277]
["Leapfrog","PGE",4,22,0.99829839654710772]
["Leapfrog","PGE",4,23,0]
["Leapfrog","PGE",4,24,0]
["Leapfrog","PGE",5,1,0]
["Leapfrog","PGE",5,2,0]
["Leapfrog","PGE",5,3,0]
["Leapfrog","PGE",5,4,0]
["Leapfrog","PGE",5,5,0]
["Leapfrog","PGE",5,6,0]
["Leapfrog","PGE",5,7,0]
["Leapfrog","PGE",5,8,0]
["Leapfrog","PGE",5,9,0]
["Leapfrog","PGE",5,10,0]
["Leapfrog","PGE",5,11,0]
["Leapfrog","PGE",5,12,0]
["Leapfrog","PGE",5,13,0]
["Leapfrog","PGE",5,14,0]
["Leapfrog","PGE",5,15,0]
["Leapfrog","PGE",5,16,0]
["Leapfrog","PGE",5,17,0]
["Leapfrog","PGE",5,18,0.90167031797081276]
["Leapfrog","PGE",5,19,0.9392924403397197]
["Leapfrog","PGE",5,20,1.0955586241704349]
["Leapfrog","PGE",5,21,1.0551006986981355]
["Leapfrog","PGE",5,22,1.0083779165456832]
["Leapfrog","PGE",5,23,0]
["Leapfrog","PGE",5,24,0]
["Leapfrog","PGE",6,1,0]
["Leapfrog","PGE",6,2,0]
["Leapfrog","PGE",6,3,0]
["Leapfrog","PGE",6,4,0]
["Leapfrog","PGE",6,5,0]
["Leapfrog","PGE",6,6,0]
["Leapfrog","PGE",6,7,0]
["Leapfrog","PGE",6,8,0]
["Leapfrog","PGE",6,9,0]
["Leapfrog","PGE",6,10,0]
["Leapfrog","PGE",6,11,0]
["Leapfrog","PGE",6,12,0]
["Leapfrog","PGE",6,13,0]
["Leapfrog","PGE",6,14,0]
["Leapfrog","PGE",6,15,0]
["Leapfrog","PGE",6,16,0]
["Leapfrog","PGE",6,17,0.90870242370987842]
["Leapfrog","PGE",6,18,1.0488617783247911]
["Leapfrog","PGE",6,19,1.0955214179164021]
["Leapfrog","PGE",6,20,0.99369878849805127]
["Leapfrog","PGE",6,21,0.95321558734477285]
["Leapfrog","PGE",6,22,0]
["Leapfrog","PGE",6,23,0]
["Leapfrog","PGE",6,24,0]
["Leapfrog","PGE",7,1,0]
["Leapfrog","PGE",7,2,0]
["Leapfrog","PGE",7,3,0]
["Leapfrog","PGE",7,4,0]
["Leapfrog","PGE",7,5,0]
["Leapfrog","PGE",7,6,0]
["Leapfrog","PGE",7,7,0]
["Leapfrog","PGE",7,8,0]
["Leapfrog","PGE",7,9,0]
["Leapfrog","PGE",7,10,0]
["Leapfrog","PGE",7,11,0]
["Leapfrog","PGE",7,12,0]
["Leapfrog","PGE",7,13,0]
["Leapfrog","PGE",7,14,0]
["Leapfrog","PGE",7,15,0]
["Leapfrog","PGE",7,16,0]
["Leapfrog","PGE",7,17,1.1868644378112962]
["Leapfrog","PGE",7,18,0.98425179719958544]
["Leapfrog","PGE",7,19,1.0394729408434784]
["Leapfrog","PGE",7,20,0.93348815083941272]
["Leapfrog","PGE",7,21,0.85592267519504872]
["Leapfrog","PGE",7,22,0]
["Leapfrog","PGE",7,23,0]
["Leapfrog","PGE",7,24,0]
["Leapfrog","PGE",8,1,0]
["Leapfrog","PGE",8,2,0]
["Leapfrog","PGE",8,3,0]
["Leapfrog","PGE",8,4,0]
["Leapfrog","PGE",8,5,0]
["Leapfrog","PGE",8,6,0]
["Leapfrog","PGE",8,7,0]
["Leapfrog","PGE",8,8,0]
["Leapfrog","PGE",8,9,0]
["Leapfrog","PGE",8,10,0]
["Leapfrog","PGE",8,11,0]
["Leapfrog","PGE",8,12,0]
["Leapfrog","PGE",8,13,0]
["Leapfrog","PGE",8,14,0]
["Leapfrog","PGE",8,15,0]
["Leapfrog","PGE",8,16,0]
["Leapfrog","PGE",8,17,1.204329453767206]
["Leapfrog","PGE",8,18,0.98714532311119441]
["Leapfrog","PGE",8,19,1.0363899541195332]
["Leapfrog","PGE",8,20,0.92223182421420691]
["Leapfrog","PGE",8,21,0.84990344012486718]
["Leapfrog","PGE",8,22,0]
["Leapfrog","PGE",8,23,0]
["Leapfrog","PGE",8,24,0]
["Leapfrog","PGE",9,1,0]
["Leapfrog","PGE",9,2,0]
["Leapfrog","PGE",9,3,0]
["Leapfrog","PGE",9,4,0]
["Leapfrog","PGE",9,5,0]
["Leapfrog","PGE",9,6,0]
["Leapfrog","PGE",9,7,0]
["Leapfrog","PGE",9,8,0]
["Leapfrog","PGE",9,9,0]
["Leapfrog","PGE",9,10,0]
["Leapfrog","PGE",9,11,0]
["Leapfrog","PGE",9,12,0]
["Leapfrog","PGE",9,13,0]
["Leapfrog","PGE",9,14,0]
["Leapfrog","PGE",9,15,0]
["Leapfrog","PGE",9,16,0]
["Leapfrog","PGE",9,17,1.1504165147507455]
["Leapfrog","PGE",9,18,0.97117291783111426]
["Leapfrog","PGE",9,19,1.0641426403354435]
["Leapfrog","PGE",9,20,0.94270616093104009]
["Leapfrog","PGE",9,21,0.87156177254234224]
["Leapfrog","PGE",9,22,0]
["Leapfrog","PGE",9,23,0]
["Leapfrog","PGE",9,24,0]
["Leapfrog","PGE",10,1,0]
["Leapfrog","PGE",10,2,0]
["Leapfrog","PGE",10,3,0]
["Leapfrog","PGE",10,4,0]
["Leapfrog","PGE",10,5,0]
["Leapfrog","PGE",10,6,0]
["Leapfrog","PGE",10,7,0]
["Leapfrog","PGE",10,8,0]
["Leapfrog","PGE",10,9,0]
["Leapfrog","PGE",10,10,0]
["Leapfrog","PGE",10,11,0]
["Leapfrog","PGE",10,12,0]
["Leapfrog","PGE",10,13,0]
["Leapfrog","PGE",10,14,0]
["Leapfrog","PGE",10,15,0]
["Leapfrog","PGE",10,16,0]
["Leapfrog","PGE",10,17,1.1224342107765779]
["Leapfrog","PGE",10,18,0.94631624621791544]
["Leapfrog","PGE",10,19,1.0319762369373224]
["Leapfrog","PGE",10,20,0.95322408631621447]
["Leapfrog","PGE",10,21,0.94604921829867905]
["Leapfrog","PGE",10,22,0]
["Leapfrog","PGE",10,23,0]
["Leapfrog","PGE",10,24,0]
["Leapfrog","PGE",11,1,0]
["Leapfrog","PGE",11,2,0]
["Leapfrog","PGE",11,3,0]
["Leapfrog","PGE",11,4,0]
["Leapfrog","PGE",11,5,0]
["Leapfrog","PGE",11,6,0]
["Leapfrog","PGE",11,7,0]
["Leapfrog","PGE",11,8,0]
["Leapfrog","PGE",11,9,0]
["Leapfrog","PGE",11,10,0]
["Leapfrog","PGE",11,11,0]
["Leapfrog","PGE",11,12,0]
["Leapfrog","PGE",11,13,0]
["Leapfrog","PGE",11,14,0]
["Leapfrog","PGE",11,15,0]
["Leapfrog","PGE",11,16,0]
["Leapfrog","PGE",11,17,0.93284100545181448]
["Leapfrog","PGE",11,18,1.1501444339582558]
["Leapfrog","PGE",11,19,1.1688229457606947]
["Leapfrog","PGE",11,20,0.99720857648343986]
["Leapfrog","PGE",11,21,0.75098303777683206]
["Leapfrog","PGE",11,22,0]
["Leapfrog","PGE",11,23,0]
["Leapfrog","PGE",11,24,0]
["Leapfrog","PGE",12,1,0]
["Leapfrog","PGE",12,2,0]
["Leapfrog","PGE",12,3,0]
["Leapfrog","PGE",12,4,0]
["Leapfrog","PGE",12,5,0]
["Leapfrog","PGE",12,6,0]
["Leapfrog","PGE",12,7,0]
["Leapfrog","PGE",12,8,0]
["Leapfrog","PGE",12,9,0]
["Leapfrog","PGE",12,10,0]
["Leapfrog","PGE",12,11,0]
["Leapfrog","PGE",12,12,0]
["Leapfrog","PGE",12,13,0]
["Leapfrog","PGE",12,14,0]
["Leapfrog","PGE",12,15,0]
["Leapfrog","PGE",12,16,0]
["Leapfrog","PGE",12,17,0.8558092542834016]
["Leapfrog","PGE",12,18,1.1153205049996686]
["Leapfrog","PGE",12,19,1.1876634530750247]
["Leapfrog","PGE",12,20,1.0289116200307806]
["Leapfrog","PGE",12,21,0.81229515632032123]
["Leapfrog","PGE",12,22,0]
["Leapfrog","PGE",12,23,0]
["Leapfrog","PGE",12,24,0]
["Leapfrog","SCE",1,1,0]
["Leapfrog","SCE",1,2,0]
["Leapfrog","SCE",1,3,0]
["Leapfrog","SCE",1,4,0]
["Leapfrog","SCE",1,5,0]
["Leapfrog","SCE",1,6,0]
["Leapfrog","SCE",1,7,0]
["Leapfrog","SCE",1,8,0]
["Leapfrog","SCE",1,9,0]
["Leapfrog","SCE",1,10,0]
["Leapfrog","SCE",1,11,0]
["Leapfrog","SCE",1,12,0]
["Leapfrog","SCE",1,13,0]
["Leapfrog","SCE",1,14,0]
["Leapfrog","SCE",1,15,0]
["Leapfrog","SCE",1,16,0]
["Leapfrog","SCE",1,17,1.4615609748093825]
["Leapfrog","SCE",1,18,1.5016256243437118]
["Leapfrog","SCE",1,19,0.68377702532886009]
["Leapfrog","SCE",1,20,0.67878658603644382]
["Leapfrog","SCE",1,21,0.67424978563936955]
["Leapfrog","SCE",1,22,0]
["Leapfrog","SCE",1,23,0]
["Leapfrog","SCE",1,24,0]
["Leapfrog","SCE",2,1,0]
["Leapfrog","SCE",2,2,0]
["Leapfrog","SCE",2,3,0]
["Leapfrog","SCE",2,4,0]
["Leapfrog","SCE",2,5,0]
["Leapfrog","SCE",2,6,0]
["Leapfrog","SCE",2,7,0]
["Leapfrog","SCE",2,8,0]
["Leapfrog","SCE",2,9,0]
["Leapfrog","SCE",2,10,0]
["Leapfrog","SCE",2,11,0]
["Leapfrog","SCE",2,12,0]
["Leapfrog","SCE",2,13,0]
["Leapfrog","SCE",2,14,0]
["Leapfrog","SCE",2,15,0]
["Leapfrog","SCE",2,16,0]
["Leapfrog","SCE",2,17,1.456887584137613]
["Leapfrog","SCE",2,18,1.5148383708849313]
["Leapfrog","SCE",2,19,0.68035698952613488]
["Leapfrog","SCE",2,20,0.6761073835878082]
["Leapfrog","SCE",2,21,0.6718096761443012]
["Leapfrog","SCE",2,22,0]
["Leapfrog","SCE",2,23,0]
["Leapfrog","SCE",2,24,0]
["Leapfrog","SCE",3,1,0]
["Leapfrog","SCE",3,2,0]
["Leapfrog","SCE",3,3,0]
["Leapfrog","SCE",3,4,0]
["Leapfrog","SCE",3,5,0]
["Leapfrog","SCE",3,6,0]
["Leapfrog","SCE",3,7,0]
["Leapfrog","SCE",3,8,0]
["Leapfrog","SCE",3,9,0]
["Leapfrog","SCE",3,10,0]
["Leapfrog","SCE",3,11,0]
["Leapfrog","SCE",3,12,0]
["Leapfrog","SCE",3,13,0]
["Leapfrog","SCE",3,14,0]
["Leapfrog","SCE",3,15,0]
["Leapfrog","SCE",3,16,0]
["Leapfrog","SCE",3,17,0]
["Leapfrog","SCE",3,18,1.4515136953043801]
["Leapfrog","SCE",3,19,1.4976742848657387]
["Leapfrog","SCE",3,20,0.68903575963239605]
["Leapfrog","SCE",3,21,0.68317176169483995]
["Leapfrog","SCE",3,22,0.67860449694461966]
["Leapfrog","SCE",3,23,0]
["Leapfrog","SCE",3,24,0]
["Leapfrog","SCE",4,1,0]
["Leapfrog","SCE",4,2,0]
["Leapfrog","SCE",4,3,0]
["Leapfrog","SCE",4,4,0]
["Leapfrog","SCE",4,5,0]
["Leapfrog","SCE",4,6,0]
["Leapfrog","SCE",4,7,0]
["Leapfrog","SCE",4,8,0]
["Leapfrog","SCE",4,9,0]
["Leapfrog","SCE",4,10,0]
["Leapfrog","SCE",4,11,0]
["Leapfrog","SCE",4,12,0]
["Leapfrog","SCE",4,13,0]
["Leapfrog","SCE",4,14,0]
["Leapfrog","SCE",4,15,0]
["Leapfrog","SCE",4,16,0]
["Leapfrog","SCE",4,17,0]
["Leapfrog","SCE",4,18,0.97205288200922912]
["Leapfrog","SCE",4,19,1.1338373715804766]
["Leapfrog","SCE",4,20,1.0462843027071145]
["Leapfrog","SCE",4,21,0.94196249586539371]
["Leapfrog","SCE",4,22,0.90586295073720724]
["Leapfrog","SCE",4,23,0]
["Leapfrog","SCE",4,24,0]
["Leapfrog","SCE",5,1,0]
["Leapfrog","SCE",5,2,0]
["Leapfrog","SCE",5,3,0]
["Leapfrog","SCE",5,4,0]
["Leapfrog","SCE",5,5,0]
["Leapfrog","SCE",5,6,0]
["Leapfrog","SCE",5,7,0]
["Leapfrog","SCE",5,8,0]
["Leapfrog","SCE",5,9,0]
["Leapfrog","SCE",5,10,0]
["Leapfrog","SCE",5,11,0]
["Leapfrog","SCE",5,12,0]
["Leapfrog","SCE",5,13,0]
["Leapfrog","SCE",5,14,0]
["Leapfrog","SCE",5,15,0]
["Leapfrog","SCE",5,16,0]
["Leapfrog","SCE",5,17,0]
["Leapfrog","SCE",5,18,0.90538556353220723]
["Leapfrog","SCE",5,19,1.120555147821749]
["Leapfrog","SCE",5,20,1.0735503243497131]
["Leapfrog","SCE",5,21,0.99017569732024402]
["Leapfrog","SCE",5,22,0.91033326257019831]
["Leapfrog","SCE",5,23,0]
["Leapfrog","SCE",5,24,0]
["Leapfrog","SCE",6,1,0]
["Leapfrog","SCE",6,2,0]
["Leapfrog","SCE",6,3,0]
["Leapfrog","SCE",6,4,0]
["Leapfrog","SCE",6,5,0]
["Leapfrog","SCE",6,6,0]
["Leapfrog","SCE",6,7,0]
["Leapfrog","SCE",6,8,0]
["Leapfrog","SCE",6,9,0]
["Leapfrog","SCE",6,10,0]
["Leapfrog","SCE",6,11,0]
["Leapfrog","SCE",6,12,0]
["Leapfrog","SCE",6,13,0]
["Leapfrog","SCE",6,14,0]
["Leapfrog","SCE",6,15,0]
["Leapfrog","SCE",6,16,0]
["Leapfrog","SCE",6,17,0.93553034826524273]
["Leapfrog","SCE",6,18,1.0844063615122737]
["Leapfrog","SCE",6,19,1.0723607432302811]
["Leapfrog","SCE",6,20,1.00059153472622]
["Leapfrog","SCE",6,21,0.90711101646956271]
["Leapfrog","SCE",6,22,0]
["Leapfrog","SCE",6,23,0]
["Leapfrog","SCE",6,24,0]
["Leapfrog","SCE",7,1,0]
["Leapfrog","SCE",7,2,0]
["Leapfrog","SCE",7,3,0]
["Leapfrog","SCE",7,4,0]
["Leapfrog","SCE",7,5,0]
["Leapfrog","SCE",7,6,0]
["Leapfrog","SCE",7,7,0]
["Leapfrog","SCE",7,8,0]
["Leapfrog","SCE",7,9,0]
["Leapfrog","SCE",7,10,0]
["Leapfrog","SCE",7,11,0]
["Leapfrog","SCE",7,12,0]
["Leapfrog","SCE",7,13,0]
["Leapfrog","SCE",7,14,0]
["Leapfrog","SCE",7,15,0]
["Leapfrog","SCE",7,16,0]
["Leapfrog","SCE",7,17,1.1149373672209566]
["Leapfrog","SCE",7,18,1.0808124746504308]
["Leapfrog","SCE",7,19,1.0316407183081122]
["Leapfrog","SCE",7,20,0.93633716971103065]
["Leapfrog","SCE",7,21,0.8362722733240503]
["Leapfrog","SCE",7,22,0]
["Leapfrog","SCE",7,23,0]
["Leapfrog","SCE",7,24,0]
["Leapfrog","SCE",8,1,0]
["Leapfrog","SCE",8,2,0]
["Leapfrog","SCE",8,3,0]
["Leapfrog","SCE",8,4,0]
["Leapfrog","SCE",8,5,0]
["Leapfrog","SCE",8,6,0]
["Leapfrog","SCE",8,7,0]
["Leapfrog","SCE",8,8,0]
["Leapfrog","SCE",8,9,0]
["Leapfrog","SCE",8,10,0]
["Leapfrog","SCE",8,11,0]
["Leapfrog","SCE",8,12,0]
["Leapfrog","SCE",8,13,0]
["Leapfrog","SCE",8,14,0]
["Leapfrog","SCE",8,15,0]
["Leapfrog","SCE",8,16,0]
["Leapfrog","SCE",8,17,1.1022318957831065]
["Leapfrog","SCE",8,18,1.0588040779938843]
["Leapfrog","SCE",8,19,1.0198366969878352]
["Leapfrog","SCE",8,20,0.95482055601968407]
["Leapfrog","SCE",8,21,0.86430677449838988]
["Leapfrog","SCE",8,22,0]
["Leapfrog","SCE",8,23,0]
["Leapfrog","SCE",8,24,0]
["Leapfrog","SCE",9,1,0]
["Leapfrog","SCE",9,2,0]
["Leapfrog","SCE",9,3,0]
["Leapfrog","SCE",9,4,0]
["Leapfrog","SCE",9,5,0]
["Leapfrog","SCE",9,6,0]
["Leapfrog","SCE",9,7,0]
["Leapfrog","SCE",9,8,0]
["Leapfrog","SCE",9,9,0]
["Leapfrog","SCE",9,10,0]
["Leapfrog","SCE",9,11,0]
["Leapfrog","SCE",9,12,0]
["Leapfrog","SCE",9,13,0]
["Leapfrog","SCE",9,14,0]
["Leapfrog","SCE",9,15,0]
["Leapfrog","SCE",9,16,0]
["Leapfrog","SCE",9,17,1.0982458750154525]
["Leapfrog","SCE",9,18,1.0629152006782505]
["Leapfrog","SCE",9,19,1.0339235634204906]
["Leapfrog","SCE",9,20,0.94745178751699477]
["Leapfrog","SCE",9,21,0.85746357254876071]
["Leapfrog","SCE",9,22,0]
["Leapfrog","SCE",9,23,0]
["Leapfrog","SCE",9,24,0]
["Leapfrog","SCE",10,1,0]
["Leapfrog","SCE",10,2,0]
["Leapfrog","SCE",10,3,0]
["Leapfrog","SCE",10,4,0]
["Leapfrog","SCE",10,5,0]
["Leapfrog","SCE",10,6,0]
["Leapfrog","SCE",10,7,0]
["Leapfrog","SCE",10,8,0]
["Leapfrog","SCE",10,9,0]
["Leapfrog","SCE",10,10,0]
["Leapfrog","SCE",10,11,0]
["Leapfrog","SCE",10,12,0]
["Leapfrog","SCE",10,13,0]
["Leapfrog","SCE",10,14,0]
["Leapfrog","SCE",10,15,0]
["Leapfrog","SCE",10,16,0]
["Leapfrog","SCE",10,17,1.0892932763911429]
["Leapfrog","SCE",10,18,1.0668945460628187]
["Leapfrog","SCE",10,19,1.0461258361743948]
["Leapfrog","SCE",10,20,0.93488618218200692]
["Leapfrog","SCE",10,21,0.86280016642639712]
["Leapfrog","SCE",10,22,0]
["Leapfrog","SCE",10,23,0]
["Leapfrog","SCE",10,24,0]
["Leapfrog","SCE",11,1,0]
["Leapfrog","SCE",11,2,0]
["Leapfrog","SCE",11,3,0]
["Leapfrog","SCE",11,4,0]
["Leapfrog","SCE",11,5,0]
["Leapfrog","SCE",11,6,0]
["Leapfrog","SCE",11,7,0]
["Leapfrog","SCE",11,8,0]
["Leapfrog","SCE",11,9,0]
["Leapfrog","SCE",11,10,0]
["Leapfrog","SCE",11,11,0]
["Leapfrog","SCE",11,12,0]
["Leapfrog","SCE",11,13,0]
["Leapfrog","SCE",11,14,0]
["Leapfrog","SCE",11,15,0]
["Leapfrog","SCE",11,16,0]
["Leapfrog","SCE",11,17,1.0208474154256644]
["Leapfrog","SCE",11,18,1.0638248484827881]
["Leapfrog","SCE",11,19,1.049635093722352]
["Leapfrog","SCE",11,20,0.96276399106014021]
["Leapfrog","SCE",11,21,0.90292865522619226]
["Leapfrog","SCE",11,22,0]
["Leapfrog","SCE",11,23,0]
["Leapfrog","SCE",11,24,0]
["Leapfrog","SCE",12,1,0]
["Leapfrog","SCE",12,2,0]
["Leapfrog","SCE",12,3,0]
["Leapfrog","SCE",12,4,0]
["Leapfrog","SCE",12,5,0]
["Leapfrog","SCE",12,6,0]
["Leapfrog","SCE",12,7,0]
["Leapfrog","SCE",12,8,0]
["Leapfrog","SCE",12,9,0]
["Leapfrog","SCE",12,10,0]
["Leapfrog","SCE",12,11,0]
["Leapfrog","SCE",12,12,0]
["Leapfrog","SCE",12,13,0]
["Leapfrog","SCE",12,14,0]
["Leapfrog","SCE",12,15,0]
["Leapfrog","SCE",12,16,0]
["Leapfrog","SCE",12,17,0.82975407091530429]
["Leapfrog","SCE",12,18,0.96898126805305429]
["Leapfrog","SCE",12,19,1.0805988958511852]
["Leapfrog","SCE",12,20,1.0540775701391003]
["Leapfrog","SCE",12,21,1.0665882041954933]
["Leapfrog","SCE",12,22,0]
["Leapfrog","SCE",12,23,0]
["Leapfrog","SCE",12,24,0]
["Leapfrog","SDGE",1,1,0]
["Leapfrog","SDGE",1,2,0]
["Leapfrog","SDGE",1,3,0]
["Leapfrog","SDGE",1,4,0]
["Leapfrog","SDGE",1,5,0]
["Leapfrog","SDGE",1,6,0]
["Leapfrog","SDGE",1,7,0]
["Leapfrog","SDGE",1,8,0]
["Leapfrog","SDGE",1,9,0]
["Leapfrog","SDGE",1,10,0]
["Leapfrog","SDGE",1,11,0]
["Leapfrog","SDGE",1,12,0]
["Leapfrog","SDGE",1,13,0]
["Leapfrog","SDGE",1,14,0]
["Leapfrog","SDGE",1,15,0]
["Leapfrog","SDGE",1,16,0]
["Leapfrog","SDGE",1,17,2.2764879972255998]
["Leapfrog","SDGE",1,18,1.1345616391833471]
["Leapfrog","SDGE",1,19,0.54553077695855456]
["Leapfrog","SDGE",1,20,0.52859416275975213]
["Leapfrog","SDGE",1,21,0.51482541872402998]
["Leapfrog","SDGE",1,22,0]
["Leapfrog","SDGE",1,23,0]
["Leapfrog","SDGE",1,24,0]
["Leapfrog","SDGE",2,1,0]
["Leapfrog","SDGE",2,2,0]
["Leapfrog","SDGE",2,3,0]
["Leapfrog","SDGE",2,4,0]
["Leapfrog","SDGE",2,5,0]
["Leapfrog","SDGE",2,6,0]
["Leapfrog","SDGE",2,7,0]
["Leapfrog","SDGE",2,8,0]
["Leapfrog","SDGE",2,9,0]
["Leapfrog","SDGE",2,10,0]
["Leapfrog","SDGE",2,11,0]
["Leapfrog","SDGE",2,12,0]
["Leapfrog","SDGE",2,13,0]
["Leapfrog","SDGE",2,14,0]
["Leapfrog","SDGE",2,15,0]
["Leapfrog","SDGE",2,16,0]
["Leapfrog","SDGE",2,17,2.2773802981609994]
["Leapfrog","SDGE",2,18,1.1392003552740437]
["Leapfrog","SDGE",2,19,0.54296880841865813]
["Leapfrog","SDGE",2,20,0.52739349276043002]
["Leapfrog","SDGE",2,21,0.51305707415194135]
["Leapfrog","SDGE",2,22,0]
["Leapfrog","SDGE",2,23,0]
["Leapfrog","SDGE",2,24,0]
["Leapfrog","SDGE",3,1,0]
["Leapfrog","SDGE",3,2,0]
["Leapfrog","SDGE",3,3,0]
["Leapfrog","SDGE",3,4,0]
["Leapfrog","SDGE",3,5,0]
["Leapfrog","SDGE",3,6,0]
["Leapfrog","SDGE",3,7,0]
["Leapfrog","SDGE",3,8,0]
["Leapfrog","SDGE",3,9,0]
["Leapfrog","SDGE",3,10,0]
["Leapfrog","SDGE",3,11,0]
["Leapfrog","SDGE",3,12,0]
["Leapfrog","SDGE",3,13,0]
["Leapfrog","SDGE",3,14,0]
["Leapfrog","SDGE",3,15,0]
["Leapfrog","SDGE",3,16,0]
["Leapfrog","SDGE",3,17,0]
["Leapfrog","SDGE",3,18,2.233836791508105]
["Leapfrog","SDGE",3,19,1.134802121514829]
["Leapfrog","SDGE",3,20,0.5591719698385953]
["Leapfrog","SDGE",3,21,0.5439957651718994]
["Leapfrog","SDGE",3,22,0.52819334607991364]
["Leapfrog","SDGE",3,23,0]
["Leapfrog","SDGE",3,24,0]
["Leapfrog","SDGE",4,1,0]
["Leapfrog","SDGE",4,2,0]
["Leapfrog","SDGE",4,3,0]
["Leapfrog","SDGE",4,4,0]
["Leapfrog","SDGE",4,5,0]
["Leapfrog","SDGE",4,6,0]
["Leapfrog","SDGE",4,7,0]
["Leapfrog","SDGE",4,8,0]
["Leapfrog","SDGE",4,9,0]
["Leapfrog","SDGE",4,10,0]
["Leapfrog","SDGE",4,11,0]
["Leapfrog","SDGE",4,12,0]
["Leapfrog","SDGE",4,13,0]
["Leapfrog","SDGE",4,14,0]
["Leapfrog","SDGE",4,15,0]
["Leapfrog","SDGE",4,16,0]
["Leapfrog","SDGE",4,17,0]
["Leapfrog","SDGE",4,18,0.96969299690559074]
["Leapfrog","SDGE",4,19,1.1377848060586375]
["Leapfrog","SDGE",4,20,1.0542387405335707]
["Leapfrog","SDGE",4,21,0.95459976037565919]
["Leapfrog","SDGE",4,22,0.88419960240975659]
["Leapfrog","SDGE",4,23,0]
["Leapfrog","SDGE",4,24,0]
["Leapfrog","SDGE",5,1,0]
["Leapfrog","SDGE",5,2,0]
["Leapfrog","SDGE",5,3,0]
["Leapfrog","SDGE",5,4,0]
["Leapfrog","SDGE",5,5,0]
["Leapfrog","SDGE",5,6,0]
["Leapfrog","SDGE",5,7,0]
["Leapfrog","SDGE",5,8,0]
["Leapfrog","SDGE",5,9,0]
["Leapfrog","SDGE",5,10,0]
["Leapfrog","SDGE",5,11,0]
["Leapfrog","SDGE",5,12,0]
["Leapfrog","SDGE",5,13,0]
["Leapfrog","SDGE",5,14,0]
["Leapfrog","SDGE",5,15,0]
["Leapfrog","SDGE",5,16,0]
["Leapfrog","SDGE",5,17,0]
["Leapfrog","SDGE",5,18,0.95568996816804408]
["Leapfrog","SDGE",5,19,1.1379815895755989]
["Leapfrog","SDGE",5,20,1.054994918948621]
["Leapfrog","SDGE",5,21,0.9673377702856889]
["Leapfrog","SDGE",5,22,0.88399581003105743]
["Leapfrog","SDGE",5,23,0]
["Leapfrog","SDGE",5,24,0]
["Leapfrog","SDGE",6,1,0]
["Leapfrog","SDGE",6,2,0]
["Leapfrog","SDGE",6,3,0]
["Leapfrog","SDGE",6,4,0]
["Leapfrog","SDGE",6,5,0]
["Leapfrog","SDGE",6,6,0]
["Leapfrog","SDGE",6,7,0]
["Leapfrog","SDGE",6,8,0]
["Leapfrog","SDGE",6,9,0]
["Leapfrog","SDGE",6,10,0]
["Leapfrog","SDGE",6,11,0]
["Leapfrog","SDGE",6,12,0]
["Leapfrog","SDGE",6,13,0]
["Leapfrog","SDGE",6,14,0]
["Leapfrog","SDGE",6,15,0]
["Leapfrog","SDGE",6,16,0]
["Leapfrog","SDGE",6,17,0.88458204469665525]
["Leapfrog","SDGE",6,18,1.0634209316440857]
["Leapfrog","SDGE",6,19,1.0640695062803724]
["Leapfrog","SDGE",6,20,1.0287962110222508]
["Leapfrog","SDGE",6,21,0.9591312964367692]
["Leapfrog","SDGE",6,22,0]
["Leapfrog","SDGE",6,23,0]
["Leapfrog","SDGE",6,24,0]
["Leapfrog","SDGE",7,1,0]
["Leapfrog","SDGE",7,2,0]
["Leapfrog","SDGE",7,3,0]
["Leapfrog","SDGE",7,4,0]
["Leapfrog","SDGE",7,5,0]
["Leapfrog","SDGE",7,6,0]
["Leapfrog","SDGE",7,7,0]
["Leapfrog","SDGE",7,8,0]
["Leapfrog","SDGE",7,9,0]
["Leapfrog","SDGE",7,10,0]
["Leapfrog","SDGE",7,11,0]
["Leapfrog","SDGE",7,12,0]
["Leapfrog","SDGE",7,13,0]
["Leapfrog","SDGE",7,14,0]
["Leapfrog","SDGE",7,15,0]
["Leapfrog","SDGE",7,16,0]
["Leapfrog","SDGE",7,17,1.1934142338682183]
["Leapfrog","SDGE",7,18,0.82022979409416885]
["Leapfrog","SDGE",7,19,0.72942133072184245]
["Leapfrog","SDGE",7,20,1.1897554779192061]
["Leapfrog","SDGE",7,21,1.0671790035864035]
["Leapfrog","SDGE",7,22,0]
["Leapfrog","SDGE",7,23,0]
["Leapfrog","SDGE",7,24,0]
["Leapfrog","SDGE",8,1,0]
["Leapfrog","SDGE",8,2,0]
["Leapfrog","SDGE",8,3,0]
["Leapfrog","SDGE",8,4,0]
["Leapfrog","SDGE",8,5,0]
["Leapfrog","SDGE",8,6,0]
["Leapfrog","SDGE",8,7,0]
["Leapfrog","SDGE",8,8,0]
["Leapfrog","SDGE",8,9,0]
["Leapfrog","SDGE",8,10,0]
["Leapfrog","SDGE",8,11,0]
["Leapfrog","SDGE",8,12,0]
["Leapfrog","SDGE",8,13,0]
["Leapfrog","SDGE",8,14,0]
["Leapfrog","SDGE",8,15,0]
["Leapfrog","SDGE",8,16,0]
["Leapfrog","SDGE",8,17,1.2474718679820613]
["Leapfrog","SDGE",8,18,0.73817969761238877]
["Leapfrog","SDGE",8,19,0.60876231908001943]
["Leapfrog","SDGE",8,20,1.2583140664417589]
["Leapfrog","SDGE",8,21,1.1472721153060579]
["Leapfrog","SDGE",8,22,0]
["Leapfrog","SDGE",8,23,0]
["Leapfrog","SDGE",8,24,0]
["Leapfrog","SDGE",9,1,0]
["Leapfrog","SDGE",9,2,0]
["Leapfrog","SDGE",9,3,0]
["Leapfrog","SDGE",9,4,0]
["Leapfrog","SDGE",9,5,0]
["Leapfrog","SDGE",9,6,0]
["Leapfrog","SDGE",9,7,0]
["Leapfrog","SDGE",9,8,0]
["Leapfrog","SDGE",9,9,0]
["Leapfrog","SDGE",9,10,0]
["Leapfrog","SDGE",9,11,0]
["Leapfrog","SDGE",9,12,0]
["Leapfrog","SDGE",9,13,0]
["Leapfrog","SDGE",9,14,0]
["Leapfrog","SDGE",9,15,0]
["Leapfrog","SDGE",9,16,0]
["Leapfrog","SDGE",9,17,1.104831205664953]
["Leapfrog","SDGE",9,18,0.71637394256791753]
["Leapfrog","SDGE",9,19,0.67213890360198225]
["Leapfrog","SDGE",9,20,1.3005830663783606]
["Leapfrog","SDGE",9,21,1.2060728307043751]
["Leapfrog","SDGE",9,22,0]
["Leapfrog","SDGE",9,23,0]
["Leapfrog","SDGE",9,24,0]
["Leapfrog","SDGE",10,1,0]
["Leapfrog","SDGE",10,2,0]
["Leapfrog","SDGE",10,3,0]
["Leapfrog","SDGE",10,4,0]
["Leapfrog","SDGE",10,5,0]
["Leapfrog","SDGE",10,6,0]
["Leapfrog","SDGE",10,7,0]
["Leapfrog","SDGE",10,8,0]
["Leapfrog","SDGE",10,9,0]
["Leapfrog","SDGE",10,10,0]
["Leapfrog","SDGE",10,11,0]
["Leapfrog","SDGE",10,12,0]
["Leapfrog","SDGE",10,13,0]
["Leapfrog","SDGE",10,14,0]
["Leapfrog","SDGE",10,15,0]
["Leapfrog","SDGE",10,16,0]
["Leapfrog","SDGE",10,17,1.1579174890395356]
["Leapfrog","SDGE",10,18,0.72331983694672919]
["Leapfrog","SDGE",10,19,0.66825653616298109]
["Leapfrog","SDGE",10,20,1.2971664390206239]
["Leapfrog","SDGE",10,21,1.153339646416941]
["Leapfrog","SDGE",10,22,0]
["Leapfrog","SDGE",10,23,0]
["Leapfrog","SDGE",10,24,0]
["Leapfrog","SDGE",11,1,0]
["Leapfrog","SDGE",11,2,0]
["Leapfrog","SDGE",11,3,0]
["Leapfrog","SDGE",11,4,0]
["Leapfrog","SDGE",11,5,0]
["Leapfrog","SDGE",11,6,0]
["Leapfrog","SDGE",11,7,0]
["Leapfrog","SDGE",11,8,0]
["Leapfrog","SDGE",11,9,0]
["Leapfrog","SDGE",11,10,0]
["Leapfrog","SDGE",11,11,0]
["Leapfrog","SDGE",11,12,0]
["Leapfrog","SDGE",11,13,0]
["Leapfrog","SDGE",11,14,0]
["Leapfrog","SDGE",11,15,0]
["Leapfrog","SDGE",11,16,0]
["Leapfrog","SDGE",11,17,1.5583517528675523]
["Leapfrog","SDGE",11,18,1.515896764678319]
["Leapfrog","SDGE",11,19,0.98258211785607186]
["Leapfrog","SDGE",11,20,0.50666275386714466]
["Leapfrog","SDGE",11,21,0.43650659887546484]
["Leapfrog","SDGE",11,22,0]
["Leapfrog","SDGE",11,23,0]
["Leapfrog","SDGE",11,24,0]
["Leapfrog","SDGE",12,1,0]
["Leapfrog","SDGE",12,2,0]
["Leapfrog","SDGE",12,3,0]
["Leapfrog","SDGE",12,4,0]
["Leapfrog","SDGE",12,5,0]
["Leapfrog","SDGE",12,6,0]
["Leapfrog","SDGE",12,7,0]
["Leapfrog","SDGE",12,8,0]
["Leapfrog","SDGE",12,9,0]
["Leapfrog","SDGE",12,10,0]
["Leapfrog","SDGE",12,11,0]
["Leapfrog","SDGE",12,12,0]
["Leapfrog","SDGE",12,13,0]
["Leapfrog","SDGE",12,14,0]
["Leapfrog","SDGE",12,15,0]
["Leapfrog","SDGE",12,16,0]
["Leapfrog","SDGE",12,17,1.5383944205377551]
["Leapfrog","SDGE",12,18,1.5423325859699124]
["Leapfrog","SDGE",12,19,0.88800286103806481]
["Leapfrog","SDGE",12,20,0.41456633867654002]
["Leapfrog","SDGE",12,21,0.61670379180881896]
["Leapfrog","SDGE",12,22,0]
["Leapfrog","SDGE",12,23,0]
["Leapfrog","SDGE",12,24,0]
["Voltus","PGE",1,1,0]
["Voltus","PGE",1,2,0]
["Voltus","PGE",1,3,0]
["Voltus","PGE",1,4,0]
["Voltus","PGE",1,5,0]
["Voltus","PGE",1,6,0]
["Voltus","PGE",1,7,0]
["Voltus","PGE",1,8,0]
["Voltus","PGE",1,9,0]
["Voltus","PGE",1,10,0]
["Voltus","PGE",1,11,0]
["Voltus","PGE",1,12,0]
["Voltus","PGE",1,13,0]
["Voltus","PGE",1,14,0]
["Voltus","PGE",1,15,0]
["Voltus","PGE",1,16,0]
["Voltus","PGE",1,17,1.1749561291193766]
["Voltus","PGE",1,18,1.1268951178477726]
["Voltus","PGE",1,19,0.94356783302640601]
["Voltus","PGE",1,20,0.91311121117470351]
["Voltus","PGE",1,21,0.84146970883174199]
["Voltus","PGE",1,22,0]
["Voltus","PGE",1,23,0]
["Voltus","PGE",1,24,0]
["Voltus","PGE",2,1,0]
["Voltus","PGE",2,2,0]
["Voltus","PGE",2,3,0]
["Voltus","PGE",2,4,0]
["Voltus","PGE",2,5,0]
["Voltus","PGE",2,6,0]
["Voltus","PGE",2,7,0]
["Voltus","PGE",2,8,0]
["Voltus","PGE",2,9,0]
["Voltus","PGE",2,10,0]
["Voltus","PGE",2,11,0]
["Voltus","PGE",2,12,0]
["Voltus","PGE",2,13,0]
["Voltus","PGE",2,14,0]
["Voltus","PGE",2,15,0]
["Voltus","PGE",2,16,0]
["Voltus","PGE",2,17,1.1749561291193766]
["Voltus","PGE",2,18,1.1268951178477726]
["Voltus","PGE",2,19,0.94356783302640601]
["Voltus","PGE",2,20,0.91311121117470351]
["Voltus","PGE",2,21,0.84146970883174199]
["Voltus","PGE",2,22,0]
["Voltus","PGE",2,23,0]
["Voltus","PGE",2,24,0]
["Voltus","PGE",3,1,0]
["Voltus","PGE",3,2,0]
["Voltus","PGE",3,3,0]
["Voltus","PGE",3,4,0]
["Voltus","PGE",3,5,0]
["Voltus","PGE",3,6,0]
["Voltus","PGE",3,7,0]
["Voltus","PGE",3,8,0]
["Voltus","PGE",3,9,0]
["Voltus","PGE",3,10,0]
["Voltus","PGE",3,11,0]
["Voltus","PGE",3,12,0]
["Voltus","PGE",3,13,0]
["Voltus","PGE",3,14,0]
["Voltus","PGE",3,15,0]
["Voltus","PGE",3,16,0]
["Voltus","PGE",3,17,0]
["Voltus","PGE",3,18,0.99308203086915836]
["Voltus","PGE",3,19,1.0707053410348244]
["Voltus","PGE",3,20,0.97307446836527678]
["Voltus","PGE",3,21,1.0042407297117069]
["Voltus","PGE",3,22,0.95889743001903371]
["Voltus","PGE",3,23,0]
["Voltus","PGE",3,24,0]
["Voltus","PGE",4,1,0]
["Voltus","PGE",4,2,0]
["Voltus","PGE",4,3,0]
["Voltus","PGE",4,4,0]
["Voltus","PGE",4,5,0]
["Voltus","PGE",4,6,0]
["Voltus","PGE",4,7,0]
["Voltus","PGE",4,8,0]
["Voltus","PGE",4,9,0]
["Voltus","PGE",4,10,0]
["Voltus","PGE",4,11,0]
["Voltus","PGE",4,12,0]
["Voltus","PGE",4,13,0]
["Voltus","PGE",4,14,0]
["Voltus","PGE",4,15,0]
["Voltus","PGE",4,16,0]
["Voltus","PGE",4,17,0]
["Voltus","PGE",4,18,0.99308203086915836]
["Voltus","PGE",4,19,1.0707053410348244]
["Voltus","PGE",4,20,0.97307446836527678]
["Voltus","PGE",4,21,1.0042407297117069]
["Voltus","PGE",4,22,0.95889743001903371]
["Voltus","PGE",4,23,0]
["Voltus","PGE",4,24,0]
["Voltus","PGE",5,1,0]
["Voltus","PGE",5,2,0]
["Voltus","PGE",5,3,0]
["Voltus","PGE",5,4,0]
["Voltus","PGE",5,5,0]
["Voltus","PGE",5,6,0]
["Voltus","PGE",5,7,0]
["Voltus","PGE",5,8,0]
["Voltus","PGE",5,9,0]
["Voltus","PGE",5,10,0]
["Voltus","PGE",5,11,0]
["Voltus","PGE",5,12,0]
["Voltus","PGE",5,13,0]
["Voltus","PGE",5,14,0]
["Voltus","PGE",5,15,0]
["Voltus","PGE",5,16,0]
["Voltus","PGE",5,17,0]
["Voltus","PGE",5,18,0.98748784352970465]
["Voltus","PGE",5,19,1.030662673336219]
["Voltus","PGE",5,20,0.99740479435116125]
["Voltus","PGE",5,21,1.0134956797148664]
["Voltus","PGE",5,22,0.97094900906804904]
["Voltus","PGE",5,23,0]
["Voltus","PGE",5,24,0]
["Voltus","PGE",6,1,0]
["Voltus","PGE",6,2,0]
["Voltus","PGE",6,3,0]
["Voltus","PGE",6,4,0]
["Voltus","PGE",6,5,0]
["Voltus","PGE",6,6,0]
["Voltus","PGE",6,7,0]
["Voltus","PGE",6,8,0]
["Voltus","PGE",6,9,0]
["Voltus","PGE",6,10,0]
["Voltus","PGE",6,11,0]
["Voltus","PGE",6,12,0]
["Voltus","PGE",6,13,0]
["Voltus","PGE",6,14,0]
["Voltus","PGE",6,15,0]
["Voltus","PGE",6,16,0]
["Voltus","PGE",6,17,0.98260199805405901]
["Voltus","PGE",6,18,1.024000010975626]
["Voltus","PGE",6,19,0.9952261620005739]
["Voltus","PGE",6,20,1.0196190533988907]
["Voltus","PGE",6,21,0.97855277557084985]
["Voltus","PGE",6,22,0]
["Voltus","PGE",6,23,0]
["Voltus","PGE",6,24,0]
["Voltus","PGE",7,1,0]
["Voltus","PGE",7,2,0]
["Voltus","PGE",7,3,0]
["Voltus","PGE",7,4,0]
["Voltus","PGE",7,5,0]
["Voltus","PGE",7,6,0]
["Voltus","PGE",7,7,0]
["Voltus","PGE",7,8,0]
["Voltus","PGE",7,9,0]
["Voltus","PGE",7,10,0]
["Voltus","PGE",7,11,0]
["Voltus","PGE",7,12,0]
["Voltus","PGE",7,13,0]
["Voltus","PGE",7,14,0]
["Voltus","PGE",7,15,0]
["Voltus","PGE",7,16,0]
["Voltus","PGE",7,17,1.1422221115359998]
["Voltus","PGE",7,18,1.1205508565196487]
["Voltus","PGE",7,19,0.9292441935740865]
["Voltus","PGE",7,20,0.93307404480940437]
["Voltus","PGE",7,21,0.8749087935608606]
["Voltus","PGE",7,22,0]
["Voltus","PGE",7,23,0]
["Voltus","PGE",7,24,0]
["Voltus","PGE",8,1,0]
["Voltus","PGE",8,2,0]
["Voltus","PGE",8,3,0]
["Voltus","PGE",8,4,0]
["Voltus","PGE",8,5,0]
["Voltus","PGE",8,6,0]
["Voltus","PGE",8,7,0]
["Voltus","PGE",8,8,0]
["Voltus","PGE",8,9,0]
["Voltus","PGE",8,10,0]
["Voltus","PGE",8,11,0]
["Voltus","PGE",8,12,0]
["Voltus","PGE",8,13,0]
["Voltus","PGE",8,14,0]
["Voltus","PGE",8,15,0]
["Voltus","PGE",8,16,0]
["Voltus","PGE",8,17,1.1093029660700771]
["Voltus","PGE",8,18,1.08146105386727]
["Voltus","PGE",8,19,0.94008127945586295]
["Voltus","PGE",8,20,0.9550080692691415]
["Voltus","PGE",8,21,0.91414663133764884]
["Voltus","PGE",8,22,0]
["Voltus","PGE",8,23,0]
["Voltus","PGE",8,24,0]
["Voltus","PGE",9,1,0]
["Voltus","PGE",9,2,0]
["Voltus","PGE",9,3,0]
["Voltus","PGE",9,4,0]
["Voltus","PGE",9,5,0]
["Voltus","PGE",9,6,0]
["Voltus","PGE",9,7,0]
["Voltus","PGE",9,8,0]
["Voltus","PGE",9,9,0]
["Voltus","PGE",9,10,0]
["Voltus","PGE",9,11,0]
["Voltus","PGE",9,12,0]
["Voltus","PGE",9,13,0]
["Voltus","PGE",9,14,0]
["Voltus","PGE",9,15,0]
["Voltus","PGE",9,16,0]
["Voltus","PGE",9,17,1.1356528855011032]
["Voltus","PGE",9,18,1.1014585338282841]
["Voltus","PGE",9,19,0.96580155347502128]
["Voltus","PGE",9,20,0.94286866164566541]
["Voltus","PGE",9,21,0.85421836554992581]
["Voltus","PGE",9,22,0]
["Voltus","PGE",9,23,0]
["Voltus","PGE",9,24,0]
["Voltus","PGE",10,1,0]
["Voltus","PGE",10,2,0]
["Voltus","PGE",10,3,0]
["Voltus","PGE",10,4,0]
["Voltus","PGE",10,5,0]
["Voltus","PGE",10,6,0]
["Voltus","PGE",10,7,0]
["Voltus","PGE",10,8,0]
["Voltus","PGE",10,9,0]
["Voltus","PGE",10,10,0]
["Voltus","PGE",10,11,0]
["Voltus","PGE",10,12,0]
["Voltus","PGE",10,13,0]
["Voltus","PGE",10,14,0]
["Voltus","PGE",10,15,0]
["Voltus","PGE",10,16,0]
["Voltus","PGE",10,17,1.1749561291193766]
["Voltus","PGE",10,18,1.1268951178477726]
["Voltus","PGE",10,19,0.94356783302640601]
["Voltus","PGE",10,20,0.91311121117470351]
["Voltus","PGE",10,21,0.84146970883174199]
["Voltus","PGE",10,22,0]
["Voltus","PGE",10,23,0]
["Voltus","PGE",10,24,0]
["Voltus","PGE",11,1,0]
["Voltus","PGE",11,2,0]
["Voltus","PGE",11,3,0]
["Voltus","PGE",11,4,0]
["Voltus","PGE",11,5,0]
["Voltus","PGE",11,6,0]
["Voltus","PGE",11,7,0]
["Voltus","PGE",11,8,0]
["Voltus","PGE",11,9,0]
["Voltus","PGE",11,10,0]
["Voltus","PGE",11,11,0]
["Voltus","PGE",11,12,0]
["Voltus","PGE",11,13,0]
["Voltus","PGE",11,14,0]
["Voltus","PGE",11,15,0]
["Voltus","PGE",11,16,0]
["Voltus","PGE",11,17,1.1749561291193766]
["Voltus","PGE",11,18,1.1268951178477726]
["Voltus","PGE",11,19,0.94356783302640601]
["Voltus","PGE",11,20,0.91311121117470351]
["Voltus","PGE",11,21,0.84146970883174199]
["Voltus","PGE",11,22,0]
["Voltus","PGE",11,23,0]
["Voltus","PGE",11,24,0]
["Voltus","PGE",12,1,0]
["Voltus","PGE",12,2,0]
["Voltus","PGE",12,3,0]
["Voltus","PGE",12,4,0]
["Voltus","PGE",12,5,0]
["Voltus","PGE",12,6,0]
["Voltus","PGE",12,7,0]
["Voltus","PGE",12,8,0]
["Voltus","PGE",12,9,0]
["Voltus","PGE",12,10,0]
["Voltus","PGE",12,11,0]
["Voltus","PGE",12,12,0]
["Voltus","PGE",12,13,0]
["Voltus","PGE",12,14,0]
["Voltus","PGE",12,15,0]
["Voltus","PGE",12,16,0]
["Voltus","PGE",12,17,1.1749561291193766]
["Voltus","PGE",12,18,1.1268951178477726]
["Voltus","PGE",12,19,0.94356783302640601]
["Voltus","PGE",12,20,0.91311121117470351]
["Voltus","PGE",12,21,0.84146970883174199]
["Voltus","PGE",12,22,0]
["Voltus","PGE",12,23,0]
["Voltus","PGE",12,24,0]
["Nostromo","SCE",1,1,0]
["Nostromo","SCE",1,2,0]
["Nostromo","SCE",1,3,0]
["Nostromo","SCE",1,4,0]
["Nostromo","SCE",1,5,0]
["Nostromo","SCE",1,6,0]
["Nostromo","SCE",1,7,0]
["Nostromo","SCE",1,8,0]
["Nostromo","SCE",1,9,0]
["Nostromo","SCE",1,10,0]
["Nostromo","SCE",1,11,0]
["Nostromo","SCE",1,12,0]
["Nostromo","SCE",1,13,0]
["Nostromo","SCE",1,14,0]
["Nostromo","SCE",1,15,0]
["Nostromo","SCE",1,16,0]
["Nostromo","SCE",1,17,1.3253452365611198]
["Nostromo","SCE",1,18,1.3047272063778279]
["Nostromo","SCE",1,19,0.86119135423914184]
["Nostromo","SCE",1,20,0.79644663883021205]
["Nostromo","SCE",1,21,0.7122895639916994]
["Nostromo","SCE",1,22,0]
["Nostromo","SCE",1,23,0]
["Nostromo","SCE",1,24,0]
["Nostromo","SCE",2,1,0]
["Nostromo","SCE",2,2,0]
["Nostromo","SCE",2,3,0]
["Nostromo","SCE",2,4,0]
["Nostromo","SCE",2,5,0]
["Nostromo","SCE",2,6,0]
["Nostromo","SCE",2,7,0]
["Nostromo","SCE",2,8,0]
["Nostromo","SCE",2,9,0]
["Nostromo","SCE",2,10,0]
["Nostromo","SCE",2,11,0]
["Nostromo","SCE",2,12,0]
["Nostromo","SCE",2,13,0]
["Nostromo","SCE",2,14,0]
["Nostromo","SCE",2,15,0]
["Nostromo","SCE",2,16,0]
["Nostromo","SCE",2,17,1.4771183714599179]
["Nostromo","SCE",2,18,1.4407515552247678]
["Nostromo","SCE",2,19,0.74742046381172]
["Nostromo","SCE",2,20,0.70120806420465054]
["Nostromo","SCE",2,21,0.6335015452989442]
["Nostromo","SCE",2,22,0]
["Nostromo","SCE",2,23,0]
["Nostromo","SCE",2,24,0]
["Nostromo","SCE",3,1,0]
["Nostromo","SCE",3,2,0]
["Nostromo","SCE",3,3,0]
["Nostromo","SCE",3,4,0]
["Nostromo","SCE",3,5,0]
["Nostromo","SCE",3,6,0]
["Nostromo","SCE",3,7,0]
["Nostromo","SCE",3,8,0]
["Nostromo","SCE",3,9,0]
["Nostromo","SCE",3,10,0]
["Nostromo","SCE",3,11,0]
["Nostromo","SCE",3,12,0]
["Nostromo","SCE",3,13,0]
["Nostromo","SCE",3,14,0]
["Nostromo","SCE",3,15,0]
["Nostromo","SCE",3,16,0]
["Nostromo","SCE",3,17,0]
["Nostromo","SCE",3,18,1.4830974257726681]
["Nostromo","SCE",3,19,0.91155863403080795]
["Nostromo","SCE",3,20,0.88107046876761297]
["Nostromo","SCE",3,21,0.86922474860102183]
["Nostromo","SCE",3,22,0.85504872282788891]
["Nostromo","SCE",3,23,0]
["Nostromo","SCE",3,24,0]
["Nostromo","SCE",4,1,0]
["Nostromo","SCE",4,2,0]
["Nostromo","SCE",4,3,0]
["Nostromo","SCE",4,4,0]
["Nostromo","SCE",4,5,0]
["Nostromo","SCE",4,6,0]
["Nostromo","SCE",4,7,0]
["Nostromo","SCE",4,8,0]
["Nostromo","SCE",4,9,0]
["Nostromo","SCE",4,10,0]
["Nostromo","SCE",4,11,0]
["Nostromo","SCE",4,12,0]
["Nostromo","SCE",4,13,0]
["Nostromo","SCE",4,14,0]
["Nostromo","SCE",4,15,0]
["Nostromo","SCE",4,16,0]
["Nostromo","SCE",4,17,0]
["Nostromo","SCE",4,18,1.1068964322898625]
["Nostromo","SCE",4,19,1.0559825658699902]
["Nostromo","SCE",4,20,1.0037152689059936]
["Nostromo","SCE",4,21,0.94274441627967076]
["Nostromo","SCE",4,22,0.89066131665448256]
["Nostromo","SCE",4,23,0]
["Nostromo","SCE",4,24,0]
["Nostromo","SCE",5,1,0]
["Nostromo","SCE",5,2,0]
["Nostromo","SCE",5,3,0]
["Nostromo","SCE",5,4,0]
["Nostromo","SCE",5,5,0]
["Nostromo","SCE",5,6,0]
["Nostromo","SCE",5,7,0]
["Nostromo","SCE",5,8,0]
["Nostromo","SCE",5,9,0]
["Nostromo","SCE",5,10,0]
["Nostromo","SCE",5,11,0]
["Nostromo","SCE",5,12,0]
["Nostromo","SCE",5,13,0]
["Nostromo","SCE",5,14,0]
["Nostromo","SCE",5,15,0]
["Nostromo","SCE",5,16,0]
["Nostromo","SCE",5,17,0]
["Nostromo","SCE",5,18,1.0734346971904631]
["Nostromo","SCE",5,19,0.99056619188182693]
["Nostromo","SCE",5,20,0.95796558688654299]
["Nostromo","SCE",5,21,0.90459882685070503]
["Nostromo","SCE",5,22,0.85355431094103196]
["Nostromo","SCE",5,23,0]
["Nostromo","SCE",5,24,0]
["Nostromo","SCE",6,1,0]
["Nostromo","SCE",6,2,0]
["Nostromo","SCE",6,3,0]
["Nostromo","SCE",6,4,0]
["Nostromo","SCE",6,5,0]
["Nostromo","SCE",6,6,0]
["Nostromo","SCE",6,7,0]
["Nostromo","SCE",6,8,0]
["Nostromo","SCE",6,9,0]
["Nostromo","SCE",6,10,0]
["Nostromo","SCE",6,11,0]
["Nostromo","SCE",6,12,0]
["Nostromo","SCE",6,13,0]
["Nostromo","SCE",6,14,0]
["Nostromo","SCE",6,15,0]
["Nostromo","SCE",6,16,0]
["Nostromo","SCE",6,17,1.0031820874383801]
["Nostromo","SCE",6,18,1.0031820874383801]
["Nostromo","SCE",6,19,0.99647893781534902]
["Nostromo","SCE",6,20,1.0031820874383801]
["Nostromo","SCE",6,21,0.99397479986951176]
["Nostromo","SCE",6,22,0]
["Nostromo","SCE",6,23,0]
["Nostromo","SCE",6,24,0]
["Nostromo","SCE",7,1,0]
["Nostromo","SCE",7,2,0]
["Nostromo","SCE",7,3,0]
["Nostromo","SCE",7,4,0]
["Nostromo","SCE",7,5,0]
["Nostromo","SCE",7,6,0]
["Nostromo","SCE",7,7,0]
["Nostromo","SCE",7,8,0]
["Nostromo","SCE",7,9,0]
["Nostromo","SCE",7,10,0]
["Nostromo","SCE",7,11,0]
["Nostromo","SCE",7,12,0]
["Nostromo","SCE",7,13,0]
["Nostromo","SCE",7,14,0]
["Nostromo","SCE",7,15,0]
["Nostromo","SCE",7,16,0]
["Nostromo","SCE",7,17,1.011285764420045]
["Nostromo","SCE",7,18,1.011285764420045]
["Nostromo","SCE",7,19,1.011285764420045]
["Nostromo","SCE",7,20,1.0057906500921561]
["Nostromo","SCE",7,21,0.96035205664770917]
["Nostromo","SCE",7,22,0]
["Nostromo","SCE",7,23,0]
["Nostromo","SCE",7,24,0]
["Nostromo","SCE",8,1,0]
["Nostromo","SCE",8,2,0]
["Nostromo","SCE",8,3,0]
["Nostromo","SCE",8,4,0]
["Nostromo","SCE",8,5,0]
["Nostromo","SCE",8,6,0]
["Nostromo","SCE",8,7,0]
["Nostromo","SCE",8,8,0]
["Nostromo","SCE",8,9,0]
["Nostromo","SCE",8,10,0]
["Nostromo","SCE",8,11,0]
["Nostromo","SCE",8,12,0]
["Nostromo","SCE",8,13,0]
["Nostromo","SCE",8,14,0]
["Nostromo","SCE",8,15,0]
["Nostromo","SCE",8,16,0]
["Nostromo","SCE",8,17,1.0051486465647714]
["Nostromo","SCE",8,18,1.0051486465647714]
["Nostromo","SCE",8,19,1.0051486465647714]
["Nostromo","SCE",8,20,1.0051486465647714]
["Nostromo","SCE",8,21,0.97940541374091405]
["Nostromo","SCE",8,22,0]
["Nostromo","SCE",8,23,0]
["Nostromo","SCE",8,24,0]
["Nostromo","SCE",9,1,0]
["Nostromo","SCE",9,2,0]
["Nostromo","SCE",9,3,0]
["Nostromo","SCE",9,4,0]
["Nostromo","SCE",9,5,0]
["Nostromo","SCE",9,6,0]
["Nostromo","SCE",9,7,0]
["Nostromo","SCE",9,8,0]
["Nostromo","SCE",9,9,0]
["Nostromo","SCE",9,10,0]
["Nostromo","SCE",9,11,0]
["Nostromo","SCE",9,12,0]
["Nostromo","SCE",9,13,0]
["Nostromo","SCE",9,14,0]
["Nostromo","SCE",9,15,0]
["Nostromo","SCE",9,16,0]
["Nostromo","SCE",9,17,1]
["Nostromo","SCE",9,18,1]
["Nostromo","SCE",9,19,1]
["Nostromo","SCE",9,20,1]
["Nostromo","SCE",9,21,1]
["Nostromo","SCE",9,22,0]
["Nostromo","SCE",9,23,0]
["Nostromo","SCE",9,24,0]
["Nostromo","SCE",10,1,0]
["Nostromo","SCE",10,2,0]
["Nostromo","SCE",10,3,0]
["Nostromo","SCE",10,4,0]
["Nostromo","SCE",10,5,0]
["Nostromo","SCE",10,6,0]
["Nostromo","SCE",10,7,0]
["Nostromo","SCE",10,8,0]
["Nostromo","SCE",10,9,0]
["Nostromo","SCE",10,10,0]
["Nostromo","SCE",10,11,0]
["Nostromo","SCE",10,12,0]
["Nostromo","SCE",10,13,0]
["Nostromo","SCE",10,14,0]
["Nostromo","SCE",10,15,0]
["Nostromo","SCE",10,16,0]
["Nostromo","SCE",10,17,1.0092475959224487]
["Nostromo","SCE",10,18,1.0092475959224487]
["Nostromo","SCE",10,19,1.0092475959224487]
["Nostromo","SCE",10,20,1.006912654869857]
["Nostromo","SCE",10,21,0.96534455736279645]
["Nostromo","SCE",10,22,0]
["Nostromo","SCE",10,23,0]
["Nostromo","SCE",10,24,0]
["Nostromo","SCE",11,1,0]
["Nostromo","SCE",11,2,0]
["Nostromo","SCE",11,3,0]
["Nostromo","SCE",11,4,0]
["Nostromo","SCE",11,5,0]
["Nostromo","SCE",11,6,0]
["Nostromo","SCE",11,7,0]
["Nostromo","SCE",11,8,0]
["Nostromo","SCE",11,9,0]
["Nostromo","SCE",11,10,0]
["Nostromo","SCE",11,11,0]
["Nostromo","SCE",11,12,0]
["Nostromo","SCE",11,13,0]
["Nostromo","SCE",11,14,0]
["Nostromo","SCE",11,15,0]
["Nostromo","SCE",11,16,0]
["Nostromo","SCE",11,17,1.0702800975885687]
["Nostromo","SCE",11,18,1.0702800975885687]
["Nostromo","SCE",11,19,1.0003453567974543]
["Nostromo","SCE",11,20,0.94758071066542326]
["Nostromo","SCE",11,21,0.91151373735998475]
["Nostromo","SCE",11,22,0]
["Nostromo","SCE",11,23,0]
["Nostromo","SCE",11,24,0]
["Nostromo","SCE",12,1,0]
["Nostromo","SCE",12,2,0]
["Nostromo","SCE",12,3,0]
["Nostromo","SCE",12,4,0]
["Nostromo","SCE",12,5,0]
["Nostromo","SCE",12,6,0]
["Nostromo","SCE",12,7,0]
["Nostromo","SCE",12,8,0]
["Nostromo","SCE",12,9,0]
["Nostromo","SCE",12,10,0]
["Nostromo","SCE",12,11,0]
["Nostromo","SCE",12,12,0]
["Nostromo","SCE",12,13,0]
["Nostromo","SCE",12,14,0]
["Nostromo","SCE",12,15,0]
["Nostromo","SCE",12,16,0]
["Nostromo","SCE",12,17,1.5261431854256633]
["Nostromo","SCE",12,18,1.4774384864489229]
["Nostromo","SCE",12,19,0.75250714593294732]
["Nostromo","SCE",12,20,0.66455807801150935]
["Nostromo","SCE",12,21,0.57935310418095642]
["Nostromo","SCE",12,22,0]
["Nostromo","SCE",12,23,0]
["Nostromo","SCE",12,24,0]
["Nostromo","SDGE",1,1,0]
["Nostromo","SDGE",1,2,0]
["Nostromo","SDGE",1,3,0]
["Nostromo","SDGE",1,4,0]
["Nostromo","SDGE",1,5,0]
["Nostromo","SDGE",1,6,0]
["Nostromo","SDGE",1,7,0]
["Nostromo","SDGE",1,8,0]
["Nostromo","SDGE",1,9,0]
["Nostromo","SDGE",1,10,0]
["Nostromo","SDGE",1,11,0]
["Nostromo","SDGE",1,12,0]
["Nostromo","SDGE",1,13,0]
["Nostromo","SDGE",1,14,0]
["Nostromo","SDGE",1,15,0]
["Nostromo","SDGE",1,16,0]
["Nostromo","SDGE",1,17,1.0188068426143035]
["Nostromo","SDGE",1,18,1.0101710397458528]
["Nostromo","SDGE",1,19,0.9997164349788441]
["Nostromo","SDGE",1,20,0.98905620693034524]
["Nostromo","SDGE",1,21,0.98224947573065369]
["Nostromo","SDGE",1,22,0]
["Nostromo","SDGE",1,23,0]
["Nostromo","SDGE",1,24,0]
["Nostromo","SDGE",2,1,0]
["Nostromo","SDGE",2,2,0]
["Nostromo","SDGE",2,3,0]
["Nostromo","SDGE",2,4,0]
["Nostromo","SDGE",2,5,0]
["Nostromo","SDGE",2,6,0]
["Nostromo","SDGE",2,7,0]
["Nostromo","SDGE",2,8,0]
["Nostromo","SDGE",2,9,0]
["Nostromo","SDGE",2,10,0]
["Nostromo","SDGE",2,11,0]
["Nostromo","SDGE",2,12,0]
["Nostromo","SDGE",2,13,0]
["Nostromo","SDGE",2,14,0]
["Nostromo","SDGE",2,15,0]
["Nostromo","SDGE",2,16,0]
["Nostromo","SDGE",2,17,1.0202861898039499]
["Nostromo","SDGE",2,18,1.0089271120004402]
["Nostromo","SDGE",2,19,0.99838353548278125]
["Nostromo","SDGE",2,20,0.99385038522864821]
["Nostromo","SDGE",2,21,0.97855277748418046]
["Nostromo","SDGE",2,22,0]
["Nostromo","SDGE",2,23,0]
["Nostromo","SDGE",2,24,0]
["Nostromo","SDGE",3,1,0]
["Nostromo","SDGE",3,2,0]
["Nostromo","SDGE",3,3,0]
["Nostromo","SDGE",3,4,0]
["Nostromo","SDGE",3,5,0]
["Nostromo","SDGE",3,6,0]
["Nostromo","SDGE",3,7,0]
["Nostromo","SDGE",3,8,0]
["Nostromo","SDGE",3,9,0]
["Nostromo","SDGE",3,10,0]
["Nostromo","SDGE",3,11,0]
["Nostromo","SDGE",3,12,0]
["Nostromo","SDGE",3,13,0]
["Nostromo","SDGE",3,14,0]
["Nostromo","SDGE",3,15,0]
["Nostromo","SDGE",3,16,0]
["Nostromo","SDGE",3,17,0]
["Nostromo","SDGE",3,18,1.0133883146189886]
["Nostromo","SDGE",3,19,1.0096173980368703]
["Nostromo","SDGE",3,20,1.0029959381587539]
["Nostromo","SDGE",3,21,0.99051046431144685]
["Nostromo","SDGE",3,22,0.98348788487394101]
["Nostromo","SDGE",3,23,0]
["Nostromo","SDGE",3,24,0]
["Nostromo","SDGE",4,1,0]
["Nostromo","SDGE",4,2,0]
["Nostromo","SDGE",4,3,0]
["Nostromo","SDGE",4,4,0]
["Nostromo","SDGE",4,5,0]
["Nostromo","SDGE",4,6,0]
["Nostromo","SDGE",4,7,0]
["Nostromo","SDGE",4,8,0]
["Nostromo","SDGE",4,9,0]
["Nostromo","SDGE",4,10,0]
["Nostromo","SDGE",4,11,0]
["Nostromo","SDGE",4,12,0]
["Nostromo","SDGE",4,13,0]
["Nostromo","SDGE",4,14,0]
["Nostromo","SDGE",4,15,0]
["Nostromo","SDGE",4,16,0]
["Nostromo","SDGE",4,17,0]
["Nostromo","SDGE",4,18,1.0342852391573156]
["Nostromo","SDGE",4,19,1.0270184578705779]
["Nostromo","SDGE",4,20,1.0005371585437568]
["Nostromo","SDGE",4,21,0.97599659900548374]
["Nostromo","SDGE",4,22,0.96216254542286617]
["Nostromo","SDGE",4,23,0]
["Nostromo","SDGE",4,24,0]
["Nostromo","SDGE",5,1,0]
["Nostromo","SDGE",5,2,0]
["Nostromo","SDGE",5,3,0]
["Nostromo","SDGE",5,4,0]
["Nostromo","SDGE",5,5,0]
["Nostromo","SDGE",5,6,0]
["Nostromo","SDGE",5,7,0]
["Nostromo","SDGE",5,8,0]
["Nostromo","SDGE",5,9,0]
["Nostromo","SDGE",5,10,0]
["Nostromo","SDGE",5,11,0]
["Nostromo","SDGE",5,12,0]
["Nostromo","SDGE",5,13,0]
["Nostromo","SDGE",5,14,0]
["Nostromo","SDGE",5,15,0]
["Nostromo","SDGE",5,16,0]
["Nostromo","SDGE",5,17,0]
["Nostromo","SDGE",5,18,1.026008852597706]
["Nostromo","SDGE",5,19,1.0210392869787115]
["Nostromo","SDGE",5,20,1.0009661089436936]
["Nostromo","SDGE",5,21,0.98020635455981064]
["Nostromo","SDGE",5,22,0.97177939692007786]
["Nostromo","SDGE",5,23,0]
["Nostromo","SDGE",5,24,0]
["Nostromo","SDGE",6,1,0]
["Nostromo","SDGE",6,2,0]
["Nostromo","SDGE",6,3,0]
["Nostromo","SDGE",6,4,0]
["Nostromo","SDGE",6,5,0]
["Nostromo","SDGE",6,6,0]
["Nostromo","SDGE",6,7,0]
["Nostromo","SDGE",6,8,0]
["Nostromo","SDGE",6,9,0]
["Nostromo","SDGE",6,10,0]
["Nostromo","SDGE",6,11,0]
["Nostromo","SDGE",6,12,0]
["Nostromo","SDGE",6,13,0]
["Nostromo","SDGE",6,14,0]
["Nostromo","SDGE",6,15,0]
["Nostromo","SDGE",6,16,0]
["Nostromo","SDGE",6,17,1.0141701699922743]
["Nostromo","SDGE",6,18,1.0107140309697682]
["Nostromo","SDGE",6,19,1.0055298224360094]
["Nostromo","SDGE",6,20,0.9934333358572387]
["Nostromo","SDGE",6,21,0.9761526407447092]
["Nostromo","SDGE",6,22,0]
["Nostromo","SDGE",6,23,0]
["Nostromo","SDGE",6,24,0]
["Nostromo","SDGE",7,1,0]
["Nostromo","SDGE",7,2,0]
["Nostromo","SDGE",7,3,0]
["Nostromo","SDGE",7,4,0]
["Nostromo","SDGE",7,5,0]
["Nostromo","SDGE",7,6,0]
["Nostromo","SDGE",7,7,0]
["Nostromo","SDGE",7,8,0]
["Nostromo","SDGE",7,9,0]
["Nostromo","SDGE",7,10,0]
["Nostromo","SDGE",7,11,0]
["Nostromo","SDGE",7,12,0]
["Nostromo","SDGE",7,13,0]
["Nostromo","SDGE",7,14,0]
["Nostromo","SDGE",7,15,0]
["Nostromo","SDGE",7,16,0]
["Nostromo","SDGE",7,17,1.0155349507316298]
["Nostromo","SDGE",7,18,1.0065291814573893]
["Nostromo","SDGE",7,19,0.99977485534599864]
["Nostromo","SDGE",7,20,0.99302052923460804]
["Nostromo","SDGE",7,21,0.98514048323037451]
["Nostromo","SDGE",7,22,0]
["Nostromo","SDGE",7,23,0]
["Nostromo","SDGE",7,24,0]
["Nostromo","SDGE",8,1,0]
["Nostromo","SDGE",8,2,0]
["Nostromo","SDGE",8,3,0]
["Nostromo","SDGE",8,4,0]
["Nostromo","SDGE",8,5,0]
["Nostromo","SDGE",8,6,0]
["Nostromo","SDGE",8,7,0]
["Nostromo","SDGE",8,8,0]
["Nostromo","SDGE",8,9,0]
["Nostromo","SDGE",8,10,0]
["Nostromo","SDGE",8,11,0]
["Nostromo","SDGE",8,12,0]
["Nostromo","SDGE",8,13,0]
["Nostromo","SDGE",8,14,0]
["Nostromo","SDGE",8,15,0]
["Nostromo","SDGE",8,16,0]
["Nostromo","SDGE",8,17,1.0197119747972851]
["Nostromo","SDGE",8,18,1.0130674887612452]
["Nostromo","SDGE",8,19,0.99977851668916617]
["Nostromo","SDGE",8,20,0.98981178763510724]
["Nostromo","SDGE",8,21,0.9776302321171958]
["Nostromo","SDGE",8,22,0]
["Nostromo","SDGE",8,23,0]
["Nostromo","SDGE",8,24,0]
["Nostromo","SDGE",9,1,0]
["Nostromo","SDGE",9,2,0]
["Nostromo","SDGE",9,3,0]
["Nostromo","SDGE",9,4,0]
["Nostromo","SDGE",9,5,0]
["Nostromo","SDGE",9,6,0]
["Nostromo","SDGE",9,7,0]
["Nostromo","SDGE",9,8,0]
["Nostromo","SDGE",9,9,0]
["Nostromo","SDGE",9,10,0]
["Nostromo","SDGE",9,11,0]
["Nostromo","SDGE",9,12,0]
["Nostromo","SDGE",9,13,0]
["Nostromo","SDGE",9,14,0]
["Nostromo","SDGE",9,15,0]
["Nostromo","SDGE",9,16,0]
["Nostromo","SDGE",9,17,1.0191419088158966]
["Nostromo","SDGE",9,18,1.0158415797097073]
["Nostromo","SDGE",9,19,1.0048404837891864]
["Nostromo","SDGE",9,20,0.98943894686019518]
["Nostromo","SDGE",9,21,0.97073708082501475]
["Nostromo","SDGE",9,22,0]
["Nostromo","SDGE",9,23,0]
["Nostromo","SDGE",9,24,0]
["Nostromo","SDGE",10,1,0]
["Nostromo","SDGE",10,2,0]
["Nostromo","SDGE",10,3,0]
["Nostromo","SDGE",10,4,0]
["Nostromo","SDGE",10,5,0]
["Nostromo","SDGE",10,6,0]
["Nostromo","SDGE",10,7,0]
["Nostromo","SDGE",10,8,0]
["Nostromo","SDGE",10,9,0]
["Nostromo","SDGE",10,10,0]
["Nostromo","SDGE",10,11,0]
["Nostromo","SDGE",10,12,0]
["Nostromo","SDGE",10,13,0]
["Nostromo","SDGE",10,14,0]
["Nostromo","SDGE",10,15,0]
["Nostromo","SDGE",10,16,0]
["Nostromo","SDGE",10,17,1.0252032792896304]
["Nostromo","SDGE",10,18,1.0206208659356206]
["Nostromo","SDGE",10,19,1.0068736224367811]
["Nostromo","SDGE",10,20,0.98510715127241233]
["Nostromo","SDGE",10,21,0.96219508106555596]
["Nostromo","SDGE",10,22,0]
["Nostromo","SDGE",10,23,0]
["Nostromo","SDGE",10,24,0]
["Nostromo","SDGE",11,1,0]
["Nostromo","SDGE",11,2,0]
["Nostromo","SDGE",11,3,0]
["Nostromo","SDGE",11,4,0]
["Nostromo","SDGE",11,5,0]
["Nostromo","SDGE",11,6,0]
["Nostromo","SDGE",11,7,0]
["Nostromo","SDGE",11,8,0]
["Nostromo","SDGE",11,9,0]
["Nostromo","SDGE",11,10,0]
["Nostromo","SDGE",11,11,0]
["Nostromo","SDGE",11,12,0]
["Nostromo","SDGE",11,13,0]
["Nostromo","SDGE",11,14,0]
["Nostromo","SDGE",11,15,0]
["Nostromo","SDGE",11,16,0]
["Nostromo","SDGE",11,17,1.0329996410253341]
["Nostromo","SDGE",11,18,1.0160524191002913]
["Nostromo","SDGE",11,19,0.99216943972343785]
["Nostromo","SDGE",11,20,0.98324619601833319]
["Nostromo","SDGE",11,21,0.97553230413260339]
["Nostromo","SDGE",11,22,0]
["Nostromo","SDGE",11,23,0]
["Nostromo","SDGE",11,24,0]
["Nostromo","SDGE",12,1,0]
["Nostromo","SDGE",12,2,0]
["Nostromo","SDGE",12,3,0]
["Nostromo","SDGE",12,4,0]
["Nostromo","SDGE",12,5,0]
["Nostromo","SDGE",12,6,0]
["Nostromo","SDGE",12,7,0]
["Nostromo","SDGE",12,8,0]
["Nostromo","SDGE",12,9,0]
["Nostromo","SDGE",12,10,0]
["Nostromo","SDGE",12,11,0]
["Nostromo","SDGE",12,12,0]
["Nostromo","SDGE",12,13,0]
["Nostromo","SDGE",12,14,0]
["Nostromo","SDGE",12,15,0]
["Nostromo","SDGE",12,16,0]
["Nostromo","SDGE",12,17,1.0282559974706931]
["Nostromo","SDGE",12,18,1.0128752765052766]
["Nostromo","SDGE",12,19,0.99746131672948402]
["Nostromo","SDGE",12,20,0.98699706808752896]
["Nostromo","SDGE",12,21,0.97441034120701697]
["Nostromo","SDGE",12,22,0]
["Nostromo","SDGE",12,23,0]
["Nostromo","SDGE",12,24,0]
["CPower","PGE",1,1,0]
["CPower","PGE",1,2,0]
["CPower","PGE",1,3,0]
["CPower","PGE",1,4,0]
["CPower","PGE",1,5,0]
["CPower","PGE",1,6,0]
["CPower","PGE",1,7,0]
["CPower","PGE",1,8,0]
["CPower","PGE",1,9,0]
["CPower","PGE",1,10,0]
["CPower","PGE",1,11,0]
["CPower","PGE",1,12,0]
["CPower","PGE",1,13,0]
["CPower","PGE",1,14,0]
["CPower","PGE",1,15,0]
["CPower","PGE",1,16,0]
["CPower","PGE",1,17,0]
["CPower","PGE",1,18,0]
["CPower","PGE",1,19,0]
["CPower","PGE",1,20,0]
["CPower","PGE",1,21,0]
["CPower","PGE",1,22,0]
["CPower","PGE",1,23,0]
["CPower","PGE",1,24,0]
["CPower","PGE",2,1,0]
["CPower","PGE",2,2,0]
["CPower","PGE",2,3,0]
["CPower","PGE",2,4,0]
["CPower","PGE",2,5,0]
["CPower","PGE",2,6,0]
["CPower","PGE",2,7,0]
["CPower","PGE",2,8,0]
["CPower","PGE",2,9,0]
["CPower","PGE",2,10,0]
["CPower","PGE",2,11,0]
["CPower","PGE",2,12,0]
["CPower","PGE",2,13,0]
["CPower","PGE",2,14,0]
["CPower","PGE",2,15,0]
["CPower","PGE",2,16,0]
["CPower","PGE",2,17,0]
["CPower","PGE",2,18,0]
["CPower","PGE",2,19,0]
["CPower","PGE",2,20,0]
["CPower","PGE",2,21,0]
["CPower","PGE",2,22,0]
["CPower","PGE",2,23,0]
["CPower","PGE",2,24,0]
["CPower","PGE",3,1,0]
["CPower","PGE",3,2,0]
["CPower","PGE",3,3,0]
["CPower","PGE",3,4,0]
["CPower","PGE",3,5,0]
["CPower","PGE",3,6,0]
["CPower","PGE",3,7,0]
["CPower","PGE",3,8,0]
["CPower","PGE",3,9,0]
["CPower","PGE",3,10,0]
["CPower","PGE",3,11,0]
["CPower","PGE",3,12,0]
["CPower","PGE",3,13,0]
["CPower","PGE",3,14,0]
["CPower","PGE",3,15,0]
["CPower","PGE",3,16,0]
["CPower","PGE",3,17,0]
["CPower","PGE",3,18,0]
["CPower","PGE",3,19,0]
["CPower","PGE",3,20,0]
["CPower","PGE",3,21,0]
["CPower","PGE",3,22,0]
["CPower","PGE",3,23,0]
["CPower","PGE",3,24,0]
["CPower","PGE",4,1,0]
["CPower","PGE",4,2,0]
["CPower","PGE",4,3,0]
["CPower","PGE",4,4,0]
["CPower","PGE",4,5,0]
["CPower","PGE",4,6,0]
["CPower","PGE",4,7,0]
["CPower","PGE",4,8,0]
["CPower","PGE",4,9,0]
["CPower","PGE",4,10,0]
["CPower","PGE",4,11,0]
["CPower","PGE",4,12,0]
["CPower","PGE",4,13,0]
["CPower","PGE",4,14,0]
["CPower","PGE",4,15,0]
["CPower","PGE",4,16,0]
["CPower","PGE",4,17,0]
["CPower","PGE",4,18,0]
["CPower","PGE",4,19,0]
["CPower","PGE",4,20,0]
["CPower","PGE",4,21,0]
["CPower","PGE",4,22,0]
["CPower","PGE",4,23,0]
["CPower","PGE",4,24,0]
["CPower","PGE",5,1,0]
["CPower","PGE",5,2,0]
["CPower","PGE",5,3,0]
["CPower","PGE",5,4,0]
["CPower","PGE",5,5,0]
["CPower","PGE",5,6,0]
["CPower","PGE",5,7,0]
["CPower","PGE",5,8,0]
["CPower","PGE",5,9,0]
["CPower","PGE",5,10,0]
["CPower","PGE",5,11,0]
["CPower","PGE",5,12,0]
["CPower","PGE",5,13,0]
["CPower","PGE",5,14,0]
["CPower","PGE",5,15,0]
["CPower","PGE",5,16,0]
["CPower","PGE",5,17,0]
["CPower","PGE",5,18,1.1203124560168893]
["CPower","PGE",5,19,1.1383335679099225]
["CPower","PGE",5,20,1.2900112596762841]
["CPower","PGE",5,21,1.1721231527093596]
["CPower","PGE",5,22,0.27955249824067552]
["CPower","PGE",5,23,0]
["CPower","PGE",5,24,0]
["CPower","PGE",6,1,0]
["CPower","PGE",6,2,0]
["CPower","PGE",6,3,0]
["CPower","PGE",6,4,0]
["CPower","PGE",6,5,0]
["CPower","PGE",6,6,0]
["CPower","PGE",6,7,0]
["CPower","PGE",6,8,0]
["CPower","PGE",6,9,0]
["CPower","PGE",6,10,0]
["CPower","PGE",6,11,0]
["CPower","PGE",6,12,0]
["CPower","PGE",6,13,0]
["CPower","PGE",6,14,0]
["CPower","PGE",6,15,0]
["CPower","PGE",6,16,0]
["CPower","PGE",6,17,1.2611491542798561]
["CPower","PGE",6,18,0.95816709379805209]
["CPower","PGE",6,19,1.1233305996924652]
["CPower","PGE",6,20,1.0845007688364938]
["CPower","PGE",6,21,0.57205638134290104]
["CPower","PGE",6,22,0]
["CPower","PGE",6,23,0]
["CPower","PGE",6,24,0]
["CPower","PGE",7,1,0]
["CPower","PGE",7,2,0]
["CPower","PGE",7,3,0]
["CPower","PGE",7,4,0]
["CPower","PGE",7,5,0]
["CPower","PGE",7,6,0]
["CPower","PGE",7,7,0]
["CPower","PGE",7,8,0]
["CPower","PGE",7,9,0]
["CPower","PGE",7,10,0]
["CPower","PGE",7,11,0]
["CPower","PGE",7,12,0]
["CPower","PGE",7,13,0]
["CPower","PGE",7,14,0]
["CPower","PGE",7,15,0]
["CPower","PGE",7,16,0]
["CPower","PGE",7,17,0.91518408360128611]
["CPower","PGE",7,18,0.82529533762057883]
["CPower","PGE",7,19,1.5781993569131829]
["CPower","PGE",7,20,1.1253247588424438]
["CPower","PGE",7,21,0.55657258842443724]
["CPower","PGE",7,22,0]
["CPower","PGE",7,23,0]
["CPower","PGE",7,24,0]
["CPower","PGE",8,1,0]
["CPower","PGE",8,2,0]
["CPower","PGE",8,3,0]
["CPower","PGE",8,4,0]
["CPower","PGE",8,5,0]
["CPower","PGE",8,6,0]
["CPower","PGE",8,7,0]
["CPower","PGE",8,8,0]
["CPower","PGE",8,9,0]
["CPower","PGE",8,10,0]
["CPower","PGE",8,11,0]
["CPower","PGE",8,12,0]
["CPower","PGE",8,13,0]
["CPower","PGE",8,14,0]
["CPower","PGE",8,15,0]
["CPower","PGE",8,16,0]
["CPower","PGE",8,17,1.3166994189117802]
["CPower","PGE",8,18,1.0455810882197571]
["CPower","PGE",8,19,1.07883676703645]
["CPower","PGE",8,20,0.91086740623349172]
["CPower","PGE",8,21,0.64707659799260431]
["CPower","PGE",8,22,0]
["CPower","PGE",8,23,0]
["CPower","PGE",8,24,0]
["CPower","PGE",9,1,0]
["CPower","PGE",9,2,0]
["CPower","PGE",9,3,0]
["CPower","PGE",9,4,0]
["CPower","PGE",9,5,0]
["CPower","PGE",9,6,0]
["CPower","PGE",9,7,0]
["CPower","PGE",9,8,0]
["CPower","PGE",9,9,0]
["CPower","PGE",9,10,0]
["CPower","PGE",9,11,0]
["CPower","PGE",9,12,0]
["CPower","PGE",9,13,0]
["CPower","PGE",9,14,0]
["CPower","PGE",9,15,0]
["CPower","PGE",9,16,0]
["CPower","PGE",9,17,0.83714994720168945]
["CPower","PGE",9,18,1.0264382259767686]
["CPower","PGE",9,19,1.1081251319957761]
["CPower","PGE",9,20,1.0230580781414993]
["CPower","PGE",9,21,1.0055939809926082]
["CPower","PGE",9,22,5.3676747624076024E-2]
["CPower","PGE",9,23,0]
["CPower","PGE",9,24,0]
["CPower","PGE",10,1,0]
["CPower","PGE",10,2,0]
["CPower","PGE",10,3,0]
["CPower","PGE",10,4,0]
["CPower","PGE",10,5,0]
["CPower","PGE",10,6,0]
["CPower","PGE",10,7,0]
["CPower","PGE",10,8,0]
["CPower","PGE",10,9,0]
["CPower","PGE",10,10,0]
["CPower","PGE",10,11,0]
["CPower","PGE",10,12,0]
["CPower","PGE",10,13,0]
["CPower","PGE",10,14,0]
["CPower","PGE",10,15,0]
["CPower","PGE",10,16,0]
["CPower","PGE",10,17,1.0588977803738315]
["CPower","PGE",10,18,0.83752021028037371]
["CPower","PGE",10,19,0.95693446261682225]
["CPower","PGE",10,20,1.1138682242990652]
["CPower","PGE",10,21,1.0318488317757009]
["CPower","PGE",10,22,0.13910887850467288]
["CPower","PGE",10,23,0]
["CPower","PGE",10,24,0]
["CPower","PGE",11,1,0]
["CPower","PGE",11,2,0]
["CPower","PGE",11,3,0]
["CPower","PGE",11,4,0]
["CPower","PGE",11,5,0]
["CPower","PGE",11,6,0]
["CPower","PGE",11,7,0]
["CPower","PGE",11,8,0]
["CPower","PGE",11,9,0]
["CPower","PGE",11,10,0]
["CPower","PGE",11,11,0]
["CPower","PGE",11,12,0]
["CPower","PGE",11,13,0]
["CPower","PGE",11,14,0]
["CPower","PGE",11,15,0]
["CPower","PGE",11,16,0]
["CPower","PGE",11,17,0]
["CPower","PGE",11,18,0]
["CPower","PGE",11,19,0]
["CPower","PGE",11,20,0]
["CPower","PGE",11,21,0]
["CPower","PGE",11,22,0]
["CPower","PGE",11,23,0]
["CPower","PGE",11,24,0]
["CPower","PGE",12,1,0]
["CPower","PGE",12,2,0]
["CPower","PGE",12,3,0]
["CPower","PGE",12,4,0]
["CPower","PGE",12,5,0]
["CPower","PGE",12,6,0]
["CPower","PGE",12,7,0]
["CPower","PGE",12,8,0]
["CPower","PGE",12,9,0]
["CPower","PGE",12,10,0]
["CPower","PGE",12,11,0]
["CPower","PGE",12,12,0]
["CPower","PGE",12,13,0]
["CPower","PGE",12,14,0]
["CPower","PGE",12,15,0]
["CPower","PGE",12,16,0]
["CPower","PGE",12,17,0]
["CPower","PGE",12,18,0]
["CPower","PGE",12,19,0]
["CPower","PGE",12,20,0]
["CPower","PGE",12,21,0]
["CPower","PGE",12,22,0]
["CPower","PGE",12,23,0]
["CPower","PGE",12,24,0]
["CPower","SCE",1,1,0]
["CPower","SCE",1,2,0]
["CPower","SCE",1,3,0]
["CPower","SCE",1,4,0]
["CPower","SCE",1,5,0]
["CPower","SCE",1,6,0]
["CPower","SCE",1,7,0]
["CPower","SCE",1,8,0]
["CPower","SCE",1,9,0]
["CPower","SCE",1,10,0]
["CPower","SCE",1,11,0]
["CPower","SCE",1,12,0]
["CPower","SCE",1,13,0]
["CPower","SCE",1,14,0]
["CPower","SCE",1,15,0]
["CPower","SCE",1,16,0]
["CPower","SCE",1,17,0]
["CPower","SCE",1,18,0]
["CPower","SCE",1,19,0]
["CPower","SCE",1,20,0]
["CPower","SCE",1,21,0]
["CPower","SCE",1,22,0]
["CPower","SCE",1,23,0]
["CPower","SCE",1,24,0]
["CPower","SCE",2,1,0]
["CPower","SCE",2,2,0]
["CPower","SCE",2,3,0]
["CPower","SCE",2,4,0]
["CPower","SCE",2,5,0]
["CPower","SCE",2,6,0]
["CPower","SCE",2,7,0]
["CPower","SCE",2,8,0]
["CPower","SCE",2,9,0]
["CPower","SCE",2,10,0]
["CPower","SCE",2,11,0]
["CPower","SCE",2,12,0]
["CPower","SCE",2,13,0]
["CPower","SCE",2,14,0]
["CPower","SCE",2,15,0]
["CPower","SCE",2,16,0]
["CPower","SCE",2,17,0]
["CPower","SCE",2,18,0]
["CPower","SCE",2,19,0]
["CPower","SCE",2,20,0]
["CPower","SCE",2,21,0]
["CPower","SCE",2,22,0]
["CPower","SCE",2,23,0]
["CPower","SCE",2,24,0]
["CPower","SCE",3,1,0]
["CPower","SCE",3,2,0]
["CPower","SCE",3,3,0]
["CPower","SCE",3,4,0]
["CPower","SCE",3,5,0]
["CPower","SCE",3,6,0]
["CPower","SCE",3,7,0]
["CPower","SCE",3,8,0]
["CPower","SCE",3,9,0]
["CPower","SCE",3,10,0]
["CPower","SCE",3,11,0]
["CPower","SCE",3,12,0]
["CPower","SCE",3,13,0]
["CPower","SCE",3,14,0]
["CPower","SCE",3,15,0]
["CPower","SCE",3,16,0]
["CPower","SCE",3,17,0]
["CPower","SCE",3,18,0]
["CPower","SCE",3,19,0]
["CPower","SCE",3,20,0]
["CPower","SCE",3,21,0]
["CPower","SCE",3,22,0]
["CPower","SCE",3,23,0]
["CPower","SCE",3,24,0]
["CPower","SCE",4,1,0]
["CPower","SCE",4,2,0]
["CPower","SCE",4,3,0]
["CPower","SCE",4,4,0]
["CPower","SCE",4,5,0]
["CPower","SCE",4,6,0]
["CPower","SCE",4,7,0]
["CPower","SCE",4,8,0]
["CPower","SCE",4,9,0]
["CPower","SCE",4,10,0]
["CPower","SCE",4,11,0]
["CPower","SCE",4,12,0]
["CPower","SCE",4,13,0]
["CPower","SCE",4,14,0]
["CPower","SCE",4,15,0]
["CPower","SCE",4,16,0]
["CPower","SCE",4,17,0]
["CPower","SCE",4,18,0]
["CPower","SCE",4,19,0]
["CPower","SCE",4,20,0]
["CPower","SCE",4,21,0]
["CPower","SCE",4,22,0]
["CPower","SCE",4,23,0]
["CPower","SCE",4,24,0]
["CPower","SCE",5,1,0]
["CPower","SCE",5,2,0]
["CPower","SCE",5,3,0]
["CPower","SCE",5,4,0]
["CPower","SCE",5,5,0]
["CPower","SCE",5,6,0]
["CPower","SCE",5,7,0]
["CPower","SCE",5,8,0]
["CPower","SCE",5,9,0]
["CPower","SCE",5,10,0]
["CPower","SCE",5,11,0]
["CPower","SCE",5,12,0]
["CPower","SCE",5,13,0]
["CPower","SCE",5,14,0]
["CPower","SCE",5,15,0]
["CPower","SCE",5,16,0]
["CPower","SCE",5,17,0]
["CPower","SCE",5,18,1.6187459697303037]
["CPower","SCE",5,19,1.0810605773242803]
["CPower","SCE",5,20,1.0298524447141826]
["CPower","SCE",5,21,1.0070932746652506]
["CPower","SCE",5,22,0.26324773356598263]
["CPower","SCE",5,23,0]
["CPower","SCE",5,24,0]
["CPower","SCE",6,1,0]
["CPower","SCE",6,2,0]
["CPower","SCE",6,3,0]
["CPower","SCE",6,4,0]
["CPower","SCE",6,5,0]
["CPower","SCE",6,6,0]
["CPower","SCE",6,7,0]
["CPower","SCE",6,8,0]
["CPower","SCE",6,9,0]
["CPower","SCE",6,10,0]
["CPower","SCE",6,11,0]
["CPower","SCE",6,12,0]
["CPower","SCE",6,13,0]
["CPower","SCE",6,14,0]
["CPower","SCE",6,15,0]
["CPower","SCE",6,16,0]
["CPower","SCE",6,17,1.4524922118380061]
["CPower","SCE",6,18,1.0519581664441477]
["CPower","SCE",6,19,0.97963951935914562]
["CPower","SCE",6,20,0.91121495327102797]
["CPower","SCE",6,21,0.60469514908767241]
["CPower","SCE",6,22,0]
["CPower","SCE",6,23,0]
["CPower","SCE",6,24,0]
["CPower","SCE",7,1,0]
["CPower","SCE",7,2,0]
["CPower","SCE",7,3,0]
["CPower","SCE",7,4,0]
["CPower","SCE",7,5,0]
["CPower","SCE",7,6,0]
["CPower","SCE",7,7,0]
["CPower","SCE",7,8,0]
["CPower","SCE",7,9,0]
["CPower","SCE",7,10,0]
["CPower","SCE",7,11,0]
["CPower","SCE",7,12,0]
["CPower","SCE",7,13,0]
["CPower","SCE",7,14,0]
["CPower","SCE",7,15,0]
["CPower","SCE",7,16,0]
["CPower","SCE",7,17,1.1861413043478262]
["CPower","SCE",7,18,0.99728260869565222]
["CPower","SCE",7,19,1.2235054347826089]
["CPower","SCE",7,20,0.90149456521739135]
["CPower","SCE",7,21,0.69157608695652173]
["CPower","SCE",7,22,0]
["CPower","SCE",7,23,0]
["CPower","SCE",7,24,0]
["CPower","SCE",8,1,0]
["CPower","SCE",8,2,0]
["CPower","SCE",8,3,0]
["CPower","SCE",8,4,0]
["CPower","SCE",8,5,0]
["CPower","SCE",8,6,0]
["CPower","SCE",8,7,0]
["CPower","SCE",8,8,0]
["CPower","SCE",8,9,0]
["CPower","SCE",8,10,0]
["CPower","SCE",8,11,0]
["CPower","SCE",8,12,0]
["CPower","SCE",8,13,0]
["CPower","SCE",8,14,0]
["CPower","SCE",8,15,0]
["CPower","SCE",8,16,0]
["CPower","SCE",8,17,1.4544908638586254]
["CPower","SCE",8,18,1.039718624002745]
["CPower","SCE",8,19,0.99596808784421376]
["CPower","SCE",8,20,0.81410311400875002]
["CPower","SCE",8,21,0.69571931028566525]
["CPower","SCE",8,22,0]
["CPower","SCE",8,23,0]
["CPower","SCE",8,24,0]
["CPower","SCE",9,1,0]
["CPower","SCE",9,2,0]
["CPower","SCE",9,3,0]
["CPower","SCE",9,4,0]
["CPower","SCE",9,5,0]
["CPower","SCE",9,6,0]
["CPower","SCE",9,7,0]
["CPower","SCE",9,8,0]
["CPower","SCE",9,9,0]
["CPower","SCE",9,10,0]
["CPower","SCE",9,11,0]
["CPower","SCE",9,12,0]
["CPower","SCE",9,13,0]
["CPower","SCE",9,14,0]
["CPower","SCE",9,15,0]
["CPower","SCE",9,16,0]
["CPower","SCE",9,17,0.91721496612000386]
["CPower","SCE",9,18,1.0375135028969851]
["CPower","SCE",9,19,1.111165668270647]
["CPower","SCE",9,20,0.98644800157124624]
["CPower","SCE",9,21,0.9476578611411175]
["CPower","SCE",9,22,0]
["CPower","SCE",9,23,0]
["CPower","SCE",9,24,0]
["CPower","SCE",10,1,0]
["CPower","SCE",10,2,0]
["CPower","SCE",10,3,0]
["CPower","SCE",10,4,0]
["CPower","SCE",10,5,0]
["CPower","SCE",10,6,0]
["CPower","SCE",10,7,0]
["CPower","SCE",10,8,0]
["CPower","SCE",10,9,0]
["CPower","SCE",10,10,0]
["CPower","SCE",10,11,0]
["CPower","SCE",10,12,0]
["CPower","SCE",10,13,0]
["CPower","SCE",10,14,0]
["CPower","SCE",10,15,0]
["CPower","SCE",10,16,0]
["CPower","SCE",10,17,1.2833744095296773]
["CPower","SCE",10,18,1.1802988293284042]
["CPower","SCE",10,19,0.96272335181762159]
["CPower","SCE",10,20,0.85104744300677748]
["CPower","SCE",10,21,0.72255596631751884]
["CPower","SCE",10,22,0]
["CPower","SCE",10,23,0]
["CPower","SCE",10,24,0]
["CPower","SCE",11,1,0]
["CPower","SCE",11,2,0]
["CPower","SCE",11,3,0]
["CPower","SCE",11,4,0]
["CPower","SCE",11,5,0]
["CPower","SCE",11,6,0]
["CPower","SCE",11,7,0]
["CPower","SCE",11,8,0]
["CPower","SCE",11,9,0]
["CPower","SCE",11,10,0]
["CPower","SCE",11,11,0]
["CPower","SCE",11,12,0]
["CPower","SCE",11,13,0]
["CPower","SCE",11,14,0]
["CPower","SCE",11,15,0]
["CPower","SCE",11,16,0]
["CPower","SCE",11,17,0]
["CPower","SCE",11,18,0]
["CPower","SCE",11,19,0]
["CPower","SCE",11,20,0]
["CPower","SCE",11,21,0]
["CPower","SCE",11,22,0]
["CPower","SCE",11,23,0]
["CPower","SCE",11,24,0]
["CPower","SCE",12,1,0]
["CPower","SCE",12,2,0]
["CPower","SCE",12,3,0]
["CPower","SCE",12,4,0]
["CPower","SCE",12,5,0]
["CPower","SCE",12,6,0]
["CPower","SCE",12,7,0]
["CPower","SCE",12,8,0]
["CPower","SCE",12,9,0]
["CPower","SCE",12,10,0]
["CPower","SCE",12,11,0]
["CPower","SCE",12,12,0]
["CPower","SCE",12,13,0]
["CPower","SCE",12,14,0]
["CPower","SCE",12,15,0]
["CPower","SCE",12,16,0]
["CPower","SCE",12,17,0]
["CPower","SCE",12,18,0]
["CPower","SCE",12,19,0]
["CPower","SCE",12,20,0]
["CPower","SCE",12,21,0]
["CPower","SCE",12,22,0]
["CPower","SCE",12,23,0]
["CPower","SCE",12,24,0]
["CPower","SDGE",1,1,0]
["CPower","SDGE",1,2,0]
["CPower","SDGE",1,3,0]
["CPower","SDGE",1,4,0]
["CPower","SDGE",1,5,0]
["CPower","SDGE",1,6,0]
["CPower","SDGE",1,7,0]
["CPower","SDGE",1,8,0]
["CPower","SDGE",1,9,0]
["CPower","SDGE",1,10,0]
["CPower","SDGE",1,11,0]
["CPower","SDGE",1,12,0]
["CPower","SDGE",1,13,0]
["CPower","SDGE",1,14,0]
["CPower","SDGE",1,15,0]
["CPower","SDGE",1,16,0]
["CPower","SDGE",1,17,0]
["CPower","SDGE",1,18,0]
["CPower","SDGE",1,19,0]
["CPower","SDGE",1,20,0]
["CPower","SDGE",1,21,0]
["CPower","SDGE",1,22,0]
["CPower","SDGE",1,23,0]
["CPower","SDGE",1,24,0]
["CPower","SDGE",2,1,0]
["CPower","SDGE",2,2,0]
["CPower","SDGE",2,3,0]
["CPower","SDGE",2,4,0]
["CPower","SDGE",2,5,0]
["CPower","SDGE",2,6,0]
["CPower","SDGE",2,7,0]
["CPower","SDGE",2,8,0]
["CPower","SDGE",2,9,0]
["CPower","SDGE",2,10,0]
["CPower","SDGE",2,11,0]
["CPower","SDGE",2,12,0]
["CPower","SDGE",2,13,0]
["CPower","SDGE",2,14,0]
["CPower","SDGE",2,15,0]
["CPower","SDGE",2,16,0]
["CPower","SDGE",2,17,0]
["CPower","SDGE",2,18,0]
["CPower","SDGE",2,19,0]
["CPower","SDGE",2,20,0]
["CPower","SDGE",2,21,0]
["CPower","SDGE",2,22,0]
["CPower","SDGE",2,23,0]
["CPower","SDGE",2,24,0]
["CPower","SDGE",3,1,0]
["CPower","SDGE",3,2,0]
["CPower","SDGE",3,3,0]
["CPower","SDGE",3,4,0]
["CPower","SDGE",3,5,0]
["CPower","SDGE",3,6,0]
["CPower","SDGE",3,7,0]
["CPower","SDGE",3,8,0]
["CPower","SDGE",3,9,0]
["CPower","SDGE",3,10,0]
["CPower","SDGE",3,11,0]
["CPower","SDGE",3,12,0]
["CPower","SDGE",3,13,0]
["CPower","SDGE",3,14,0]
["CPower","SDGE",3,15,0]
["CPower","SDGE",3,16,0]
["CPower","SDGE",3,17,0]
["CPower","SDGE",3,18,0]
["CPower","SDGE",3,19,0]
["CPower","SDGE",3,20,0]
["CPower","SDGE",3,21,0]
["CPower","SDGE",3,22,0]
["CPower","SDGE",3,23,0]
["CPower","SDGE",3,24,0]
["CPower","SDGE",4,1,0]
["CPower","SDGE",4,2,0]
["CPower","SDGE",4,3,0]
["CPower","SDGE",4,4,0]
["CPower","SDGE",4,5,0]
["CPower","SDGE",4,6,0]
["CPower","SDGE",4,7,0]
["CPower","SDGE",4,8,0]
["CPower","SDGE",4,9,0]
["CPower","SDGE",4,10,0]
["CPower","SDGE",4,11,0]
["CPower","SDGE",4,12,0]
["CPower","SDGE",4,13,0]
["CPower","SDGE",4,14,0]
["CPower","SDGE",4,15,0]
["CPower","SDGE",4,16,0]
["CPower","SDGE",4,17,0]
["CPower","SDGE",4,18,0]
["CPower","SDGE",4,19,0]
["CPower","SDGE",4,20,0]
["CPower","SDGE",4,21,0]
["CPower","SDGE",4,22,0]
["CPower","SDGE",4,23,0]
["CPower","SDGE",4,24,0]
["CPower","SDGE",5,1,0]
["CPower","SDGE",5,2,0]
["CPower","SDGE",5,3,0]
["CPower","SDGE",5,4,0]
["CPower","SDGE",5,5,0]
["CPower","SDGE",5,6,0]
["CPower","SDGE",5,7,0]
["CPower","SDGE",5,8,0]
["CPower","SDGE",5,9,0]
["CPower","SDGE",5,10,0]
["CPower","SDGE",5,11,0]
["CPower","SDGE",5,12,0]
["CPower","SDGE",5,13,0]
["CPower","SDGE",5,14,0]
["CPower","SDGE",5,15,0]
["CPower","SDGE",5,16,0]
["CPower","SDGE",5,17,0]
["CPower","SDGE",5,18,2.0667586530839914]
["CPower","SDGE",5,19,0.98332501541261774]
["CPower","SDGE",5,20,0.9912515045650705]
["CPower","SDGE",5,21,0.95866482693832022]
["CPower","SDGE",5,22,0]
["CPower","SDGE",5,23,0]
["CPower","SDGE",5,24,0]
["CPower","SDGE",6,1,0]
["CPower","SDGE",6,2,0]
["CPower","SDGE",6,3,0]
["CPower","SDGE",6,4,0]
["CPower","SDGE",6,5,0]
["CPower","SDGE",6,6,0]
["CPower","SDGE",6,7,0]
["CPower","SDGE",6,8,0]
["CPower","SDGE",6,9,0]
["CPower","SDGE",6,10,0]
["CPower","SDGE",6,11,0]
["CPower","SDGE",6,12,0]
["CPower","SDGE",6,13,0]
["CPower","SDGE",6,14,0]
["CPower","SDGE",6,15,0]
["CPower","SDGE",6,16,0]
["CPower","SDGE",6,17,2.1188463374447579]
["CPower","SDGE",6,18,1.0193868280439171]
["CPower","SDGE",6,19,0.80842610985355956]
["CPower","SDGE",6,20,0.70879721593446365]
["CPower","SDGE",6,21,0.34454350872330275]
["CPower","SDGE",6,22,0]
["CPower","SDGE",6,23,0]
["CPower","SDGE",6,24,0]
["CPower","SDGE",7,1,0]
["CPower","SDGE",7,2,0]
["CPower","SDGE",7,3,0]
["CPower","SDGE",7,4,0]
["CPower","SDGE",7,5,0]
["CPower","SDGE",7,6,0]
["CPower","SDGE",7,7,0]
["CPower","SDGE",7,8,0]
["CPower","SDGE",7,9,0]
["CPower","SDGE",7,10,0]
["CPower","SDGE",7,11,0]
["CPower","SDGE",7,12,0]
["CPower","SDGE",7,13,0]
["CPower","SDGE",7,14,0]
["CPower","SDGE",7,15,0]
["CPower","SDGE",7,16,0]
["CPower","SDGE",7,17,1.712594153931992]
["CPower","SDGE",7,18,0.90279284585102748]
["CPower","SDGE",7,19,1.1011747930938283]
["CPower","SDGE",7,20,0.79352778897120346]
["CPower","SDGE",7,21,0.48991041815194819]
["CPower","SDGE",7,22,0]
["CPower","SDGE",7,23,0]
["CPower","SDGE",7,24,0]
["CPower","SDGE",8,1,0]
["CPower","SDGE",8,2,0]
["CPower","SDGE",8,3,0]
["CPower","SDGE",8,4,0]
["CPower","SDGE",8,5,0]
["CPower","SDGE",8,6,0]
["CPower","SDGE",8,7,0]
["CPower","SDGE",8,8,0]
["CPower","SDGE",8,9,0]
["CPower","SDGE",8,10,0]
["CPower","SDGE",8,11,0]
["CPower","SDGE",8,12,0]
["CPower","SDGE",8,13,0]
["CPower","SDGE",8,14,0]
["CPower","SDGE",8,15,0]
["CPower","SDGE",8,16,0]
["CPower","SDGE",8,17,1.8187895534361351]
["CPower","SDGE",8,18,0.99607808182547442]
["CPower","SDGE",8,19,0.90159550762100005]
["CPower","SDGE",8,20,0.7139673767715482]
["CPower","SDGE",8,21,0.56956948034584187]
["CPower","SDGE",8,22,0]
["CPower","SDGE",8,23,0]
["CPower","SDGE",8,24,0]
["CPower","SDGE",9,1,0]
["CPower","SDGE",9,2,0]
["CPower","SDGE",9,3,0]
["CPower","SDGE",9,4,0]
["CPower","SDGE",9,5,0]
["CPower","SDGE",9,6,0]
["CPower","SDGE",9,7,0]
["CPower","SDGE",9,8,0]
["CPower","SDGE",9,9,0]
["CPower","SDGE",9,10,0]
["CPower","SDGE",9,11,0]
["CPower","SDGE",9,12,0]
["CPower","SDGE",9,13,0]
["CPower","SDGE",9,14,0]
["CPower","SDGE",9,15,0]
["CPower","SDGE",9,16,0]
["CPower","SDGE",9,17,1.1031706089582283]
["CPower","SDGE",9,18,1.0427780573729239]
["CPower","SDGE",9,19,1.1077000503271262]
["CPower","SDGE",9,20,0.95571212883744328]
["CPower","SDGE",9,21,0.79063915450427769]
["CPower","SDGE",9,22,0]
["CPower","SDGE",9,23,0]
["CPower","SDGE",9,24,0]
["CPower","SDGE",10,1,0]
["CPower","SDGE",10,2,0]
["CPower","SDGE",10,3,0]
["CPower","SDGE",10,4,0]
["CPower","SDGE",10,5,0]
["CPower","SDGE",10,6,0]
["CPower","SDGE",10,7,0]
["CPower","SDGE",10,8,0]
["CPower","SDGE",10,9,0]
["CPower","SDGE",10,10,0]
["CPower","SDGE",10,11,0]
["CPower","SDGE",10,12,0]
["CPower","SDGE",10,13,0]
["CPower","SDGE",10,14,0]
["CPower","SDGE",10,15,0]
["CPower","SDGE",10,16,0]
["CPower","SDGE",10,17,1.9548276317527407]
["CPower","SDGE",10,18,1.1468101968035926]
["CPower","SDGE",10,19,0.96965394267600036]
["CPower","SDGE",10,20,0.73702285035001969]
["CPower","SDGE",10,21,0.19168537841764627]
["CPower","SDGE",10,22,0]
["CPower","SDGE",10,23,0]
["CPower","SDGE",10,24,0]
["CPower","SDGE",11,1,0]
["CPower","SDGE",11,2,0]
["CPower","SDGE",11,3,0]
["CPower","SDGE",11,4,0]
["CPower","SDGE",11,5,0]
["CPower","SDGE",11,6,0]
["CPower","SDGE",11,7,0]
["CPower","SDGE",11,8,0]
["CPower","SDGE",11,9,0]
["CPower","SDGE",11,10,0]
["CPower","SDGE",11,11,0]
["CPower","SDGE",11,12,0]
["CPower","SDGE",11,13,0]
["CPower","SDGE",11,14,0]
["CPower","SDGE",11,15,0]
["CPower","SDGE",11,16,0]
["CPower","SDGE",11,17,0]
["CPower","SDGE",11,18,0]
["CPower","SDGE",11,19,0]
["CPower","SDGE",11,20,0]
["CPower","SDGE",11,21,0]
["CPower","SDGE",11,22,0]
["CPower","SDGE",11,23,0]
["CPower","SDGE",11,24,0]
["CPower","SDGE",12,1,0]
["CPower","SDGE",12,2,0]
["CPower","SDGE",12,3,0]
["CPower","SDGE",12,4,0]
["CPower","SDGE",12,5,0]
["CPower","SDGE",12,6,0]
["CPower","SDGE",12,7,0]
["CPower","SDGE",12,8,0]
["CPower","SDGE",12,9,0]
["CPower","SDGE",12,10,0]
["CPower","SDGE",12,11,0]
["CPower","SDGE",12,12,0]
["CPower","SDGE",12,13,0]
["CPower","SDGE",12,14,0]
["CPower","SDGE",12,15,0]
["CPower","SDGE",12,16,0]
["CPower","SDGE",12,17,0]
["CPower","SDGE",12,18,0]
["CPower","SDGE",12,19,0]
["CPower","SDGE",12,20,0]
["CPower","SDGE",12,21,0]
["CPower","SDGE",12,22,0]
["CPower","SDGE",12,23,0]
["CPower","SDGE",12,24,0]
["Voltus","SCE",1,1,0]
["Voltus","SCE",1,2,0]
["Voltus","SCE",1,3,0]
["Voltus","SCE",1,4,0]
["Voltus","SCE",1,5,0]
["Voltus","SCE",1,6,0]
["Voltus","SCE",1,7,0]
["Voltus","SCE",1,8,0]
["Voltus","SCE",1,9,0]
["Voltus","SCE",1,10,0]
["Voltus","SCE",1,11,0]
["Voltus","SCE",1,12,0]
["Voltus","SCE",1,13,0]
["Voltus","SCE",1,14,0]
["Voltus","SCE",1,15,0]
["Voltus","SCE",1,16,0]
["Voltus","SCE",1,17,1.1749561291193766]
["Voltus","SCE",1,18,1.1268951178477726]
["Voltus","SCE",1,19,0.94356783302640601]
["Voltus","SCE",1,20,0.91311121117470351]
["Voltus","SCE",1,21,0.84146970883174199]
["Voltus","SCE",1,22,0]
["Voltus","SCE",1,23,0]
["Voltus","SCE",1,24,0]
["Voltus","SCE",2,1,0]
["Voltus","SCE",2,2,0]
["Voltus","SCE",2,3,0]
["Voltus","SCE",2,4,0]
["Voltus","SCE",2,5,0]
["Voltus","SCE",2,6,0]
["Voltus","SCE",2,7,0]
["Voltus","SCE",2,8,0]
["Voltus","SCE",2,9,0]
["Voltus","SCE",2,10,0]
["Voltus","SCE",2,11,0]
["Voltus","SCE",2,12,0]
["Voltus","SCE",2,13,0]
["Voltus","SCE",2,14,0]
["Voltus","SCE",2,15,0]
["Voltus","SCE",2,16,0]
["Voltus","SCE",2,17,1.1749561291193766]
["Voltus","SCE",2,18,1.1268951178477726]
["Voltus","SCE",2,19,0.94356783302640601]
["Voltus","SCE",2,20,0.91311121117470351]
["Voltus","SCE",2,21,0.84146970883174199]
["Voltus","SCE",2,22,0]
["Voltus","SCE",2,23,0]
["Voltus","SCE",2,24,0]
["Voltus","SCE",3,1,0]
["Voltus","SCE",3,2,0]
["Voltus","SCE",3,3,0]
["Voltus","SCE",3,4,0]
["Voltus","SCE",3,5,0]
["Voltus","SCE",3,6,0]
["Voltus","SCE",3,7,0]
["Voltus","SCE",3,8,0]
["Voltus","SCE",3,9,0]
["Voltus","SCE",3,10,0]
["Voltus","SCE",3,11,0]
["Voltus","SCE",3,12,0]
["Voltus","SCE",3,13,0]
["Voltus","SCE",3,14,0]
["Voltus","SCE",3,15,0]
["Voltus","SCE",3,16,0]
["Voltus","SCE",3,17,0]
["Voltus","SCE",3,18,0.99308203086915836]
["Voltus","SCE",3,19,1.0707053410348244]
["Voltus","SCE",3,20,0.97307446836527678]
["Voltus","SCE",3,21,1.0042407297117069]
["Voltus","SCE",3,22,0.95889743001903371]
["Voltus","SCE",3,23,0]
["Voltus","SCE",3,24,0]
["Voltus","SCE",4,1,0]
["Voltus","SCE",4,2,0]
["Voltus","SCE",4,3,0]
["Voltus","SCE",4,4,0]
["Voltus","SCE",4,5,0]
["Voltus","SCE",4,6,0]
["Voltus","SCE",4,7,0]
["Voltus","SCE",4,8,0]
["Voltus","SCE",4,9,0]
["Voltus","SCE",4,10,0]
["Voltus","SCE",4,11,0]
["Voltus","SCE",4,12,0]
["Voltus","SCE",4,13,0]
["Voltus","SCE",4,14,0]
["Voltus","SCE",4,15,0]
["Voltus","SCE",4,16,0]
["Voltus","SCE",4,17,0]
["Voltus","SCE",4,18,0.99308203086915836]
["Voltus","SCE",4,19,1.0707053410348244]
["Voltus","SCE",4,20,0.97307446836527678]
["Voltus","SCE",4,21,1.0042407297117069]
["Voltus","SCE",4,22,0.95889743001903371]
["Voltus","SCE",4,23,0]
["Voltus","SCE",4,24,0]
["Voltus","SCE",5,1,0]
["Voltus","SCE",5,2,0]
["Voltus","SCE",5,3,0]
["Voltus","SCE",5,4,0]
["Voltus","SCE",5,5,0]
["Voltus","SCE",5,6,0]
["Voltus","SCE",5,7,0]
["Voltus","SCE",5,8,0]
["Voltus","SCE",5,9,0]
["Voltus","SCE",5,10,0]
["Voltus","SCE",5,11,0]
["Voltus","SCE",5,12,0]
["Voltus","SCE",5,13,0]
["Voltus","SCE",5,14,0]
["Voltus","SCE",5,15,0]
["Voltus","SCE",5,16,0]
["Voltus","SCE",5,17,0]
["Voltus","SCE",5,18,0.98748784352970465]
["Voltus","SCE",5,19,1.030662673336219]
["Voltus","SCE",5,20,0.99740479435116125]
["Voltus","SCE",5,21,1.0134956797148664]
["Voltus","SCE",5,22,0.97094900906804904]
["Voltus","SCE",5,23,0]
["Voltus","SCE",5,24,0]
["Voltus","SCE",6,1,0]
["Voltus","SCE",6,2,0]
["Voltus","SCE",6,3,0]
["Voltus","SCE",6,4,0]
["Voltus","SCE",6,5,0]
["Voltus","SCE",6,6,0]
["Voltus","SCE",6,7,0]
["Voltus","SCE",6,8,0]
["Voltus","SCE",6,9,0]
["Voltus","SCE",6,10,0]
["Voltus","SCE",6,11,0]
["Voltus","SCE",6,12,0]
["Voltus","SCE",6,13,0]
["Voltus","SCE",6,14,0]
["Voltus","SCE",6,15,0]
["Voltus","SCE",6,16,0]
["Voltus","SCE",6,17,0.98260199805405901]
["Voltus","SCE",6,18,1.024000010975626]
["Voltus","SCE",6,19,0.9952261620005739]
["Voltus","SCE",6,20,1.0196190533988907]
["Voltus","SCE",6,21,0.97855277557084985]
["Voltus","SCE",6,22,0]
["Voltus","SCE",6,23,0]
["Voltus","SCE",6,24,0]
["Voltus","SCE",7,1,0]
["Voltus","SCE",7,2,0]
["Voltus","SCE",7,3,0]
["Voltus","SCE",7,4,0]
["Voltus","SCE",7,5,0]
["Voltus","SCE",7,6,0]
["Voltus","SCE",7,7,0]
["Voltus","SCE",7,8,0]
["Voltus","SCE",7,9,0]
["Voltus","SCE",7,10,0]
["Voltus","SCE",7,11,0]
["Voltus","SCE",7,12,0]
["Voltus","SCE",7,13,0]
["Voltus","SCE",7,14,0]
["Voltus","SCE",7,15,0]
["Voltus","SCE",7,16,0]
["Voltus","SCE",7,17,1.1422221115359998]
["Voltus","SCE",7,18,1.1205508565196487]
["Voltus","SCE",7,19,0.9292441935740865]
["Voltus","SCE",7,20,0.93307404480940437]
["Voltus","SCE",7,21,0.8749087935608606]
["Voltus","SCE",7,22,0]
["Voltus","SCE",7,23,0]
["Voltus","SCE",7,24,0]
["Voltus","SCE",8,1,0]
["Voltus","SCE",8,2,0]
["Voltus","SCE",8,3,0]
["Voltus","SCE",8,4,0]
["Voltus","SCE",8,5,0]
["Voltus","SCE",8,6,0]
["Voltus","SCE",8,7,0]
["Voltus","SCE",8,8,0]
["Voltus","SCE",8,9,0]
["Voltus","SCE",8,10,0]
["Voltus","SCE",8,11,0]
["Voltus","SCE",8,12,0]
["Voltus","SCE",8,13,0]
["Voltus","SCE",8,14,0]
["Voltus","SCE",8,15,0]
["Voltus","SCE",8,16,0]
["Voltus","SCE",8,17,1.1093029660700771]
["Voltus","SCE",8,18,1.08146105386727]
["Voltus","SCE",8,19,0.94008127945586295]
["Voltus","SCE",8,20,0.9550080692691415]
["Voltus","SCE",8,21,0.91414663133764884]
["Voltus","SCE",8,22,0]
["Voltus","SCE",8,23,0]
["Voltus","SCE",8,24,0]
["Voltus","SCE",9,1,0]
["Voltus","SCE",9,2,0]
["Voltus","SCE",9,3,0]
["Voltus","SCE",9,4,0]
["Voltus","SCE",9,5,0]
["Voltus","SCE",9,6,0]
["Voltus","SCE",9,7,0]
["Voltus","SCE",9,8,0]
["Voltus","SCE",9,9,0]
["Voltus","SCE",9,10,0]
["Voltus","SCE",9,11,0]
["Voltus","SCE",9,12,0]
["Voltus","SCE",9,13,0]
["Voltus","SCE",9,14,0]
["Voltus","SCE",9,15,0]
["Voltus","SCE",9,16,0]
["Voltus","SCE",9,17,1.1356528855011032]
["Voltus","SCE",9,18,1.1014585338282841]
["Voltus","SCE",9,19,0.96580155347502128]
["Voltus","SCE",9,20,0.94286866164566541]
["Voltus","SCE",9,21,0.85421836554992581]
["Voltus","SCE",9,22,0]
["Voltus","SCE",9,23,0]
["Voltus","SCE",9,24,0]
["Voltus","SCE",10,1,0]
["Voltus","SCE",10,2,0]
["Voltus","SCE",10,3,0]
["Voltus","SCE",10,4,0]
["Voltus","SCE",10,5,0]
["Voltus","SCE",10,6,0]
["Voltus","SCE",10,7,0]
["Voltus","SCE",10,8,0]
["Voltus","SCE",10,9,0]
["Voltus","SCE",10,10,0]
["Voltus","SCE",10,11,0]
["Voltus","SCE",10,12,0]
["Voltus","SCE",10,13,0]
["Voltus","SCE",10,14,0]
["Voltus","SCE",10,15,0]
["Voltus","SCE",10,16,0]
["Voltus","SCE",10,17,1.1749561291193766]
["Voltus","SCE",10,18,1.1268951178477726]
["Voltus","SCE",10,19,0.94356783302640601]
["Voltus","SCE",10,20,0.91311121117470351]
["Voltus","SCE",10,21,0.84146970883174199]
["Voltus","SCE",10,22,0]
["Voltus","SCE",10,23,0]
["Voltus","SCE",10,24,0]
["Voltus","SCE",11,1,0]
["Voltus","SCE",11,2,0]
["Voltus","SCE",11,3,0]
["Voltus","SCE",11,4,0]
["Voltus","SCE",11,5,0]
["Voltus","SCE",11,6,0]
["Voltus","SCE",11,7,0]
["Voltus","SCE",11,8,0]
["Voltus","SCE",11,9,0]
["Voltus","SCE",11,10,0]
["Voltus","SCE",11,11,0]
["Voltus","SCE",11,12,0]
["Voltus","SCE",11,13,0]
["Voltus","SCE",11,14,0]
["Voltus","SCE",11,15,0]
["Voltus","SCE",11,16,0]
["Voltus","SCE",11,17,1.1749561291193766]
["Voltus","SCE",11,18,1.1268951178477726]
["Voltus","SCE",11,19,0.94356783302640601]
["Voltus","SCE",11,20,0.91311121117470351]
["Voltus","SCE",11,21,0.84146970883174199]
["Voltus","SCE",11,22,0]
["Voltus","SCE",11,23,0]
["Voltus","SCE",11,24,0]
["Voltus","SCE",12,1,0]
["Voltus","SCE",12,2,0]
["Voltus","SCE",12,3,0]
["Voltus","SCE",12,4,0]
["Voltus","SCE",12,5,0]
["Voltus","SCE",12,6,0]
["Voltus","SCE",12,7,0]
["Voltus","SCE",12,8,0]
["Voltus","SCE",12,9,0]
["Voltus","SCE",12,10,0]
["Voltus","SCE",12,11,0]
["Voltus","SCE",12,12,0]
["Voltus","SCE",12,13,0]
["Voltus","SCE",12,14,0]
["Voltus","SCE",12,15,0]
["Voltus","SCE",12,16,0]
["Voltus","SCE",12,17,1.1749561291193766]
["Voltus","SCE",12,18,1.1268951178477726]
["Voltus","SCE",12,19,0.94356783302640601]
["Voltus","SCE",12,20,0.91311121117470351]
["Voltus","SCE",12,21,0.84146970883174199]
["Voltus","SCE",12,22,0]
["Voltus","SCE",12,23,0]
["Voltus","SCE",12,24,0]

{"sheet":"Regions","index":24,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":true,"merged":[]}
["Path 26 Designation","Balancing Authority Area","Region"]
["North","CISO","Norcal"]
["South","CISO","Socal"]
[null,"CISO"]
["South","IID","Socal"]
[null,"IID","Socal"]
["South","SRP","AZ"]
[null,"SRP","AZ"]
["South","AZPS","AZ"]
[null,"AZPS","AZ"]
["South","PNM","NM"]
[null,"PNM","NM"]
["South","WALC","AZ"]
[null,"WALC","AZ"]
["North","BPAT","WA/OR"]
[null,"BPAT","WA/OR"]
["South","LADWP","Socal"]
[null,"LADWP","Socal"]
["North","PGE","PGE"]
["South","SCE","SCE"]
["South","SDGE","SDGE"]

{"sheet":"Expanded Default Profiles","index":25,"n_rows":55,"n_cols":26,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["Profile Category","Region","MW HE 1","MW HE 2","MW HE 3","MW HE 4","MW HE 5","MW HE 6","MW HE 7","MW HE 8","MW HE 9","MW HE 10","MW HE 11","MW HE 12","MW HE 13","MW HE 14","MW HE 15","MW HE 16","MW HE 17","MW HE 18","MW HE 19","MW HE 20","MW HE 21","MW HE 22","MW HE 23","MW HE 24"]
["Battery Storage","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","AZ",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","NM",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","Norcal",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","Socal",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["Battery Storage","WA/OR",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,0,0,0]
["CAM Peaker","",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","AZ",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","NM",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","Norcal",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","Socal",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CAM Peaker","WA/OR",0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0]
["CPower","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CPower","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CPower","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Enersponse","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0]
["Enersponse","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0]
["Enersponse","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0]
["Leapfrog","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0.85580000000000001,1.1153,1.1877,1.0288999999999999,0.81230000000000002,0,0,0]
["Leapfrog","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0.82979999999999998,0.96899999999999997,1.0806,1.0541,1.0666,0,0,0]
["Leapfrog","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.5384,1.5423,0.88800000000000001,0.41460000000000002,0.61670000000000003,0,0,0]
["NexusRenewables","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0]
["Nostromo","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.5261,1.4774,0.75249999999999995,0.66459999999999997,0.57940000000000003,0,0,0]
["Nostromo","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.0283,1.0128999999999999,0.99750000000000005,0.98699999999999999,0.97440000000000004,0,0,0]
["OhmConnect","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.1442000000000001,1.0984,1.0297000000000001,0.98399999999999999,0.74370000000000003,0,0,0]
["OhmConnect","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.1442000000000001,1.0984,1.0297000000000001,0.98399999999999999,0.74370000000000003,0,0,0]
["OhmConnect","SDGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.1442000000000001,1.0984,1.0297000000000001,0.98399999999999999,0.74370000000000003,0,0,0]
["Other","",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","AZ",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","NM",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","Norcal",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","PGE",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","SCE",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","SDGE",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","Socal",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Other","WA/OR",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["Solar Fixed","Norcal",0,0,0,0,0,0,0,3.9E-2,0.22520000000000001,0.39240000000000003,0.48399999999999999,0.51700000000000002,0.49430000000000002,0.44669999999999999,0.4108,0.21179999999999999,2.5899999999999999E-2,0,0,0,0,0,0,0]
["Solar Fixed","Socal",0,0,0,0,0,0,3.0000000000000001E-3,0.1424,0.39979999999999999,0.53520000000000001,0.58989999999999998,0.621,0.60209999999999997,0.55300000000000005,0.45079999999999998,0.20169999999999999,1.24E-2,0,0,0,0,0,0,0]
["Solar Thermal","Socal",0,0,0,0,0,0,0,0,1.2999999999999999E-2,0.1081,0.17030000000000001,0.1807,0.1789,0.18529999999999999,0.183,0.13120000000000001,2.98E-2,0,0,0,0,0,0,0]
["Solar Tracking","Norcal",0,0,0,0,0,0,0,2.52E-2,0.18729999999999999,0.30659999999999998,0.36720000000000003,0.40200000000000002,0.39610000000000001,0.38159999999999999,0.32079999999999997,0.1709,2.01E-2,0,0,0,0,0,0,0]
["Solar Tracking","Socal",0,0,0,0,0,0,1.1000000000000001E-3,0.1323,0.41670000000000001,0.52229999999999999,0.51480000000000004,0.49519999999999997,0.51549999999999996,0.50729999999999997,0.46739999999999998,0.25540000000000002,2.1000000000000001E-2,0,0,0,0,0,0,0]
["Voltus","PGE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.175,1.1269,0.94359999999999999,0.91310000000000002,0.84150000000000003,0,0,0]
["Voltus","SCE",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,1.175,1.1269,0.94359999999999999,0.91310000000000002,0.84150000000000003,0,0,0]
["Wind","AZ",0.31119999999999998,0.30059999999999998,0.32240000000000002,0.29060000000000002,0.2606,0.27,0.2606,0.26,0.25059999999999999,0.26,0.26,0.22,0.1706,0.14000000000000001,0.15,0.13239999999999999,0.17,0.19,0.15060000000000001,0.16,0.17180000000000001,0.16059999999999999,0.22,0.26]
["Wind","NM",0.49070000000000003,0.51900000000000002,0.4556,0.43409999999999999,0.4536,0.48130000000000001,0.50960000000000005,0.49070000000000003,0.42730000000000001,0.42530000000000001,0.45300000000000001,0.44350000000000001,0.43409999999999999,0.46239999999999998,0.4718,0.48130000000000001,0.50149999999999995,0.52849999999999997,0.52849999999999997,0.50270000000000004,0.51900000000000002,0.55679999999999996,0.52259999999999995,0.49070000000000003]
["Wind","Norcal",5.4699999999999999E-2,5.45E-2,5.2499999999999998E-2,4.6600000000000003E-2,5.0799999999999998E-2,5.2299999999999999E-2,4.5600000000000002E-2,5.1999999999999998E-2,4.8800000000000003E-2,0.04,3.7900000000000003E-2,3.2099999999999997E-2,3.27E-2,3.1699999999999999E-2,3.4000000000000002E-2,3.5999999999999997E-2,3.3399999999999999E-2,3.4200000000000001E-2,4.2799999999999998E-2,5.1499999999999997E-2,5.91E-2,5.67E-2,5.2200000000000003E-2,0.06]
["Wind","Socal",3.73E-2,3.6200000000000003E-2,3.5499999999999997E-2,4.07E-2,3.9899999999999998E-2,4.0500000000000001E-2,4.02E-2,3.7400000000000003E-2,3.5099999999999999E-2,3.5000000000000003E-2,3.4700000000000002E-2,3.7900000000000003E-2,3.7699999999999997E-2,3.4799999999999998E-2,3.32E-2,3.4799999999999998E-2,3.85E-2,4.0599999999999997E-2,4.5900000000000003E-2,4.2999999999999997E-2,4.87E-2,4.3799999999999999E-2,4.1399999999999999E-2,4.1000000000000002E-2]
["Wind","WA/OR",0.31119999999999998,0.30059999999999998,0.32240000000000002,0.29060000000000002,0.2606,0.27,0.2606,0.26,0.25059999999999999,0.26,0.26,0.22,0.1706,0.14000000000000001,0.15,0.13239999999999999,0.17,0.19,0.15060000000000001,0.16,0.17180000000000001,0.16059999999999999,0.22,0.26]

{"sheet":"Resource Profile Categories","index":26,"n_rows":37,"n_cols":3,"rows_kept":37,"cut":false,"hidden":true,"merged":[]}
["Resource Type","Profile Category","Chart Category"]
["Battery Storage","Battery Storage","Battery Storage"]
["Biogas","Other","Biogas"]
["Biomass","Other","Biomass"]
["CAM Peaker","CAM Peaker","Thermal"]
["CCGT","Other","Thermal"]
["CHP","Other","CHP"]
["Coal","Other","Thermal"]
["Demand Response","Demand Response","Demand Response"]
["Fuel Cell","Other","Fuel Cell"]
["Geothermal","Other","Geothermal"]
["Hybrid_Solar1Axis","Solar Tracking","Solar"]
["Hybrid_SolarFixed","Solar Fixed","Solar"]
["Hybrid_Storage","Battery Storage","Battery Storage"]
["Hydro","Other","Hydro"]
["Nuclear","Other","Nuclear"]
["Paired_BattStorage","Battery Storage","Battery Storage"]
["Paired_Solar_1Axis","Solar Tracking","Solar"]
["Paired_Solar_Fixed","Solar Fixed","Solar"]
["Paired_Solar_Thermal","Solar Thermal","Solar"]
["Peaker","Other","Thermal"]
["Pump","Other","Pumped Hydro"]
["Pumped Hydro","Other","Pumped Hydro"]
["Reciprocating Engine","Other","Thermal"]
["Solar_1Axis","Solar Tracking","Solar"]
["Solar_2Axis","Solar Tracking","Solar"]
["Solar_Fixed","Solar Fixed","Solar"]
["Solar_Thermal","Solar Thermal","Solar"]
["Steam Turbine","Other","Thermal"]
["Wind","Wind","Wind"]
["Enersponse Demand Response","Enersponse","Demand Response"]
["Leapfrog Demand Response","Leapfrog","Demand Response"]
["OhmConnect Demand Response","OhmConnect","Demand Response"]
["Voltus Demand Response","Voltus","Demand Response"]
["NexusRenewables Demand Response","NexusRenewables","Demand Response"]
["Nostromo Demand Response","Nostromo","Demand Response"]
["CPower Demand Response","CPower","Demand Response"]

{"sheet":"VER Categories","index":27,"n_rows":5,"n_cols":1,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["Profile Category"]
["Solar Tracking"]
["Solar Fixed"]
["Solar Thermal"]
["Wind"]

{"sheet":"Query Statuses","index":28,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":true,"merged":[[13,6,18,8]]}
[]
[null,"Worksheet","Upstream Query Tables","Downstream Query Tables","Status",null,"Output Query Table","Worksheet","Status"]
[null,"README",null,null,"COMMITTED",null,"ExpandedResourceDefaultProfiles","Expanded Default Profiles","FRESH"]
[null,"Certification",null,null,"COMMITTED",null,"UnoptimizedShowing","Unoptimized Showing","FRESH"]
[null,"Certification Table",null,null,"COMMITTED",null,"StorageProperties","Profile Optimization","FRESH"]
[null,"LSE Showing",null,"UnoptimizedShowing,\nStorageProperties,\nSODProfilesForSOC,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED",null,"SODProfilesForSOC","Profile Optimization","FRESH"]
[null,"Resource Custom Profiles",null,"UnoptimizedShowing,\nStorageProperties,\nSODProfilesForSOC,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED",null,"LSEShowingComplete","LSE Showing Complete","FRESH"]
[null,"Unoptimized Showing","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing","LSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED",null,"CheckCapacity","Check Capacity","FRESH"]
[null,"Profile Optimization","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing","LSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED",null,"CheckCustomProfiles","Check Custom Profiles","FRESH"]
[null,"Validation Overview","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability",null,"COMMITTED",null,"CheckStorageSOC","Check Storage SOC","FRESH"]
[null,"Check Capacity","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity",null,"COMMITTED",null,"CheckGroupedResources","Check Grouped Resources","FRESH"]
[null,"Check Custom Profiles","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckCustomProfiles",null,"COMMITTED",null,"CheckHybridDeliverability","Check Hybrid Deliverability","FRESH"]
[null,"Check Storage SOC","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckStorageSOC","CheckCapacity","COMMITTED"]
[null,"Check Grouped Resources","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckGroupedResources",null,"COMMITTED",null,"This worksheet controls when and which query tables refresh upon opening certain worksheets. Each worksheet in the workbook is listed in the lefthand table, and each query table is listed in the righthand table. When any worksheet is opened, e.g., by clicking on a worksheet tab, a script loops through all query tables listed in the \"Upstream Query Tables\" column, refreshing and setting the corresponding \"Status\" column value in the left table to \"FRESH\" if previously \"STALE\". When any change occurs on a worksheet, a script loops through all query tables listed in the \"Downstream Query Tables\" column and sets the corresponding values in the \"Status\" column to \"STALE\". When a user navigates through the workbook without making changes, they should thus only experience one refresh for each query table, rather than repeatedly."]
[null,"Check Hybrid Deliverability","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckHybridDeliverability",null,"COMMITTED"]
[null,"Check Demand Response","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity",null,"COMMITTED"]
[null,"LSE Showing Complete","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nUnoptimizedShowing,\nLSEShowingComplete","CheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED"]
[null,"Hourly Availability Chart","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity",null,"COMMITTED"]
[null,"Hourly Availability","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nCheckStorageSOC,\nCheckCapacity",null,"COMMITTED"]
[null,"Local Availability Chart","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing",null,"COMMITTED"]
[null,"Local Availability","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing",null,"COMMITTED"]
[null,"Flex Availability Chart","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing",null,"COMMITTED"]
[null,"Flex Availability","ExpandedResourceDefaultProfiles,\nUnoptimizedShowing",null,"COMMITTED"]
[null,"Requirements and Allocations",null,"UnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","EDITED"]
[null,"Resource Database",null,"ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED"]
[null,"Resource Default Profiles",null,"ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED"]
[null,"Query Statuses",null,null,"COMMITTED"]
[null,"Resource Profile Categories",null,"ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED"]
[null,"Regions",null,"ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED"]
[null,"VER Categories",null,"ExpandedResourceDefaultProfiles,\nUnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","COMMITTED"]
[null,"Expanded Default Profiles","ExpandedResourceDefaultProfiles","UnoptimizedShowing,\nLSEShowingComplete,\nStorageProperties,\nSODProfilesForSOC,\nCheckStorageSOC,\nCheckCapacity,\nCheckCustomProfiles,\nCheckGroupedResources,\nCheckHybridDeliverability","EDITED"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,11]